{"text_format":"3","workbook":"xlsx","n_sheets":13,"sheets":["Lighting Project Tool","Input Tables","Table3","Lookups","Criteria","Deemed Savings","Measure List","Industry Std Cost","2025 Default Wattage Guide","S&G Interior Measures","S&G Exterior Measures","Ag Measures","Wattage Guide"],"not_rendered":{"images":1,"macros":1,"external_links":19,"defined_names":617,"comments":7},"read":"whole","date_system":"1900"}

{"sheet":"Lighting Project Tool","index":0,"n_rows":123,"n_cols":66,"rows_kept":123,"merged":[[1,1,2,14],[1,29,1,30],[2,17,2,20],[3,11,3,13],[3,17,3,20],[4,11,4,13],[4,17,5,20],[5,5,5,6],[5,11,7,13],[6,5,6,6],[6,17,7,20],[8,11,8,13],[8,17,9,20],[9,11,9,13],[10,11,11,13],[10,17,11,20],[12,11,13,13],[12,17,13,20],[14,11,15,13],[14,17,14,20],[16,41,16,65],[17,1,17,14],[49,5,49,6],[50,5,50,6],[51,5,51,6],[52,5,52,6],[53,5,53,6],[54,5,54,6],[55,5,55,6],[60,9,60,12],[61,5,61,6],[74,22,74,23],[74,24,74,25],[74,26,74,27],[77,16,78,16],[77,17,78,17],[77,18,77,19]]}
[]
[null,"2026 FOCUS ON ENERGY®  Lighting Savings Tool",{"$nulls":43},"CFL","HID","Linear Lamp","Linear Fixture","Data Validation Formula"]
[{"$nulls":28},"Measures","Sectors","Measure Tables",{"$nulls":14},"Fixture List Selection Formula"]
[{"$nulls":9},"Color Coding Legend:",null,"PLEASE READ",{"$nulls":16},"L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer","Schools & Gov - Interior",null,"1099:1134",{"$nulls":14},{"$f":"IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$9),C20=$AD$24),Table83[HIDSGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$9),C20=$AD$25),Table83[HIDSGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$7),C20=$AD$24),Table83[HIDSGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$7),C20=$AD$25),Table82[HIDSGEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$5),C20=$AD$24),Table83[HIDSGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$5),C20=$AD$25),Table82[HIDSGEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$3),C20=$AD$24),Table79[HIDAGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$3),C20=$AD$25),Table78[HIDAGEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$9),C20=$AD$24),Table83[HIDSGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$9),C20=$AD$25),Table82[HIDSGEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$7),C20=$AD$24),Table83[HIDSGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$7),C20=$AD$25),Table82[HIDSGEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$5),C20=$AD$24),Table83[HIDSGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$5),C20=$AD$25),Table82[HIDSGEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$3),C20=$AD$24),Table79[HIDAGINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$3),C20=$AD$25),Table78[HIDAGEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$10),C20=$AD$24),Table81[HIDSGNCINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$10),C20=$AD$25),Table80[HIDSGNCEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$8),C20=$AD$24),Table81[HIDSGNCINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$8),C20=$AD$25),Table80[HIDSGNCEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$6),C20=$AD$24),Table81[HIDSGNCINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$6),C20=$AD$25),Table80[HIDSGNCEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$4),C20=$AD$24),Table77[HIDAGNCINT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$4),C20=$AD$25),Table76[HIDAGNCEXT],\"ERROR\"))))))))))))))))))))))))","v":"ERROR"},{"$f":"IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$9),C20=$AD$24),Table84[FLSGINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$9),C20=$AD$25),Table85[FLSGEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$7),C20=$AD$24),Table86[FLSGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$7),C20=$AD$25),Table87[FLSGNCEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$5),C20=$AD$24),Table86[FLSGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$5),C20=$AD$25),Table87[FLSGNCEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$3),C20=$AD$24),Table88[FLAGINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$3),C20=$AD$25),Table89[FLAGEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$9),C20=$AD$24),Table86[FLSGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$9),C20=$AD$25),Table87[FLSGNCEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$7),C20=$AD$24),Table86[FLSGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$7),C20=$AD$25),Table87[FLSGNCEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$5),C20=$AD$24),Table86[FLSGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$5),C20=$AD$25),Table87[FLSGNCEXT],IF(AND(COUNTIF(D20,\"*HID\")=1,($F$9=Lookups!$B$3),C20=$AD$24),Table88[FLAGINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$3),C20=$AD$25),Table89[FLAGEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$10),C20=$AD$24),Table86[FLSGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$10),C20=$AD$25),Table87[FLSGNCEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$8),C20=$AD$24),Table86[FLSGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$8),C20=$AD$25),Table87[FLSGNCEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$6),C20=$AD$24),Table86[FLSGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$6),C20=$AD$25),Table87[FLSGNCEXT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$4),C20=$AD$24),Table91[FLAGNCINT],IF(AND(COUNTIF(D20,\"*Lamp\")=1,($F$9=Lookups!$B$4),C20=$AD$25),Table92[FLAGNCEXT],\"ERROR\"))))))))))))))))))))))))","v":"ERROR"},{"$f":"IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$9),C20=$AD$24),Table100[T8SGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$9),C20=$AD$25),Table100[T8SGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$7),C20=$AD$24),Table100[T8SGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$7),C20=$AD$25),Table99[T8SGEXT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$5),C20=$AD$24),Table100[T8SGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$5),C20=$AD$25),Table99[T8SGEXT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$3),C20=$AD$24),Table96[T8AGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$3),C20=$AD$25),Table95[T8AGEXT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$9),C20=$AD$24),Table100[T8SGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$9),C20=$AD$25),Table99[T8SGEXT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$7),C20=$AD$24),Table100[T8SGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$7),C20=$AD$25),Table99[T8SGEXT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$5),C20=$AD$24),Table100[T8SGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$5),C20=$AD$25),Table99[T8SGEXT],IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$3),C20=$AD$24),Table96[T8AGINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$3),C20=$AD$25),Table95[T8AGEXT],IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$10),C20=$AD$24),Table98[T8SGNCINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$10),C20=$AD$25),Table97[T8SGNCEXT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$8),C20=$AD$24),Table98[T8SGNCINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$8),C20=$AD$25),Table97[T8SGNCEXT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$6),C20=$AD$24),Table98[T8SGNCINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$6),C20=$AD$25),Table97[T8SGNCEXT],IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$4),C20=$AD$24),Table94[T8AGNCINT], IF(AND(COUNTIF(D20,\"*Fixture\")=1,($F$9=Lookups!$B$4),C20=$AD$25),Table2[T8AGNCEXT],\"ERROR\"))))))))))))))))))))))))","v":"ERROR"},{"$f":"IF(COUNTIF(D20,\"*CFL\")=1, $AT$5:$AT$28, IF(COUNTIF(D20,\"*HID\")=1,$AU$4:$AU$28,IF(COUNTIF(D20,\"*Lamp\")=1,$AV$4:$AV$28,IF(COUNTIF(D20,\"*Fixture\")=1,$AW$4:$AW$28,\"ERROR\"))))","v":"ERROR"}]
[{"$nulls":4},"Project Information",{"$nulls":4},"User Input (Required)",null,"THESE ARE ESTIMATES AND MAY NOT REFLECT ACTUAL SAVINGS",{"$nulls":16},"L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","Schools & Gov - NC - Interior",null,"1155:1168",null,null,0,{"$nulls":10},{"$f":"IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$9),C20=$AD$24),Table101[CFLSGINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$9),C20=$AD$25),Table69[CFLSGEXT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$7),C20=$AD$24),Table101[CFLSGINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$7),C20=$AD$25),Table69[CFLSGEXT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$5),C20=$AD$24),Table101[CFLSGINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$5),C20=$AD$25),Table69[CFLSGEXT],IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$3),C20=$AD$24),Table72[CFLAGINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$3),C20=$AD$25),Table73[CFLAGEXT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$9),C20=$AD$24),Table101[CFLSGINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$9),C20=$AD$25),Table69[CFLSGEXT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$7),C20=$AD$24),Table101[CFLSGINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$7),C20=$AD$25),Table69[CFLSGEXT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$5),C20=$AD$24),Table101[CFLSGINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$5),C20=$AD$25),Table69[CFLSGEXT],IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$3),C20=$AD$24),Table72[CFLAGINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$3),C20=$AD$25),Table73[CFLAGEXT],IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$10),C20=$AD$24),Table70[CFLSGNCINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$10),C20=$AD$25),Table71[CFLSGNCEXT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$8),C20=$AD$24),Table70[CFLSGNCINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$8),C20=$AD$25),Table71[CFLSGNCEXT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$6),C20=$AD$24),Table70[CFLSGNCINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$6),C20=$AD$25),Table71[CFLSGNCEXT],IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$4),C20=$AD$24),Table74[CFLAGNCINT], IF(AND(COUNTIF(D20,\"*CFL\")=1,($F$9=Lookups!$B$4),C20=$AD$25),Table75[CFLAGNCEXT],\"ERROR\"))))))))))))))))))))))))","v":"ERROR"}]
[{"$nulls":4},"Customer Name:",{"$nulls":4},"User Input (Optional)",null,"Contact your local Energy Advisor to learn about rebate opportunities for updating your lighting. Non 1 for 1 lighting replacement projects will either qualify for Wattage Reduction/Fixture Elimination or Custom measures. ",{"$nulls":16},"L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","Ag - Interior",null,"1181:1204",null,null,0]
[{"$nulls":4},"Facility Name:",{"$nulls":4},"Calc Output",{"$nulls":18},"L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","Ag - NC - Interior",null,"1216:1230",null,null,0]
[{"$nulls":8},"Project Totals",{"$nulls":19},"L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior","Schools & Gov - Exterior",null,"1142:1154",null,null,0]
[{"$nulls":4},"Sector:",null,"Used for Annual Run Hours & Controls Saving Fraction",null,"Annual kWh Savings",{"$f":"K45","v":0},null,"For L3903 and L3904 - Instead of Existing Quantity, Enter Proposed Installed Wattage",{"$nulls":16},"L10282: 4' LED Linear Ambient Fixture, Interior","Schools & Gov - NC - Exterior",null,"1168:1180",null,null,0]
[{"$nulls":4},"Annual Run Hours:","Default Sector Hours",null,null,"Rebate ",{"$f":"L45","v":0},null,"For (N)L4813, instead of fixture quantity, enter in total watts reduced for project. ",{"$nulls":16},"L10283: 8' LED Linear Ambient Fixture, Interior","Ag - Exterior",null,"1205:1215",null,null,0]
[{"$nulls":4},"Sector for Utility Rates:",{"$nulls":3},"Annual Utility Savings",{"$f":"M45","v":0},null,"For Flourescent T8, T12 Lamp replacement - Manually enter in Existing bulb wattage (L5451, L5452,L5453, L5454, L5456, L5458)",{"$nulls":16},"L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","Ag - NC - Exterior",null,"1231:1238",null,null,0]
[{"$nulls":4},"Interior or 24/7 (On-Peak) Utility Rate:",{"$f":"IFERROR(VLOOKUP(F11,L51:M53,2,FALSE),\"Select Sector for Utilty Rates\")","v":"Select Sector for Utilty Rates"},"Actual, if known.",null,"Payback (Years)",{"$f":"(G45-J10)/J11","v":{"$error":"#DIV/0!"}},{"$nulls":18},"L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture",{"$nulls":5},0]
[null,null,{"$f":"IF(AND(F9=\"Schools & Gov\",E20=\"Interior\"),Table5_1[Column1.1],IF(AND(F9=\"Schools & Gov\",E20=\"Exterior\"),Table7_1[Column1.1],IF(AND(F9=\"AG\",E20=\"Interior\"),'Ag Measures'!A2:A25:'Ag Measures'!A27:'Ag Measures'!A42:A49:'Ag Measures'!A67:A71,IF(AND(F9=\"AG\",E20=\"Exterior\"),'Ag Measures'!A28:A41:'Ag Measures'!A50:A66,\"\"))))","v":""},null,"Exterior (Off-Peak) Utility Rate:",{"$f":"M53","v":{"v":0.08,"d":"$0.0800"}},"Actual, if known.",{"$nulls":4},"Energy Savings are calculated for by using Existing and Proposed Wattages for fixtures/lamp types. Entering actual project values with give more accurate savings. ",{"$nulls":16},"L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID",{"$nulls":5},0]
[{"$nulls":28},"L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID","B&I",{"$nulls":4},0]
[{"$nulls":11},"Project Payback is calculated using estimated project costs, entering the actual project cost will give a more accurate payback. ",{"$nulls":16},"L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID","B&I-NC",{"$nulls":4},0]
[{"$nulls":28},"L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID"]
[null,null,"Last Updated: ",{"$f":"MAX($G$115:$G$132)","v":"2026-02-18"},{"$nulls":24},"L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID","Large Industrial",{"$nulls":4},0,{"$nulls":6},"Data Validation for Cell F"]
[null," LIGHTING PROJECT INFORMATION",{"$nulls":26},"L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID","Large Industrial-NC",null,null,"CFL Interior","HID Interior","Lamp Interior","Fixture Interior",{"$f":"IF(AND($F$9=$AD$19,C20=$AD$24), $AD$4, IF(AND($F$9=$AD$19,C20=$AD$25), $AD$8, IF(AND($F$9=$AD$20,C20=$AD$24), $AD$5, IF(AND($F$9=$AD$20,C20=$AD$25), $AD$9, IF(AND($F$9=$AD$21,C20=$AD$24), $AD$6, IF(AND($F$9=$AD$21,C20=$AD$25), $AD$10, IF(AND($F$9=$AD$22,C20=$AD$24), $AD$7, IF(AND($F$9=$AD$22,C20=$AD$25), $AD$11, \"ERROR\"))))))))","v":"ERROR"},{"$f":"IF($AK$18=$AD$4,$AD$8, IF($AK$18=$AD$5, $AD$9, IF($AK$18=$AD$6, $AD10, IF($AK$18=$AD$7, $AD$11, IF($AK$18=$AD$8,$AD$4, IF($AK$18=$AD$9, $AD$5, IF($AK$18=$AD$10, $AD6, IF($AK$18=$AD$11, $AD$7, \"ERROR\"))))))))","v":"ERROR"},null,"DV Interior",null,1,{"$f":"AP18+1","v":2},{"$f":"AQ18+1","v":3},4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25]
[null,"Line #","Interior or Exterior?","Existing Lighting Fixture/Lamp","Quantity","Proposed Lighting Technology","Project Cost (Default Industry Standard Cost) (Can be Overidden)","Exisiting Wattage\n(Can be overridden)","Proposed Wattage\n(Manual Entry)",{"$f":"IF(F10=\"Default Sector Hours\", \"Annual Run Hours (Sector Default)\", \"Annual Run Hours '(Manual Entry)\")","v":"Annual Run Hours (Sector Default)"},"Annual kWh Savings","Rebate","Annual Utility Savings","Project Payback (Years)","Measure Rebate Cap",{"$nulls":13},"L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12","Schools & Government",null,null,{"$f":"IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*CFL\")=0),Table101[CFLSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*CFL\")=0),Table70[CFLSGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*CFL\")=1),Table101[CFLSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*CFL\")=1),Table70[CFLSGNCINT],IF(AND($F$9=$AD$21,C20=$AD$24),Table72[CFLAGINT],IF(AND($F$9=$AD$22,C20=$AD$24),Table74[CFLAGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*CFL\")=0),Table101[CFLSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*CFL\")=0),Table70[CFLSGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*CFL\")=1),Table101[CFLSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*CFL\")=1),Table70[CFLSGNCINT],IF(AND($F$9=$AD$21,C20=$AD$25),Table72[CFLAGINT],IF(AND($F$9=$AD$22,C20=$AD$25),Table74[CFLAGNCINT],\"ERROR\"))))))))))))","v":"ERROR"},{"$f":"IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*HID\")=0),Table83[HIDSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*HID\")=0),Table81[HIDSGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*HID\")=1),Table83[HIDSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*HID\")=1),Table81[HIDSGNCINT],IF(AND($F$9=$AD$21,C20=$AD$24),Table79[HIDAGINT],IF(AND($F$9=$AD$22,C20=$AD$24),Table77[HIDAGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*HID\")=0),Table83[HIDSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*HID\")=0),Table81[HIDSGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*HID\")=1),Table83[HIDSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*HID\")=1),Table81[HIDSGNCINT],IF(AND($F$9=$AD$21,C20=$AD$25),Table79[HIDAGINT],IF(AND($F$9=$AD$22,C20=$AD$25),Table77[HIDAGNCINT],\"ERROR\"))))))))))))","v":"ERROR"},{"$f":"IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*LAMP\")=0),Table84[FLSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*LAMP\")=0),Table86[FLSGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*LAMP\")=1),Table84[FLSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*LAMP\")=1),Table86[FLSGNCINT],IF(AND($F$9=$AD$21,C20=$AD$24),Table88[FLAGINT],IF(AND($F$9=$AD$22,C20=$AD$24),Table91[FLAGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*LAMP\")=0),Table84[FLSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*LAMP\")=0),Table86[FLSGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*LAMP\")=1),Table84[FLSGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*LAMP\")=1),Table86[FLSGNCINT],IF(AND($F$9=$AD$21,C20=$AD$25),Table88[FLAGINT],IF(AND($F$9=$AD$22,C20=$AD$25),Table91[FLAGNCINT],\"ERROR\"))))))))))))","v":"ERROR"},{"$f":"IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*FIXTURE\")=0),Table100[T8SGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*FIXTURE\")=0),Table98[T8SGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*FIXTURE\")=1),Table100[T8SGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*FIXTURE\")=1),Table98[T8SGNCINT],IF(AND($F$9=$AD$21,C20=$AD$24),Table96[T8AGINT],IF(AND($F$9=$AD$22,C20=$AD$24),Table94[T8AGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*FIXTURE\")=0),Table100[T8SGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*FIXTURE\")=0),Table98[T8SGNCINT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*FIXTURE\")=1),Table100[T8SGINT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*FIXTURE\")=1),Table98[T8SGNCINT],IF(AND($F$9=$AD$21,C20=$AD$25),Table96[T8AGINT],IF(AND($F$9=$AD$22,C20=$AD$25),Table94[T8AGNCINT],\"ERROR\"))))))))))))","v":"ERROR"},{"$f":"IF($AK$18=$AD$4,$AC$4:$AC$31, IF($AK$18=$AD$5,$AC$4:$AC$30, IF( $AK$18=$AD$6,$AC$4:$AC$31, IF($AK$18=$AD$7, $AC$4:$AC$30,\"ERROR\"))))","v":"ERROR"},{"$f":"IF($AL$18=$AD$8,$AC$41:$AC$44,IF($AL$18=$AD$9,$AC$32:$AC$44,IF($AL$18=$AD$10,$AC$78:$AC$92,IF($AL$18=$AD$11,$AC$80:$AC$91,\"Error\"))))","v":"Error"},null,{"$f":"IF(COUNTIF(D20,\"*CFL\")=1,_xlfn.ANCHORARRAY( $AG$19), IF(COUNTIF(D20,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), IF(COUNTIF(D20,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),IF(COUNTIF(D20,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19), \"ERROR\"))))","v":"ERROR"},null,{"$f":"IF(C20=$AD$24, _xlfn.IFS(COUNTIF(D20,\"*CFL\")=1,_xlfn.ANCHORARRAY( $AG$19),COUNTIF(D20,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D20,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D20,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)), IF(C20=$AD$25, _xlfn.IFS(COUNTIF(D20,\"*CFL\")=1,_xlfn.ANCHORARRAY( $AG$41), COUNTIF(D20,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41), COUNTIF(D20,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D20,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C21=$AD$24, _xlfn.IFS(COUNTIF(D21,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D21,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D21,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D21,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C21=$AD$25,_xlfn.IFS(COUNTIF(D21,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D21,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D21,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D21,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C22=$AD$24, _xlfn.IFS(COUNTIF(D22,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D22,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D22,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D22,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C22=$AD$25,_xlfn.IFS(COUNTIF(D22,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D22,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D22,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D22,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C23=$AD$24, _xlfn.IFS(COUNTIF(D23,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D23,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D23,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D23,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C23=$AD$25,_xlfn.IFS(COUNTIF(D23,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D23,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D23,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D23,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C24=$AD$24, _xlfn.IFS(COUNTIF(D24,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D24,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D24,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D24,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C24=$AD$25,_xlfn.IFS(COUNTIF(D24,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D24,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D24,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D24,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C25=$AD$24, _xlfn.IFS(COUNTIF(D25,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D25,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D25,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D25,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C25=$AD$25,_xlfn.IFS(COUNTIF(D25,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D25,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D25,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D25,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C26=$AD$24, _xlfn.IFS(COUNTIF(D26,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D26,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D26,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D26,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C26=$AD$25,_xlfn.IFS(COUNTIF(D26,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D26,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D26,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D26,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C27=$AD$24, _xlfn.IFS(COUNTIF(D27,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D27,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D27,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D27,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C27=$AD$25,_xlfn.IFS(COUNTIF(D27,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D27,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D27,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D27,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C28=$AD$24, _xlfn.IFS(COUNTIF(D28,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D28,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D28,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D28,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C28=$AD$25,_xlfn.IFS(COUNTIF(D28,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D28,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D28,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D28,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C29=$AD$24, _xlfn.IFS(COUNTIF(D29,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D29,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D29,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D29,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C29=$AD$25,_xlfn.IFS(COUNTIF(D29,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D29,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D29,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D29,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C30=$AD$24, _xlfn.IFS(COUNTIF(D30,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D30,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D30,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D30,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C30=$AD$25,_xlfn.IFS(COUNTIF(D30,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D30,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D30,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D30,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C31=$AD$24, _xlfn.IFS(COUNTIF(D31,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D31,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D31,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D31,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C31=$AD$25,_xlfn.IFS(COUNTIF(D31,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D31,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D31,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D31,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C32=$AD$24, _xlfn.IFS(COUNTIF(D32,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D32,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D32,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D32,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C32=$AD$25,_xlfn.IFS(COUNTIF(D32,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D32,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D32,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D32,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C33=$AD$24, _xlfn.IFS(COUNTIF(D33,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D33,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D33,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D33,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C33=$AD$25,_xlfn.IFS(COUNTIF(D33,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D33,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D33,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D33,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C34=$AD$24, _xlfn.IFS(COUNTIF(D34,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D34,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D34,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D34,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C34=$AD$25,_xlfn.IFS(COUNTIF(D34,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D34,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D34,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D34,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C35=$AD$24, _xlfn.IFS(COUNTIF(D35,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D35,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D35,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D35,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C35=$AD$25,_xlfn.IFS(COUNTIF(D35,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D35,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D35,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D35,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C36=$AD$24, _xlfn.IFS(COUNTIF(D36,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D36,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D36,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D36,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C36=$AD$25,_xlfn.IFS(COUNTIF(D36,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D36,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D36,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D36,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C37=$AD$24, _xlfn.IFS(COUNTIF(D37,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D37,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D37,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D37,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C37=$AD$25,_xlfn.IFS(COUNTIF(D37,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D37,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D37,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D37,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C38=$AD$24, _xlfn.IFS(COUNTIF(D38,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D38,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D38,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D38,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C38=$AD$25,_xlfn.IFS(COUNTIF(D38,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D38,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D38,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D38,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C39=$AD$24, _xlfn.IFS(COUNTIF(D39,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D39,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D39,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D39,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C39=$AD$25,_xlfn.IFS(COUNTIF(D39,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D39,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D39,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D39,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C40=$AD$24, _xlfn.IFS(COUNTIF(D40,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D40,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D40,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D40,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C40=$AD$25,_xlfn.IFS(COUNTIF(D40,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D40,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D40,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D40,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C41=$AD$24, _xlfn.IFS(COUNTIF(D41,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D41,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D41,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D41,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C41=$AD$25,_xlfn.IFS(COUNTIF(D41,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D41,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D41,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D41,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C42=$AD$24, _xlfn.IFS(COUNTIF(D42,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D42,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D42,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D42,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C42=$AD$25,_xlfn.IFS(COUNTIF(D42,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D42,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D42,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D42,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C43=$AD$24, _xlfn.IFS(COUNTIF(D43,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D43,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D43,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D43,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C43=$AD$25,_xlfn.IFS(COUNTIF(D43,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D43,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D43,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D43,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"},{"$f":"IF(C44=$AD$24, _xlfn.IFS(COUNTIF(D44,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$19),COUNTIF(D44,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$19), COUNTIF(D44,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$19),COUNTIF(D44,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$19)),IF(C44=$AD$25,_xlfn.IFS(COUNTIF(D44,\"*CFL\")=1,_xlfn.ANCHORARRAY($AG$41),COUNTIF(D44,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41),COUNTIF(D44,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),COUNTIF(D44,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41)), \"ERROR\"))","v":"ERROR"}]
[null,1,{"$nulls":4},{"$f":"IF(ISBLANK(F20),\"\",E20*(_xlfn.XLOOKUP(F20,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F20),ISBLANK(E20)),\"\",_xlfn.XLOOKUP(D20,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,{"$f":"IF($F$10=\"Manual Input\", \"Manual Input\",IF(C20=\"Interior\", _xlfn.XLOOKUP($F$9,$W$52:$W$59,$X$52:$X$59, \"NOT FOUND\",0,1), IF(C20=\"Exterior\",$X$60,\"\")))","v":""},{"$f":"IF(ISBLANK(F20),\"\",IF(ISBLANK(I20),\"Enter Proposed Watts\",(E20*((H20-I20)*J20/1000))))","v":""},{"$f":"IF(ISBLANK(F20),\"\",IF(G20<=E20*IF(LEFT(F20,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F20,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F20,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F20,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F20,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F20,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F20,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F20,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G20, E20*IF(LEFT(F20,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F20,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F20,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F20,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F20,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F20,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F20,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F20,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},{"$f":"IF(ISBLANK(F20),\"\",IF(C20=$AD$24,K20*$F$12, K20*$F$13))","v":""},{"$f":"IF(ISBLANK(F20),\"\",IF(C20=$AD$24,(G20-L20)/(M20),IF(C20=$AD$25,(G20-L20)/M20,\"Enter in Estimated Cost\")))","v":""},{"$f":"IFERROR(IF(F20=VLOOKUP(F20, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":6},"",null,"",{"$nulls":4},"L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO","Schools & Government-NC"]
[null,2,{"$nulls":4},{"$f":"IF(ISBLANK(F21),\"\",E21*(_xlfn.XLOOKUP(F21,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F21),ISBLANK(E21)),\"\",_xlfn.XLOOKUP(D21,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"",{"$f":"IF(ISBLANK(F21),\"\",IF(ISBLANK(I21),\"Enter Proposed Watts\",(E21*((H21-I21)*J21/1000))))","v":""},{"$f":"IF(ISBLANK(F21),\"\",IF(G21<=E21*IF(LEFT(F21,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F21,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F21,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F21,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F21,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F21,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F21,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F21,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G21, E21*IF(LEFT(F21,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F21,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F21,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F21,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F21,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F21,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F21,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F21,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F21=VLOOKUP(F21, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO","Agribusiness",null,{"$f":"1141-1109","v":32}]
[null,3,{"$nulls":4},{"$f":"IF(ISBLANK(F22),\"\",E22*(_xlfn.XLOOKUP(F22,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F22),ISBLANK(E22)),\"\",_xlfn.XLOOKUP(D22,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F22),\"\",IF(G22<=E22*IF(LEFT(F22,6)=\"L4813:\",Criteria!$V$17,IF(LEFT(F22,6)=\"NL4813:\",Criteria!$Z$17,IF(LEFT(F22,6)=\"L3903:\",Criteria!$V$18,IF(LEFT(F22,6)=\"L3904:\",Criteria!$V$19, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F22,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F22,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F22,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F22,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G22, E22*IF(LEFT(F22,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F22,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F22,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F22,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F22,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F22,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F22,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F22,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F22=VLOOKUP(F22, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO","Agribusiness-NC",null,{"$f":"1168-1155","v":13}]
[null,4,{"$nulls":4},{"$f":"IF(ISBLANK(F23),\"\",E23*(_xlfn.XLOOKUP(F23,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F23),ISBLANK(E23)),\"\",_xlfn.XLOOKUP(D23,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F23),\"\",IF(G23<=E23*IF(LEFT(F23,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F23,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F23,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F23,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F23,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F23,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F23,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F23,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G23, E23*IF(LEFT(F23,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F23,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F23,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F23,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F23,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F23,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F23,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F23,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F23=VLOOKUP(F23, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO",null,null,{"$f":"1204-1181","v":23}]
[null,5,{"$nulls":4},{"$f":"IF(ISBLANK(F24),\"\",E24*(_xlfn.XLOOKUP(F24,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F24),ISBLANK(E24)),\"\",_xlfn.XLOOKUP(D24,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F24),\"\",IF(G24<=E24*IF(LEFT(F24,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F24,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F24,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F24,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F24,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F24,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F24,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F24,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G24, E24*IF(LEFT(F24,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F24,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F24,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F24,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F24,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F24,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F24,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F24,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F24=VLOOKUP(F24, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO","Interior",null,{"$f":"1230-1216","v":14}]
[null,6,{"$nulls":4},{"$f":"IF(ISBLANK(F25),\"\",E25*(_xlfn.XLOOKUP(F25,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F25),ISBLANK(E25)),\"\",_xlfn.XLOOKUP(D25,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F25),\"\",IF(G25<=E25*IF(LEFT(F25,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F25,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F25,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F25,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F25,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F25,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F25,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F25,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G25, E25*IF(LEFT(F25,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F25,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F25,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F25,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F25,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F25,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F25,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F25,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F25=VLOOKUP(F25, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":6},"",null,"",{"$nulls":4},"L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID","Exterior",null,{"$f":"1154-1142","v":12}]
[null,7,{"$nulls":4},{"$f":"IF(ISBLANK(F26),\"\",E26*(_xlfn.XLOOKUP(F26,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F26),ISBLANK(E26)),\"\",_xlfn.XLOOKUP(D26,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F26),\"\",IF(G26<=E26*IF(LEFT(F26,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F26,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F26,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F26,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F26,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F26,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F26,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F26,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G26, E26*IF(LEFT(F26,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F26,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F26,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F26,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F26,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F26,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F26,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F26,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F26=VLOOKUP(F26, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L10039: Four-pin base LED Lamp Replacing CFL",null,null,{"$f":"1180-1168","v":12}]
[null,8,{"$nulls":4},{"$f":"IF(ISBLANK(F27),\"\",E27*(_xlfn.XLOOKUP(F27,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F27),ISBLANK(E27)),\"\",_xlfn.XLOOKUP(D27,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F27),\"\",IF(G27<=E27*IF(LEFT(F27,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F27,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F27,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F27,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F27,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F27,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F27,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F27,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G27, E27*IF(LEFT(F27,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F27,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F27,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F27,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F27,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F27,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F27,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F27,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F27=VLOOKUP(F27, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp",null,null,{"$f":"1215-1205","v":10}]
[null,9,{"$nulls":4},{"$f":"IF(ISBLANK(F28),\"\",E28*(_xlfn.XLOOKUP(F28,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F28),ISBLANK(E28)),\"\",_xlfn.XLOOKUP(D28,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F28),\"\",IF(G28<=E28*IF(LEFT(F28,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F28,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F28,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F28,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F28,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F28,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F28,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F28,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G28, E28*IF(LEFT(F28,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F28,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F28,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F28,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F28,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F28,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F28,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F28,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F28=VLOOKUP(F28, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L5452: 4' TLED, replacing 4' T5HO Lamp",null,null,{"$f":"1238-1231","v":7}]
[null,10,{"$nulls":4},{"$f":"IF(ISBLANK(F29),\"\",E29*(_xlfn.XLOOKUP(F29,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F29),ISBLANK(E29)),\"\",_xlfn.XLOOKUP(D29,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F29),\"\",IF(G29<=E29*IF(LEFT(F29,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F29,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F29,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F29,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F29,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F29,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F29,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F29,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G29, E29*IF(LEFT(F29,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F29,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F29,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F29,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F29,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F29,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F29,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F29,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F29=VLOOKUP(F29, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L4797: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp"]
[null,11,{"$nulls":4},{"$f":"IF(ISBLANK(F30),\"\",E30*(_xlfn.XLOOKUP(F30,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F30),ISBLANK(E30)),\"\",_xlfn.XLOOKUP(D30,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F30),\"\",IF(G30<=E30*IF(LEFT(F30,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F30,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F30,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F30,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F30,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F30,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F30,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F30,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G30, E30*IF(LEFT(F30,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F30,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F30,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F30,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F30,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F30,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F30,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F30,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F30=VLOOKUP(F30, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L4809: 8' TLED, replacing 8' T8 or T12 Lamp"]
[null,12,{"$nulls":4},{"$f":"IF(ISBLANK(F31),\"\",E31*(_xlfn.XLOOKUP(F31,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F31),ISBLANK(E31)),\"\",_xlfn.XLOOKUP(D31,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F31),\"\",IF(G31<=E31*IF(LEFT(F31,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F31,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F31,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F31,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F31,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F31,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F31,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F31,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G31, E31*IF(LEFT(F31,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F31,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F31,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F31,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F31,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F31,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F31,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F31,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F31=VLOOKUP(F31, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":6},"",null,"",{"$nulls":4},"L3903: Interior LED Signage"]
[null,13,{"$nulls":4},{"$f":"IF(ISBLANK(F32),\"\",E32*(_xlfn.XLOOKUP(F32,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F32),ISBLANK(E32)),\"\",_xlfn.XLOOKUP(D32,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F32),\"\",IF(G32<=E32*IF(LEFT(F32,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F32,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F32,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F32,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F32,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F32,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F32,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F32,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G32, E32*IF(LEFT(F32,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F32,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F32,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F32,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F32,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F32,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F32,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F32,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F32=VLOOKUP(F32, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
[null,14,{"$nulls":4},{"$f":"IF(ISBLANK(F33),\"\",E33*(_xlfn.XLOOKUP(F33,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F33),ISBLANK(E33)),\"\",_xlfn.XLOOKUP(D33,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F33),\"\",IF(G33<=E33*IF(LEFT(F33,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F33,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F33,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F33,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F33,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F33,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F33,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F33,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G33, E33*IF(LEFT(F33,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F33,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F33,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F33,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F33,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F33,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F33,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F33,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F33=VLOOKUP(F33, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L10285: 4' LED Linear Ambient Fixture, Exterior"]
[null,15,{"$nulls":4},{"$f":"IF(ISBLANK(F34),\"\",E34*(_xlfn.XLOOKUP(F34,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F34),ISBLANK(E34)),\"\",_xlfn.XLOOKUP(D34,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F34),\"\",IF(G34<=E34*IF(LEFT(F34,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F34,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F34,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F34,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F34,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F34,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F34,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F34,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G34, E34*IF(LEFT(F34,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F34,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F34,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F34,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F34,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F34,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F34,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F34,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F34=VLOOKUP(F34, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L10286: 8' LED Linear Ambient Fixture, Exterior"]
[null,16,{"$nulls":4},{"$f":"IF(ISBLANK(F35),\"\",E35*(_xlfn.XLOOKUP(F35,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F35),ISBLANK(E35)),\"\",_xlfn.XLOOKUP(D35,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F35),\"\",IF(G35<=E35*IF(LEFT(F35,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F35,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F35,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F35,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F35,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F35,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F35,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F35,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G35, E35*IF(LEFT(F35,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F35,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F35,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F35,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F35,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F35,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F35,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F35,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F35=VLOOKUP(F35, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
[null,17,{"$nulls":4},{"$f":"IF(ISBLANK(F36),\"\",E36*(_xlfn.XLOOKUP(F36,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F36),ISBLANK(E36)),\"\",_xlfn.XLOOKUP(D36,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F36),\"\",IF(G36<=E36*IF(LEFT(F36,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F36,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F36,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F36,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F36,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F36,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F36,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F36,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G36, E36*IF(LEFT(F36,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F36,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F36,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F36,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F36,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F36,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F36,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F36,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F36=VLOOKUP(F36, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L3904: Exterior LED Signage"]
[null,18,{"$nulls":4},{"$f":"IF(ISBLANK(F37),\"\",E37*(_xlfn.XLOOKUP(F37,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F37),ISBLANK(E37)),\"\",_xlfn.XLOOKUP(D37,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F37),\"\",IF(G37<=E37*IF(LEFT(F37,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F37,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F37,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F37,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F37,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F37,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F37,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F37,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G37, E37*IF(LEFT(F37,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F37,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F37,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F37,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F37,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F37,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F37,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F37,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F37=VLOOKUP(F37, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
[null,19,{"$nulls":4},{"$f":"IF(ISBLANK(F38),\"\",E38*(_xlfn.XLOOKUP(F38,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F38),ISBLANK(E38)),\"\",_xlfn.XLOOKUP(D38,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F38),\"\",IF(G38<=E38*IF(LEFT(F38,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F38,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F38,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F38,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F38,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F38,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F38,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F38,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G38, E38*IF(LEFT(F38,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F38,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F38,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F38,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F38,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F38,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F38,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F38,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F38=VLOOKUP(F38, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":6},"",null,"",{"$nulls":4},"L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
[null,20,{"$nulls":4},{"$f":"IF(ISBLANK(F39),\"\",E39*(_xlfn.XLOOKUP(F39,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F39),ISBLANK(E39)),\"\",_xlfn.XLOOKUP(D39,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F39),\"\",IF(G39<=E39*IF(LEFT(F39,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F39,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F39,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F39,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F39,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F39,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F39,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F39,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G39, E39*IF(LEFT(F39,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F39,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F39,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F39,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F39,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F39,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F39,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F39,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F39=VLOOKUP(F39, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
[null,21,{"$nulls":4},{"$f":"IF(ISBLANK(F40),\"\",E40*(_xlfn.XLOOKUP(F40,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F40),ISBLANK(E40)),\"\",_xlfn.XLOOKUP(D40,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F40),\"\",IF(G40<=E40*IF(LEFT(F40,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F40,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F40,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F40,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F40,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F40,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F40,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F40,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G40, E40*IF(LEFT(F40,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F40,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F40,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F40,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F40,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F40,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F40,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F40,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F40=VLOOKUP(F40, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",{"$nulls":3},"CFL Exterior","HID Exterior","Lamp Exterior","Fixture Exterior",{"$nulls":3},"DV Exterior"]
[null,22,{"$nulls":4},{"$f":"IF(ISBLANK(F41),\"\",E41*(_xlfn.XLOOKUP(F41,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F41),ISBLANK(E41)),\"\",_xlfn.XLOOKUP(D41,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F41),\"\",IF(G41<=E41*IF(LEFT(F41,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F41,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F41,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F41,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F41,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F41,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F41,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F41,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G41, E41*IF(LEFT(F41,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F41,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F41,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F41,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F41,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F41,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F41,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F41,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F41=VLOOKUP(F41, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior",{"$nulls":3},{"$f":"IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*CFL\")=0),Table69[CFLSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*CFL\")=0),Table71[CFLSGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*CFL\")=1),Table69[CFLSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*CFL\")=1),Table71[CFLSGNCEXT],IF(AND($F$9=$AD$21,C20=$AD$25),Table73[CFLAGEXT],IF(AND($F$9=$AD$22,C20=$AD$25),Table75[CFLAGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*CFL\")=0),Table69[CFLSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*CFL\")=0),Table71[CFLSGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*CFL\")=1),Table69[CFLSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*CFL\")=1),Table71[CFLSGNCEXT],IF(AND($F$9=$AD$21,C20=$AD$24),Table73[CFLAGEXT],IF(AND($F$9=$AD$22,C20=$AD$24),Table75[CFLAGNCEXT],\"ERROR\"))))))))))))","v":"ERROR"},{"$f":"IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*HID\")=0),Table82[HIDSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*HID\")=0),Table80[HIDSGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*HID\")=1),Table82[HIDSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*HID\")=1),Table80[HIDSGNCEXT],IF(AND($F$9=$AD$21,C20=$AD$25),Table78[HIDAGEXT],IF(AND($F$9=$AD$22,C20=$AD$25),Table76[HIDAGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*HID\")=0),Table82[HIDSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*HID\")=0),Table80[HIDSGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*HID\")=1),Table82[HIDSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*HID\")=1),Table80[HIDSGNCEXT],IF(AND($F$9=$AD$21,C20=$AD$24),Table78[HIDAGEXT],IF(AND($F$9=$AD$22,C20=$AD$24),Table76[HIDAGNCEXT],\"ERROR\"))))))))))))","v":"ERROR"},{"$f":"IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*LAMP\")=0),Table85[FLSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*LAMP\")=0),Table87[FLSGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*LAMP\")=1),Table85[FLSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*LAMP\")=1),Table87[FLSGNCEXT],IF(AND($F$9=$AD$21,C20=$AD$25),Table89[FLAGEXT],IF(AND($F$9=$AD$22,C20=$AD$25),Table92[FLAGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*LAMP\")=0),Table85[FLSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*LAMP\")=0),Table87[FLSGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*LAMP\")=1),Table85[FLSGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*LAMP\")=1),Table87[FLSGNCEXT],IF(AND($F$9=$AD$21,C20=$AD$24),Table89[FLAGEXT],IF(AND($F$9=$AD$22,C20=$AD$24),Table92[FLAGNCEXT],\"ERROR\"))))))))))))","v":"ERROR"},{"$f":"IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*FIXTURE\")=0),Table99[T8SGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*FIXTURE\")=0),Table97[T8SGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$25,COUNTIF(D20,\"*FIXTURE\")=1),Table99[T8SGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$25,COUNTIF(D20,\"*FIXTURE\")=1),Table97[T8SGNCEXT],IF(AND($F$9=$AD$21,C20=$AD$25),Table95[T8AGEXT],IF(AND($F$9=$AD$22,C20=$AD$25),Table2[T8AGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*FIXTURE\")=0),Table99[T8SGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*FIXTURE\")=0),Table97[T8SGNCEXT],IF(AND(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),C20=$AD$24,COUNTIF(D20,\"*FIXTURE\")=1),Table99[T8SGEXT],IF(AND(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),C20=$AD$24,COUNTIF(D20,\"*FIXTURE\")=1),Table97[T8SGNCEXT],IF(AND($F$9=$AD$21,C20=$AD$24),Table95[T8AGEXT],IF(AND($F$9=$AD$22,C20=$AD$24),Table2[T8AGNCEXT],\"ERROR\"))))))))))))","v":"ERROR"},{"$nulls":3},{"$f":"IF(COUNTIF(D20,\"*CFL\")=1,_xlfn.ANCHORARRAY( $AG$41), IF(COUNTIF(D20,\"*HID\")=1,_xlfn.ANCHORARRAY($AH$41), IF(COUNTIF(D20,\"*LAMP\")=1,_xlfn.ANCHORARRAY($AI$41),IF(COUNTIF(D20,\"*FIXTURE\")=1,_xlfn.ANCHORARRAY($AJ$41), \"ERROR\"))))","v":"ERROR"}]
[null,23,{"$nulls":4},{"$f":"IF(ISBLANK(F42),\"\",E42*(_xlfn.XLOOKUP(F42,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F42),ISBLANK(E42)),\"\",_xlfn.XLOOKUP(D42,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F42),\"\",IF(G42<=E42*IF(LEFT(F42,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F42,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F42,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F42,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F42,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F42,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F42,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F42,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G42, E42*IF(LEFT(F42,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F42,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F42,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F42,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F42,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F42,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F42,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F42,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F42=VLOOKUP(F42, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L10040: Four-pin base LED Lamp Replacing CFL, Exterior"]
[null,24,{"$nulls":4},{"$f":"IF(ISBLANK(F43),\"\",E43*(_xlfn.XLOOKUP(F43,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F43),ISBLANK(E43)),\"\",_xlfn.XLOOKUP(D43,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F43),\"\",IF(G43<=E43*IF(LEFT(F43,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F43,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F43,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F43,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F43,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F43,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F43,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F43,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G43, E43*IF(LEFT(F43,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F43,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F43,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F43,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F43,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F43,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F43,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F43,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F43=VLOOKUP(F43, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":13},"L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
[null,25,{"$nulls":4},{"$f":"IF(ISBLANK(F44),\"\",E44*(_xlfn.XLOOKUP(F44,'Industry Std Cost'!$E$4:$E$44,'Industry Std Cost'!$G$4:$G$44,\"NOT FOUND\",0,1)))","v":""},{"$f":"IF(OR(ISBLANK(F44),ISBLANK(E44)),\"\",_xlfn.XLOOKUP(D44,'2025 Default Wattage Guide'!$B$67:$B$131, '2025 Default Wattage Guide'!$C$67:$C$131, \"NOT FOUND\",0,1))","v":""},null,"","",{"$f":"IF(ISBLANK(F44),\"\",IF(G44<=E44*IF(LEFT(F44,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F44,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F44,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F44,6)=\"L3904:\",Criteria!$V$23, IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F44,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F44,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$21),_xlfn.XLOOKUP(LEFT(F44,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$22,_xlfn.XLOOKUP(LEFT(F44,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1),\"ERROR\")))))))),G44, E44*IF(LEFT(F44,6)=\"L4813:\",Criteria!$V$21,IF(LEFT(F44,6)=\"NL4813\",Criteria!$Z$21,IF(LEFT(F44,6)=\"L3903:\",Criteria!$V$22,IF(LEFT(F44,6)=\"L3904:\",Criteria!$V$23,IF(OR($F$9=$AD$14,$F$9=$AD$17,$F$9=$AD$19),_xlfn.XLOOKUP(LEFT(F44,6),Criteria!$A$5:$A$333,Criteria!$V$5:$V$333,\"NOT FOUND\",-1,1),IF(OR($F$9=$AD$15,$F$9=$AD$18,$F$9=$AD$20),_xlfn.XLOOKUP(LEFT(F44,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),IF($F$9=$AD$21,_xlfn.XLOOKUP(LEFT(F44,6),Criteria!$B$5:$B$333,Criteria!$X$5:$X$333,\"NOT FOUND\",-1,1), IF($F$9=$AD$22, _xlfn.XLOOKUP(LEFT(F44,6),Criteria!$C$5:$C$333,Criteria!$Z$5:$Z$333,\"NOT FOUND\",-1,1),\"ERROR\"))))))))))","v":""},"","",{"$f":"IFERROR(IF(F44=VLOOKUP(F44, Criteria!$E$37:$E$46, 1, FALSE), \"This measure Incentive will be capped at 50% project cost.\", \"\"), \"\")","v":""},{"$nulls":6},"",null,"",{"$nulls":4},"L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]
[{"$nulls":5},"Project Totals",{"$f":"SUM(IFERROR(G20:G44, 0))","v":0},{"$nulls":3},{"$f":"SUM(IFERROR(K20:K44, 0))","v":0},{"$f":"SUM(IFERROR(L20:L44, 0))","v":0},{"$f":"SUM(IFERROR(M20:M44, 0))","v":0},{"$f":"(G45-L45)/M45","v":{"$error":"#DIV/0!"}},{"$nulls":14},"L5459: 1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer","AG Starts Here"]
[{"$nulls":28},"L3111: 2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer"]
[{"$nulls":28},"L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
[{"$nulls":28},"L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
[{"$nulls":11},"Default Utility Rates",{"$nulls":16},"L10028: LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture"]
[{"$nulls":11},"Sector","$/kWh",{"$nulls":15},"L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
[{"$nulls":11},"Commercial / Schools & Government / Agriculture",{"v":0.1287,"d":"$0.1287"},{"$nulls":9},"Sector","HOU","CF","NLC SF","SF by Sector Column Index",null,"L10282: 4' LED Linear Ambient Fixture, Interior"]
[{"$nulls":11},"Industrial",{"v":0.0872,"d":"$0.0872"},{"$nulls":9},"Agribusiness",4698,0.67,0.45,null,null,"L10283: 8' LED Linear Ambient Fixture, Interior"]
[{"$nulls":11},"Exterior(Off Peak)",{"v":0.08,"d":"$0.0800"},{"$nulls":9},"Agribusiness-NC",4698,0.67,0.45,null,null,"AG4695: LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture"]
[{"$nulls":22},"B&I",3730,0.77,0.56,null,null,"AG4696: LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture"]
[{"$nulls":22},"B&I-NC",3730,0.77,0.56,null,null,"AG4697: LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
[{"$nulls":22},"Large Industrial",4745,0.77,0.49,null,null,"AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
[{"$nulls":22},"Large Industrial-NC",4745,0.77,0.49,null,null,"AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture"]
[{"$nulls":22},"Schools & Government",3239,0.64,0.41,null,null,"AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture"]
[{"$nulls":22},"Schools & Government-NC",3239,0.64,0.41,null,null,"AG4699: LED Fixture, ≤500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture"]
[{"$nulls":22},"Exterior",{"v":4380,"d":"4,380"},0,0.5,null,null,"AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
[{"$nulls":28},"AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture"]
[{"$nulls":28},"AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture"]
[{"$nulls":28},"L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing existing E39 base lamp"]
[{"$nulls":28},"L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp"]
[{"$nulls":28},"L5452: 4' TLED, replacing 4' T5HO Lamp"]
[{"$nulls":28},"L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp"]
[{"$nulls":28},"L5454: 8' TLED, replacing 8' T8 or T12 Lamp"]
[{"$nulls":28},"AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture"]
[{"$nulls":28},"AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture"]
[{"$nulls":28},"AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture"]
[{"$nulls":28},"AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture"]
[{"$nulls":28},"AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture"]
[{"$nulls":10},"Exterior",{"$nulls":17},"N-AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture"]
[{"$nulls":10},"Interior",{"$nulls":17},"N-AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture"]
[{"$nulls":28},"N-AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture"]
[{"$nulls":28},"N-AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture"]
[{"$nulls":28},"N-AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture"]
[{"$nulls":28},"L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
[{"$nulls":28},"L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]
[{"$nulls":28},"L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
[{"$nulls":28},"L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
[{"$nulls":28},"L10285: 4' LED Linear Ambient Fixture, Exterior"]
[{"$nulls":28},"L10286: 8' LED Linear Ambient Fixture, Exterior"]
[{"$nulls":28},"L4280: Outdoor LED Fixture or Retrofit Kit – Low Output"]
[{"$nulls":28},"L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output"]
[{"$nulls":28},"L4282: Outdoor LED Fixture or Retrofit Kit – High Output "]
[{"$nulls":28},"L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output"]
[{"$nulls":28},"N-L4280: Outdoor LED Fixture or Retrofit Kit – Low Output"]
[{"$nulls":28},"N-L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output"]
[{"$nulls":28},"N-L4282: Outdoor LED Fixture or Retrofit Kit – High Output "]
[{"$nulls":28},"N-L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output"]
[{"$nulls":28},"L10043: Mogul Screw-in Base (E39) replacing existing E39 base lamp, Exterior"]
[{"$nulls":28},"L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
[{"$nulls":28},"L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]
{"$rows_empty":18}
[{"$nulls":5},"Version History"]
[{"$nulls":5},"Program Year","Date of Revision","Description of Changes","Updated By:"]
[{"$nulls":5},2025,"2024-12-16","Still Creating Initial Tool","Evan Croft"]
[{"$nulls":5},2025,"2025-01-16","Editing Existing and proposed fixutre options, will add in deemed savings for proposed, and ISC for project costs","Evan Croft"]
[{"$nulls":5},2025,"2025-02-19","Added in input tables for S&G, B&I, Commercial, Ag measures with breakdowns for existing fixture type. ","Evan Croft"]
[{"$nulls":5},2025,"2025-02-26","Added in Deemed Savings Formulas","Evan Croft"]
[{"$nulls":5},2025,"2025-02-27","Added Payback Formula ","Evan Croft"]
[{"$nulls":5},2025,"2025-03-11","Added in remaining ISC from SPECTRUM","Evan Croft"]
[{"$nulls":5},2025,"2025-07-22","Made multiple edits: added in new kwh savings formula(removing deemed savings formula), Made multiple other small, clerical edits. ","Evan Croft"]
[{"$nulls":5},2025,"2025-08-05","Removed extra tables and formulas that are from the shell calc we used to create the tool. ","Evan Croft"]
[{"$nulls":5},2026,"2026-02-18","Updated for 2026, changed incentive rates, measure lists, ISC, etc.","Evan Croft"]

{"sheet":"Input Tables","index":1,"n_rows":396,"n_cols":11,"rows_kept":396,"hidden":true,"merged":[[1,0,1,1],[1,3,1,5]]}
[]
["Default Wattage",null,null,"Matching Measure"]
["Select Fixture/Lamp"]
["*******FOR CFL DOWNLIGHTS*******","Wattage",null,"CFLSGINT","CFLSGEXT","CFLSGNCINT","CFLSGNCEXT","CFLAGINT","CFLAGEXT","CFLAGNCINT","CFLAGNCEXT"]
["(1) 13W CFL",16,null,"L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior","NL10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","NL10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior","L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior","NL10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","NL10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["(1) 18W CFL",23,null,"L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture","L10040: Four-pin base LED Lamp Replacing CFL, Exterior","NL4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture","NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens","L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture","L10040: Four-pin base LED Lamp Replacing CFL, Exterior","NL4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture","NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["(1) 26W CFL",31,null,"L10039: Four-pin base LED Lamp Replacing CFL","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens","L10039: Four-pin base LED Lamp Replacing CFL","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["(1) 32W CFL",35,null,"L3903: Interior LED Signage","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens","L3903: Interior LED Signage","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["(1) 42W CFL",46,null," ","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["(1) 36/39W 2G11 CFL",51,null,null,"L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC",null,"L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["(1) 40W 2G11 CFL",48,null,null,"L3904: Exterior LED Signage",null,"NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC",null,"L3904: Exterior LED Signage",null,"NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["(1) 55W 2G11 CFL",58,{"$nulls":4},"NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC",{"$nulls":3},"NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["(2) 13W CFL",32,{"$nulls":4},"NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC",{"$nulls":3},"NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
["(2) 18 W CFL",46]
["(2) 26W CFL",62]
["(2) 32W CFL",70]
{"$rows_empty":8}
["*******FOR HID SYSTEMS*******",null,null,"HIDSGINT","HIDSGEXT","HIDSGNCINT","HIDSGNCEXT","HIDAGINT","HIDAGEXT","HIDAGNCINT","HIDAGNCEXT"]
["50W HID",65,null,"L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior","NL10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","NL10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior","L10028: LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture","L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior","NL10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","NL10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["70W HID",94,null,"L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture","L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior","NL4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture","NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens","AG4695: LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture","L3903: Interior LED Signage","NL4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture","NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["100W HID",126,null,"L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens","AG4696: LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["125W HID",146,null,"L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens","AG4697: LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["150W HID",179,null,"L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens","AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["175W HID",210,null,"L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC","AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["200W HID",232,null,"L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID","L3904: Exterior LED Signage",null,"NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC","AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture","L3904: Exterior LED Signage",null,"NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["250W HID",293,null,"L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID",null,null,"NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC","AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture",null,null,"NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["320W HID",356,null,"L10215: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID, w/LLLC",null,null,"NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC","AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture",null,null,"NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
["400W HID",455,null,"L10216: ≤ 250W LED High Bay/Low Bay, replacing 400W HID, w/LLLC",{"$nulls":3},"AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture"]
["750W HID",812,null,"L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID"]
["1,000W HID",{"v":1079,"d":"1,079"},null,"L3903: Interior LED Signage"]
{"$rows_empty":9}
[{"$nulls":3},"FLSGINT","FLSGEXT","FLSGNCINT","FLSGNCEXT","FLAGINT","FLAGEXT","FLAGNCINT","FLAGNCEXT"]
["*******FOR LINEAR FLUORESCENT SYSTEMS*******",null,null,"L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp","L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior","No Lamp S&G NC Interior Measures","NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens","L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp","L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior","No Lamp AG NC Interior Measures","NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["*******Linear Replacement Lamps********",null,null,"L5452: 4' TLED, replacing 4' T5HO Lamp","L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior",null,"NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens","L5452: 4' TLED, replacing 4' T5HO Lamp","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["4' or U-Bend T5, T8, or T12 Lamp",null,null,"L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens","L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["4' T5HO Lamp",null,null,"L5454: 8' TLED, replacing 8' T8 or T12 Lamp","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens","L5454: 8' TLED, replacing 8' T8 or T12 Lamp","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["2' or 3' T8 or T12 Lamp",null,null,"L3903: Interior LED Signage","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC","L3903: Interior LED Signage","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["8' T8 or T12 Lamp",{"$nulls":3},"L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC",null,"L3904: Exterior LED Signage",null,"NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
[{"$nulls":4},"L3904: Exterior LED Signage",null,"NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC",null,"L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior",null,"NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
[{"$nulls":6},"NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC",{"$nulls":3},"NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
{"$rows_empty":8}
["*******4-Foot Fixtures*******",null,null,"T8SGINT","T8SGEXT","T8SGNCINT","T8SGNCEXT","T8AGINT","T8AGEXT","T8AGNCINT","T8AGNCEXT"]
["1L F32 T8 Normal BF Fixture",33,null,"L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer","L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior","NL5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer","NL10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior","L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer","L10285: 4' LED Linear Ambient Fixture, Exterior","NL5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer","NL10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["1L F34 T12 Fixture",39,null,"L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","L10285: 4' LED Linear Ambient Fixture, Exterior","NL3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","NL10285: 4' LED Linear Ambient Fixture, Exterior","L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","L10286: 8' LED Linear Ambient Fixture, Exterior","NL3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","NL10285: 4' LED Linear Ambient Fixture, Exterior"]
["1L F40 T12 Fixture",39,null,"L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","L10286: 8' LED Linear Ambient Fixture, Exterior","NL3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","NL10286: 8' LED Linear Ambient Fixture, Exterior","L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior","NL3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","NL10286: 8' LED Linear Ambient Fixture, Exterior"]
["1L F54 T5HO Fixture",62,null,"L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens","NL3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens","L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens","NL3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["2L F32 T8 Normal BF Fixture",61,null,"L10214: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer, w/LLLC","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens","NL10281: 1’ to 3’ LED Linear Ambient Fixture, Interior","NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens","L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens","NL10281: 1’ to 3’ LED Linear Ambient Fixture, Interior","NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["2L FU32T8/6 Fixture",55,null,"L10213: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer, w/LLLC","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens","NL10282: 4' LED Linear Ambient Fixture, Interior","NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens","L10282: 4' LED Linear Ambient Fixture, Interior","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens","NL10282: 4' LED Linear Ambient Fixture, Interior","NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["2L F34 T12 Fixture",66,null,"L10211: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps, w/LLLC","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens","NL10283: 8' LED Linear Ambient Fixture, Interior","NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens","L10283: 8' LED Linear Ambient Fixture, Interior","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens","NL10283: 8' LED Linear Ambient Fixture, Interior","NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["2L F40 T12 Fixture",79,null,"L10212: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps, w/LLLC","L3904: Exterior LED Signage","NL5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12","NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC","L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior","L3904: Exterior LED Signage","NL5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12","NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["2L FU40T12 Fixture",72,null,"L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior",null,"NL3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO","NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC","L3903: Interior LED Signage",null,"NL3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO","NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["2L F54 T5HO Fixture",117,null,"L10282: 4' LED Linear Ambient Fixture, Interior",null,"NL4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO","NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC","L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12",null,"NL4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO","NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["3L F32 T8 Normal BF Fixture",91,null,"L10283: 8' LED Linear Ambient Fixture, Interior",null,"NL4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO","NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC","L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO",null,"NL4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO","NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
["3L F34 T12 Fixture",103,null,"L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12",null,"NL4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO",null,"L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO",null,"NL4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["3L F40 T12 Fixture",124,null,"L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO",{"$nulls":3},"L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO",null,"NL5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"]
["4L F54 T5HO Fixture",234,null,"L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO",{"$nulls":3},"L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO",null,"NL3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO"]
["4L F32 T8 Normal BF Fixture",120,null,"L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO",{"$nulls":3},"L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO",null,"NL4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO"]
["4L F32 T8 High BF Fixture",151,null,"L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO",{"$nulls":3},"L10217: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO, w/LLLC",null,"NL4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO"]
["4L F34 T12 Fixture",136,null,"L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO",{"$nulls":3},"L10218: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO, w/LLLC",null,"NL4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["4L F40 T12 Fixture",153,null,"L10217: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO, w/LLLC",{"$nulls":3},"AG4697: LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
["6L F54 T5HO Fixture",355,null,"L10218: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO, w/LLLC",{"$nulls":3},"AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
["6L F32 T8 High BF Fixture",224,null,"L3903: Interior LED Signage",{"$nulls":3},"AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture"]
["8L F54 T5HO Fixture",468,{"$nulls":5},"AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture"]
["8L F32 T8 High BF Fixture",291]
["10L F54 T5HO Fixture",585]
["10L F32 T8 High BF Fixture",368]
["12L F32 T8 High BF Fixture",442]
["*******8-Foot Fixtures*******"]
["1L F96T8 Fixture",61]
["2L F96T8 Fixture",107]
["1L F96T12 Fixture",69]
["1L F96T12/HO Fixture",115]
["2L F96T12 Fixture",109]
["2L F96T12/HO Fixture",190]
["Other Fixture(Non DLC/ES Listed, different end use appliaction, not listed)","Manual Input"]
[]
[]
["Measures","Measure Selection","Measure Tables",{"$nulls":3},"Fixture List Specification",null,null,"Fixture List Specification"]
["L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer","Schools & Government - Interior",null,"69:104",{"$f":"IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$118,'Lighting Project Tool'!C20='Input Tables'!$B$127),$B$101,IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$118,'Lighting Project Tool'!C20='Input Tables'!$B$128),$B$109,IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$119,'Lighting Project Tool'!C20='Input Tables'!$B$127),$B$102,IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$119,'Lighting Project Tool'!C20='Input Tables'!$B$128),$B$110,IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$120,'Lighting Project Tool'!C20='Input Tables'!$B$127),$B$103,IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$120,'Lighting Project Tool'!C20='Input Tables'!$B$128),$B$111,IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$121,'Lighting Project Tool'!C20='Input Tables'!$B$127),$B$104,IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$121,'Lighting Project Tool'!C20='Input Tables'!$B$128),$B$112,IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$122,'Lighting Project Tool'!C20='Input Tables'!$B$127),$B$105, IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$122,'Lighting Project Tool'!C20='Input Tables'!$B$128),$B$113, IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$123,'Lighting Project Tool'!C20='Input Tables'!$B$127),$B$106, IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$123,'Lighting Project Tool'!C20='Input Tables'!$B$128),$B$114, IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$124,'Lighting Project Tool'!C20='Input Tables'!$B$127),$B$107, IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$124,'Lighting Project Tool'!C20='Input Tables'!$B$128),$B$115, IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$125,'Lighting Project Tool'!C20='Input Tables'!$B$127),$B$108, IF(AND('Lighting Project Tool'!$F$9='Input Tables'!$B$125,'Lighting Project Tool'!C20='Input Tables'!$B$128),$B$116,\"PLEASE SELECT SECTOR OR INTERIOR/EXTERIOR\"))))))))))))))))","v":"PLEASE SELECT SECTOR OR INTERIOR/EXTERIOR"},{"$f":"IF($E$101=$B$101,$A$101:$A$136, IF($E$101=$B$102, $A$150:$A$163, IF($E$101=$B$103,$A$176:$A$203, IF($E$101=$B$104, $A$217:$A$232, IF($E$101=$B$109,$A$137:$A$149, IF($E$101 = $B$110, $A$164:$A$175, IF($E$101=$B$111,$A$204:$A$216, IF($E$101=$B$112,$A$233:$A$244,IF($E$101=$B$105,$A$101:$A$136, IF($E$101=$B$106,$A$150:$A$163,IF($E$101=$B$107,$A$101:$A$136, IF($E$101=$B$108,$A$150:$A$163,IF($E$101=$B$113,$A$137:$A$149, IF($E$101=$B$114,$A$164:$A$175,IF($E$101=$B$115,$A$137:$A$149, IF($E$101=$B$116,$A$164:$A$175,\"PLEASE SELECT SECTOR OR INTERIOR/EXTERIOR\"))))))))))))))))","v":"PLEASE SELECT SECTOR OR INTERIOR/EXTERIOR"},null,{"$f":"IF($E$101=$B$101,$B$109,IF($E$101=$B$102,$B$110,IF($E$101=$B$103,$B$111,IF($E$101=$B$104,$B$112,IF($E$101=$B$109,$B$101,IF($E$101=$B$110,$B$102,IF($E$101=$B$111,$B$103,IF($E$101=$B$112,$B$104,IF($E$101 = $B$105, $B$113, IF($E$101=$B$106, $B$114, IF($E$101=$B$107,$B$115, IF($E$101=$B$108, $B$116, IF($E$101 = $B$113, $B$105, IF($E$101=$B$114, $B$106, IF($E$101 = $B$115, $B$107, IF($E$101=$B$116, $B$108, \"PLEASE SELECT SECTOR OR INTERIOR/EXTERIOR\"))))))))))))))))","v":"PLEASE SELECT SECTOR OR INTERIOR/EXTERIOR"},{"$f":"IF($H$101=$B$101,$A$101:$A$136, IF($H$101=$B$102, $A$150:$A$163, IF($H$101=$B$103,$A$176:$A$203, IF($H$101=$B$104, $A$217:$A$232, IF($H$101=$B$109,$A$137:$A$149, IF($H$101 = $B$110, $A$164:$A$175, IF($H$101=$B$111,$A$204:$A$216, IF($H$101=$B$112,$A$233:$A$244,IF($H$101=$B$105,$A$101:$A$136, IF($H$101=$B$106,$A$150:$A$163,IF($H$101=$B$107,$A$101:$A$136, IF($H$101=$B$108,$A$150:$A$163,IF($H$101=$B$113,$A$137:$A$149, IF($H$101=$B$114,$A$164:$A$175,IF($H$101=$B$115,$A$137:$A$149, IF($H$101=$B$116,$A$164:$A$175,\"PLEASE SELECT SECTOR OR INTERIOR/EXTERIOR\"))))))))))))))))","v":"PLEASE SELECT SECTOR OR INTERIOR/EXTERIOR"}]
["L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","Schools & Government - NC - Interior",null,"118:131",{"$nulls":3},0]
["L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","Agribusiness - Interior",null,"144:171",{"$nulls":3},0]
["L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","Agribusiness - NC - Interior",null,"185:200",{"$nulls":3},0]
["L10214: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer, w/LLLC","B&I - Interior",null,"69:104",{"$nulls":3},0]
["L10213: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer, w/LLLC","B&I - NC - Interior",null,"118:131",{"$nulls":3},0]
["L10211: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps, w/LLLC","Large Industrial - Interior",null,"69:104",{"$nulls":3},0]
["L10212: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps, w/LLLC","Large Industrial - NC - Interior",null,"118:131",{"$nulls":3},0]
["L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior","Schools & Government - Exterior",null,"105:117",{"$nulls":3},0]
["L10282: 4' LED Linear Ambient Fixture, Interior","Schools & Government - NC - Exterior",null,"132:143",{"$nulls":3},0]
["L10283: 8' LED Linear Ambient Fixture, Interior","Agribusiness - Exterior",null,"172:184",{"$nulls":3},0]
["L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture","Agribusiness - NC - Exterior",null,"201:212",{"$nulls":3},0]
["L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture","B&I - Exterior",null,"105:117",{"$nulls":3},0]
["L3903: Interior LED Signage","B&I - NC - Exterior",null,"132:143",{"$nulls":3},0]
["L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID","Large Industrial - Exterior",null,"105:117",{"$nulls":3},0]
["L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID","Large Industrial - NC - Exterior",null,"132:143",{"$nulls":3},0]
["L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID",{"$nulls":6},0]
["L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID","Schools & Government",{"$nulls":5},0]
["L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID","Schools & Government-NC",{"$nulls":5},0]
["L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID","Agribusiness",{"$nulls":5},0]
["L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12","Agribusiness-NC",{"$nulls":5},0]
["L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO","B&I",{"$nulls":5},0]
["L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO","B&I-NC",{"$nulls":5},0]
["L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO","Large Industrial",{"$nulls":5},0]
["L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO","Large Industrial-NC",{"$nulls":5},0]
["L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO",{"$nulls":6},0]
["L10215: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID, w/LLLC","Interior",{"$nulls":5},0]
["L10216: ≤ 250W LED High Bay/Low Bay, replacing 400W HID, w/LLLC","Exterior",{"$nulls":5},0]
["L10217: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO, w/LLLC",{"$nulls":6},0]
["L10218: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO, w/LLLC",{"$nulls":6},0]
["L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID",{"$nulls":6},0]
["L10039: Four-pin base LED Lamp Replacing CFL",{"$nulls":6},0]
["L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp",{"$nulls":6},0]
["L5452: 4' TLED, replacing 4' T5HO Lamp",{"$nulls":6},0]
["L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp",{"$nulls":6},0]
["L5454: 8' TLED, replacing 8' T8 or T12 Lamp",{"$nulls":6},0]
["L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior",{"$nulls":6},0]
["L10285: 4' LED Linear Ambient Fixture, Exterior",{"$nulls":6},0]
["L10286: 8' LED Linear Ambient Fixture, Exterior",{"$nulls":6},0]
["L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior",{"$nulls":6},0]
["L3904: Exterior LED Signage",{"$nulls":6},0]
["L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",{"$nulls":6},0]
["L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior"]
["L10040: Four-pin base LED Lamp Replacing CFL, Exterior"]
["L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["NL5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"]
["NL3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer"]
["NL3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["NL3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["NL10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["NL10282: 4' LED Linear Ambient Fixture, Interior"]
["NL10283: 8' LED Linear Ambient Fixture, Interior"]
["NL10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"]
["NL4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"]
["NL5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"]
["NL3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO"]
["NL4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO"]
["NL4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO"]
["NL4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["NL10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["NL10285: 4' LED Linear Ambient Fixture, Exterior"]
["NL10286: 8' LED Linear Ambient Fixture, Exterior"]
["NL10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
["L5459: 1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer"]
["L3111: 2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer"]
["L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["L10028: LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture"]
["L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["L10282: 4' LED Linear Ambient Fixture, Interior"]
["L10283: 8' LED Linear Ambient Fixture, Interior"]
["AG4695: LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture"]
["AG4696: LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture"]
["AG4697: LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
["AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
["AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture"]
["AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture"]
["L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing existing E39 base lamp"]
["L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp"]
["L5452: 4' TLED, replacing 4' T5HO Lamp"]
["L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp"]
["L5454: 8' TLED, replacing 8' T8 or T12 Lamp"]
["AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture"]
["AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture"]
["AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture"]
["AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture"]
["AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture"]
["AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture"]
["AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture"]
["L10289: Fixture Elimination, Interior"]
["L10287: General Wattage Reduction, Interior"]
["L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["L10285: 4' LED Linear Ambient Fixture, Exterior"]
["L10286: 8' LED Linear Ambient Fixture, Exterior"]
["L4280: Outdoor LED Fixture or Retrofit Kit – Low Output"]
["L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output"]
["L4282: Outdoor LED Fixture or Retrofit Kit – High Output "]
["L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output"]
["L10043: Mogul Screw-in Base (E39) replacing existing E39 base lamp, Exterior"]
["L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["L10290: Fixture Elimination, Exterior"]
["L10288: General Wattage Reduction, Exterior"]
["NL5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"]
["NL3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer"]
["NL3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["NL3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["NL10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["NL10282: 4' LED Linear Ambient Fixture, Interior"]
["NL10283: 8' LED Linear Ambient Fixture, Interior"]
["NL10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"]
["NL4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"]
["NL5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"]
["NL3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO"]
["NL4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO"]
["NL4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO"]
["NL4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["N-AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture"]
["N-AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture"]
["NL10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["NL10285: 4' LED Linear Ambient Fixture, Exterior"]
["NL10286: 8' LED Linear Ambient Fixture, Exterior"]
["NL10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
{"$rows_empty":7}
["Measures with ISC"]
["L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"]
["L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer"]
["L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["L10214: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer, w/LLLC"]
["L10213: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer, w/LLLC"]
["L10211: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps, w/LLLC"]
["L10212: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps, w/LLLC"]
["L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["L10282: 4' LED Linear Ambient Fixture, Interior"]
["L10283: 8' LED Linear Ambient Fixture, Interior"]
["L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"]
["L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"]
["L3903: Interior LED Signage"]
["L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID"]
["L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID"]
["L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID"]
["L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID"]
["L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID"]
["L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID"]
["L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"]
["L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO"]
["L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO"]
["L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO"]
["L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO"]
["L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["L10215: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID, w/LLLC"]
["L10216: ≤ 250W LED High Bay/Low Bay, replacing 400W HID, w/LLLC"]
["L10217: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO, w/LLLC"]
["L10218: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO, w/LLLC"]
["L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID"]
["L10039: Four-pin base LED Lamp Replacing CFL"]
["L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp"]
["L5452: 4' TLED, replacing 4' T5HO Lamp"]
["L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp"]
["L5454: 8' TLED, replacing 8' T8 or T12 Lamp"]
["L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["L10285: 4' LED Linear Ambient Fixture, Exterior"]
["L10286: 8' LED Linear Ambient Fixture, Exterior"]
["L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["L3904: Exterior LED Signage"]
["L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior"]
["L10040: Four-pin base LED Lamp Replacing CFL, Exterior"]
["L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["NL5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"]
["NL3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer"]
["NL3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["NL3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["NL10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["NL10282: 4' LED Linear Ambient Fixture, Interior"]
["NL10283: 8' LED Linear Ambient Fixture, Interior"]
["NL10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"]
["NL4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"]
["NL5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"]
["NL3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO"]
["NL4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO"]
["NL4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO"]
["NL4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["NL10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["NL10285: 4' LED Linear Ambient Fixture, Exterior"]
["NL10286: 8' LED Linear Ambient Fixture, Exterior"]
["NL10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
["L5459: 1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer"]
["L3111: 2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer"]
["L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["L10028: LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture"]
["L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["L10282: 4' LED Linear Ambient Fixture, Interior"]
["L10283: 8' LED Linear Ambient Fixture, Interior"]
["AG4695: LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture"]
["AG4696: LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture"]
["AG4697: LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
["AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
["AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture"]
["AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture"]
["L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing existing E39 base lamp"]
["L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp"]
["L5452: 4' TLED, replacing 4' T5HO Lamp"]
["L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp"]
["L5454: 8' TLED, replacing 8' T8 or T12 Lamp"]
["AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture"]
["AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture"]
["AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture"]
["AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture"]
["AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture"]
["AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture"]
["AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture"]
["L10289: Fixture Elimination, Interior"]
["L10287: General Wattage Reduction, Interior"]
["L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["L10285: 4' LED Linear Ambient Fixture, Exterior"]
["L10286: 8' LED Linear Ambient Fixture, Exterior"]
["L4280: Outdoor LED Fixture or Retrofit Kit – Low Output"]
["L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output"]
["L4282: Outdoor LED Fixture or Retrofit Kit – High Output "]
["L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output"]
["L10043: Mogul Screw-in Base (E39) replacing existing E39 base lamp, Exterior"]
["L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["L10290: Fixture Elimination, Exterior"]
["L10288: General Wattage Reduction, Exterior"]
["NL5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"]
["NL3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer"]
["NL3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["NL3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["NL10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["NL10282: 4' LED Linear Ambient Fixture, Interior"]
["NL10283: 8' LED Linear Ambient Fixture, Interior"]
["NL10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"]
["NL4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"]
["NL5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"]
["NL3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO"]
["NL4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO"]
["NL4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO"]
["NL4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["N-AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture"]
["N-AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture"]
["NL10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["NL10285: 4' LED Linear Ambient Fixture, Exterior"]
["NL10286: 8' LED Linear Ambient Fixture, Exterior"]
["NL10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["NL4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["NL4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["NL4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["NL4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["NL5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["NL5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["NL5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["NL5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]

{"sheet":"Table3","index":2,"n_rows":4,"n_cols":1,"rows_kept":4,"hidden":true}
["Existing Exterior Fixture List"]
["Outdoor Pole/Arm-mounted Area & Roadway Luminaires"]
["Outdoor Wall-mounted Area Luminaires"]
["Other Outdoor LED Fixtures"]

{"sheet":"Lookups","index":3,"n_rows":90,"n_cols":13,"rows_kept":90,"hidden":true,"merged":[[30,0,30,1],[59,0,59,7]]}
[]
["Unit of Measure lookup","Program Name Lookup","Short","Incentive Codes to Use"]
["# of Rooms","Agribusiness","AG","Ag"]
["Boiler Capacity (MBh)","Agribusiness-NC","BNC","Ag"]
["Boiler hp","B&I","BI","Business"]
["Bushels/Hr","B&I-NC","BNC","NewConstruction"]
["Capacity (input MBh)","Large Industrial","BI","Business"]
["CFM","Large Industrial-NC","BNC","NewConstruction"]
["Compressor HP","Schools & Government","BI","Business"]
["Computers","Schools & Government-NC","BNC","NewConstruction"]
["Cu Ft","Ag-Propane","AGP","Ag"]
["Fan Diameter (Inches)"]
["Fan Motors Controlled"]
["Fixtures Controlled"]
["HP","Measure Labels",null,"Incentive Code Types"]
["HP of Load Shifted","Use Numbers",null,"Business"]
["Hrs/Yr","Use Letters",null,"Ag"]
["kW Controlled",null,null,"NewConstruction"]
["kW of Exist. Heater Bands"]
["Linear Feet","Cost Types",null,null,"Start Row on Criteria Tab"]
["MBh","Invoice",null,null,"Business","$4"]
["Sq Ft","Ind Std Cost",null,null,"Ag","$265"]
["Million BTU/HR"," TRM",null,null,"Ag Propane","$410"]
["Tons","Prorate by Qty/Cap"]
[null,"Other",null,null,"Last Row on Criteria Tab",{"v":454,"d":"$454"}]
[]
[null,"True/False Questions"]
[null,"Yes"]
[null,"No"]
[]
["Letter to Number Conversion"]
[1,"A"]
[2,"B"]
[3,"C"]
[4,"D"]
[5,"E"]
[6,"F"]
[7,"G"]
[8,"H"]
[9,"I"]
[10,"J"]
[11,"K"]
[12,"L"]
[13,"M"]
[14,"N"]
[15,"O"]
[16,"P"]
[17,"Q"]
[18,"R"]
[19,"S"]
[20,"T"]
[21,"U"]
[22,"V"]
[23,"W"]
[24,"X"]
[25,"Y"]
[]
[]
[]
["These lists are used to populate the \"Browse by Incentive Catalog\" dropdown on the Review Sheet tab and translate each item to a named range on the measure list tab. Update as needed. "]
["B&I, LI, and S&G APPLICATION LIST",null,null,"AGRIBUSINESS APPLICATION LIST",null,null,"NEW CONSTRUCTION APPLICATION LIST",null,null,"Unique UOM Question - UOM Lookup"]
["Incentive Application","Named Range",null,"Incentive Application","Named Range",null,"Incentive Application","Named Range",null,"Measure Master ID","Measure Master Name","Unit of Measure Question","Quantity Description"]
["Special Offers B&I","SpecialOffersBI",null,"Agribusiness Catalog: Milking Equipment","AgCatalogMilkingEquipAG",null,"Lighting Catalog: LED Fixtures","LightingCatalogLEDFixturesBNC",null,3909,"A/C Split System, Condensing Unit Only, High Efficiency","Enter Unit Total Incentive","Enter # of Condensing Units"]
["Lighting Catalog: LED Fixtures","LightingCatalogLEDFixturesBI",null,"Agribusiness Catalog: Specialty Equipment","AgCatalogSpecialtyEquipAG",null,"Lighting Catalog: Other Lighting Solutions","LightingCatalogOtherLightingSolutionsBNC",null,4368,"A/C Split or Packaged System, High Efficiency, ≥ 5.42 to < 11.25 tons ","Enter Unit Total Incentive","Enter # of Split Systems or RTUs"]
["Lighting Catalog: LED Lamps","LightingCatalogLEDLampsBI",null,"Agribusiness Catalog: Lighting","AgCatalogLightingAG",null,"HVAC Catalog: Heating Systems","HvacCatalogHeatingSystemsBNC",null,4369,"A/C Split or Packaged System, High Efficiency, ≥ 11.25 to < 20.00 tons","Enter Unit Total Incentive","Enter # of Split Systems or RTUs"]
["Lighting Catalog: Controls","LightingCatalogControlsBI",null,"Agribusiness Catalog: Ventilation Equipment","AgCatalogVentilationAG",null,"HVAC Catalog: Cooling Systems","HvacCatalogCoolingSystemsBNC",null,4370,"A/C Split or Packaged System, High Efficiency, ≥ 20.00 to < 63.33 tons","Enter Unit Total Incentive","Enter # of Split Systems or RTUs"]
["Lighting Catalog: Other Lighting Solutions","LightingCatalogOtherLightingSolutionsBI",null,"Agribusiness Catalog: VFD and Compressed Air","AgCatalogVFDandCompressedAirAG",null,"HVAC Catalog: Ventilation and Controls","HvacCatalogVentilationControlsBNC",null,4371,"A/C Split or Packaged System, High Efficiency, ≥ 63.33 tons","Enter Unit Total Incentive","Enter # of Split Systems or RTUs"]
["HVAC Catalog: Heating Systems","HvacCatalogHeatingSystemsBI",null,"Agribusiness Catalog: Cooling and Space Heating Equipment","AgCatalogCoolingSpaceHeatingAG",null,"HVAC Catalog: Plumbing","HvacCatalogPlumbingBNC",null,10025,"Commercial Air Source Heat Pumps, ≥ 5.42 to < 11.25 tons","Enter Unit Total Incentive","Enter # of Split Systems or RTUs"]
["HVAC Catalog: Cooling Systems","HvacCatalogCoolingSystemsBI",null,"Agribusiness Catalog: Water Heating Equipment","AgCatalogWaterHeatingAG",null,"HVAC Catalog: Building Envelope","HvacCatalogBuildingEnvelopeBNC",null,10026,"Commercial Air Source Heat Pumps, ≥ 11.25 to < 20.00 tons","Enter Unit Total Incentive","Enter # of Split Systems or RTUs"]
["HVAC Catalog: Ventilation and Controls","HvacCatalogVentilationControlsBI",null,"Ag-Propane Catalog: Specialty Equipment","AgPropCatalogSpecialtyEquipAGP",null,"Commercial Refrig Catalog: Non Self-Contained","RefrigerationCatalogNonSelfContainBNC",null,10027,"Commercial Air Source Heat Pumps, ≥ 20.00 to < 63.33 tons,","Enter Unit Total Incentive","Enter # of Split Systems or RTUs"]
["HVAC Catalog: Building Envelope","HvacCatalogBuildingEnvelopeBI",null,"Ag-Propane Catalog: VFDs and Compressed Air","AgPropCatalogVfdCompAirAGP",null,"Commercial Refrig Catalog: Controls","RefrigerationCatalogControlsBNC",null,4712,"Chiller, Air-Cooled <150 tons, Path A","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Commercial Refrig Catalog: Non Self-Contained","RefrigerationCatalogNonSelfContainBI",null,"Ag-Propane Catalog: Water Heating Equipment","AgPropCatalogWaterHeatingAGP",null,"Process Systems Catalog: Compressed Air","ProcessCatalogCompressedAirBNC",null,4713,"Chiller, Air-Cooled ≥150 tons, Path A","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Commercial Refrig Catalog: Controls","RefrigerationCatalogControlsBI",null,"Ag-Propane Catalog: Space Heating Equipment","AgPropCatalogSpaceHeatingAGP",null,"Process Systems Catalog: Steam Systems","ProcessCatalogSteamSystemsBNC",null,4714,"Chiller, Air-Cooled <150 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Process Systems Catalog: Compressed Air","ProcessCatalogCompressedAirBI",null,"Lighting Catalog: LED Fixtures","LightingCatalogLEDFixturesAG",null,"Process Systems Catalog: VFDs","ProcessCatalogVFDsBNC",null,4715,"Chiller, Air-Cooled ≥150 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Process Systems Catalog: Steam Systems","ProcessCatalogSteamSystemsBI",null,"Lighting Catalog: LED Lamps","LightingCatalogLEDLampsAG",null,"Process Systems Catalog: Process Specialty Equip","ProcessCatalogProcessSpecialtyEquipBNC",null,4716,"Chiller, Positive Displacement, Water-Cooled <75 tons, Path A","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Process Systems Catalog: VFDs","ProcessCatalogVFDsBI",null,"Lighting Catalog: Controls","LightingCatalogControlsAG",{"$nulls":4},4721,"Chiller, Positive Displacement, Water-Cooled <75 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Process Systems Catalog: Data Center and Telecom Facilities","ProcessCatalogDataCenterTelecomBI",null,"Lighting Catalog: Other Lighting Solutions","LightingCatalogOtherLightingSolutionsAG",{"$nulls":4},4722,"Chiller, Positive Displacement, Water-Cooled ≥75 and <150 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Process Systems Catalog: Process Specialty Equip","ProcessCatalogProcessSpecialtyEquipBI",null,"HVAC Catalog: Heating Systems","HvacCatalogHeatingSystemsAG",{"$nulls":4},4723,"Chiller, Positive Displacement, Water-Cooled ≥150 and <300 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Special Offers LI","SpecialOffersLI",null,"HVAC Catalog: Cooling Systems","HvacCatalogCoolingSystemsAG",{"$nulls":4},4724,"Chiller, Positive Displacement, Water-Cooled ≥300 and <600 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
["Special Offers S&G","SpecialOffersSG",null,"HVAC Catalog: Ventilation and Controls","HvacCatalogVentilationControlsAG",null,"Process Catalog VFDs not listed as they are all eligible under B&I. Above items are for equipment eligible under BNC.",null,null,4725,"Chiller, Positive Displacement, Water-Cooled ≥600, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
[{"$nulls":3},"HVAC Catalog: Plumbing","HvacCatalogPlumbingAG",{"$nulls":4},4726,"Chiller, Centrifugal, Water-Cooled <150 tons, Path A","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
[{"$nulls":3},"HVAC Catalog: Building Envelope","HvacCatalogBuildingEnvelopeAG",{"$nulls":4},4730,"Chiller, Centrifugal, Water-Cooled ≥600, Path A","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
[{"$nulls":3},"Commercial Refrig Catalog: Non Self-Contained","RefrigerationCatalogNonSelfContainAG",{"$nulls":4},4731,"Chiller, Centrifugal, Water-Cooled <150 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
[{"$nulls":3},"Commercial Refrig Catalog: Controls","RefrigerationCatalogControlsAG",{"$nulls":4},4732,"Chiller, Centrifugal, Water-Cooled ≥150 and <300 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
[{"$nulls":3},"Process Systems Catalog: Compressed Air","ProcessCatalogCompressedAirAG",{"$nulls":4},4733,"Chiller, Centrifugal, Water-Cooled ≥300 and <400 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
[{"$nulls":3},"Process Systems Catalog: Steam Systems","ProcessCatalogSteamSystemsAG",{"$nulls":4},4734,"Chiller, Centrifugal, Water-Cooled ≥400 and <600 tons, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
[{"$nulls":3},"Process Systems Catalog: VFDs","ProcessCatalogVFDsAG",{"$nulls":4},4735,"Chiller, Centrifugal, Water-Cooled ≥600, Path B","Enter Incentive Per Ton","Enter total chiller tons (tons each x qty)"]
[{"$nulls":3},"Process Systems Catalog: Data Center and Telecom Facilities","ProcessCatalogDataCenterTelecomAG"]
[{"$nulls":3},"Process Systems Catalog: Process Specialty Equip","ProcessCatalogProcessSpecialtyEquipAG",{"$nulls":4},"Regular UOM & Qty Description:","** This is the UOM & Qty that appear on the application **"]
[{"$nulls":3},"Special Offers Ag","SpecialOffersAG",{"$nulls":4},"SPECTRUM UOM & Qty Description:","** This is the Unit of Measure and Qty that get entered in SPECTRUM **"]

{"sheet":"Criteria","index":4,"n_rows":471,"n_cols":45,"rows_kept":471,"hidden":true,"merged":[[0,0,0,5]]}
["This tab is the main lookup table to find incentives, units of measure, new construction eligibility, and key requirements for each measure. \nUpdate Instructions: need to manually go thru each catalog and copy in measure codes, measure descriptions, and Criteria. Some criteria may need to be combined or shortened to fit in allocated # of Critera columns. Inserting rows before the end or after the start of a section is the best way, as it keeps the new row in the intended Named Range. When done, verify that the \"Criteria_Array\" named range (columns E thru J, all rows but not headings) is still accurate and covers all rows. After measure list here is complete, also need to update Measure List tab. Measure List tab should contain all eligible measure codes and measure names in separate columns for Business / LI / S&G, AgV2, and New Construction (i.e., columns A, B, C of this tab, but with the \"Not Eligible\" rows removed). \nAlso, check the Vlookup functions on the Review Sheet tab to ensure they cover the last row of this tab. Do a find and replace to fix as there are 100's of references to the measure list on this tab. ",{"$nulls":5},"Agribusiness"]
[1,2,3,4,5,6,7,8,9,10,{"$f":"J2+1","v":11},{"$f":"K2+1","v":12},13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45]
["Business Catalog Code","Agribusiness Catalog Code","New Construction Catalog Code","Measure Text","Measure Code & Name","Criteria 1","Criteria 2","Criteria 3","Criteria 4","Criteria 5","Criteria 6","Criteria 7","Criteria 8","Criteria 9","Interpretations and Clarifications","PI Guidance-Photos","PI Guidance 1","PI Guidance 2","PI Guidance 3","PI Guidance 4","PI Guidance 5","B&I Incentive","B&I Incentive per…","Ag Incentive","Ag Incentive per…","NC Incentive","NC Incentive Per","B&I MMID","Ag MMID","NC MMID","B&I NC Eligible","Ag NC Eligible","BNC Eligible","B&I % of  Project Cost Limit","Ag % of  Project Cost Limit","Business NC % of  Project Cost Limit","Requires Unique SPECTRUM Data Entry for UOM & Qty","Measure Text for Hybrid Calc & Tech Review Pivot Table","Hybrid Calc required","Tech Review Required","Unit of Measure for Savings","Unit of Measure Range Minimum","Unit of Measure Range Maximum","Catalog Name","Page No."]
[{"$nulls":3},"----------------------LIGHTING CATALOG: LED FIXTURES----------------------------",{"$f":"IF(ISBLANK(A4),\"\",IF(FOEPrgm=IncentCodeTypeNC,C4,IF(FOEIncentCodeType=IncentCodeTypeAg,B4,A4))&\": \") &D4","v":"----------------------LIGHTING CATALOG: LED FIXTURES----------------------------"},{"$nulls":32},{"$f":"IF(ISBLANK(A4),\"\",IF(A4<>\"Not Eligible\",A4,IF(B4<>\"Not Eligible\",B4,C4))&\": \") &D4","v":"----------------------LIGHTING CATALOG: LED FIXTURES----------------------------"},{"$nulls":3},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR4=\"Agribusiness\", $AR4=\"Ag\",$AR4=\"Propane\", $AR4=\"Ag Propane\", $AR4=\"Ag-Propane\"),$AC4,  $AB4),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR4=\"Agribusiness\", $AR4=\"Ag\",$AR4=\"Propane\", $AR4=\"Ag Propane\", $AR4=\"Ag-Propane\"),$AC4,  $AB4),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting"]
["L5459","L5459","N-L5459","LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer",{"$f":"IF(ISBLANK(A5),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C5,IF(FOEIncentCodeType=IncentCodeTypeAg,B5,A5))&\": \") &D5","v":"L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"},"For 1-for-1 replacement of T12 or standard T8 fluorescent fixtures","Must be DLC TRT V5.0 or higher listed in the \"Troffer\" general application.","New fixture must consume ≤ 43W.","Other LED configurations may qualify for a custom incentive.",{"$nulls":5},"Other LED configurations may qualify for custom incentive.","Provide clear photo(s) of: fixture layout and (if possible) fixture packaging label.","Verify fixture size by comparing to grid ceiling as reference.",{"$nulls":4},{"v":10,"d":"$10.00"},"Fixture",{"$f":"V5","v":{"v":10,"d":"$10.00"}},"Fixture",{"v":7,"d":"$7.00"},{"$f":"W5","v":"Fixture"},5459,{"$f":"AB5","v":5459},5459,"Yes",{"$f":"AE5","v":"Yes"},"Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A5),\"\",IF(A5<>\"Not Eligible\",A5,IF(B5<>\"Not Eligible\",B5,C5))&\": \") &D5","v":"L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR5=\"Agribusiness\", $AR5=\"Ag\",$AR5=\"Propane\", $AR5=\"Ag Propane\", $AR5=\"Ag-Propane\"),$AC5,  $AB5),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR5=\"Agribusiness\", $AR5=\"Ag\",$AR5=\"Propane\", $AR5=\"Ag Propane\", $AR5=\"Ag-Propane\"),$AC5,  $AB5),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L3111","L3111","N-L3111","LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","For 1-for-1 replacement of T12 or standard T8 fluorescent fixtures","Must be DLC TRT V5.0 or higher listed in the \"Troffer\" general application.","New fixture must consume ≤ 55W","Other LED configurations may qualify for a custom incentive.",{"$nulls":5},"Work paper is based on 3 and 4 lamp fixtures only. ","Provide clear photo(s) of: fixture layout and (if possible) fixture packaging label.","Verify fixture size by comparing to grid ceiling as reference.",{"$nulls":4},{"v":25,"d":"$25.00"},"Fixture",{"v":25,"d":"$25.00"},"Fixture",{"v":20,"d":"$20.00"},"Fixture",3111,3111,3111,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR6=\"Agribusiness\", $AR6=\"Ag\",$AR6=\"Propane\", $AR6=\"Ag Propane\", $AR6=\"Ag-Propane\"),$AC6,  $AB6),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR6=\"Agribusiness\", $AR6=\"Ag\",$AR6=\"Propane\", $AR6=\"Ag Propane\", $AR6=\"Ag-Propane\"),$AC6,  $AB6),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L3400","L3400","N-L3400","2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","For 1-for-1 replacement of T12 or standard T8 fluorescent fixtures","Must be DLC TRT V5.0 or higher listed in the \"Troffer\" general application.","New fixture must consume ≤ 39W.","Other LED configurations may qualify for a custom incentive.",{"$nulls":6},"Provide clear photo(s) of: fixture layout and (if possible) fixture packaging label.","Verify fixture size by comparing to grid ceiling as reference.",{"$nulls":4},{"v":15,"d":"$15.00"},"Fixture",{"v":15,"d":"$15.00"},"Fixture",{"v":10,"d":"$10.00"},"Fixture",3400,3400,3400,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR7=\"Agribusiness\", $AR7=\"Ag\",$AR7=\"Propane\", $AR7=\"Ag Propane\", $AR7=\"Ag-Propane\"),$AC7,  $AB7),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR7=\"Agribusiness\", $AR7=\"Ag\",$AR7=\"Propane\", $AR7=\"Ag Propane\", $AR7=\"Ag-Propane\"),$AC7,  $AB7),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L3401","L3401","N-L3401","2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","For 1-for-1 replacement of T12 or standard T8 fluorescent fixtures","Must be DLC TRT V5.0 or higher listed in the \"Troffer\" general application.","New fixture must consume ≤ 85W.","2G11 base lamps replaced must have a nominal lamp wattage between 40-55 watts.","Other LED configurations may qualify for a custom incentive.",{"$nulls":5},"Provide clear photo(s) of: fixture layout and (if possible) fixture packaging label.","Verify fixture size by comparing to grid ceiling as reference.",{"$nulls":4},{"v":30,"d":"$30.00"},"Fixture",{"v":30,"d":"$30.00"},"Fixture",{"v":20,"d":"$20.00"},"Fixture",3401,3401,3401,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR8=\"Agribusiness\", $AR8=\"Ag\",$AR8=\"Propane\", $AR8=\"Ag Propane\", $AR8=\"Ag-Propane\"),$AC8,  $AB8),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR8=\"Agribusiness\", $AR8=\"Ag\",$AR8=\"Propane\", $AR8=\"Ag Propane\", $AR8=\"Ag-Propane\"),$AC8,  $AB8),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L10281","L10281","N-L10281","1’ to 3’ LED Linear Ambient Fixture, Interior","L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":6,"d":"$6.00"},"Fixture",{"v":6,"d":"$6.00"},"Fixture",{"v":4,"d":"$4.00"},"Fixture",10281,10281,{"$f":"AB9","v":10281},"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR9=\"Agribusiness\", $AR9=\"Ag\",$AR9=\"Propane\", $AR9=\"Ag Propane\", $AR9=\"Ag-Propane\"),$AC9,  $AB9),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR9=\"Agribusiness\", $AR9=\"Ag\",$AR9=\"Propane\", $AR9=\"Ag Propane\", $AR9=\"Ag-Propane\"),$AC9,  $AB9),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L10282","L10282","N-L10282","4' LED Linear Ambient Fixture, Interior","L10282: 4' LED Linear Ambient Fixture, Interior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":12,"d":"$12.00"},"Fixture",{"v":12,"d":"$12.00"},"Fixture",{"v":8,"d":"$8.00"},"Fixture",10282,10282,{"$f":"AB10","v":10282},"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10282: 4' LED Linear Ambient Fixture, Interior","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR10=\"Agribusiness\", $AR10=\"Ag\",$AR10=\"Propane\", $AR10=\"Ag Propane\", $AR10=\"Ag-Propane\"),$AC10,  $AB10),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR10=\"Agribusiness\", $AR10=\"Ag\",$AR10=\"Propane\", $AR10=\"Ag Propane\", $AR10=\"Ag-Propane\"),$AC10,  $AB10),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L10283","L10283","N-L10283","8' LED Linear Ambient Fixture, Interior","L10283: 8' LED Linear Ambient Fixture, Interior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":24,"d":"$24.00"},"Fixture",{"v":24,"d":"$24.00"},"Fixture",{"v":16,"d":"$16.00"},"Fixture",10283,10283,10283,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10283: 8' LED Linear Ambient Fixture, Interior","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR11=\"Agribusiness\", $AR11=\"Ag\",$AR11=\"Propane\", $AR11=\"Ag Propane\", $AR11=\"Ag-Propane\"),$AC11,  $AB11),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR11=\"Agribusiness\", $AR11=\"Ag\",$AR11=\"Propane\", $AR11=\"Ag Propane\", $AR11=\"Ag-Propane\"),$AC11,  $AB11),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L10284","L10284","N-L10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":6,"d":"$6.00"},"Fixture",{"v":6,"d":"$6.00"},"Fixture",{"v":4,"d":"$4.00"},"Fixture",10284,10284,10284,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR12=\"Agribusiness\", $AR12=\"Ag\",$AR12=\"Propane\", $AR12=\"Ag Propane\", $AR12=\"Ag-Propane\"),$AC12,  $AB12),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR12=\"Agribusiness\", $AR12=\"Ag\",$AR12=\"Propane\", $AR12=\"Ag Propane\", $AR12=\"Ag-Propane\"),$AC12,  $AB12),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L10285","L10285","N-L10285","4' LED Linear Ambient Fixture, Exterior","L10285: 4' LED Linear Ambient Fixture, Exterior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":12,"d":"$12.00"},"Fixture",{"v":12,"d":"$12.00"},"Fixture",{"v":8,"d":"$8.00"},"Fixture",10285,10285,10285,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10285: 4' LED Linear Ambient Fixture, Exterior","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR13=\"Agribusiness\", $AR13=\"Ag\",$AR13=\"Propane\", $AR13=\"Ag Propane\", $AR13=\"Ag-Propane\"),$AC13,  $AB13),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR13=\"Agribusiness\", $AR13=\"Ag\",$AR13=\"Propane\", $AR13=\"Ag Propane\", $AR13=\"Ag-Propane\"),$AC13,  $AB13),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L10286","L10286","N-L10286","8' LED Linear Ambient Fixture, Exterior","L10286: 8' LED Linear Ambient Fixture, Exterior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":24,"d":"$24.00"},"Fixture",{"v":24,"d":"$24.00"},"Fixture",{"v":16,"d":"$16.00"},"Fixture",10286,10286,10286,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10286: 8' LED Linear Ambient Fixture, Exterior","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR14=\"Agribusiness\", $AR14=\"Ag\",$AR14=\"Propane\", $AR14=\"Ag Propane\", $AR14=\"Ag-Propane\"),$AC14,  $AB14),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR14=\"Agribusiness\", $AR14=\"Ag\",$AR14=\"Propane\", $AR14=\"Ag Propane\", $AR14=\"Ag-Propane\"),$AC14,  $AB14),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",11]
["L10028","L10028","N-L10028","LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture",{"$f":"IF(ISBLANK(A15),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C15,IF(FOEIncentCodeType=IncentCodeTypeAg,B15,A15))&\": \") &D15","v":"L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"},"Fixture must be listed on ENERGY STAR as a “Downlight Recessed,” “Downlight Solid State Retrofit,” “Downlight Surface Mount,” \"Ceiling Mount,\" or \"LED Surface Mount Ceiling Retrofit\" fixture type and be intended for commercial use.","Fixtures that are intended for residential use may be used in multifamily buildings.","For replacement of incandescent, CFL or HID fixtures in interior applications.","Low voltage or decorative LED fixtures that do not meet the criteria below may be eligible for custom incentives.",{"$nulls":12},{"v":13,"d":"$13.00"},"Fixture",{"v":13,"d":"$13.00"},"Fixture",{"v":7,"d":"$7.00"},{"$f":"W15","v":"Fixture"},10028,{"$f":"AB15","v":10028},10028,"Yes",{"$f":"AE15","v":"Yes"},"Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A15),\"\",IF(A15<>\"Not Eligible\",A15,IF(B15<>\"Not Eligible\",B15,C15))&\": \") &D15","v":"L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"},"No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR15=\"Agribusiness\", $AR15=\"Ag\",$AR15=\"Propane\", $AR15=\"Ag Propane\", $AR15=\"Ag-Propane\"),$AC15,  $AB15),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR15=\"Agribusiness\", $AR15=\"Ag\",$AR15=\"Propane\", $AR15=\"Ag Propane\", $AR15=\"Ag-Propane\"),$AC15,  $AB15),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",12]
["L10029","L10029","N-L10029","LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior",{"$f":"IF(ISBLANK(A16),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C16,IF(FOEIncentCodeType=IncentCodeTypeAg,B16,A16))&\": \") &D16","v":"L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"},"For businesses, fixture must be listed on ENERGY STAR as a Downlight Recessed, Downlight Solid State Retrofit, …","... or Downlight Surface Mount fixture type and be intended for commercial use.","For multifamily buildings, must be listed on ENERGY STAR as a Downlight Recessed, Downlight Solid State Retrofit, or Downlight Surface Mount fixture type and be intended for commercial and/or residential use.","For replacement of incandescent, CFL or HID fixtures in exterior applications.",{"$nulls":12},{"v":20,"d":"$20.00"},"Fixture",{"v":20,"d":"$20.00"},"Fixture",{"v":10,"d":"$10.00"},{"$f":"W16","v":"Fixture"},10029,{"$f":"AB16","v":10029},10029,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A16),\"\",IF(A16<>\"Not Eligible\",A16,IF(B16<>\"Not Eligible\",B16,C16))&\": \") &D16","v":"L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"},"No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR16=\"Agribusiness\", $AR16=\"Ag\",$AR16=\"Propane\", $AR16=\"Ag Propane\", $AR16=\"Ag-Propane\"),$AC16,  $AB16),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR16=\"Agribusiness\", $AR16=\"Ag\",$AR16=\"Propane\", $AR16=\"Ag Propane\", $AR16=\"Ag-Propane\"),$AC16,  $AB16),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",12]
["L4813","L4813","N-L4813","LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture",{"$f":"IF(ISBLANK(A17),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C17,IF(FOEIncentCodeType=IncentCodeTypeAg,B17,A17))&\": \") &D17","v":"L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"},"Complete Table A of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Watts reduced calculation uses system wattage table on page 10 of Lighting Catalog for baseline inputs.","Fixture may be listed on ENERGY STAR and in a category not defined by linear ambient (pg. 10) or downlight (pg. 13) measures. ","Eligible fixtures may also be DLC TRT V5.0 or higher listed in either the \"Track or Mono-point Luminaires, or \"Wall-wash Luminaires\" primary use categories. Fixtures must be intended for commercial use.","Must be permanently wired fixtures and include housing, lens, heat sink, driver and light source.",{"$nulls":11},{"v":0.3,"d":"$0.30"},"Watt Reduced",{"v":0.3,"d":"$0.30"},"Watt Reduced",{"v":0.2,"d":"$0.20"},{"$f":"W17","v":"Watt Reduced"},4813,{"$f":"AB17","v":4813},4813,"Yes",{"$f":"AE17","v":"Yes"},"Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A17),\"\",IF(A17<>\"Not Eligible\",A17,IF(B17<>\"Not Eligible\",B17,C17))&\": \") &D17","v":"L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"},"No","Optional (yes if baseline watts not from input wattage table in lighting catalog)","Watts Reduced",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR17=\"Agribusiness\", $AR17=\"Ag\",$AR17=\"Propane\", $AR17=\"Ag Propane\", $AR17=\"Ag-Propane\"),$AC17,  $AB17),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR17=\"Agribusiness\", $AR17=\"Ag\",$AR17=\"Propane\", $AR17=\"Ag Propane\", $AR17=\"Ag-Propane\"),$AC17,  $AB17),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"Lighting",12]
["L3903","L3903","Not Eligible","Interior LED Signage",{"$f":"IF(ISBLANK(A18),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C18,IF(FOEIncentCodeType=IncentCodeTypeAg,B18,A18))&\": \") &D18","v":"L3903: Interior LED Signage"},"Applications include, but are not limited to, channel lettering, backlit displays and menu boards.","Signs illuminated by screw-in or pin-based lamps, track lights, or flood lights  should refer to the corresponding incentive.",{"$nulls":8},"Provide clear photo(s) of: fixture, fixture packaging label (if possible).","Verify sign is installed in interior application.","Verify whether retrofit is dedicated LED system or simply screw-in or pin-based replacement lamps.",{"$nulls":3},{"v":0.5,"d":"$0.50"},"Watt Installed",{"$f":"V18","v":{"v":0.5,"d":"$0.50"}},"Watt Installed","N/a","Watt Installed",3903,{"$f":"AB18","v":3903},3903,"No",{"$f":"AE18","v":"No"},"No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A18),\"\",IF(A18<>\"Not Eligible\",A18,IF(B18<>\"Not Eligible\",B18,C18))&\": \") &D18","v":"L3903: Interior LED Signage"},"No","Optional (if applied wattage does not match invoice)",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR18=\"Agribusiness\", $AR18=\"Ag\",$AR18=\"Propane\", $AR18=\"Ag Propane\", $AR18=\"Ag-Propane\"),$AC18,  $AB18),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR18=\"Agribusiness\", $AR18=\"Ag\",$AR18=\"Propane\", $AR18=\"Ag Propane\", $AR18=\"Ag-Propane\"),$AC18,  $AB18),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",12]
["L3904","L3904","Not Eligible","Exterior LED Signage",{"$f":"IF(ISBLANK(A19),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C19,IF(FOEIncentCodeType=IncentCodeTypeAg,B19,A19))&\": \") &D19","v":"L3904: Exterior LED Signage"},"Applications include, but are not limited to, channel lettering, backlit displays and menu boards.","Signs illuminated by screw-in or pin-based lamps, track lights, or flood lights  should refer to the corresponding incentive.",{"$nulls":8},"Provide photo(s) of: fixture, fixture packaging label (if possible).","Verify sign is installed in exterior application.","Verify whether retrofit is dedicated LED system or simply screw-in or pin-based replacement lamps.",{"$nulls":3},{"v":0.5,"d":"$0.50"},"Watt Installed",{"$f":"V19","v":{"v":0.5,"d":"$0.50"}},"Watt Installed","N/A","Watt Installed",3904,{"$f":"AB19","v":3904},3904,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3904: Exterior LED Signage","No","Optional (if applied wattage does not match invoice)",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR19=\"Agribusiness\", $AR19=\"Ag\",$AR19=\"Propane\", $AR19=\"Ag Propane\", $AR19=\"Ag-Propane\"),$AC19,  $AB19),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR19=\"Agribusiness\", $AR19=\"Ag\",$AR19=\"Propane\", $AR19=\"Ag Propane\", $AR19=\"Ag-Propane\"),$AC19,  $AB19),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",12]
["L3091","L3091","Not Eligible","≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID","L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 155W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive. Agriculture customers eligible for MMID AG4695.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":65,"d":"$65.00"},"Fixture",{"v":65,"d":"$65.00"},"Fixture","N/A","Fixture",3091,3091,3091,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR20=\"Agribusiness\", $AR20=\"Ag\",$AR20=\"Propane\", $AR20=\"Ag Propane\", $AR20=\"Ag-Propane\"),$AC20,  $AB20),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR20=\"Agribusiness\", $AR20=\"Ag\",$AR20=\"Propane\", $AR20=\"Ag Propane\", $AR20=\"Ag-Propane\"),$AC20,  $AB20),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L3092","L3092","Not Eligible","≤ 250W LED High Bay/Low Bay, instead of 320-399W HID","L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 250W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive. Agriculture customers eligible for MMID AG4696.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":75,"d":"$75.00"},"Fixture",{"v":75,"d":"$75.00"},"Fixture","N/A","Fixture",3092,3092,3092,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR21=\"Agribusiness\", $AR21=\"Ag\",$AR21=\"Propane\", $AR21=\"Ag Propane\", $AR21=\"Ag-Propane\"),$AC21,  $AB21),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR21=\"Agribusiness\", $AR21=\"Ag\",$AR21=\"Propane\", $AR21=\"Ag Propane\", $AR21=\"Ag-Propane\"),$AC21,  $AB21),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L3093","L3093","Not Eligible","≤ 250W LED High Bay/Low Bay, replacing 400W HID","L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 250W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive. Agriculture customers eligible for MMID AG4697.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":100,"d":"$100.00"},"Fixture",{"v":100,"d":"$100.00"},"Fixture","N/A","Fixture",3093,3093,3093,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR22=\"Agribusiness\", $AR22=\"Ag\",$AR22=\"Propane\", $AR22=\"Ag Propane\", $AR22=\"Ag-Propane\"),$AC22,  $AB22),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR22=\"Agribusiness\", $AR22=\"Ag\",$AR22=\"Propane\", $AR22=\"Ag Propane\", $AR22=\"Ag-Propane\"),$AC22,  $AB22),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L3094","L3094","Not Eligible","≤ 365W LED High Bay/Low Bay, replacing 400W HID","L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 365W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive. Agriculture customers eligible for MMID AG4698.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":65,"d":"$65.00"},"Fixture",{"v":65,"d":"$65.00"},"Fixture","N/A","Fixture",3094,3094,3094,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR23=\"Agribusiness\", $AR23=\"Ag\",$AR23=\"Propane\", $AR23=\"Ag Propane\", $AR23=\"Ag-Propane\"),$AC23,  $AB23),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR23=\"Agribusiness\", $AR23=\"Ag\",$AR23=\"Propane\", $AR23=\"Ag Propane\", $AR23=\"Ag-Propane\"),$AC23,  $AB23),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L3095","L3095","Not Eligible","≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID","L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","≤500W refers to LED total system watts and may consist of up to two fixtures replacing a single HID fixture.","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive. Agriculture customers eligible for MMID AG4699.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":175,"d":"$175.00"},"Fixture",{"v":175,"d":"$175.00"},"Fixture","N/A","Fixture",3095,3095,3095,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR24=\"Agribusiness\", $AR24=\"Ag\",$AR24=\"Propane\", $AR24=\"Ag Propane\", $AR24=\"Ag-Propane\"),$AC24,  $AB24),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR24=\"Agribusiness\", $AR24=\"Ag\",$AR24=\"Propane\", $AR24=\"Ag Propane\", $AR24=\"Ag-Propane\"),$AC24,  $AB24),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L3096","L3096","Not Eligible","≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID","L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","≤800W refers to LED total system watts and may consist of up to two fixtures replacing a single HID fixture.","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive. Agriculture customers eligible for MMID AG4700.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":125,"d":"$125.00"},"Fixture",{"v":125,"d":"$125.00"},"Fixture","N/A","Fixture",3096,3096,3096,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR25=\"Agribusiness\", $AR25=\"Ag\",$AR25=\"Propane\", $AR25=\"Ag Propane\", $AR25=\"Ag-Propane\"),$AC25,  $AB25),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR25=\"Agribusiness\", $AR25=\"Ag\",$AR25=\"Propane\", $AR25=\"Ag Propane\", $AR25=\"Ag-Propane\"),$AC25,  $AB25),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L5460","L5460","N-L5460","≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12",{"$f":"IF(ISBLANK(A26),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C26,IF(FOEIncentCodeType=IncentCodeTypeAg,B26,A26))&\": \") &D26","v":"L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"},"Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 85W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":4},"Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":20,"d":"$20.00"},"Fixture",{"$f":"V26","v":{"v":20,"d":"$20.00"}},{"$f":"W26","v":"Fixture"},{"v":13,"d":"$13.00"},"Fixture",5460,{"$f":"AB26","v":5460},5460,"Yes",{"$f":"AE26","v":"Yes"},"Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A26),\"\",IF(A26<>\"Not Eligible\",A26,IF(B26<>\"Not Eligible\",B26,C26))&\": \") &D26","v":"L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR26=\"Agribusiness\", $AR26=\"Ag\",$AR26=\"Propane\", $AR26=\"Ag Propane\", $AR26=\"Ag-Propane\"),$AC26,  $AB26),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR26=\"Agribusiness\", $AR26=\"Ag\",$AR26=\"Propane\", $AR26=\"Ag Propane\", $AR26=\"Ag-Propane\"),$AC26,  $AB26),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L5461","L5461","Not Eligible","≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO",{"$f":"IF(ISBLANK(A27),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C27,IF(FOEIncentCodeType=IncentCodeTypeAg,B27,A27))&\": \") &D27","v":"L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO"},"Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 125W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":4},"Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":50,"d":"$50.00"},"Fixture",{"$f":"V27","v":{"v":50,"d":"$50.00"}},{"$f":"W27","v":"Fixture"},"N/A","Fixture",5461,{"$f":"AB27","v":5461},5461,"No",{"$f":"AE27","v":"No"},{"$f":"AF27","v":"No"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A27),\"\",IF(A27<>\"Not Eligible\",A27,IF(B27<>\"Not Eligible\",B27,C27))&\": \") &D27","v":"L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR27=\"Agribusiness\", $AR27=\"Ag\",$AR27=\"Propane\", $AR27=\"Ag Propane\", $AR27=\"Ag-Propane\"),$AC27,  $AB27),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR27=\"Agribusiness\", $AR27=\"Ag\",$AR27=\"Propane\", $AR27=\"Ag Propane\", $AR27=\"Ag-Propane\"),$AC27,  $AB27),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L3393","L3393","N-L3393","≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO","L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 180W.  ","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive. Agriculture customers eligible for MMID AG4701.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":50,"d":"$50.00"},"Fixture",{"v":50,"d":"$50.00"},"Fixture",{"v":30,"d":"$30.00"},"Fixture",3393,3393,3393,"Yes",{"$f":"AE28","v":"Yes"},"Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR28=\"Agribusiness\", $AR28=\"Ag\",$AR28=\"Propane\", $AR28=\"Ag Propane\", $AR28=\"Ag-Propane\"),$AC28,  $AB28),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR28=\"Agribusiness\", $AR28=\"Ag\",$AR28=\"Propane\", $AR28=\"Ag Propane\", $AR28=\"Ag-Propane\"),$AC28,  $AB28),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L4347","L4347","N-L4347","≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO","L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 250W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive. Agriculture customers eligible for MMID AG4702.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":75,"d":"$75.00"},"Fixture",{"v":75,"d":"$75.00"},"Fixture",{"v":50,"d":"$50.00"},"Fixture",4347,4347,4347,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR29=\"Agribusiness\", $AR29=\"Ag\",$AR29=\"Propane\", $AR29=\"Ag Propane\", $AR29=\"Ag-Propane\"),$AC29,  $AB29),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR29=\"Agribusiness\", $AR29=\"Ag\",$AR29=\"Propane\", $AR29=\"Ag Propane\", $AR29=\"Ag-Propane\"),$AC29,  $AB29),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L4795","L4795","N-L4795","≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO","L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 300W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":120,"d":"$120.00"},"Fixture",{"v":120,"d":"$120.00"},"Fixture",{"v":65,"d":"$65.00"},"Fixture",4795,4795,4795,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR30=\"Agribusiness\", $AR30=\"Ag\",$AR30=\"Propane\", $AR30=\"Ag Propane\", $AR30=\"Ag-Propane\"),$AC30,  $AB30),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR30=\"Agribusiness\", $AR30=\"Ag\",$AR30=\"Propane\", $AR30=\"Ag Propane\", $AR30=\"Ag-Propane\"),$AC30,  $AB30),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L4796","L4796","N-L4796","≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO","L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO","Retrofit products must be listed on the DLC TRT V5.0 or higher qualified product list under the High-Bay or Low-Bay General Application and be permanently wired or applicable cord and plug.","New fixtures must be DLC TRT V5.0 or higher listed under the High-Bay or Low-Bay General Application. ","Fixture must consume ≤ 350W","Integral ballast screw-based retrofit products are not eligible. Refer to page 18 for High/Low-Bay Mogul Screw-base (E39) LED lamps.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general category,... ","\"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" PUD, if they provide sufficient lighting and meet wattage requirements.",{"$nulls":3},"Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","Provide clear photo(s) of: fixture, sensor (if applicable), fixture packaging label (if possible).","Verify fixture is dedicated LED and not a replacement, screw-in lamp.",{"$nulls":4},{"v":170,"d":"$170.00"},"Fixture",{"v":170,"d":"$170.00"},"Fixture",{"v":90,"d":"$90.00"},"Fixture",4796,4796,4796,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR31=\"Agribusiness\", $AR31=\"Ag\",$AR31=\"Propane\", $AR31=\"Ag Propane\", $AR31=\"Ag-Propane\"),$AC31,  $AB31),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR31=\"Agribusiness\", $AR31=\"Ag\",$AR31=\"Propane\", $AR31=\"Ag Propane\", $AR31=\"Ag-Propane\"),$AC31,  $AB31),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",13]
["L4280","L4280","N-L4280","Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",{"$f":"IF(ISBLANK(A32),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C32,IF(FOEIncentCodeType=IncentCodeTypeAg,B32,A32))&\": \") &D32","v":"L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"},"Must be DLC SSL QPL listed (TRT V5.0 or higher) in an “Outdoor” General Application Category.","Must be permanently wired. Integral ballast screw-based lamp retrofit products of any technology are not eligible.","Stadium lighting is not eligible for prescriptive incentives.  Contact your Energy Advisor to determine eligibility for a custom incentive.","Customers applying for municipal roadway lighting MUST submit a copy of utililty bill verifying customer is on a utility rate for customer owned street lights. Utility owned street lights are not eligible for incentives.","For interior stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","**Ignore lumen levels in measure name.  Use DLC category to qualify equipment**","Fixtures equipped with light shields are eligible if the equivalent shieldless fixture is DLC listed.",{"$nulls":9},{"v":30,"d":"$30.00"},"Fixture",{"$f":"V32","v":{"v":30,"d":"$30.00"}},"Fixture",{"v":20,"d":"$20.00"},{"$f":"W32","v":"Fixture"},4280,{"$f":"AB32","v":4280},4280,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A32),\"\",IF(A32<>\"Not Eligible\",A32,IF(B32<>\"Not Eligible\",B32,C32))&\": \") &D32","v":"L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR32=\"Agribusiness\", $AR32=\"Ag\",$AR32=\"Propane\", $AR32=\"Ag Propane\", $AR32=\"Ag-Propane\"),$AC32,  $AB32),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR32=\"Agribusiness\", $AR32=\"Ag\",$AR32=\"Propane\", $AR32=\"Ag Propane\", $AR32=\"Ag-Propane\"),$AC32,  $AB32),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",14]
["L4281","L4281","N-L4281","Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens","Must be DLC SSL QPL listed (TRT V5.0 or higher) in an “Outdoor” General Application Category.","Must be permanently wired. Integral ballast screw-based lamp retrofit products of any technology are not eligible.","Stadium lighting is not eligible for prescriptive incentives.  Contact your Energy Advisor to determine eligibility for a custom incentive.","Customers applying for municipal roadway lighting MUST submit a copy of utililty bill verifying customer is on a utility rate for customer owned street lights. Utility owned street lights are not eligible for incentives.","For interior stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","**Ignore lumen levels in measure name.  Use DLC category to qualify equipment**","Fixtures equipped with light shields are eligible if the equivalent shieldless fixture is DLC listed.",{"$nulls":9},{"v":55,"d":"$55.00"},"Fixture",{"v":55,"d":"$55.00"},"Fixture",{"v":35,"d":"$35.00"},{"$f":"W33","v":"Fixture"},4281,{"$f":"AB33","v":4281},4281,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A33),\"\",IF(A33<>\"Not Eligible\",A33,IF(B33<>\"Not Eligible\",B33,C33))&\": \") &D33","v":"L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR33=\"Agribusiness\", $AR33=\"Ag\",$AR33=\"Propane\", $AR33=\"Ag Propane\", $AR33=\"Ag-Propane\"),$AC33,  $AB33),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR33=\"Agribusiness\", $AR33=\"Ag\",$AR33=\"Propane\", $AR33=\"Ag Propane\", $AR33=\"Ag-Propane\"),$AC33,  $AB33),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",14]
["L4282","L4282","N-L4282","Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens","Must be DLC SSL QPL listed (TRT V5.0 or higher) in an “Outdoor” General Application Category.","Must be permanently wired. Integral ballast screw-based lamp retrofit products of any technology are not eligible.","Stadium lighting is not eligible for prescriptive incentives.  Contact your Energy Advisor to determine eligibility for a custom incentive.","Customers applying for municipal roadway lighting MUST submit a copy of utililty bill verifying customer is on a utility rate for customer owned street lights. Utility owned street lights are not eligible for incentives.","For interior stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","**Ignore lumen levels in measure name.  Use DLC category to qualify equipment**","Fixtures equipped with light shields are eligible if the equivalent shieldless fixture is DLC listed.",{"$nulls":9},{"v":100,"d":"$100.00"},"Fixture",{"v":100,"d":"$100.00"},"Fixture",{"v":90,"d":"$90.00"},{"$f":"W34","v":"Fixture"},4282,{"$f":"AB34","v":4282},4282,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A34),\"\",IF(A34<>\"Not Eligible\",A34,IF(B34<>\"Not Eligible\",B34,C34))&\": \") &D34","v":"L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR34=\"Agribusiness\", $AR34=\"Ag\",$AR34=\"Propane\", $AR34=\"Ag Propane\", $AR34=\"Ag-Propane\"),$AC34,  $AB34),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR34=\"Agribusiness\", $AR34=\"Ag\",$AR34=\"Propane\", $AR34=\"Ag Propane\", $AR34=\"Ag-Propane\"),$AC34,  $AB34),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",14]
["L4283","L4283","N-L4283","Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens","Must be DLC SSL QPL listed (TRT V5.0 or higher) in an “Outdoor” General Application Category.","Must be permanently wired. Integral ballast screw-based lamp retrofit products of any technology are not eligible.","Stadium lighting is not eligible for prescriptive incentives.  Contact your Energy Advisor to determine eligibility for a custom incentive.","Customers applying for municipal roadway lighting MUST submit a copy of utililty bill verifying customer is on a utility rate for customer owned street lights. Utility owned street lights are not eligible for incentives.","For interior stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","**Ignore lumen levels in measure name.  Use DLC category to qualify equipment**","Fixtures equipped with light shields are eligible if the equivalent shieldless fixture is DLC listed.",{"$nulls":9},{"v":250,"d":"$250.00"},"Fixture",{"v":250,"d":"$250.00"},"Fixture",{"v":200,"d":"$200.00"},{"$f":"W35","v":"Fixture"},4283,{"$f":"AB35","v":4283},4283,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A35),\"\",IF(A35<>\"Not Eligible\",A35,IF(B35<>\"Not Eligible\",B35,C35))&\": \") &D35","v":"L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR35=\"Agribusiness\", $AR35=\"Ag\",$AR35=\"Propane\", $AR35=\"Ag Propane\", $AR35=\"Ag-Propane\"),$AC35,  $AB35),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR35=\"Agribusiness\", $AR35=\"Ag\",$AR35=\"Propane\", $AR35=\"Ag Propane\", $AR35=\"Ag-Propane\"),$AC35,  $AB35),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",14]
[{"$nulls":3},"----------------------LIGHTING CATALOG: LED LAMPS----------------------------","----------------------LIGHTING CATALOG: LED LAMPS----------------------------",{"$nulls":32},{"$f":"IF(ISBLANK(A36),\"\",IF(A36<>\"Not Eligible\",A36,IF(B36<>\"Not Eligible\",B36,C36))&\": \") &D36","v":"----------------------LIGHTING CATALOG: LED LAMPS----------------------------"},null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR36=\"Agribusiness\", $AR36=\"Ag\",$AR36=\"Propane\", $AR36=\"Ag Propane\", $AR36=\"Ag-Propane\"),$AC36,  $AB36),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR36=\"Agribusiness\", $AR36=\"Ag\",$AR36=\"Propane\", $AR36=\"Ag Propane\", $AR36=\"Ag-Propane\"),$AC36,  $AB36),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["L10042","L10042","Not Eligible","DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID",{"$f":"IF(ISBLANK(A37),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C37,IF(FOEIncentCodeType=IncentCodeTypeAg,B37,A37))&\": \") &D37","v":"L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID"},"Must be DLC TRT V5.0 or higher in the \"Mogul (E39) Screw-Base Reaplcements for HID Lamps\" category.","Interior medium screw-base (E26) lamps may be eligible if E39 option is DLC listed. Contact Focus on Energy for assistance.","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":7},"lighting layout, close-up of lamp, lamp model number (if available)","Provide clear photo(s) of: lamp(s) and lamp packaging label (if possible).","Verify lamp is installed in high/low-bay fixture.",{"$nulls":3},{"v":30,"d":"$30.00"},"Lamp",{"$f":"V37","v":{"v":30,"d":"$30.00"}},"Lamp","N/A",{"$f":"W37","v":"Lamp"},10042,{"$f":"AB37","v":10042},10042,"No",{"$f":"AE37","v":"No"},"No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR37=\"Agribusiness\", $AR37=\"Ag\",$AR37=\"Propane\", $AR37=\"Ag Propane\", $AR37=\"Ag-Propane\"),$AC37,  $AB37),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR37=\"Agribusiness\", $AR37=\"Ag\",$AR37=\"Propane\", $AR37=\"Ag Propane\", $AR37=\"Ag-Propane\"),$AC37,  $AB37),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L10043","L10043","Not Eligible","DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior","L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior","Must be DLC TRT V5.0 or higher in the \"Mogul (E39) Screw-Base Reaplcements for HID Lamps\" category.","Interior medium screw-base (E26) lamps may be eligible if E39 option is DLC listed. Contact Focus on Energy for assistance.","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":7},"Provide photo(s) of: lamp, lamp packaging label (if possible).","Verify lamp is installed in DLC-listed application.",{"$nulls":4},{"v":30,"d":"$30.00"},"Lamp",{"v":30,"d":"$30.00"},"Lamp","N/A","Lamp",10043,10043,10043,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR38=\"Agribusiness\", $AR38=\"Ag\",$AR38=\"Propane\", $AR38=\"Ag Propane\", $AR38=\"Ag-Propane\"),$AC38,  $AB38),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR38=\"Agribusiness\", $AR38=\"Ag\",$AR38=\"Propane\", $AR38=\"Ag Propane\", $AR38=\"Ag-Propane\"),$AC38,  $AB38),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L10039","L10039","Not Eligible","Four-pin base LED Lamp Replacing CFL","L10039: Four-pin base LED Lamp Replacing CFL","Must be DLC TRT V5.0 or higher in the \"Four Pin-Base Replacement Lamps for CFLs\" category.","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":8},"lighting layout, close-up of lamp, lamp model number (if available)","Provide clear photo(s) of: lamp(s) and lamp packaging label (if possible).",{"$nulls":4},{"v":5,"d":"$5.00"},"Lamp",{"v":5,"d":"$5.00"},"Lamp","N/A","Lamp",10039,10039,10039,"No",{"$f":"AE39","v":"No"},"No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L10039: Four-pin base LED Lamp Replacing CFL","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR39=\"Agribusiness\", $AR39=\"Ag\",$AR39=\"Propane\", $AR39=\"Ag Propane\", $AR39=\"Ag-Propane\"),$AC39,  $AB39),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR39=\"Agribusiness\", $AR39=\"Ag\",$AR39=\"Propane\", $AR39=\"Ag Propane\", $AR39=\"Ag-Propane\"),$AC39,  $AB39),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L10040","L10040","Not Eligible","Four-pin base LED Lamp Replacing CFL, Exterior","L10040: Four-pin base LED Lamp Replacing CFL, Exterior","Must be DLC TRT V5.0 or higher in the \"Four Pin-Base Replacement Lamps for CFLs\" category.","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":8},"lighting layout, close-up of lamp, lamp model number (if available)","Provide clear photo(s) of: lamp(s) and lamp packaging label (if possible).",{"$nulls":4},{"v":5,"d":"$5.00"},"Lamp",{"v":5,"d":"$5.00"},"Lamp","N/A","Lamp",10040,10040,10040,"No",{"$f":"AE40","v":"No"},"No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L10040: Four-pin base LED Lamp Replacing CFL, Exterior","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR40=\"Agribusiness\", $AR40=\"Ag\",$AR40=\"Propane\", $AR40=\"Ag Propane\", $AR40=\"Ag-Propane\"),$AC40,  $AB40),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR40=\"Agribusiness\", $AR40=\"Ag\",$AR40=\"Propane\", $AR40=\"Ag Propane\", $AR40=\"Ag-Propane\"),$AC40,  $AB40),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L5451","L5451","Not Eligible","4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp","L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)","Measures can be used for 8' retrofit products.  Apply for the corresponding quantity installed.",{"$nulls":5},"Provide clear photo(s): of lamp, lamp packaging label (if possible).","Verify lamp is 4ft in length or is a U-Bend",null,"Verify lamp installed matches spec sheets, invoicing, and QPL provided.",null,null,{"v":3.25,"d":"$3.25"},"Lamp",{"v":1.5,"d":"$1.50"},"Lamp","N/A","Lamp",5451,5451,5451,"No",{"$f":"AE41","v":"No"},"No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR41=\"Agribusiness\", $AR41=\"Ag\",$AR41=\"Propane\", $AR41=\"Ag Propane\", $AR41=\"Ag-Propane\"),$AC41,  $AB41),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR41=\"Agribusiness\", $AR41=\"Ag\",$AR41=\"Propane\", $AR41=\"Ag Propane\", $AR41=\"Ag-Propane\"),$AC41,  $AB41),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L5452","L5452","Not Eligible","4' TLED, replacing 4' T5HO Lamp","L5452: 4' TLED, replacing 4' T5HO Lamp","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)","Measures can be used for 8' retrofit products.  Apply for the corresponding quantity installed.",{"$nulls":5},"Provide clear photo(s): of lamp, lamp packaging label (if possible).",{"$nulls":5},{"v":7,"d":"$7.00"},"Lamp",{"v":3,"d":"$3.00"},"Lamp","N/A","Lamp",5452,5452,5452,"No",{"$f":"AE42","v":"No"},"No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5452: 4' TLED, replacing 4' T5HO Lamp","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR42=\"Agribusiness\", $AR42=\"Ag\",$AR42=\"Propane\", $AR42=\"Ag Propane\", $AR42=\"Ag-Propane\"),$AC42,  $AB42),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR42=\"Agribusiness\", $AR42=\"Ag\",$AR42=\"Propane\", $AR42=\"Ag Propane\", $AR42=\"Ag-Propane\"),$AC42,  $AB42),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L5453","L4797","Not Eligible","2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp","L4797: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":6},"Provide clear photo(s): of lamp, lamp packaging label (if possible).","Verify lamp is 2ft in length.",{"$nulls":4},{"v":2.75,"d":"$2.75"},"Lamp",{"v":1.25,"d":"$1.25"},"Lamp","N/A","Lamp",5453,5453,5453,"No",{"$f":"AE43","v":"No"},"No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR43=\"Agribusiness\", $AR43=\"Ag\",$AR43=\"Propane\", $AR43=\"Ag Propane\", $AR43=\"Ag-Propane\"),$AC43,  $AB43),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR43=\"Agribusiness\", $AR43=\"Ag\",$AR43=\"Propane\", $AR43=\"Ag Propane\", $AR43=\"Ag-Propane\"),$AC43,  $AB43),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L5454","L4809","Not Eligible","8' TLED, replacing 8' T8 or T12 Lamp","L4809: 8' TLED, replacing 8' T8 or T12 Lamp","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":6},"Provide clear photo(s): of lamp, lamp packaging label (if possible).","Verify lamp is 8ft in length.",{"$nulls":4},{"v":7,"d":"$7.00"},"Lamp",{"v":3,"d":"$3.00"},"Lamp","N/A","Lamp",5454,5454,5454,"No",{"$f":"AE44","v":"No"},"No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5454: 8' TLED, replacing 8' T8 or T12 Lamp","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR44=\"Agribusiness\", $AR44=\"Ag\",$AR44=\"Propane\", $AR44=\"Ag Propane\", $AR44=\"Ag-Propane\"),$AC44,  $AB44),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR44=\"Agribusiness\", $AR44=\"Ag\",$AR44=\"Propane\", $AR44=\"Ag Propane\", $AR44=\"Ag-Propane\"),$AC44,  $AB44),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L5456","L5456","Not Eligible","4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior","L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)","Measures can be used for 8' retrofit products.  Apply for the corresponding quantity installed.",{"$nulls":5},"Provide clear photo(s): of lamp, lamp packaging label (if possible).",{"$nulls":5},{"v":3.25,"d":"$3.25"},"Lamp",{"$f":"V45","v":{"v":3.25,"d":"$3.25"}},"Lamp","N/A","Lamp",5456,5456,5456,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR45=\"Agribusiness\", $AR45=\"Ag\",$AR45=\"Propane\", $AR45=\"Ag Propane\", $AR45=\"Ag-Propane\"),$AC45,  $AB45),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR45=\"Agribusiness\", $AR45=\"Ag\",$AR45=\"Propane\", $AR45=\"Ag Propane\", $AR45=\"Ag-Propane\"),$AC45,  $AB45),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
["L5458","L5458","Not Eligible","8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior","L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":6},"Provide clear photo(s): of lamp, lamp packaging label (if possible).",{"$nulls":5},{"v":7,"d":"$7.00"},"Lamp",{"$f":"V46","v":{"v":7,"d":"$7.00"}},"Lamp","N/A","Lamp",5458,5458,5458,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR46=\"Agribusiness\", $AR46=\"Ag\",$AR46=\"Propane\", $AR46=\"Ag Propane\", $AR46=\"Ag-Propane\"),$AC46,  $AB46),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR46=\"Agribusiness\", $AR46=\"Ag\",$AR46=\"Propane\", $AR46=\"Ag Propane\", $AR46=\"Ag-Propane\"),$AC46,  $AB46),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",15]
[{"$nulls":3},"----------------------LIGHTING CATALOG: CONTROLS----------------------------",{"$f":"IF(ISBLANK(A47),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C47,IF(FOEIncentCodeType=IncentCodeTypeAg,B47,A47))&\": \") &D47","v":"----------------------LIGHTING CATALOG: CONTROLS----------------------------"},{"$nulls":25},"No","No","No",{"$nulls":4},"----------------------LIGHTING CATALOG: CONTROLS----------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR47=\"Agribusiness\", $AR47=\"Ag\",$AR47=\"Propane\", $AR47=\"Ag Propane\", $AR47=\"Ag-Propane\"),$AC47,  $AB47),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR47=\"Agribusiness\", $AR47=\"Ag\",$AR47=\"Propane\", $AR47=\"Ag Propane\", $AR47=\"Ag-Propane\"),$AC47,  $AB47),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting"]
["L10223","L10223","N-L10223","Advanced Lighting Controls, Interior","L10223: Advanced Lighting Controls, Interior","Installation of NLC or LLLC not otherwise specified in catalog. ","NLC systems must be DLC NLC QPL (NLC5 or higher) with the following capabilities setup and operational for individual fixturesL","Occupancy sensing, zoning, and individual addressability","Measure cannot be commbined with other controls meaures.","Complete Table B of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Control costs should be itemized separately on invoice",{"$nulls":4},"Provide clear photo of sensor(s) and controller (if possible).","If customer is comfortable with software, may be able to demonstrate functionalities.",{"$nulls":4},{"v":15,"d":"$15.00"},"Fixture Controlled",{"v":15,"d":"$15.00"},"Fixture Controlled",{"v":10,"d":"$10.00"},"Fixture Controlled",10223,{"$f":"AB48","v":10223},10223,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10223: Advanced Lighting Controls, Interior","No","Yes","Watt Controlled",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR48=\"Agribusiness\", $AR48=\"Ag\",$AR48=\"Propane\", $AR48=\"Ag Propane\", $AR48=\"Ag-Propane\"),$AC48,  $AB48),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR48=\"Agribusiness\", $AR48=\"Ag\",$AR48=\"Propane\", $AR48=\"Ag Propane\", $AR48=\"Ag-Propane\"),$AC48,  $AB48),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Lighting",16]
["L10224","L10224","N-L10224","Advanced Lighting Controls, Exterior","L10224: Advanced Lighting Controls, Exterior","Installation of NLC or LLLC not otherwise specified in catalog. ","NLC systems must be DLC NLC QPL (NLC5 or higher) with the following capabilities setup and operational for individual fixturesL","Occupancy sensing, zoning, and individual addressability","Measure cannot be commbined with other controls meaures.","Complete Table B of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Control costs should be itemized separately on invoice",{"$nulls":4},"Provide clear photo of sensor(s) and controller (if possible).","If customer is comfortable with software, may be able to demonstrate functionalities.",{"$nulls":4},{"v":15,"d":"$15.00"},"Fixture Controlled",{"v":15,"d":"$15.00"},"Fixture Controlled",{"v":10,"d":"$10.00"},"Fixture Controlled",10224,10224,10224,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10224: Advanced Lighting Controls, Exterior","No","Yes","Watt Controlled",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR49=\"Agribusiness\", $AR49=\"Ag\",$AR49=\"Propane\", $AR49=\"Ag Propane\", $AR49=\"Ag-Propane\"),$AC49,  $AB49),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR49=\"Agribusiness\", $AR49=\"Ag\",$AR49=\"Propane\", $AR49=\"Ag Propane\", $AR49=\"Ag-Propane\"),$AC49,  $AB49),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Lighting",16]
["L10432","L10432","N-L10432","ANSI Controls System Configuration Report",{"$f":"IF(ISBLANK(A50),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C50,IF(FOEIncentCodeType=IncentCodeTypeAg,B50,A50))&\": \") &D50","v":"L10432: ANSI Controls System Configuration Report"},"Must be submitted along with Advanced Lighting Controls measures.",{"$nulls":9},"Provide clear photo of sensor(s) and controller (if possible).","If customer is comfortable with software, may be able to demonstrate functionalities.",{"$nulls":4},{"v":500,"d":"$500.00"},"Report",{"v":500,"d":"$500.00"},"Report",{"v":500,"d":"$500.00"},"Report",10225,10225,10225,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10432: ANSI Controls System Configuration Report","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR50=\"Agribusiness\", $AR50=\"Ag\",$AR50=\"Propane\", $AR50=\"Ag Propane\", $AR50=\"Ag-Propane\"),$AC50,  $AB50),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR50=\"Agribusiness\", $AR50=\"Ag\",$AR50=\"Propane\", $AR50=\"Ag Propane\", $AR50=\"Ag-Propane\"),$AC50,  $AB50),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting",16]
["L10431","L10431","Not Eligible","Standard Lighting Controls, Interior","L10431: Standard Lighting Controls, Interior","For Occupancy and Interior Bi-level Controls: Must be ultrasonic, infrared, microwave, or dual technology. Socket-based DNQ.","For Daylighting Controls: Must be step dimmed with at least one level in addition to full power and off or continuous dimming.","Controls using both Occupancy and Daylighting should apply for L10223.","For retrofit situations where spec sheets aren't available for existing fixtures, program default wattages will be used for calculating incentives. Reference Default Wattage Table or contact Tech Lead to obtain a system not listed.","Complete Table B of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Control costs should be itemized separately on invoice",{"$nulls":4},"Provide clear photo of sensor(s) (if possible).","Verify timers are NOT being used for prescriptive measures.",{"$nulls":4},{"v":5,"d":"$5.00"},"Fixture Controlled",{"$f":"V51","v":{"v":5,"d":"$5.00"}},"Fixture Controlled","N/A",{"$f":"W51","v":"Fixture Controlled"},10431,10431,10431,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10431: Standard Lighting Controls, Interior","No","Yes","Watt Controlled",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR51=\"Agribusiness\", $AR51=\"Ag\",$AR51=\"Propane\", $AR51=\"Ag Propane\", $AR51=\"Ag-Propane\"),$AC51,  $AB51),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR51=\"Agribusiness\", $AR51=\"Ag\",$AR51=\"Propane\", $AR51=\"Ag Propane\", $AR51=\"Ag-Propane\"),$AC51,  $AB51),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Lighting",16]
["L10430","L10430","Not Eligible","Standard Lighting Controls, Exterior","L10430: Standard Lighting Controls, Exterior","Eligible for parking garage or stairwells.  High quantities in non-parking garages sould be reviewed thoroughly.","If PIR and/or ultrasonic technology are used, must fail in \"on\" position.","Fixtures must operate in low-standy light levels during low occupancy periods; cannot exceed 50% during unoccupied.","For retrofit situations where spec sheets aren't available for existing fixtures, program default wattages will be used for calculating incentives. Reference Default Wattage Table or contact Tech Lead to obtain a system not listed.","Complete Table B of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Control costs should be itemized separately on invoice",{"$nulls":4},"Provide clear photo of sensor(s) (if possible).","Verify timers are NOT being used for prescriptive measures.",{"$nulls":4},{"v":5,"d":"$5.00"},"Fixture Controlled",{"v":5,"d":"$5.00"},"Fixture Controlled","N/A","Fixture Controlled",10430,10430,10430,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10430: Standard Lighting Controls, Exterior","No","Yes","Watt Controlled",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR52=\"Agribusiness\", $AR52=\"Ag\",$AR52=\"Propane\", $AR52=\"Ag Propane\", $AR52=\"Ag-Propane\"),$AC52,  $AB52),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR52=\"Agribusiness\", $AR52=\"Ag\",$AR52=\"Propane\", $AR52=\"Ag Propane\", $AR52=\"Ag-Propane\"),$AC52,  $AB52),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Lighting",16]
[{"$nulls":3},"----------------------LIGHTING CATALOG: OTHER LIGHTING SOLUTIONS----------------------------",{"$f":"IF(ISBLANK(A53),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C53,IF(FOEIncentCodeType=IncentCodeTypeAg,B53,A53))&\": \") &D53","v":"----------------------LIGHTING CATALOG: OTHER LIGHTING SOLUTIONS----------------------------"},{"$nulls":32},"----------------------LIGHTING CATALOG: OTHER LIGHTING SOLUTIONS----------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR53=\"Agribusiness\", $AR53=\"Ag\",$AR53=\"Propane\", $AR53=\"Ag Propane\", $AR53=\"Ag-Propane\"),$AC53,  $AB53),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR53=\"Agribusiness\", $AR53=\"Ag\",$AR53=\"Propane\", $AR53=\"Ag Propane\", $AR53=\"Ag-Propane\"),$AC53,  $AB53),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Lighting"]
["Eligible under NC","Eligible under NC","N-L4948","Lighting Power Density (LPD) better than code requirements",{"$f":"IF(ISBLANK(A54),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C54,IF(FOEIncentCodeType=IncentCodeTypeAg,B54,A54))&\": \") &D54","v":"Eligible under NC: Lighting Power Density (LPD) better than code requirements"},"Complete LPD workbook submitted.","Incentives are based on current Wisconsin Energy Code (IECC 2021 with WI Amendments found in SPS Chapter 363) LPD requirements. ","Lighting levels should meet the current IESNA recommendations for delivered light level and uniformity. ","Incentive is for interior lighting only.","Upon completion, must include documentation to verify total connected wattage as-built (COMcheck or professional lighting layout indicating where fixtures are installed PLUS fixture cut sheets for all installed fixtures)","Ok to reference spec sheet, DLC (reported or tested), or ES wattage.","Ok to include exit light wattage if already part of COMcheck - don't need to pull it out and recalculate LPD. Do not include exit lights if creating COMcheck/workbook.","Wisconsin Adendums references IECC 2015 requirements",null,null,"Verify COMcheck/layout/others are accurate as-built.  Ask if anything differs from submitted documents.",{"$nulls":5},"N/A","kWh Reduced","N/A",{"$f":"W54","v":"kWh Reduced"},{"v":0.05,"d":"$0.05"},{"$f":"W54","v":"kWh Reduced"},4948,{"$f":"AB54","v":4948},4948,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","Eligible under NC: Lighting Power Density (LPD) better than code requirements","Yes","Yes","kWh below code",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR54=\"Agribusiness\", $AR54=\"Ag\",$AR54=\"Propane\", $AR54=\"Ag Propane\", $AR54=\"Ag-Propane\"),$AC54,  $AB54),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR54=\"Agribusiness\", $AR54=\"Ag\",$AR54=\"Propane\", $AR54=\"Ag Propane\", $AR54=\"Ag-Propane\"),$AC54,  $AB54),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":10000000,"d":"10,000,000.00"}},"Lighting",17]
["R5235","R5235","N-R5235","Refrigeration Savings for Lighting Upgrades in Freezers","R5235: Refrigeration Savings for Lighting Upgrades in Freezers","Complete Table A of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","For refrigerated warehouse spaces only. Walk-in coolers and freezers are not eligible. ","Only heat load reduction due to lighting upgrade from HID or fluorescent fixtures to LED fixtures are eligible. Lighting upgrade limited to fixtures that are eligible for the high and low bay measures on page 12 and the linear ambient measures on page 11.","Refrigeration savings measure must be submitted at the same time the incentive application for the lighting upgrade is submitted","Lamp only lighting upgrades are not eligible.","Freezer space is defined as having evaporator temperatures from -25 to 15°F.","Not for standard air-conditioned spaces or refrigerated spaces with evaporator temperatures above 35°F.","Watts reduced is fixture wattage reduction only; do not include additional wattage reduction for occupancy sensors (if installed).","For new construction, baseline determined by multiplying installed fixture wattage 2x.",null,"Verify quantities of respective 1-for-1 measures.",{"$nulls":5},{"v":0.2,"d":"$0.20"},"Watt Reduced",{"$f":"V55","v":{"v":0.2,"d":"$0.20"}},{"$f":"W55","v":"Watt Reduced"},{"v":0.15,"d":"$0.15"},{"$f":"W55","v":"Watt Reduced"},5235,5235,5235,"Yes",{"$f":"AE55","v":"Yes"},"Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A55),\"\",IF(A55<>\"Not Eligible\",A55,IF(B55<>\"Not Eligible\",B55,C55))&\": \") &D55","v":"R5235: Refrigeration Savings for Lighting Upgrades in Freezers"},"No","Yes","Watt Reduced",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR55=\"Agribusiness\", $AR55=\"Ag\",$AR55=\"Propane\", $AR55=\"Ag Propane\", $AR55=\"Ag-Propane\"),$AC55,  $AB55),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR55=\"Agribusiness\", $AR55=\"Ag\",$AR55=\"Propane\", $AR55=\"Ag Propane\", $AR55=\"Ag-Propane\"),$AC55,  $AB55),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":60000,"d":"60,000.00"}},"Lighting",18]
["R5236","R5236","N-R5236","Refrigeration Savings for Lighting Upgrades in Coolers","R5236: Refrigeration Savings for Lighting Upgrades in Coolers","Complete Table A of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","For refrigerated warehouse spaces only. Walk-in coolers and freezers are not eligible. ","Only heat load reduction due to lighting upgrade from HID or fluorescent fixtures to LED fixtures are eligible. Lighting upgrade limited to fixtures that are eligible for the high and low bay measures on page 12 and the linear ambient measures on page 11","Refrigeration savings measure must be submitted at the same time the incentive application for the lighting upgrade is submitted","Lamp only lighting upgrades are not eligible.","Cooler space is defined as having evaporator temperatures from 10 to 35°F. ","Not for standard air-conditioned spaces or refrigerated spaces with evaporator temperatures above 35°F.","Watts reduced is fixture wattage reduction only; do not include additional wattage reduction for occupancy sensors (if installed).","For new construction, baseline determined by multiplying installed fixture wattage 2x.",null,"Verify quantities of respective 1-for-1 measures.",{"$nulls":5},{"v":0.2,"d":"$0.20"},"Watt Reduced",{"$f":"V56","v":{"v":0.2,"d":"$0.20"}},{"$f":"W56","v":"Watt Reduced"},{"v":0.15,"d":"$0.15"},{"$f":"W56","v":"Watt Reduced"},5236,5236,5236,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A56),\"\",IF(A56<>\"Not Eligible\",A56,IF(B56<>\"Not Eligible\",B56,C56))&\": \") &D56","v":"R5236: Refrigeration Savings for Lighting Upgrades in Coolers"},"No","Yes","Watt Reduced",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR56=\"Agribusiness\", $AR56=\"Ag\",$AR56=\"Propane\", $AR56=\"Ag Propane\", $AR56=\"Ag-Propane\"),$AC56,  $AB56),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR56=\"Agribusiness\", $AR56=\"Ag\",$AR56=\"Propane\", $AR56=\"Ag Propane\", $AR56=\"Ag-Propane\"),$AC56,  $AB56),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":60000,"d":"60,000.00"}},"Lighting",18]
["L10287","L10287","Not Eligible","General Wattage Reduction, ≥1,500 Hours, Interior","L10287: General Wattage Reduction, ≥1,500 Hours, Interior","Complete Table A of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Intended for LED to LED upgrades, products installed outside of their intended end-use and/or products not ES or DLC listed.","Must operate at least 1,500 hours annually.","Pre-approval required if requesting >$10k of incentives.","Rebates limited to 50% of the retail product cost (cost to customer); excludes credit, shipping, and tax.","If project/area results in other prescriptive 1-for-1 fixtures, ok to treat measure as fixture elimination.  Ensure incentives (this and 1-for-1 measure) do not exceed project cost.","If Measure Cost cannot be determined; ok to assume same value as incentive as long as condition above is met.","Omnidirectional, directional, or decorative lamps are not eligible.",{"$nulls":8},{"v":0.2,"d":"$0.20"},"Watt Reduced",{"$f":"V57","v":{"v":0.2,"d":"$0.20"}},"Watt Reduced","N/A",{"$f":"W57","v":"Watt Reduced"},10287,10287,10287,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A57),\"\",IF(A57<>\"Not Eligible\",A57,IF(B57<>\"Not Eligible\",B57,C57))&\": \") &D57","v":"L10287: General Wattage Reduction, ≥1,500 Hours, Interior"},"No","Optional","Watt Reduced",{"v":5,"d":"5.00"},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR57=\"Agribusiness\", $AR57=\"Ag\",$AR57=\"Propane\", $AR57=\"Ag Propane\", $AR57=\"Ag-Propane\"),$AC57,  $AB57),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Lighting",18]
["L10433","L10433","Not Eligible","General Wattage Reduction, <1,500 Hours, Interior","L10433: General Wattage Reduction, <1,500 Hours, Interior","Complete Table A of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Intended for LED to LED upgrades, products installed outside of their intended end-use and/or products not ES or DLC listed.","Must operate less than 1,500 hours annually.","Pre-approval required if requesting >$10k of incentives.","Rebates limited to 50% of the retail product cost (cost to customer); excludes credit, shipping, and tax.","If project/area results in other prescriptive 1-for-1 fixtures, ok to treat measure as fixture elimination.  Ensure incentives (this and 1-for-1 measure) do not exceed project cost.","If Measure Cost cannot be determined; ok to assume same value as incentive as long as condition above is met.","Omnidirectional, directional, or decorative lamps are not eligible.",{"$nulls":8},{"v":0.05,"d":"$0.05"},"Watt Reduced",{"v":0.05,"d":"$0.05"},"Watt Reduced","N/A","Watt Reduced",10433,10433,10433,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10433: General Wattage Reduction, <1,500 Hours, Interior","No","Optional","Watt Reduced",{"v":5,"d":"5.00"},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR58=\"Agribusiness\", $AR58=\"Ag\",$AR58=\"Propane\", $AR58=\"Ag Propane\", $AR58=\"Ag-Propane\"),$AC58,  $AB58),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Lighting",18]
["L10288","L10288","Not Eligible","General Wattage Reduction, ≥1,500 Hours, Exterior",{"$f":"IF(ISBLANK(A59),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C59,IF(FOEIncentCodeType=IncentCodeTypeAg,B59,A59))&\": \") &D59","v":"L10288: General Wattage Reduction, ≥1,500 Hours, Exterior"},"Complete Table A of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Intended for LED to LED upgrades, products installed outside of their intended end-use and/or products not ES or DLC listed.","Must operate at least 1,500 hours annually.","Pre-approval required if requesting >$10k of incentives.","Rebates limited to 50% of the retail product cost (cost to customer); excludes credit, shipping, and tax.","If project/area results in other prescriptive 1-for-1 fixtures, ok to treat measure as fixture elimination.  Ensure incentives (this and 1-for-1 measure) do not exceed project cost.","If Measure Cost cannot be determined; ok to assume same value as incentive as long as condition above is met.","Omnidirectional, directional, or decorative lamps are not eligible.",{"$nulls":8},{"v":0.2,"d":"$0.20"},"Watt Reduced",{"v":0.2,"d":"$0.20"},"Watt Reduced","N/A","Watt Reduced",10288,10288,10288,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10288: General Wattage Reduction, ≥1,500 Hours, Exterior","No","Optional","Watt Reduced",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR59=\"Agribusiness\", $AR59=\"Ag\",$AR59=\"Propane\", $AR59=\"Ag Propane\", $AR59=\"Ag-Propane\"),$AC59,  $AB59),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR59=\"Agribusiness\", $AR59=\"Ag\",$AR59=\"Propane\", $AR59=\"Ag Propane\", $AR59=\"Ag-Propane\"),$AC59,  $AB59),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Lighting",18]
["L10437","L10437","Not Eligible","General Wattage Reduction, <1,500 Hours, Exterior","L10437: General Wattage Reduction, <1,500 Hours, Exterior","Complete Table A of the \"Lighting Incentive Catalog Supplemental Data Sheet\" for these measures.","Intended for LED to LED upgrades, products installed outside of their intended end-use and/or products not ES or DLC listed.","Must operate less than 1,500 hours annually.","Pre-approval required if requesting >$10k of incentives.","Rebates limited to 50% of the retail product cost (cost to customer); excludes credit, shipping, and tax.","If project/area results in other prescriptive 1-for-1 fixtures, ok to treat measure as fixture elimination.  Ensure incentives (this and 1-for-1 measure) do not exceed project cost.","If Measure Cost cannot be determined; ok to assume same value as incentive as long as condition above is met.","Omnidirectional, directional, or decorative lamps are not eligible.",{"$nulls":8},{"v":0.05,"d":"$0.05"},"Watt Reduced",{"v":0.05,"d":"$0.05"},"Watt Reduced","N/A","Watt Reduced",10437,10437,10437,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10437: General Wattage Reduction, <1,500 Hours, Exterior","No","Optional","Watt Reduced",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR60=\"Agribusiness\", $AR60=\"Ag\",$AR60=\"Propane\", $AR60=\"Ag Propane\", $AR60=\"Ag-Propane\"),$AC60,  $AB60),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR60=\"Agribusiness\", $AR60=\"Ag\",$AR60=\"Propane\", $AR60=\"Ag Propane\", $AR60=\"Ag-Propane\"),$AC60,  $AB60),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Lighting",18]
[{"$nulls":3},"----------------------HVAC CATALOG: HEATING SYSTEMS----------------------------","----------------------HVAC CATALOG: HEATING SYSTEMS----------------------------",{"$nulls":9},"",{"$nulls":22},"----------------------HVAC CATALOG: HEATING SYSTEMS----------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR61=\"Agribusiness\", $AR61=\"Ag\",$AR61=\"Propane\", $AR61=\"Ag Propane\", $AR61=\"Ag-Propane\"),$AC61,  $AB61),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR61=\"Agribusiness\", $AR61=\"Ag\",$AR61=\"Propane\", $AR61=\"Ag Propane\", $AR61=\"Ag-Propane\"),$AC61,  $AB61),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC"]
["H10222","H10222","N-H10222","Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","Must be ≥ 90 and <95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,null,"See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":7,"d":"$7.00"},"MBh",{"$f":"V62","v":{"v":7,"d":"$7.00"}},"MBh",{"v":7,"d":"$7.00"},{"$f":"W62","v":"MBh"},10222,{"$f":"AB62","v":10222},10222,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR62=\"Agribusiness\", $AR62=\"Ag\",$AR62=\"Propane\", $AR62=\"Ag Propane\", $AR62=\"Ag-Propane\"),$AC62,  $AB62),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR62=\"Agribusiness\", $AR62=\"Ag\",$AR62=\"Propane\", $AR62=\"Ag Propane\", $AR62=\"Ag-Propane\"),$AC62,  $AB62),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"HVAC",12]
["H10207","H10207","N-H10207","Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","Must be ≥ 95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,null,"See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":8,"d":"$8.00"},"MBh",{"v":8,"d":"$8.00"},"MBh",{"v":8,"d":"$8.00"},"MBh",10207,10207,10207,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR63=\"Agribusiness\", $AR63=\"Ag\",$AR63=\"Propane\", $AR63=\"Ag Propane\", $AR63=\"Ag-Propane\"),$AC63,  $AB63),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR63=\"Agribusiness\", $AR63=\"Ag\",$AR63=\"Propane\", $AR63=\"Ag Propane\", $AR63=\"Ag-Propane\"),$AC63,  $AB63),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"HVAC",12]
["H2221","H2221","Not Eligible","Outdoor Air Reset/Cutout Controls","H2221: Outdoor Air Reset/Cutout Controls","OA temp. boiler reset & cutout control incentives are for retrofit projects only. New boilers equipped w/ these controls DNQ.","System must have an outdoor temperature sensor installed in a shaded location on the north side of the building.","Min temp must be <10°F above boiler mfg's recommended min return temp unless unusual circumstances require higher setting","If multiple boilers, controls must stage lag boiler(s) only after 1st boiler fails to maintain water temp called for by reset control.","Provide input capacity of boilers (in MBh) controlled w/OA reset & cutoff controls per the example given.","Natural gas equipment only.",{"$nulls":4},"Controller, screenshot or control system readout (displaying data being sensed), equipment being controlled, equipment capacity",{"$nulls":5},{"v":100,"d":"$100.00"},"Control",{"v":100,"d":"$100.00"},"Control","N/A","Control",2221,2221,2221,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2221: Outdoor Air Reset/Cutout Controls","No","Yes","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR64=\"Agribusiness\", $AR64=\"Ag\",$AR64=\"Propane\", $AR64=\"Ag Propane\", $AR64=\"Ag-Propane\"),$AC64,  $AB64),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR64=\"Agribusiness\", $AR64=\"Ag\",$AR64=\"Propane\", $AR64=\"Ag Propane\", $AR64=\"Ag-Propane\"),$AC64,  $AB64),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6300,"d":"6,300.00"}},"HVAC",13]
["H2205","H2205","Not Eligible","Linkageless Controls, HVAC Boilers","H2205: Linkageless Controls, HVAC Boilers","Boiler must be natural gas-fired, forced-draft boiler used for space heating that operates a minimum of 4,000 hours per year","Installation on redundant or backup boilers does not qualify for an incentive","Boiler input capacity must be entered in boiler horsepower (BHP). To convert use 1 BHP=33.476 MBh. ","Incentive capped @ 50% of project cost, including equip and external labor (internal labor eligible for schools and gov customers). ",{"$nulls":6},"Front of boiler (including burner), burner nameplate",{"$nulls":5},{"v":35,"d":"$35.00"},"BHP",{"v":35,"d":"$35.00"},"BHP","N/A","BHP",2205,2205,2205,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","H2205: Linkageless Controls, HVAC Boilers","No","Yes","BHP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR65=\"Agribusiness\", $AR65=\"Ag\",$AR65=\"Propane\", $AR65=\"Ag Propane\", $AR65=\"Ag-Propane\"),$AC65,  $AB65),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR65=\"Agribusiness\", $AR65=\"Ag\",$AR65=\"Propane\", $AR65=\"Ag Propane\", $AR65=\"Ag-Propane\"),$AC65,  $AB65),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"HVAC",13]
["H2206","H2206","N-H2206","O₂ Trim Controls, HVAC Boilers","H2206: O₂ Trim Controls, HVAC Boilers","Boiler must be natural gas-fired, forced-draft boiler used for space heating that operates a minimum of 4,000 hours per year","Installation on redundant or backup boilers does not qualify for an incentive","Boiler input capacity must be entered in boiler horsepower (BHP). To convert use 1 BHP=33.476 MBh. ","Incentive capped @ 50% of project cost, including equip and external labor (internal labor eligible for schools and gov customers). ",{"$nulls":6},"Front of boiler (including burner), burner nameplate, oxygen sensor location (if visible), screen shot of boiler control system (if available)",{"$nulls":5},{"v":10,"d":"$10.00"},"BHP",{"v":10,"d":"$10.00"},"BHP",{"v":10,"d":"$10.00"},"BHP",2206,2206,2206,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","H2206: O₂ Trim Controls, HVAC Boilers","No","Yes","BHP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR66=\"Agribusiness\", $AR66=\"Ag\",$AR66=\"Propane\", $AR66=\"Ag Propane\", $AR66=\"Ag-Propane\"),$AC66,  $AB66),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR66=\"Agribusiness\", $AR66=\"Ag\",$AR66=\"Propane\", $AR66=\"Ag Propane\", $AR66=\"Ag-Propane\"),$AC66,  $AB66),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"HVAC",13]
["H2203","H2203","Not Eligible","High Turndown Burner, Retrofit on Existing Boiler","H2203: High Turndown Burner, Retrofit on Existing Boiler","Boiler must be natural gas-fired, forced-draft boiler used for space heating that operates a minimum of 4,000 hours per year","Installation on redundant or backup boilers does not qualify for an incentive.","Boiler input capacity must be entered in boiler horsepower (BHP). To convert use 1 BHP=33.476 MBh. ","Burners must have a minimum 10:1 firing rate.","Incentive capped @ 50% of project cost, including equip and external labor (internal labor eligible for schools and gov customers). ","For retrofitting an existing boiler only.",{"$nulls":4},"Front of boiler (including burner), burner nameplate",{"$nulls":5},{"v":20,"d":"$20.00"},"BHP",{"v":20,"d":"$20.00"},"BHP","N/A","BHP",2203,2203,2203,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","H2203: High Turndown Burner, Retrofit on Existing Boiler","No","Yes","BHP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR67=\"Agribusiness\", $AR67=\"Ag\",$AR67=\"Propane\", $AR67=\"Ag Propane\", $AR67=\"Ag-Propane\"),$AC67,  $AB67),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR67=\"Agribusiness\", $AR67=\"Ag\",$AR67=\"Propane\", $AR67=\"Ag Propane\", $AR67=\"Ag-Propane\"),$AC67,  $AB67),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"HVAC",13]
["H5237","H5237","N-H5237","High Turndown Burner, New Boiler Replacement","H5237: High Turndown Burner, New Boiler Replacement","Boiler must be natural gas-fired, forced-draft boiler used for space heating that operates a minimum of 4,000 hours per year","Installation on redundant or backup boilers does not qualify for an incentive.","Boiler input capacity must be entered in boiler horsepower (BHP). To convert use 1 BHP=33.476 MBh. ","Burners must have a minimum 10:1 firing rate.","Incentive capped @ 50% of project cost, including equip and external labor (internal labor eligible for schools and gov customers). ","For new boiler upgrades only.",{"$nulls":4},"Front of boiler (including burner), burner nameplate",{"$nulls":5},{"v":20,"d":"$20.00"},"BHP",{"v":20,"d":"$20.00"},"BHP",{"v":20,"d":"$20.00"},"BHP",5237,5237,5237,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","H5237: High Turndown Burner, New Boiler Replacement","No","Yes","BHP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR68=\"Agribusiness\", $AR68=\"Ag\",$AR68=\"Propane\", $AR68=\"Ag Propane\", $AR68=\"Ag-Propane\"),$AC68,  $AB68),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR68=\"Agribusiness\", $AR68=\"Ag\",$AR68=\"Propane\", $AR68=\"Ag Propane\", $AR68=\"Ag-Propane\"),$AC68,  $AB68),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"HVAC",13]
["H2225","H2225","Not Eligible","Steam Trap Survey (HVAC)","H2225: Steam Trap Survey (HVAC)","Survey log must include all necessary fields. Note that 2225 is now only for HVAC steam traps. Process steam trap survey = 4041.","Only systems with steam produced by natural gas equipment are eligible. Municipal steam systems DNQ.","Customer must repair or replace one trap for every five traps surveyed. If less than one trap per every five traps survayed is identified as failed, then all failed traps must be repaired or replaced.","If all identified failed traps must be repaired/replaced, customer may provide written explanation for a trap that can't be repaired or replaced & may still qualify.","Survey incentive only available once per year per steam system","Survey cost must be shown on the invoice","For projects that don't complete a steam trap survey, provide the nominal steam pressure (psig) on the application or in other supporting documentation","Steam trap survey and repair work must be recorded in a log sheet and attached to the application in order to be eligible for the survey incentive",null,"If survey incentive is being paid before repairs are complete, add a note in SPECTRUM with explaination and connect the two apps once repair measures are processed.","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":8,"d":"$8.00"},"Steam Trap",{"v":8,"d":"$8.00"},"Steam Trap","N/A","Steam Trap",2225,2225,2225,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2225: Steam Trap Survey (HVAC)","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR69=\"Agribusiness\", $AR69=\"Ag\",$AR69=\"Propane\", $AR69=\"Ag Propane\", $AR69=\"Ag-Propane\"),$AC69,  $AB69),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR69=\"Agribusiness\", $AR69=\"Ag\",$AR69=\"Propane\", $AR69=\"Ag Propane\", $AR69=\"Ag-Propane\"),$AC69,  $AB69),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",14]
["H10425","H10425","Not Eligible","Steam Trap Repair, <10 psig General Heating","H10425: Steam Trap Repair, <10 psig General Heating","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. HVAC traps only; use separate measures for process traps.","Only natural gas based steam systems are eligible. Municipal steam systems DNQ.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, if possible, that the actual system steam pressure is < 10 PSI. Do not use rated PSI of the steam trap.",null,"Customer must repair or replace one trap for every five traps surveyed. If less than one trap per every five traps survayed is identified as failed, then all failed traps must be repaired or replaced.","If all identified failed traps must be repaired/replaced, customer may provide written explanation for a trap that can't be repaired or replaced & may still qualify.",null,"Surveys are optional","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":60,"d":"$60.00"},"Steam Trap",{"v":60,"d":"$60.00"},"Steam Trap","N/A","Steam Trap",10425,10425,10425,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10425: Steam Trap Repair, <10 psig General Heating","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR70=\"Agribusiness\", $AR70=\"Ag\",$AR70=\"Propane\", $AR70=\"Ag Propane\", $AR70=\"Ag-Propane\"),$AC70,  $AB70),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR70=\"Agribusiness\", $AR70=\"Ag\",$AR70=\"Propane\", $AR70=\"Ag Propane\", $AR70=\"Ag-Propane\"),$AC70,  $AB70),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",14]
["H10427","H10427","Not Eligible","Steam Trap Repair, 10-49 psig General Heating","H10427: Steam Trap Repair, 10-49 psig General Heating","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. HVAC traps only; use separate measures for process traps.","Only natural gas based steam systems are eligible. Municipal steam systems DNQ.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, that UOM in SPECTRUM is the actual system steam pressure + 14.7 PSI. Do not use rated PSI of the steam trap as steam pressure.",null,"Customer must repair or replace one trap for every five traps surveyed. If less than one trap per every five traps survayed is identified as failed, then all failed traps must be repaired or replaced.","If all identified failed traps must be repaired/replaced, customer may provide written explanation for a trap that can't be repaired or replaced & may still qualify.",null,"Surveys are optional","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":100,"d":"$100.00"},"Steam Trap",{"v":100,"d":"$100.00"},"Steam Trap","N/A","Steam Trap",10427,10427,10427,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10427: Steam Trap Repair, 10-49 psig General Heating","No","Yes","PSIA (PSIG + 14.7)",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR71=\"Agribusiness\", $AR71=\"Ag\",$AR71=\"Propane\", $AR71=\"Ag Propane\", $AR71=\"Ag-Propane\"),$AC71,  $AB71),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR71=\"Agribusiness\", $AR71=\"Ag\",$AR71=\"Propane\", $AR71=\"Ag Propane\", $AR71=\"Ag-Propane\"),$AC71,  $AB71),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",14]
["H10428","H10428","Not Eligible","Steam Trap Repair, 50-124 psig General Heating","H10428: Steam Trap Repair, 50-124 psig General Heating","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. HVAC traps only; use separate measures for process traps.","Only natural gas based steam systems are eligible. Municipal steam systems DNQ.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, that UOM in SPECTRUM is the actual system steam pressure + 14.7 PSI. Do not use rated PSI of the steam trap as steam pressure.",null,"Customer must repair or replace one trap for every five traps surveyed. If less than one trap per every five traps survayed is identified as failed, then all failed traps must be repaired or replaced.","If all identified failed traps must be repaired/replaced, customer may provide written explanation for a trap that can't be repaired or replaced & may still qualify.",null,"Surveys are optional","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":150,"d":"$150.00"},"Steam Trap",{"v":150,"d":"$150.00"},"Steam Trap","N/A","Steam Trap",10428,10428,10428,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10428: Steam Trap Repair, 50-124 psig General Heating","No","Yes","PSIA (PSIG + 14.7)",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR72=\"Agribusiness\", $AR72=\"Ag\",$AR72=\"Propane\", $AR72=\"Ag Propane\", $AR72=\"Ag-Propane\"),$AC72,  $AB72),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR72=\"Agribusiness\", $AR72=\"Ag\",$AR72=\"Propane\", $AR72=\"Ag Propane\", $AR72=\"Ag-Propane\"),$AC72,  $AB72),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",14]
["H10426","H10426","Not Eligible","Steam Trap Repair, ≥125 psig General Heating","H10426: Steam Trap Repair, ≥125 psig General Heating","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. HVAC traps only; use separate measures for process traps.","Only natural gas based steam systems are eligible. Municipal steam systems DNQ.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, that UOM in SPECTRUM is the actual system steam pressure + 14.7 PSI. Do not use rated PSI of the steam trap as steam pressure.",null,"Customer must repair or replace one trap for every five traps surveyed. If less than one trap per every five traps survayed is identified as failed, then all failed traps must be repaired or replaced.","If all identified failed traps must be repaired/replaced, customer may provide written explanation for a trap that can't be repaired or replaced & may still qualify.",null,"Surveys are optional","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":250,"d":"$250.00"},"Steam Trap",{"v":250,"d":"$250.00"},"Steam Trap","N/A","Steam Trap",10426,10426,10426,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10426: Steam Trap Repair, ≥125 psig General Heating","No","Yes","PSIA (PSIG + 14.7)",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR73=\"Agribusiness\", $AR73=\"Ag\",$AR73=\"Propane\", $AR73=\"Ag Propane\", $AR73=\"Ag-Propane\"),$AC73,  $AB73),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR73=\"Agribusiness\", $AR73=\"Ag\",$AR73=\"Propane\", $AR73=\"Ag Propane\", $AR73=\"Ag-Propane\"),$AC73,  $AB73),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",14]
["H2429","H2429","Not Eligible","Insulation for Steam Fittings, Natural Gas","H2429: Insulation for Steam Fittings, Natural Gas","Incentive is for adding insulation to uninsulated steam piping and fittings (including traps). For natural gas generated steam only.","Insulation for fittings must be removable and reusable.","For businesses: Insulation must be ≥1.5 inches for pipes <1.5 inches in diameter and ≥3 inches for pipes >1.5 inches in diameter","Steam system being insulated must be used for space heating applications. Industrial process applications may be eligible for a custom incentive.",{"$nulls":6},"Close-up of insulation (showing thickness if possible); wide shot of piping layout; photo of boiler if possible.",{"$nulls":5},{"v":20,"d":"$20.00"},"Fitting",{"v":20,"d":"$20.00"},"Fitting","N/A","Fitting",2429,2429,2429,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2429: Insulation for Steam Fittings, Natural Gas","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR74=\"Agribusiness\", $AR74=\"Ag\",$AR74=\"Propane\", $AR74=\"Ag Propane\", $AR74=\"Ag-Propane\"),$AC74,  $AB74),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR74=\"Agribusiness\", $AR74=\"Ag\",$AR74=\"Propane\", $AR74=\"Ag Propane\", $AR74=\"Ag-Propane\"),$AC74,  $AB74),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",14]
["H2430","H2430","Not Eligible","Insulation for Steam Pipe, Natural Gas","H2430: Insulation for Steam Pipe, Natural Gas","Incentive is for adding insulation to uninsulated steam piping and fittings. For natural gas generated steam only.","For businesses: Insulation must be ≥1.5 inches for pipes <1.5 inches in diameter and ≥3 inches for pipes >1.5 inches in diameter","Steam system being insulated must be used for space heating applications. Industrial process applications may be eligible for a custom incentive.",{"$nulls":7},"Close-up of insulation (showing thickness if possible); wide shot of piping layout; photo of boiler if possible.",{"$nulls":5},{"v":10,"d":"$10.00"},"Ft of Pipe",{"v":10,"d":"$10.00"},"Ft of Pipe","N/A","Ft of Pipe",2430,2430,2430,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2430: Insulation for Steam Pipe, Natural Gas","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR75=\"Agribusiness\", $AR75=\"Ag\",$AR75=\"Propane\", $AR75=\"Ag Propane\", $AR75=\"Ag-Propane\"),$AC75,  $AB75),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR75=\"Agribusiness\", $AR75=\"Ag\",$AR75=\"Propane\", $AR75=\"Ag Propane\", $AR75=\"Ag-Propane\"),$AC75,  $AB75),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",14]
["H2422","H2422","N-H2422","Infrared Heater","H2422: Infrared Heater","Low-intensity and high-intensity units are eligible","Must have electronic ignition","Outdoor patio heating applications not eligible","For existing buildings, replacement of existing infrared heater DNQ","Propane customers should refer to the Propane and Electric Incentive Catalog for eligible measures.","Must be vented per manufacturer's requirements","Low-intensity heaters must use outside non-conditioned combustion air",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":7.5,"d":"$7.50"},"MBh",{"v":7.5,"d":"$7.50"},"MBh",{"v":6,"d":"$6.00"},"MBh",2422,2422,2422,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2422: Infrared Heater","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR76=\"Agribusiness\", $AR76=\"Ag\",$AR76=\"Propane\", $AR76=\"Ag Propane\", $AR76=\"Ag-Propane\"),$AC76,  $AB76),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR76=\"Agribusiness\", $AR76=\"Ag\",$AR76=\"Propane\", $AR76=\"Ag Propane\", $AR76=\"Ag-Propane\"),$AC76,  $AB76),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"HVAC",14]
["H5436","H5436","N-H5436","Unit Heater, ≥ 90% Thermal Efficiency","H5436: Unit Heater, ≥ 90% Thermal Efficiency","Must be ≥ 90% thermal efficiency, replacing or instead of standard efficiency unit heater (typically 80%-84% Thermal Efficiency)","Direct-fired RTUs / MUA units not eligible","Must provide a mfg's spec sheet to document efficiency level","Equipment serving process or other loads DNQ.","Must be natural gas fired only. Steam or hot water coils/systems are not eligible.  Propane customers should refer to the Propane and Electric Incentive Catalog for eligible measures.","Must replace existing non-condensing unit heater or be installed instead of a non-condensing unit heater.","Must be vented and condensate drained per manufacturer specifications",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":4,"d":"$4.00"},"MBh",{"v":4,"d":"$4.00"},"MBh",{"v":2.75,"d":"$2.75"},"MBh",5436,5436,5436,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5436: Unit Heater, ≥ 90% Thermal Efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR77=\"Agribusiness\", $AR77=\"Ag\",$AR77=\"Propane\", $AR77=\"Ag Propane\", $AR77=\"Ag-Propane\"),$AC77,  $AB77),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":50,"d":"50.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR77=\"Agribusiness\", $AR77=\"Ag\",$AR77=\"Propane\", $AR77=\"Ag Propane\", $AR77=\"Ag-Propane\"),$AC77,  $AB77),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":400,"d":"400.00"}},"HVAC",15]
["H2699","H2699","N-H2699","PTHP <8,000 BTUh, ≥10.7 EER and ≥3.1 COP   (NC =  ≥12.7 EER and ≥3.1 COP)","H2699: PTHP <8,000 BTUh, ≥10.7 EER and ≥3.1 COP   (NC =  ≥12.7 EER and ≥3.1 COP)","Must replace or be instead of a Packaged Terminal Air Conditioner (PTAC). For existing buildings, replacement of existing PTHP DNQ.","Unit must be AHRI listed as a Commercial PTHP. Window and through-the-wall air conditioners/heat pumps DNQ.","The equipment size category (BTUh) is the cooling capacity value of the unit.","Must meet both heating and cooling specifications for the equipment size category.","Verify efficiency ratings using AHRIdirectory.org","Eligibility for PTHP measures is based on customer having an eligible electric provider.",{"$nulls":4},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":120,"d":"$120.00"},"PTHP",{"$f":"V78","v":{"v":120,"d":"$120.00"}},"PTHP",{"v":110,"d":"$110.00"},"PTHP",2699,2699,2699,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2699: PTHP <8,000 BTUh, ≥10.7 EER and ≥3.1 COP   (NC =  ≥12.7 EER and ≥3.1 COP)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR78=\"Agribusiness\", $AR78=\"Ag\",$AR78=\"Propane\", $AR78=\"Ag Propane\", $AR78=\"Ag-Propane\"),$AC78,  $AB78),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR78=\"Agribusiness\", $AR78=\"Ag\",$AR78=\"Propane\", $AR78=\"Ag Propane\", $AR78=\"Ag-Propane\"),$AC78,  $AB78),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",15]
["H2702","H2702","N-H2702","PTHP 8,000-9,999 BTUh, ≥10.4 EER and ≥3.0 COP   (NC =  ≥12.1 EER and ≥3.0 COP)","H2702: PTHP 8,000-9,999 BTUh, ≥10.4 EER and ≥3.0 COP   (NC =  ≥12.1 EER and ≥3.0 COP)","Must replace or be instead of a Packaged Terminal Air Conditioner (PTAC). For existing buildings, replacement of existing PTHP DNQ.","Unit must be AHRI listed as a Commercial PTHP. Window and through-the-wall air conditioners/heat pumps DNQ.","The equipment size category (BTUh) is the cooling capacity value of the unit.","Must meet both heating and cooling specifications for the equipment size category.","Verify efficiency ratings using AHRIdirectory.org","Eligibility for PTHP measures is based on customer having an eligible electric provider.",{"$nulls":4},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":120,"d":"$120.00"},"PTHP",{"v":120,"d":"$120.00"},"PTHP",{"v":110,"d":"$110.00"},"PTHP",2702,2702,2702,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2702: PTHP 8,000-9,999 BTUh, ≥10.4 EER and ≥3.0 COP   (NC =  ≥12.1 EER and ≥3.0 COP)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR79=\"Agribusiness\", $AR79=\"Ag\",$AR79=\"Propane\", $AR79=\"Ag Propane\", $AR79=\"Ag-Propane\"),$AC79,  $AB79),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR79=\"Agribusiness\", $AR79=\"Ag\",$AR79=\"Propane\", $AR79=\"Ag Propane\", $AR79=\"Ag-Propane\"),$AC79,  $AB79),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",15]
["H2701","H2701","N-H2701","PTHP 10,000-12,999 BTUh, ≥9.9 EER and ≥2.9 COP   (NC =  ≥10.9 EER and ≥2.9 COP)","H2701: PTHP 10,000-12,999 BTUh, ≥9.9 EER and ≥2.9 COP   (NC =  ≥10.9 EER and ≥2.9 COP)","Must replace or be instead of a Packaged Terminal Air Conditioner (PTAC). For existing buildings, replacement of existing PTHP DNQ.","Unit must be AHRI listed as a Commercial PTHP. Window and through-the-wall air conditioners/heat pumps DNQ.","The equipment size category (BTUh) is the cooling capacity value of the unit.","Must meet both heating and cooling specifications for the equipment size category.","Verify efficiency ratings using AHRIdirectory.org","Eligibility for PTHP measures is based on customer having an eligible electric provider.",{"$nulls":4},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":120,"d":"$120.00"},"PTHP",{"v":120,"d":"$120.00"},"PTHP",{"v":110,"d":"$110.00"},"PTHP",2701,2701,2701,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2701: PTHP 10,000-12,999 BTUh, ≥9.9 EER and ≥2.9 COP   (NC =  ≥10.9 EER and ≥2.9 COP)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR80=\"Agribusiness\", $AR80=\"Ag\",$AR80=\"Propane\", $AR80=\"Ag Propane\", $AR80=\"Ag-Propane\"),$AC80,  $AB80),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR80=\"Agribusiness\", $AR80=\"Ag\",$AR80=\"Propane\", $AR80=\"Ag Propane\", $AR80=\"Ag-Propane\"),$AC80,  $AB80),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",15]
["H2700","H2700","N-H2700","PTHP ≥13,000 BTUh, ≥9.3 EER and ≥2.9 COP   (NC =  ≥10.3 EER and ≥2.9 COP)","H2700: PTHP ≥13,000 BTUh, ≥9.3 EER and ≥2.9 COP   (NC =  ≥10.3 EER and ≥2.9 COP)","Must replace or be instead of a Packaged Terminal Air Conditioner (PTAC). For existing buildings, replacement of existing PTHP DNQ.","Unit must be AHRI listed as a Commercial PTHP. Window and through-the-wall air conditioners/heat pumps DNQ.","The equipment size category (BTUh) is the cooling capacity value of the unit.","Must meet both heating and cooling specifications for the equipment size category.","Verify efficiency ratings using AHRIdirectory.org","Eligibility for PTHP measures is based on customer having an eligible electric provider.",{"$nulls":4},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":120,"d":"$120.00"},"PTHP",{"v":120,"d":"$120.00"},"PTHP",{"v":110,"d":"$110.00"},"PTHP",2700,2700,2700,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2700: PTHP ≥13,000 BTUh, ≥9.3 EER and ≥2.9 COP   (NC =  ≥10.3 EER and ≥2.9 COP)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR81=\"Agribusiness\", $AR81=\"Ag\",$AR81=\"Propane\", $AR81=\"Ag Propane\", $AR81=\"Ag-Propane\"),$AC81,  $AB81),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR81=\"Agribusiness\", $AR81=\"Ag\",$AR81=\"Propane\", $AR81=\"Ag Propane\", $AR81=\"Ag-Propane\"),$AC81,  $AB81),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",15]
["H5081","H5081","N-H5081","Direct Fired Make-up Air Unit, Constant Volume","H5081: Direct Fired Make-up Air Unit, Constant Volume","Complete Table A1 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.  Or Table J of the “Propane and Electric Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible. ","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":0.4,"d":"$0.40"},"CFM",{"v":0.4,"d":"$0.40"},"CFM",{"v":0.3,"d":"$0.30"},"CFM",5081,5081,5081,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5081: Direct Fired Make-up Air Unit, Constant Volume","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR82=\"Agribusiness\", $AR82=\"Ag\",$AR82=\"Propane\", $AR82=\"Ag Propane\", $AR82=\"Ag-Propane\"),$AC82,  $AB82),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR82=\"Agribusiness\", $AR82=\"Ag\",$AR82=\"Propane\", $AR82=\"Ag Propane\", $AR82=\"Ag-Propane\"),$AC82,  $AB82),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"HVAC",15]
["H10030","H10030","N-H10030","Direct Fired Make-up Air Unit, Variable Air Volume",{"$f":"IF(ISBLANK(A83),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C83,IF(FOEIncentCodeType=IncentCodeTypeAg,B83,A83))&\": \") &D83","v":"H10030: Direct Fired Make-up Air Unit, Variable Air Volume"},"Complete Table A2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.  Or Table J of the “Propane and Electric Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible. ","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.","Cannot be combined with VFD incentives.",null,null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":0.65,"d":"$0.65"},"CFM",{"v":0.65,"d":"$0.65"},"CFM",{"v":0.4,"d":"$0.40"},"CFM",10030,10030,10030,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10030: Direct Fired Make-up Air Unit, Variable Air Volume","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR83=\"Agribusiness\", $AR83=\"Ag\",$AR83=\"Propane\", $AR83=\"Ag Propane\", $AR83=\"Ag-Propane\"),$AC83,  $AB83),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":800,"d":"800.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR83=\"Agribusiness\", $AR83=\"Ag\",$AR83=\"Propane\", $AR83=\"Ag Propane\", $AR83=\"Ag-Propane\"),$AC83,  $AB83),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"HVAC",15]
["H10445","H10445","N-H10445","Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume","H10445: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume","Complete Table A2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.  Or Table J of the “Propane and Electric Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.","Cannot be combined with VFD incentives.",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":0.2,"d":"$0.20"},"CFM",{"v":0.2,"d":"$0.20"},"CFM",{"v":0.2,"d":"$0.20"},"CFM",10445,10445,10445,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10445: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume","Yes","Yes","CFM",{"v":100,"d":"100.00"},{"v":50000,"d":"50,000.00"},"HVAC",15]
[{"$nulls":3},"----------------------HVAC CATALOG: COOLING SYSTEMS----------------------------","----------------------HVAC CATALOG: COOLING SYSTEMS----------------------------",{"$nulls":10},"equipment, location, equipment nameplate (if possible)",{"$nulls":21},"----------------------HVAC CATALOG: COOLING SYSTEMS----------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR85=\"Agribusiness\", $AR85=\"Ag\",$AR85=\"Propane\", $AR85=\"Ag Propane\", $AR85=\"Ag-Propane\"),$AC85,  $AB85),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR85=\"Agribusiness\", $AR85=\"Ag\",$AR85=\"Propane\", $AR85=\"Ag Propane\", $AR85=\"Ag-Propane\"),$AC85,  $AB85),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC"]
["H5423","H5423","N-H5423","16 SEER2 A/C Split System or Single Package, < 5.42 tons","H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 16 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":75,"d":"$75.00"},"A/C Unit",{"$f":"V86","v":{"v":75,"d":"$75.00"}},"A/C Unit",{"v":50,"d":"$50.00"},{"$f":"W86","v":"A/C Unit"},5423,5423,5423,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR86=\"Agribusiness\", $AR86=\"Ag\",$AR86=\"Propane\", $AR86=\"Ag Propane\", $AR86=\"Ag-Propane\"),$AC86,  $AB86),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR86=\"Agribusiness\", $AR86=\"Ag\",$AR86=\"Propane\", $AR86=\"Ag Propane\", $AR86=\"Ag-Propane\"),$AC86,  $AB86),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"HVAC",16]
["H5424","H5424","N-H5424","17 SEER2 A/C Split System or Single Package, < 5.42 tons","H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 17 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":100,"d":"$100.00"},"A/C Unit",{"v":100,"d":"$100.00"},"A/C Unit",{"v":75,"d":"$75.00"},"A/C Unit",5424,5424,5424,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR87=\"Agribusiness\", $AR87=\"Ag\",$AR87=\"Propane\", $AR87=\"Ag Propane\", $AR87=\"Ag-Propane\"),$AC87,  $AB87),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR87=\"Agribusiness\", $AR87=\"Ag\",$AR87=\"Propane\", $AR87=\"Ag Propane\", $AR87=\"Ag-Propane\"),$AC87,  $AB87),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"HVAC",16]
["H5425","H5425","N-H5425","18 SEER2 A/C Split System or Single Package, < 5.42 tons","H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 18 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":125,"d":"$125.00"},"A/C Unit",{"v":125,"d":"$125.00"},"A/C Unit",{"v":100,"d":"$100.00"},"A/C Unit",5425,5425,5425,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR88=\"Agribusiness\", $AR88=\"Ag\",$AR88=\"Propane\", $AR88=\"Ag Propane\", $AR88=\"Ag-Propane\"),$AC88,  $AB88),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR88=\"Agribusiness\", $AR88=\"Ag\",$AR88=\"Propane\", $AR88=\"Ag Propane\", $AR88=\"Ag-Propane\"),$AC88,  $AB88),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"HVAC",16]
["H5426","H5426","N-H5426","19 SEER2 A/C Split System or Single Package, < 5.42 tons","H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 19 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":175,"d":"$175.00"},"A/C Unit",{"v":175,"d":"$175.00"},"A/C Unit",{"v":125,"d":"$125.00"},"A/C Unit",5426,5426,5426,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR89=\"Agribusiness\", $AR89=\"Ag\",$AR89=\"Propane\", $AR89=\"Ag Propane\", $AR89=\"Ag-Propane\"),$AC89,  $AB89),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR89=\"Agribusiness\", $AR89=\"Ag\",$AR89=\"Propane\", $AR89=\"Ag Propane\", $AR89=\"Ag-Propane\"),$AC89,  $AB89),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"HVAC",16]
["H5427","H5427","N-H5427","20 SEER2 A/C Split System or Single Package, < 5.42 tons","H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 20 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":200,"d":"$200.00"},"A/C Unit",{"v":200,"d":"$200.00"},"A/C Unit",{"v":150,"d":"$150.00"},"A/C Unit",5427,5427,5427,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR90=\"Agribusiness\", $AR90=\"Ag\",$AR90=\"Propane\", $AR90=\"Ag Propane\", $AR90=\"Ag-Propane\"),$AC90,  $AB90),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR90=\"Agribusiness\", $AR90=\"Ag\",$AR90=\"Propane\", $AR90=\"Ag Propane\", $AR90=\"Ag-Propane\"),$AC90,  $AB90),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"HVAC",16]
["H2820","H2820","N-H2820","Ground Source Heat Pump w/ Electric Back-Up","H2820: Ground Source Heat Pump w/ Electric Back-Up","Systems must be AHRI or ENERGY STAR listed in a geothermal category.","Primarily provides heating and cooling.  Ice/Snow melting, DHW, or non-HVAC main uses DNQ.  ","Enter Heating Capacity (MBh).  If unknown, 1 MBh cooling capacity = 0.7628 MBh heating capacity.  ",{"$nulls":7},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":750,"d":"$750.00"},"System",{"v":750,"d":"$750.00"},"System",{"v":750,"d":"$750.00"},"System",2820,2820,2820,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2820: Ground Source Heat Pump w/ Electric Back-Up","No","Yes","Heating MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR91=\"Agribusiness\", $AR91=\"Ag\",$AR91=\"Propane\", $AR91=\"Ag Propane\", $AR91=\"Ag-Propane\"),$AC91,  $AB91),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"v":50,"d":"50.00"},"HVAC",16]
["H2821","H2821","N-H2821","Ground Source Heat Pump w/ Natural Gas Back-Up","H2821: Ground Source Heat Pump w/ Natural Gas Back-Up","Systems must be AHRI or ENERGY STAR listed in a geothermal category.","Primarily provides heating and cooling.  Ice/Snow melting, DHW, or non-HVAC main uses DNQ.  ","Enter Heating Capacity (MBh).  If unknown, 1 MBh cooling capacity = 0.7628 MBh heating capacity.  ","Confirm eligible Gas Account",{"$nulls":6},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":1000,"d":"$1,000.00"},"System",{"v":1000,"d":"$1,000.00"},"System",{"v":1000,"d":"$1,000.00"},"System",2821,2821,2821,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2821: Ground Source Heat Pump w/ Natural Gas Back-Up","No","Yes","Heating MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR92=\"Agribusiness\", $AR92=\"Ag\",$AR92=\"Propane\", $AR92=\"Ag Propane\", $AR92=\"Ag-Propane\"),$AC92,  $AB92),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"v":50,"d":"50.00"},"HVAC",16]
["H4368","H4368","N-H4368","DX Cooling ≥ 5.42 to < 11.25 tons, Min. Eff. = 16.1 IEER (additional incentive on IEER)","H4368: DX Cooling ≥ 5.42 to < 11.25 tons, Min. Eff. = 16.1 IEER (additional incentive on IEER)","Complete Table B1 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be ≥ 16.1 IEER (no EER minimum). Incentive = $25/ton (existing building) or $20/ton (new construction) + $5/ton (existing building) or $3/ton (new construction) for each 1.0 IEER over 13.8.","Provide capacity and performance values to two decimal places. Standard HVAC applications only (no process cooling)","Use AHRIdirectory.org to confirm efficiency and capacity. Use AHRI capacity for incentive calc.","If split system, must be perf. Data for \"matched air handler\" or \"complete system\", NOT \"condensing unit only\"…","…and both condenser and evap. Must have coil and condenser model #'s. Coil must be replaced for retrofit projects.","SPECTRUM Unit of Measure Question = Enter Unit Total Incentive","**Ag, S&G, and BNC Programs: ENTER A PLACE HOLDER OF 1.000 for unit of measure question and QTY from Section 7. Tech Team will enter/verify values after completing hybrid calc**","Complete Cooling Eligibility Screening Tool. ","AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met. **ENTER TONNAGE IN SPECTRUM UNDER EQUIPMENT INFORMATION>ACTUAL CAPACITY**","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"$30+$5/1.0 IEER > Min","Ton","$30+$5/1.0 IEER > Min","Ton","$25+$3/1.0 IEER > Min","Ton",4368,4368,4368,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4368: DX Cooling ≥ 5.42 to < 11.25 tons, Min. Eff. = 16.1 IEER (additional incentive on IEER)","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR93=\"Agribusiness\", $AR93=\"Ag\",$AR93=\"Propane\", $AR93=\"Ag Propane\", $AR93=\"Ag-Propane\"),$AC93,  $AB93),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR93=\"Agribusiness\", $AR93=\"Ag\",$AR93=\"Propane\", $AR93=\"Ag Propane\", $AR93=\"Ag-Propane\"),$AC93,  $AB93),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",17]
["H4369","H4369","N-H4369","DX Cooling ≥ 11.25 to < 20.00 tons, Min. Eff. = 15.4 IEER (additional incentive on IEER)",{"$f":"IF(ISBLANK(A94),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C94,IF(FOEIncentCodeType=IncentCodeTypeAg,B94,A94))&\": \") &D94","v":"H4369: DX Cooling ≥ 11.25 to < 20.00 tons, Min. Eff. = 15.4 IEER (additional incentive on IEER)"},"Complete Table B1 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be ≥ 15.4 IEER (no EER minimum). Incentive = $25/ton (existing building) or $20/ton (new construction) + $5/ton (existing building) or $3/ton (new construction) for each 1.0 IEER over 13.0.","Provide capacity and performance values to two decimal places. Standard HVAC applications only (no process cooling)","Use AHRIdirectory.org to confirm efficiency and capacity. Use AHRI capacity for incentive calc.","If split system, must be perf. Data for \"matched air handler\" or \"complete system\", NOT \"condensing unit only\"…","…and both condenser and evap. Must have coil and condenser model #'s. Coil must be replaced for retrofit projects.","SPECTRUM Unit of Measure Question = Enter Unit Total Incentive","**Ag, S&G, and BNC Programs: ENTER A PLACE HOLDER OF 1.000 for unit of measure question and QTY from Section 7. Tech Team will enter/verify values after completing hybrid calc**","Complete Cooling Eligibility Screening Tool. ","AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met. **ENTER TONNAGE IN SPECTRUM UNDER EQUIPMENT INFORMATION>ACTUAL CAPACITY**","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"$30+$5/1.0 IEER > Min","Ton","$30+$5/1.0 IEER > Min","Ton","$25+$3/1.0 IEER > Min","Ton",4369,4369,4369,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4369: DX Cooling ≥ 11.25 to < 20.00 tons, Min. Eff. = 15.4 IEER (additional incentive on IEER)","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR94=\"Agribusiness\", $AR94=\"Ag\",$AR94=\"Propane\", $AR94=\"Ag Propane\", $AR94=\"Ag-Propane\"),$AC94,  $AB94),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR94=\"Agribusiness\", $AR94=\"Ag\",$AR94=\"Propane\", $AR94=\"Ag Propane\", $AR94=\"Ag-Propane\"),$AC94,  $AB94),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",17]
["H4370","H4370","N-H4370","DX Cooling ≥ 20.00 to < 63.33 tons, Min. Eff. = 14.3 IEER (additional incentive on IEER)","H4370: DX Cooling ≥ 20.00 to < 63.33 tons, Min. Eff. = 14.3 IEER (additional incentive on IEER)","Complete Table B1 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be ≥ 14.3 IEER (no EER minimum). Incentive = $25/ton (existing building) or $20/ton (new construction) + $5/ton (existing building) or $3/ton (new construction) for each 1.0 IEER over 12.1.","Provide capacity and performance values to two decimal places. Standard HVAC applications only (no process cooling)","Use AHRIdirectory.org to confirm efficiency and capacity. Use AHRI capacity for incentive calc.","If split system, must be perf. Data for \"matched air handler\" or \"complete system\", NOT \"condensing unit only\"…","…and both condenser and evap. Must have coil and condenser model #'s. Coil must be replaced for retrofit projects.","SPECTRUM Unit of Measure Question = Enter Unit Total Incentive","**Ag, S&G, and BNC Programs: ENTER A PLACE HOLDER OF 1.000 for unit of measure question and QTY from Section 7. Tech Team will enter/verify values after completing hybrid calc**","Complete Cooling Eligibility Screening Tool. ","AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met. **ENTER TONNAGE IN SPECTRUM UNDER EQUIPMENT INFORMATION>ACTUAL CAPACITY**","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"$30+$5/1.0 IEER > Min","Ton","$30+$5/1.0 IEER > Min","Ton","$25+$3/1.0 IEER > Min","Ton",4370,4370,4370,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4370: DX Cooling ≥ 20.00 to < 63.33 tons, Min. Eff. = 14.3 IEER (additional incentive on IEER)","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR95=\"Agribusiness\", $AR95=\"Ag\",$AR95=\"Propane\", $AR95=\"Ag Propane\", $AR95=\"Ag-Propane\"),$AC95,  $AB95),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR95=\"Agribusiness\", $AR95=\"Ag\",$AR95=\"Propane\", $AR95=\"Ag Propane\", $AR95=\"Ag-Propane\"),$AC95,  $AB95),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",17]
["H4371","H4371","N-H4371","DX Cooling ≥ 63.33 tons, Min. Eff. = 9.7 EER and 13.6 IEER (additional incentive on IEER)","H4371: DX Cooling ≥ 63.33 tons, Min. Eff. = 9.7 EER and 13.6 IEER (additional incentive on IEER)","Complete Table B1 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be ≥ 9.7 EER and 13.6 IEER. Incentive = $25/ton (existing building) or $20/ton (new construction) + $5/ton (existing building) or $3/ton (new construction) for each 1.0 IEER over 11.4.","Provide capacity and performance values to two decimal places. Standard HVAC applications only (no process cooling)","Use AHRIdirectory.org to confirm efficiency and capacity. Use AHRI capacity for incentive calc.","If split system, must be perf. Data for \"matched air handler\" or \"complete system\", NOT \"condensing unit only\"…","…and both condenser and evap. Must have coil and condenser model #'s. Coil must be replaced for retrofit projects.","SPECTRUM Unit of Measure Question = Enter Unit Total Incentive","**Ag, S&G, and BNC Programs: ENTER A PLACE HOLDER OF 1.000 for unit of measure question and QTY from Section 7. Tech Team will enter/verify values after completing hybrid calc**","Complete Cooling Eligibility Screening Tool. ","AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met. **ENTER TONNAGE IN SPECTRUM UNDER EQUIPMENT INFORMATION>ACTUAL CAPACITY**","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"$30+$5/1.0 IEER > Min","Ton","$30+$5/1.0 IEER > Min","Ton","$25+$3/1.0 IEER > Min","Ton",4371,4371,4371,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4371: DX Cooling ≥ 63.33 tons, Min. Eff. = 9.7 EER and 13.6 IEER (additional incentive on IEER)","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR96=\"Agribusiness\", $AR96=\"Ag\",$AR96=\"Propane\", $AR96=\"Ag Propane\", $AR96=\"Ag-Propane\"),$AC96,  $AB96),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR96=\"Agribusiness\", $AR96=\"Ag\",$AR96=\"Propane\", $AR96=\"Ag Propane\", $AR96=\"Ag-Propane\"),$AC96,  $AB96),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",17]
["H10025","H10025","N-H10025","Air Source Heat Pump ≥ 5.42 to < 11.25 tons, Min. Eff. = 15.1 IEER (additional incentive on IEER)",{"$f":"IF(ISBLANK(A97),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C97,IF(FOEIncentCodeType=IncentCodeTypeAg,B97,A97))&\": \") &D97","v":"H10025: Air Source Heat Pump ≥ 5.42 to < 11.25 tons, Min. Eff. = 15.1 IEER (additional incentive on IEER)"},"Complete Table B1 & B2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be ≥ 15.1 IEER. Incentive = $35/ton (existing building) or $20/ton (new construction) + $5/ton (existing building) or $3/ton (new construction) for each 1.0 IEER over 15.1.","Provide capacity and performance values to two decimal places. Standard HVAC applications only (no process cooling)","Use AHRIdirectory.org to confirm efficiency and capacity. Use AHRI capacity for incentive calc.","Split System must be a complete system listed on AHRI.",null,"SPECTRUM Unit of Measure Question = Enter Unit Total Incentive","**Ag, S&G, and BNC Programs: ENTER A PLACE HOLDER OF 1.000 for unit of measure question and QTY from Section 7. Tech Team will enter/verify values after completing hybrid calc**","Complete Cooling Eligibility Screening Tool. ","AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met. **ENTER TONNAGE IN SPECTRUM UNDER EQUIPMENT INFORMATION>ACTUAL CAPACITY**","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"$40+$5/1.0 IEER > Min","Ton","$40+$5/1.0 IEER > Min","Ton","$25+$3/1.0 IEER > Min","Ton",10025,10025,10025,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H10025: Air Source Heat Pump ≥ 5.42 to < 11.25 tons, Min. Eff. = 15.1 IEER (additional incentive on IEER)","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR97=\"Agribusiness\", $AR97=\"Ag\",$AR97=\"Propane\", $AR97=\"Ag Propane\", $AR97=\"Ag-Propane\"),$AC97,  $AB97),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR97=\"Agribusiness\", $AR97=\"Ag\",$AR97=\"Propane\", $AR97=\"Ag Propane\", $AR97=\"Ag-Propane\"),$AC97,  $AB97),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",17]
["H10026","H10026","N-H10026","Air Source Heat Pump ≥ 11.25 to < 20.00 tons, Min. Eff. = 14.5 IEER (additional incentive on IEER)","H10026: Air Source Heat Pump ≥ 11.25 to < 20.00 tons, Min. Eff. = 14.5 IEER (additional incentive on IEER)","Complete Table B1 & B2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be ≥ 14.5 IEER. Incentive = $35/ton (existing building) or $20/ton (new construction) + $5/ton (existing building) or $3/ton (new construction) for each 1.0 IEER over 14.5","Provide capacity and performance values to two decimal places. Standard HVAC applications only (no process cooling)","Use AHRIdirectory.org to confirm efficiency and capacity. Use AHRI capacity for incentive calc.","Split System must be a complete system listed on AHRI.",null,"SPECTRUM Unit of Measure Question = Enter Unit Total Incentive","**Ag, S&G, and BNC Programs: ENTER A PLACE HOLDER OF 1.000 for unit of measure question and QTY from Section 7. Tech Team will enter/verify values after completing hybrid calc**","Complete Cooling Eligibility Screening Tool. ","AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met. **ENTER TONNAGE IN SPECTRUM UNDER EQUIPMENT INFORMATION>ACTUAL CAPACITY**","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"$40+$5/1.0 IEER > Min","Ton","$40+$5/1.0 IEER > Min","Ton","$25+$3/1.0 IEER > Min","Ton",10026,10026,10026,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H10026: Air Source Heat Pump ≥ 11.25 to < 20.00 tons, Min. Eff. = 14.5 IEER (additional incentive on IEER)","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR98=\"Agribusiness\", $AR98=\"Ag\",$AR98=\"Propane\", $AR98=\"Ag Propane\", $AR98=\"Ag-Propane\"),$AC98,  $AB98),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR98=\"Agribusiness\", $AR98=\"Ag\",$AR98=\"Propane\", $AR98=\"Ag Propane\", $AR98=\"Ag-Propane\"),$AC98,  $AB98),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",17]
["H10027","H10027","N-H10027","Air Source Heat Pump ≥ 20.00 to < 63.33 tons, Min. Eff. = 13.5 IEER (additional incentive on IEER)","H10027: Air Source Heat Pump ≥ 20.00 to < 63.33 tons, Min. Eff. = 13.5 IEER (additional incentive on IEER)","Complete Table B1 & B2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be ≥ 13.5 IEER. Incentive = $35/ton (existing building) or $20/ton (new construction) + $5/ton (existing building) or $3/ton (new construction) for each 1.0 IEER over 13.5","Provide capacity and performance values to two decimal places. Standard HVAC applications only (no process cooling)","Use AHRIdirectory.org to confirm efficiency and capacity. Use AHRI capacity for incentive calc.","Split System must be a complete system listed on AHRI.","Units greater than 63.33 tons should go custom.","SPECTRUM Unit of Measure Question = Enter Unit Total Incentive","**Ag, S&G, and BNC Programs: ENTER A PLACE HOLDER OF 1.000 for unit of measure question and QTY from Section 7. Tech Team will enter/verify values after completing hybrid calc**","Complete Cooling Eligibility Screening Tool. ","AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met. **ENTER TONNAGE IN SPECTRUM UNDER EQUIPMENT INFORMATION>ACTUAL CAPACITY**","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"$40+$5/1.0 IEER > Min","Ton","$40+$5/1.0 IEER > Min","Ton","$25+$3/1.0 IEER > Min","Ton",10027,10027,10027,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H10027: Air Source Heat Pump ≥ 20.00 to < 63.33 tons, Min. Eff. = 13.5 IEER (additional incentive on IEER)","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR99=\"Agribusiness\", $AR99=\"Ag\",$AR99=\"Propane\", $AR99=\"Ag Propane\", $AR99=\"Ag-Propane\"),$AC99,  $AB99),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR99=\"Agribusiness\", $AR99=\"Ag\",$AR99=\"Propane\", $AR99=\"Ag Propane\", $AR99=\"Ag-Propane\"),$AC99,  $AB99),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",17]
["H3909","H3909","Not Eligible","Split System A/C Condensing Unit Only, ≥11.25 tons, ≥ 11.5 EER","H3909: Split System A/C Condensing Unit Only, ≥11.25 tons, ≥ 11.5 EER","Complete Table B3 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be ≥ 11.1 EER and ≥ 135 MBH (11.25 ton). Incentive = $20/ton (existing building) + $5/ton (existing building) for each 1.0 EER over 11.5","Provide capacity and performance values to two decimal places. Standard HVAC applications only (no process cooling)","Use AHRIdirectory.org to confirm efficiency and capacity. Use AHRI capacity for incentive calc.","Efficiency should be based off of the \"Condensing Unit Only\" rating.","Can not apply for both this incentive and the H4368-H4371 DX Cooling incentives.",null,"**Ag, S&G, and BNC Programs: ENTER A PLACE HOLDER OF 1.000 for unit of measure question and QTY from Section 7. Tech Team will enter/verify values after completing hybrid calc**","Complete Cooling Eligibility Screening Tool. ","AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met. **ENTER TONNAGE IN SPECTRUM UNDER EQUIPMENT INFORMATION>ACTUAL CAPACITY**","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"$25+$5/1.0 IEER > Min","Ton","$25+$5/1.0 IEER > Min","Ton","N/A","Ton",3909,3909,3909,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes",{"$f":"IF(ISBLANK(A100),\"\",IF(A100<>\"Not Eligible\",A100,IF(B100<>\"Not Eligible\",B100,C100))&\": \") &D100","v":"H3909: Split System A/C Condensing Unit Only, ≥11.25 tons, ≥ 11.5 EER"},"Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR100=\"Agribusiness\", $AR100=\"Ag\",$AR100=\"Propane\", $AR100=\"Ag Propane\", $AR100=\"Ag-Propane\"),$AC100,  $AB100),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR100=\"Agribusiness\", $AR100=\"Ag\",$AR100=\"Propane\", $AR100=\"Ag Propane\", $AR100=\"Ag-Propane\"),$AC100,  $AB100),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",18]
["H4712","H4712","N-H4712","Air-Cooled Chiller, Path A, < 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.880 kW/ton ","H4712: Air-Cooled Chiller, Path A, < 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.880 kW/ton ","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool. ","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4712,4712,4712,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4712: Air-Cooled Chiller, Path A, < 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.880 kW/ton ","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR101=\"Agribusiness\", $AR101=\"Ag\",$AR101=\"Propane\", $AR101=\"Ag Propane\", $AR101=\"Ag-Propane\"),$AC101,  $AB101),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR101=\"Agribusiness\", $AR101=\"Ag\",$AR101=\"Propane\", $AR101=\"Ag Propane\", $AR101=\"Ag-Propane\"),$AC101,  $AB101),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"HVAC",19]
["H4713","H4713","N-H4713","Air-Cooled Chiller, Path A, ≥ 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.860 kW/ton ","H4713: Air-Cooled Chiller, Path A, ≥ 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.860 kW/ton ","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4713,4713,4713,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4713: Air-Cooled Chiller, Path A, ≥ 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.860 kW/ton ","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR102=\"Agribusiness\", $AR102=\"Ag\",$AR102=\"Propane\", $AR102=\"Ag Propane\", $AR102=\"Ag-Propane\"),$AC102,  $AB102),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR102=\"Agribusiness\", $AR102=\"Ag\",$AR102=\"Propane\", $AR102=\"Ag Propane\", $AR102=\"Ag-Propane\"),$AC102,  $AB102),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":800,"d":"800.00"}},"HVAC",19]
["H4714","H4714","N-H4714","Air-Cooled Chiller, Path B, < 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.730 kW/ton ","H4714: Air-Cooled Chiller, Path B, < 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.730 kW/ton ","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4714,4714,4714,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4714: Air-Cooled Chiller, Path B, < 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.730 kW/ton ","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR103=\"Agribusiness\", $AR103=\"Ag\",$AR103=\"Propane\", $AR103=\"Ag Propane\", $AR103=\"Ag-Propane\"),$AC103,  $AB103),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR103=\"Agribusiness\", $AR103=\"Ag\",$AR103=\"Propane\", $AR103=\"Ag Propane\", $AR103=\"Ag-Propane\"),$AC103,  $AB103),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"HVAC",19]
["H4715","H4715","N-H4715","Air-Cooled Chiller, Path B, ≥ 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.720 kW/ton ","H4715: Air-Cooled Chiller, Path B, ≥ 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.720 kW/ton ","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4715,4715,4715,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4715: Air-Cooled Chiller, Path B, ≥ 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.720 kW/ton ","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR104=\"Agribusiness\", $AR104=\"Ag\",$AR104=\"Propane\", $AR104=\"Ag Propane\", $AR104=\"Ag-Propane\"),$AC104,  $AB104),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR104=\"Agribusiness\", $AR104=\"Ag\",$AR104=\"Propane\", $AR104=\"Ag Propane\", $AR104=\"Ag-Propane\"),$AC104,  $AB104),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":800,"d":"800.00"}},"HVAC",19]
["H4716","H4716","N-H4716","PD Water-Cooled, Path A, <75 tons, Full Load ≤0.720 kW/ton and IPLV ≤0.600 kW/ton","H4716: PD Water-Cooled, Path A, <75 tons, Full Load ≤0.720 kW/ton and IPLV ≤0.600 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4716,4716,4716,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4716: PD Water-Cooled, Path A, <75 tons, Full Load ≤0.720 kW/ton and IPLV ≤0.600 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR105=\"Agribusiness\", $AR105=\"Ag\",$AR105=\"Propane\", $AR105=\"Ag Propane\", $AR105=\"Ag-Propane\"),$AC105,  $AB105),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR105=\"Agribusiness\", $AR105=\"Ag\",$AR105=\"Propane\", $AR105=\"Ag Propane\", $AR105=\"Ag-Propane\"),$AC105,  $AB105),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4717","H4717","N-H4717","PD Water-Cooled, Path A, ≥ 75 tons and < 150 tons, Full Load ≤0.690 kW/ton and IPLV ≤0.560 kW/ton","H4717: PD Water-Cooled, Path A, ≥ 75 tons and < 150 tons, Full Load ≤0.690 kW/ton and IPLV ≤0.560 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4717,4717,4717,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4717: PD Water-Cooled, Path A, ≥ 75 tons and < 150 tons, Full Load ≤0.690 kW/ton and IPLV ≤0.560 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR106=\"Agribusiness\", $AR106=\"Ag\",$AR106=\"Propane\", $AR106=\"Ag Propane\", $AR106=\"Ag-Propane\"),$AC106,  $AB106),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":75,"d":"75.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR106=\"Agribusiness\", $AR106=\"Ag\",$AR106=\"Propane\", $AR106=\"Ag Propane\", $AR106=\"Ag-Propane\"),$AC106,  $AB106),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"HVAC",20]
["H4718","H4718","N-H4718","PD Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.630 kW/ton and IPLV ≤0.540 kW/ton","H4718: PD Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.630 kW/ton and IPLV ≤0.540 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4718,4718,4718,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4718: PD Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.630 kW/ton and IPLV ≤0.540 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR107=\"Agribusiness\", $AR107=\"Ag\",$AR107=\"Propane\", $AR107=\"Ag Propane\", $AR107=\"Ag-Propane\"),$AC107,  $AB107),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR107=\"Agribusiness\", $AR107=\"Ag\",$AR107=\"Propane\", $AR107=\"Ag Propane\", $AR107=\"Ag-Propane\"),$AC107,  $AB107),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"HVAC",20]
["H4719","H4719","N-H4719","PD Water-Cooled, Path A, ≥ 300 tons and < 600 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.520 kW/ton","H4719: PD Water-Cooled, Path A, ≥ 300 tons and < 600 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.520 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4719,4719,4719,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4719: PD Water-Cooled, Path A, ≥ 300 tons and < 600 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.520 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR108=\"Agribusiness\", $AR108=\"Ag\",$AR108=\"Propane\", $AR108=\"Ag Propane\", $AR108=\"Ag-Propane\"),$AC108,  $AB108),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR108=\"Agribusiness\", $AR108=\"Ag\",$AR108=\"Propane\", $AR108=\"Ag Propane\", $AR108=\"Ag-Propane\"),$AC108,  $AB108),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":600,"d":"600.00"}},"HVAC",20]
["H4720","H4720","N-H4720","PD Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","H4720: PD Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4720,4720,4720,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4720: PD Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR109=\"Agribusiness\", $AR109=\"Ag\",$AR109=\"Propane\", $AR109=\"Ag Propane\", $AR109=\"Ag-Propane\"),$AC109,  $AB109),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR109=\"Agribusiness\", $AR109=\"Ag\",$AR109=\"Propane\", $AR109=\"Ag Propane\", $AR109=\"Ag-Propane\"),$AC109,  $AB109),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4726","H4726","N-H4726","Centrifugal Water-Cooled, Path A, <150 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton","H4726: Centrifugal Water-Cooled, Path A, <150 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4726,4726,4726,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4726: Centrifugal Water-Cooled, Path A, <150 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR110=\"Agribusiness\", $AR110=\"Ag\",$AR110=\"Propane\", $AR110=\"Ag Propane\", $AR110=\"Ag-Propane\"),$AC110,  $AB110),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR110=\"Agribusiness\", $AR110=\"Ag\",$AR110=\"Propane\", $AR110=\"Ag Propane\", $AR110=\"Ag-Propane\"),$AC110,  $AB110),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4727","H4727","N-H4727","Centrifugal Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton","H4727: Centrifugal Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4727,4727,4727,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4727: Centrifugal Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR111=\"Agribusiness\", $AR111=\"Ag\",$AR111=\"Propane\", $AR111=\"Ag Propane\", $AR111=\"Ag-Propane\"),$AC111,  $AB111),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR111=\"Agribusiness\", $AR111=\"Ag\",$AR111=\"Propane\", $AR111=\"Ag Propane\", $AR111=\"Ag-Propane\"),$AC111,  $AB111),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"HVAC",20]
["H4728","H4728","N-H4728","Centrifugal Water-Cooled, Path A, ≥ 300 tons and < 400 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.520 kW/ton","H4728: Centrifugal Water-Cooled, Path A, ≥ 300 tons and < 400 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.520 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4728,{"$f":"AB112","v":4728},4728,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4728: Centrifugal Water-Cooled, Path A, ≥ 300 tons and < 400 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.520 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR112=\"Agribusiness\", $AR112=\"Ag\",$AR112=\"Propane\", $AR112=\"Ag Propane\", $AR112=\"Ag-Propane\"),$AC112,  $AB112),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR112=\"Agribusiness\", $AR112=\"Ag\",$AR112=\"Propane\", $AR112=\"Ag Propane\", $AR112=\"Ag-Propane\"),$AC112,  $AB112),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":400,"d":"400.00"}},"HVAC",20]
["H4729","H4729","N-H4729","Centrifugal Water-Cooled, Path A, ≥ 400 tons and < 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","H4729: Centrifugal Water-Cooled, Path A, ≥ 400 tons and < 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4729,4729,4729,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4729: Centrifugal Water-Cooled, Path A, ≥ 400 tons and < 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR113=\"Agribusiness\", $AR113=\"Ag\",$AR113=\"Propane\", $AR113=\"Ag Propane\", $AR113=\"Ag-Propane\"),$AC113,  $AB113),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":400,"d":"400.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR113=\"Agribusiness\", $AR113=\"Ag\",$AR113=\"Propane\", $AR113=\"Ag Propane\", $AR113=\"Ag-Propane\"),$AC113,  $AB113),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":600,"d":"600.00"}},"HVAC",20]
["H4730","H4730","N-H4730","Centrifugal Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","H4730: Centrifugal Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path A: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4730,4730,4730,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4730: Centrifugal Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR114=\"Agribusiness\", $AR114=\"Ag\",$AR114=\"Propane\", $AR114=\"Ag Propane\", $AR114=\"Ag-Propane\"),$AC114,  $AB114),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR114=\"Agribusiness\", $AR114=\"Ag\",$AR114=\"Propane\", $AR114=\"Ag Propane\", $AR114=\"Ag-Propane\"),$AC114,  $AB114),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4721","H4721","N-H4721","PD Water-Cooled, Path B, <75 tons, Full Load ≤0.780 kW/ton and IPLV ≤0.470 kW/ton","H4721: PD Water-Cooled, Path B, <75 tons, Full Load ≤0.780 kW/ton and IPLV ≤0.470 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4721,4721,4721,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4721: PD Water-Cooled, Path B, <75 tons, Full Load ≤0.780 kW/ton and IPLV ≤0.470 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR115=\"Agribusiness\", $AR115=\"Ag\",$AR115=\"Propane\", $AR115=\"Ag Propane\", $AR115=\"Ag-Propane\"),$AC115,  $AB115),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR115=\"Agribusiness\", $AR115=\"Ag\",$AR115=\"Propane\", $AR115=\"Ag Propane\", $AR115=\"Ag-Propane\"),$AC115,  $AB115),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":75,"d":"75.00"}},"HVAC",20]
["H4722","H4722","N-H4722","PD Water-Cooled, Path B, ≥ 75 tons and < 150 tons, Full Load ≤0.750 kW/ton and IPLV ≤0.460 kW/ton","H4722: PD Water-Cooled, Path B, ≥ 75 tons and < 150 tons, Full Load ≤0.750 kW/ton and IPLV ≤0.460 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4722,4722,4722,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4722: PD Water-Cooled, Path B, ≥ 75 tons and < 150 tons, Full Load ≤0.750 kW/ton and IPLV ≤0.460 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR116=\"Agribusiness\", $AR116=\"Ag\",$AR116=\"Propane\", $AR116=\"Ag Propane\", $AR116=\"Ag-Propane\"),$AC116,  $AB116),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR116=\"Agribusiness\", $AR116=\"Ag\",$AR116=\"Propane\", $AR116=\"Ag Propane\", $AR116=\"Ag-Propane\"),$AC116,  $AB116),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4723","H4723","N-H4723","PD Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.680 kW/ton and IPLV ≤0.410 kW/ton","H4723: PD Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.680 kW/ton and IPLV ≤0.410 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4723,4723,4723,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4723: PD Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.680 kW/ton and IPLV ≤0.410 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR117=\"Agribusiness\", $AR117=\"Ag\",$AR117=\"Propane\", $AR117=\"Ag Propane\", $AR117=\"Ag-Propane\"),$AC117,  $AB117),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR117=\"Agribusiness\", $AR117=\"Ag\",$AR117=\"Propane\", $AR117=\"Ag Propane\", $AR117=\"Ag-Propane\"),$AC117,  $AB117),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"HVAC",20]
["H4724","H4724","N-H4724","PD Water-Cooled, Path B, ≥ 300 tons and < 600 tons, Full Load ≤0.6250 kW/ton and IPLV ≤0.380 kW/ton","H4724: PD Water-Cooled, Path B, ≥ 300 tons and < 600 tons, Full Load ≤0.6250 kW/ton and IPLV ≤0.380 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4724,4724,4724,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4724: PD Water-Cooled, Path B, ≥ 300 tons and < 600 tons, Full Load ≤0.6250 kW/ton and IPLV ≤0.380 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR118=\"Agribusiness\", $AR118=\"Ag\",$AR118=\"Propane\", $AR118=\"Ag Propane\", $AR118=\"Ag-Propane\"),$AC118,  $AB118),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR118=\"Agribusiness\", $AR118=\"Ag\",$AR118=\"Propane\", $AR118=\"Ag Propane\", $AR118=\"Ag-Propane\"),$AC118,  $AB118),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4725","H4725","N-H4725","PD Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton","H4725: PD Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4725,4725,4725,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4725: PD Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR119=\"Agribusiness\", $AR119=\"Ag\",$AR119=\"Propane\", $AR119=\"Ag Propane\", $AR119=\"Ag-Propane\"),$AC119,  $AB119),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR119=\"Agribusiness\", $AR119=\"Ag\",$AR119=\"Propane\", $AR119=\"Ag Propane\", $AR119=\"Ag-Propane\"),$AC119,  $AB119),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4731","H4731","N-H4731","Centrifugal Water-Cooled, Path B, <150 tons, Full Load ≤0.695 kW/ton and IPLV ≤0.410 kW/ton","H4731: Centrifugal Water-Cooled, Path B, <150 tons, Full Load ≤0.695 kW/ton and IPLV ≤0.410 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4731,4731,4731,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4731: Centrifugal Water-Cooled, Path B, <150 tons, Full Load ≤0.695 kW/ton and IPLV ≤0.410 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR120=\"Agribusiness\", $AR120=\"Ag\",$AR120=\"Propane\", $AR120=\"Ag Propane\", $AR120=\"Ag-Propane\"),$AC120,  $AB120),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR120=\"Agribusiness\", $AR120=\"Ag\",$AR120=\"Propane\", $AR120=\"Ag Propane\", $AR120=\"Ag-Propane\"),$AC120,  $AB120),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4732","H4732","N-H4732","Centrifugal Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.635 kW/ton and IPLV ≤0.370 kW/ton","H4732: Centrifugal Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.635 kW/ton and IPLV ≤0.370 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4732,4732,4732,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4732: Centrifugal Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.635 kW/ton and IPLV ≤0.370 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR121=\"Agribusiness\", $AR121=\"Ag\",$AR121=\"Propane\", $AR121=\"Ag Propane\", $AR121=\"Ag-Propane\"),$AC121,  $AB121),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR121=\"Agribusiness\", $AR121=\"Ag\",$AR121=\"Propane\", $AR121=\"Ag Propane\", $AR121=\"Ag-Propane\"),$AC121,  $AB121),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
["H4733","H4733","N-H4733","Centrifugal Water-Cooled, Path B, ≥ 300 tons and < 400 tons, Full Load ≤0.595 kW/ton and IPLV ≤0.360 kW/ton","H4733: Centrifugal Water-Cooled, Path B, ≥ 300 tons and < 400 tons, Full Load ≤0.595 kW/ton and IPLV ≤0.360 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4733,4733,4733,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4733: Centrifugal Water-Cooled, Path B, ≥ 300 tons and < 400 tons, Full Load ≤0.595 kW/ton and IPLV ≤0.360 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR122=\"Agribusiness\", $AR122=\"Ag\",$AR122=\"Propane\", $AR122=\"Ag Propane\", $AR122=\"Ag-Propane\"),$AC122,  $AB122),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR122=\"Agribusiness\", $AR122=\"Ag\",$AR122=\"Propane\", $AR122=\"Ag Propane\", $AR122=\"Ag-Propane\"),$AC122,  $AB122),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":400,"d":"400.00"}},"HVAC",20]
["H4734","H4734","N-H4734","Centrifugal Water-Cooled, Path B, ≥ 400 tons and < 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton","H4734: Centrifugal Water-Cooled, Path B, ≥ 400 tons and < 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4734,4734,4734,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4734: Centrifugal Water-Cooled, Path B, ≥ 400 tons and < 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR123=\"Agribusiness\", $AR123=\"Ag\",$AR123=\"Propane\", $AR123=\"Ag Propane\", $AR123=\"Ag-Propane\"),$AC123,  $AB123),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":400,"d":"400.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR123=\"Agribusiness\", $AR123=\"Ag\",$AR123=\"Propane\", $AR123=\"Ag Propane\", $AR123=\"Ag-Propane\"),$AC123,  $AB123),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":600,"d":"600.00"}},"HVAC",20]
["H4735","H4735","N-H4735","Centrifugal Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585kW/ton and IPLV ≤0.350 kW/ton","H4735: Centrifugal Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585kW/ton and IPLV ≤0.350 kW/ton","Complete Table C1 & C2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must be Path B: Rated Full-load and Part-Load Values meet the minimum requirements. Count both in incentive calc even if one is > minimum.","Verify chiller data is per AHRI conditions (550/590 test procedures). Use AHRI data for incentive calc.","Backup or redundant systems are DNQ. ","For HVAC purposes only. Process cooling (including ice rinks, data centers, and refrig warehouse) is DNQ (should be custom).","Manufacturer spec sheet provided for chiller model number installed. Provide all kW/ton values to 3 decimals and round appropriately",null,null,"Complete Cooling Eligibility Screening Tool.","Use code minimum values for baseline – don’t need to get existing chiller info from customer, TA, or EA. Go to 3 decimal places. Multiple chillers installed/designed in series can use the combined AHRI test data from the manufacturer to estimate savings/incentives and not the individual chiller AHRI data. Unit of Measure Question = Total Incentive per Ton. Quantity = Total Tons ( Quantity X Tons for each unit). Edit Actual Requested Incentive to match Total Prescriptive Incentive due to rounding to nearest ton for quantity.","close-up of chiller, location, chiller nameplate (if possible)",{"$nulls":5},"$8+$125/1.0 ∆Eff < Max","Ton","$8+$125/1.0 ∆Eff < Max","Ton","$4+$90/1.0 ∆Eff < Max","Ton",4735,4735,4735,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H4735: Centrifugal Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585kW/ton and IPLV ≤0.350 kW/ton","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR124=\"Agribusiness\", $AR124=\"Ag\",$AR124=\"Propane\", $AR124=\"Ag Propane\", $AR124=\"Ag-Propane\"),$AC124,  $AB124),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR124=\"Agribusiness\", $AR124=\"Ag\",$AR124=\"Propane\", $AR124=\"Ag Propane\", $AR124=\"Ag-Propane\"),$AC124,  $AB124),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",20]
[{"$nulls":3},"----------------------HVAC CATALOG: VENTILATION AND CONTROLS----------------------------","----------------------HVAC CATALOG: VENTILATION AND CONTROLS----------------------------",{"$nulls":9},"",{"$nulls":22},"----------------------HVAC CATALOG: VENTILATION AND CONTROLS----------------------------",{"$nulls":3},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR125=\"Agribusiness\", $AR125=\"Ag\",$AR125=\"Propane\", $AR125=\"Ag Propane\", $AR125=\"Ag-Propane\"),$AC125,  $AB125),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR125=\"Agribusiness\", $AR125=\"Ag\",$AR125=\"Propane\", $AR125=\"Ag Propane\", $AR125=\"Ag-Propane\"),$AC125,  $AB125),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC"]
["H2314","H2314","N-H2314","Energy Recovery Ventilator, Sensible & Latent Heat","H2314: Energy Recovery Ventilator, Sensible & Latent Heat","Complete Table D of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","HVAC applications only. Industrial / process heat recovery is DNQ.","Areas served must be have AC during June - Sept, 2pm - 6pm and heated during winter.","Use of ERV where required by code DNQ. For existing buildings, replacement of existing ERV DNQ.","ERV must be AHRI certified to Standard 1060 (ahridirectory.org). If not found in AHRI, check if wheel / HX is different mfg than packaged ERV / RTU.","Supply airflow, summer/winter effectiveness for calc are per AHRI values. Use the lesser of the actual project CFM or AHRI CFM for incentive calc.","For equip where AHRI only lists the manufacturer's selection software, provide an output report from the software showing supply airflow and net summer/winter eff at the intended project conditions","Custom engineered ERVs, & ERVs integral to packedaged rooftop units or air handlers which use AHRI certified heat exchangers must provide documentation specific to the heat exchanger component within the overall system",null,"Tech Review - Use the Net Total % for 100% Air Flow Heating and Cooling values from AHRI certificate when calculating savings/supp data sheet. If Winter Effectiveness is 0%, ask design professional to rerun the model at a higher winter design day temp to get a usable value (non-zero). Small (residential size) ERVs can be HVI rated if not AHRI listed. See: www.hvi.org/hvi-certified-products-directory.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":1.35,"d":"$1.35"},"CFM",{"$f":"V126","v":{"v":1.35,"d":"$1.35"}},"CFM",{"v":1.25,"d":"$1.25"},{"$f":"W126","v":"CFM"},2314,{"$f":"AB126","v":2314},2314,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2314: Energy Recovery Ventilator, Sensible & Latent Heat","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR126=\"Agribusiness\", $AR126=\"Ag\",$AR126=\"Propane\", $AR126=\"Ag Propane\", $AR126=\"Ag-Propane\"),$AC126,  $AB126),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR126=\"Agribusiness\", $AR126=\"Ag\",$AR126=\"Propane\", $AR126=\"Ag Propane\", $AR126=\"Ag-Propane\"),$AC126,  $AB126),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"HVAC",21]
["H5082","H5082","N-H5082","Energy Recovery Ventilator, Sensible Heat Only","H5082: Energy Recovery Ventilator, Sensible Heat Only","Complete Table D of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","HVAC applications only. Industrial / process heat recovery is DNQ.","Areas served must be have AC during June - Sept, 2pm - 6pm and heated during winter.","Use of ERV where required by code DNQ. For existing buildings, replacement of existing ERV DNQ.","ERV must be AHRI certified to Standard 1060 (ahridirectory.org). If not found in AHRI, check if wheel / HX is different mfg than packaged ERV / RTU.","Supply airflow, summer/winter effectiveness for calc are per AHRI values. Use the lesser of the actual project CFM or AHRI CFM for incentive calc.","For equip where AHRI only lists the manufacturer's selection software, provide an output report from the software showing supply airflow and net summer/winter eff at the intended project conditions","Custom engineered ERVs, & ERVs integral to packedaged rooftop units or air handlers which use AHRI certified heat exchangers must provide documentation specific to the heat exchanger component within the overall system","Sensible only ERVs can be identified on spec sheets and AHRI performance ratings since the latent and net latent effectiveness are zero","Tech Review - Use the Net Total % for 100% Air Flow Heating and Cooling values from AHRI certificate when calculating savings/supp data sheet. If Winter Effectiveness is 0%, ask design professional to rerun the model at a higher winter design day temp to get a usable value (non-zero). Small (residential size) ERVs can be HVI rated if not AHRI listed. See: www.hvi.org/hvi-certified-products-directory.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":1.25,"d":"$1.25"},"CFM",{"v":1.25,"d":"$1.25"},"CFM",{"v":0.95,"d":"$0.95"},"CFM",5082,5082,5082,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5082: Energy Recovery Ventilator, Sensible Heat Only","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR127=\"Agribusiness\", $AR127=\"Ag\",$AR127=\"Propane\", $AR127=\"Ag Propane\", $AR127=\"Ag-Propane\"),$AC127,  $AB127),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR127=\"Agribusiness\", $AR127=\"Ag\",$AR127=\"Propane\", $AR127=\"Ag Propane\", $AR127=\"Ag-Propane\"),$AC127,  $AB127),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"HVAC",21]
["H3910","H3910","Not Eligible","HVAC Fan with ECM (≤ 1.0 hp), Heating Only","H3910: HVAC Fan with ECM (≤ 1.0 hp), Heating Only","For ECM ≤1 hp on air handling equipment such as exhaust fans, fan coil units, fan powered VAV boxes, unit heaters, & cabinet heaters.","Furnaces w/ ECM & single package vertical units w/ ECM don't qualify, as the ECM is covered by other measures for that equipment. ","New motors can be upgrade or replace of either shaded pole or permanent split capacitor motors. Not for routine replacement of existing ECM.","A manufacturer specification sheet that includes motor hp must be provided.","If motor >1hp and variable, switch to VFD HVAC measure.  Can reference TRM HOU and assume Inlet Guide Vanes as 'Controls Before' for hybrid calc.",{"$nulls":5},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":75,"d":"$75.00"},"Motor",{"v":75,"d":"$75.00"},"Motor","N/A","Motor",3910,3910,3910,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3910: HVAC Fan with ECM (≤ 1.0 hp), Heating Only","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR128=\"Agribusiness\", $AR128=\"Ag\",$AR128=\"Propane\", $AR128=\"Ag Propane\", $AR128=\"Ag-Propane\"),$AC128,  $AB128),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR128=\"Agribusiness\", $AR128=\"Ag\",$AR128=\"Propane\", $AR128=\"Ag Propane\", $AR128=\"Ag-Propane\"),$AC128,  $AB128),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},"HVAC",22]
["H3911","H3911","Not Eligible","HVAC Fan with ECM (≤ 1.0 hp), Cooling Only","H3911: HVAC Fan with ECM (≤ 1.0 hp), Cooling Only","For ECM ≤1 hp on air handling equipment such as exhaust fans, fan coil units, fan powered VAV boxes, unit heaters, & cabinet heaters.","Furnaces w/ ECM & single package vertical units w/ ECM don't qualify, as the ECM is covered by other measures for that equipment. ","New motors can be upgrade or replace of either shaded pole or permanent split capacitor motors. Not for routine replacement of existing ECM.","A manufacturer specification sheet that includes motor hp must be provided.","If motor >1hp and variable, switch to VFD HVAC measure.  Can reference TRM HOU and assume Inlet Guide Vanes as 'Controls Before' for hybrid calc.",{"$nulls":5},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":75,"d":"$75.00"},"Motor",{"v":75,"d":"$75.00"},"Motor","N/A","Motor",3911,3911,3911,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3911: HVAC Fan with ECM (≤ 1.0 hp), Cooling Only","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR129=\"Agribusiness\", $AR129=\"Ag\",$AR129=\"Propane\", $AR129=\"Ag Propane\", $AR129=\"Ag-Propane\"),$AC129,  $AB129),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR129=\"Agribusiness\", $AR129=\"Ag\",$AR129=\"Propane\", $AR129=\"Ag Propane\", $AR129=\"Ag-Propane\"),$AC129,  $AB129),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},"HVAC",22]
["H3912","H3912","Not Eligible","HVAC Fan with ECM (≤ 1.0 hp), Occupied Ventilation","H3912: HVAC Fan with ECM (≤ 1.0 hp), Occupied Ventilation","For ECM ≤1 hp on air handling equipment such as exhaust fans, fan coil units, fan powered VAV boxes, unit heaters, & cabinet heaters.","Furnaces w/ ECM & single package vertical units w/ ECM don't qualify, as the ECM is covered by other measures for that equipment. ","New motors can be upgrade or replace of either shaded pole or permanent split capacitor motors. Not for routine replacement of existing ECM.","A manufacturer specification sheet that includes motor hp must be provided.","If motor >1hp and variable, switch to VFD HVAC measure.  Can reference TRM HOU and assume Inlet Guide Vanes as 'Controls Before' for hybrid calc.",{"$nulls":5},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":75,"d":"$75.00"},"Motor",{"v":75,"d":"$75.00"},"Motor","N/A","Motor",3912,3912,3912,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3912: HVAC Fan with ECM (≤ 1.0 hp), Occupied Ventilation","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR130=\"Agribusiness\", $AR130=\"Ag\",$AR130=\"Propane\", $AR130=\"Ag Propane\", $AR130=\"Ag-Propane\"),$AC130,  $AB130),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR130=\"Agribusiness\", $AR130=\"Ag\",$AR130=\"Propane\", $AR130=\"Ag Propane\", $AR130=\"Ag-Propane\"),$AC130,  $AB130),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},"HVAC",22]
["H3913","H3913","Not Eligible","HVAC Fan with ECM (≤ 1.0 hp), 24/7 Ventilation","H3913: HVAC Fan with ECM (≤ 1.0 hp), 24/7 Ventilation","For ECM ≤1 hp on air handling equipment such as exhaust fans, fan coil units, fan powered VAV boxes, unit heaters, & cabinet heaters.","Furnaces w/ ECM & single package vertical units w/ ECM don't qualify, as the ECM is covered by other measures for that equipment. ","New motors can be upgrade or replace of either shaded pole or permanent split capacitor motors. Not for routine replacement of existing ECM.","A manufacturer specification sheet that includes motor hp must be provided.","If motor >1hp and variable, switch to VFD HVAC measure.  Can reference TRM HOU and assume Inlet Guide Vanes as 'Controls Before' for hybrid calc.",{"$nulls":5},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":75,"d":"$75.00"},"Motor",{"v":75,"d":"$75.00"},"Motor","N/A","Motor",3913,3913,3913,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3913: HVAC Fan with ECM (≤ 1.0 hp), 24/7 Ventilation","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR131=\"Agribusiness\", $AR131=\"Ag\",$AR131=\"Propane\", $AR131=\"Ag Propane\", $AR131=\"Ag-Propane\"),$AC131,  $AB131),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR131=\"Agribusiness\", $AR131=\"Ag\",$AR131=\"Propane\", $AR131=\"Ag Propane\", $AR131=\"Ag-Propane\"),$AC131,  $AB131),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},"HVAC",22]
["H5435","H5435","Not Eligible","Smart Switched Reluctance Motor, HVAC Supply Fan","H5435: Smart Switched Reluctance Motor, HVAC Supply Fan","Motor must be a high rotor switched reluctance motor with software controls that provide variable speed capability.","Incentive is per HP of the new motor.","New motors limited to motors ≤ 20 HP","Must be used as a supply fan motor in a rooftop unit or air handling unit.","Must replace an induction motor used on a single speed / constant flow supply fan.",{"$nulls":5},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":70,"d":"$70.00"},"HP",{"v":70,"d":"$70.00"},"HP","N/A","HP",5435,5435,5435,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5435: Smart Switched Reluctance Motor, HVAC Supply Fan","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR132=\"Agribusiness\", $AR132=\"Ag\",$AR132=\"Propane\", $AR132=\"Ag Propane\", $AR132=\"Ag-Propane\"),$AC132,  $AB132),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR132=\"Agribusiness\", $AR132=\"Ag\",$AR132=\"Propane\", $AR132=\"Ag Propane\", $AR132=\"Ag-Propane\"),$AC132,  $AB132),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",22]
["H3964","H3964","Not Eligible","Advanced Rooftop Unit Controllers","H3964: Advanced Rooftop Unit Controllers","Complete Table E of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Baseline equip must be constant volume unit w/ single speed fan, DX cooling, ≥ 1.0 hp fan, and ≥ 7 nominal tons cooling.","System must include: multispeed or variable speed control of fan, modulating outdoor air damper (maintain required OA as fan speed changes), …","… Demand control ventilation, and integrated economizer functionality. Facility must be occupied 1500 hrs/yr. ","Projects installing advanced rooftop unit controllers cannot also apply for the prescriptive incentives for DCV and VFDs.","Review default temperature setpoints in calc if not typical office bldg temps. If supply and return fan, add together for hp in calc.","List of qualified advanced rooftop unit controllers can be found on focusonenergy.com/qpls.","Eligibility advanced rooftop unit measure is based on customer having both eligible electric & natural gas utility. See catalog for details if only one provider is eligible.",null,"If both the supply fan and return/exhaust fan on the RTU have VFDs, the HP can be added together and entered as \"fan hp\" on SDS to claim savings for both fans.","close-up of RTU, location, RTU nameplate (if possible)",{"$nulls":5},{"v":125,"d":"$125.00"},"Ton",{"v":125,"d":"$125.00"},"Ton","N/A","Ton",3964,3964,3964,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3964: Advanced Rooftop Unit Controllers","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR133=\"Agribusiness\", $AR133=\"Ag\",$AR133=\"Propane\", $AR133=\"Ag Propane\", $AR133=\"Ag-Propane\"),$AC133,  $AB133),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":7,"d":"7.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR133=\"Agribusiness\", $AR133=\"Ag\",$AR133=\"Propane\", $AR133=\"Ag Propane\", $AR133=\"Ag-Propane\"),$AC133,  $AB133),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"HVAC",23]
["H2853","H2853","N-H2853","Demand Controlled Ventilation (DCV) for Multiple Zone RTU/AHU/Unit Ventilator","H2853: Demand Controlled Ventilation (DCV) for Multiple Zone RTU/AHU/Unit Ventilator","Complete Table F1 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must measure CO2 levels in conditioned space w/ wall-mounted sensors & provide required outside air w/o over-ventilating","New construction DCV installations required by code DNQ. All installations must comply with code requirements for ventilation.","Spaces with DCV must be heated, but aren't required to be air conditioned. Must provide additional ventilation during all occupied modes of operation.","Incentive can't exceed 50% of project cost, including equipment and external labor (internal labor eligible for S&G customers). Duct mounted sensors may be used if space mounting not possible & duct serves single zone. ","If DCV custom-built using CO2 sensor & building's existing automation system, provide copy of control sequence that was programmed into the building automation system.","Incentive is per CFM of OA when not in economizer mode, not total CFM provided by the AHU or RTU.",null,"Refer to app 1324891 for example of SDS misinterpretted when filled out, can't have '0' for new CFM rate","To convert MBH to Tons, Divide MBH by 12 to get Tons. It is OK to combine multiple units on one measure using total CFM - it is not necessary to enter individual measures for each unit where a DCV is being installed.","CO2 sensors, screen shots of control system (showing what controls do with CO2 sensor info)","Look closely to ensure it's really a CO2 sensor, and not a similar-looking smoke detector or other sensor.","CO2 sensors must be located within the space, with 1 sensor per zone. Using 1 return air CO2 sensor for the multi-zone air handler measure is not acceptable.","If the CO2 sensor itself can't be located or is inaccessible, a screen shot of the control system interface / computer is sufficient if it shows the CO2 sensor reading.","Obtain screen shots of the control system interface / computer when the CO2 sensor can be located - it helps display how the CO2 reading is being used.",null,{"v":0.5,"d":"$0.50"},"CFM Reduced",{"v":0.5,"d":"$0.50"},"CFM Reduced",{"v":0.5,"d":"$0.50"},"CFM Reduced",2853,2853,2853,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","H2853: Demand Controlled Ventilation (DCV) for Multiple Zone RTU/AHU/Unit Ventilator","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR134=\"Agribusiness\", $AR134=\"Ag\",$AR134=\"Propane\", $AR134=\"Ag Propane\", $AR134=\"Ag-Propane\"),$AC134,  $AB134),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR134=\"Agribusiness\", $AR134=\"Ag\",$AR134=\"Propane\", $AR134=\"Ag Propane\", $AR134=\"Ag-Propane\"),$AC134,  $AB134),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":40000,"d":"40,000.00"}},"HVAC",24]
["H3266","H3266","N-H3266","Demand Controlled Ventilation (DCV) for Single Zone RTU/AHU","H3266: Demand Controlled Ventilation (DCV) for Single Zone RTU/AHU","Complete Table F2 of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","Must measure CO2 levels in space or RA ductwork for zone served & provide required level of outside air w/o over-ventilating","DCV installations required by code DNQ. All installations must comply with code requirements for ventilation.","Spaces with DCV must be heated, but aren't required to be air conditioned. Must provide additional ventilation during all occupied modes of operation.","Incentive can't exceed 50% of project cost, including equipment and external labor (internal labor eligible for S&G customers). Duct mounted sensors may be used if space mounting not possible & duct serves single zone. ","If DCV custom-built using CO2 sensor & building's existing automation system, provide copy of control sequence that was added","Incentive is per CFM of OA when not in economizer mode, not total CFM provided by the AHU or RTU.",{"$nulls":3},"CO2 sensors, screen shots of control system (showing what controls do with CO2 sensor info)","Look closely to ensure it's really a CO2 sensor, and not a similar-looking smoke detector or other sensor.","CO2 sensor should be in return air duct, near the air handler/RTU. CO2 sensors mounted in open space is OK, if representative of area served by RTU/ air handler.","If the CO2 sensor itself can't be located or is inaccessible, a screen shot of the control system interface / computer is sufficient if it shows the CO2 sensor reading.","Obtain screen shots of the control system interface / computer when the CO2 sensor can be located - it helps display how the CO2 reading is being used.",null,{"v":650,"d":"$650.00"},"RTU or AHU",{"v":650,"d":"$650.00"},"RTU or AHU",{"v":650,"d":"$650.00"},"RTU or AHU",3266,3266,3266,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","H3266: Demand Controlled Ventilation (DCV) for Single Zone RTU/AHU","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR135=\"Agribusiness\", $AR135=\"Ag\",$AR135=\"Propane\", $AR135=\"Ag Propane\", $AR135=\"Ag-Propane\"),$AC135,  $AB135),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR135=\"Agribusiness\", $AR135=\"Ag\",$AR135=\"Propane\", $AR135=\"Ag Propane\", $AR135=\"Ag-Propane\"),$AC135,  $AB135),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",24]
["H2373","H2373","N-H2373","Guest Room Energy Management Control (PTAC w/ elec heat)","H2373: Guest Room Energy Management Control (PTAC w/ elec heat)","If PTAC w/electric resistance heating or PTHP, no supplemental data is needed.","Must be a lodging business","HVAC system must be a PTAC with electric heat. Use H4748 for PTHP and H2374 for all other","The incentive is for occupancy-based guest room energy management controls. Front desk only controls DNQ.","Occupancy control may be key-activated or sensed due to motion or body heat & must control HVAC system serving room.","All other HVAC systems: Both heating & cooling source need to be served by an eligible utility.","PTAC = Packaged Terminal Air Conditioner; PTHP = Packaged Terminal Heat Pump",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":65,"d":"$65.00"},"Room",{"v":65,"d":"$65.00"},"Room",{"v":65,"d":"$65.00"},"Room",2373,2373,2373,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2373: Guest Room Energy Management Control (PTAC w/ elec heat)","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR136=\"Agribusiness\", $AR136=\"Ag\",$AR136=\"Propane\", $AR136=\"Ag Propane\", $AR136=\"Ag-Propane\"),$AC136,  $AB136),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR136=\"Agribusiness\", $AR136=\"Ag\",$AR136=\"Propane\", $AR136=\"Ag Propane\", $AR136=\"Ag-Propane\"),$AC136,  $AB136),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",24]
["H4748","H4748","N-H4748","Guest Room Energy Management Control (PTHP)","H4748: Guest Room Energy Management Control (PTHP)","If PTAC w/electric resistance heating or PTHP, no supplemental data is needed.","Must be a lodging business","HVAC system must be a PTHP. Use H2373 for PTAC with electric heat. Use H2374 for PTAC with all others","The incentive is for occupancy-based guest room energy management controls. Front desk only controls DNQ.","Occupancy control may be key-activated or sensed due to motion or body heat & must control HVAC system serving room.","All other HVAC systems: Both heating & cooling source need to be served by an eligible utility.","PTAC = Packaged Terminal Air Conditioner; PTHP = Packaged Terminal Heat Pump",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":70,"d":"$70.00"},"Room",{"v":70,"d":"$70.00"},"Room",{"v":70,"d":"$70.00"},"Room",4748,4748,4748,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H4748: Guest Room Energy Management Control (PTHP)","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR137=\"Agribusiness\", $AR137=\"Ag\",$AR137=\"Propane\", $AR137=\"Ag Propane\", $AR137=\"Ag-Propane\"),$AC137,  $AB137),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR137=\"Agribusiness\", $AR137=\"Ag\",$AR137=\"Propane\", $AR137=\"Ag Propane\", $AR137=\"Ag-Propane\"),$AC137,  $AB137),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",24]
["H2374","H2374","N-H2374","Guest Room Energy Management Control (all other HVAC systems)","H2374: Guest Room Energy Management Control (all other HVAC systems)","Complete Table G of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.  If PTAC w/electric resistance heating or PTHP, no supplemental data is needed.","Must be a lodging business","HVAC system must be something other than PTAC with electric heat (such as PTHP, fan coil, WSHP). ","The incentive is for occupancy-based guest room energy management controls. Front desk only controls DNQ.","Occupancy control may be key-activated or sensed due to motion or body heat & must control HVAC system serving room.","All other HVAC systems: Both heating & cooling source need to be served by an eligible utility.","PTAC = Packaged Terminal Air Conditioner; PTHP = Packaged Terminal Heat Pump",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":65,"d":"$65.00"},"Room",{"v":65,"d":"$65.00"},"Room",{"v":65,"d":"$65.00"},"Room",2374,2374,2374,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2374: Guest Room Energy Management Control (all other HVAC systems)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR138=\"Agribusiness\", $AR138=\"Ag\",$AR138=\"Propane\", $AR138=\"Ag Propane\", $AR138=\"Ag-Propane\"),$AC138,  $AB138),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR138=\"Agribusiness\", $AR138=\"Ag\",$AR138=\"Propane\", $AR138=\"Ag Propane\", $AR138=\"Ag-Propane\"),$AC138,  $AB138),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",24]
["H10041","H10041","Not Eligible","Smart Thermostat Controlling Natural Gas Heat",{"$f":"IF(ISBLANK(A139),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C139,IF(FOEIncentCodeType=IncentCodeTypeAg,B139,A139))&\": \") &D139","v":"H10041: Smart Thermostat Controlling Natural Gas Heat"},"Must be certified as an ENERGY STAR smart thermostat.  ","Eligibility ok if found on \"retired\" QPL.","Ineligible if purchased through online marketplace.","Confirm eligible Gas Account",{"$nulls":6},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":50,"d":"$50.00"},"Tstat",{"v":50,"d":"$50.00"},"Tstat",{"v":50,"d":"$50.00"},"Tstat",10041,10041,10041,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10041: Smart Thermostat Controlling Natural Gas Heat","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR139=\"Agribusiness\", $AR139=\"Ag\",$AR139=\"Propane\", $AR139=\"Ag Propane\", $AR139=\"Ag-Propane\"),$AC139,  $AB139),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR139=\"Agribusiness\", $AR139=\"Ag\",$AR139=\"Propane\", $AR139=\"Ag Propane\", $AR139=\"Ag-Propane\"),$AC139,  $AB139),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",24]
["H2640","H2640","N-H2640","Variable Torque VFD, Boiler Draft Fan","H2640: Variable Torque VFD, Boiler Draft Fan","Complete Table H of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load","Must operate ≥ 2,000 hours & be ≤ 500 hp. Speed must be automatically controlled by diff pressure, flow, temp (variable signal)","Use on chillers, kitchen ventilation, and air compressor DNQ.  Refer to \"Cooling Systems\" section if installing chiller w/VFD, Process Systems catalog for VFD air compressor, or apply for a custom incentive, if installing VFD elsewhere.","Staged air volume systems (using VFD to achieve two-speed fan control on RTU) not eligible, but maybe eligible for custom incentive.","See VFD section of Process Systems catalog for constant torque and variable torque VFD incentives for industrial and process uses.","For VFD for agribusiness equipment, see Agribusiness catalog.",null,null,"New Construction via core program, not BNC if process equipment. OK if VFD is sized larger than motor - question if VFD is smaller than motor.","VFD, VFD nameplate, equipment being controlled by VFD. 1 photo showing VFD & equipment controlled is OK if information is clearly visible.","VFDs will generally be located on the wall or a support column close (say 5-20 feet) to the fan or pump that it is controlling.","Locate some industrial process VFDs in motor control center away from equipment (large gray box on floor - dimensions will vary with # of motors).","On new air-handlers/RTUs, find VFDs installed on unit exterior or within control panel section. If not visible, take clear photo of equipment nameplate & model #.","Generally the VFD will be labeled with what it controls (AHU-1, Pump CW-2, etc.)…make sure that is visible in the picture.","Verify VFD is in \"auto\" mode with output display varying (% or Hz). If unit isn't displaying this or constantly shows 60Hz, inquire about functionality/system issues.",{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP",{"v":45,"d":"$45.00"},"HP",2640,2640,2640,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2640: Variable Torque VFD, Boiler Draft Fan","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR140=\"Agribusiness\", $AR140=\"Ag\",$AR140=\"Propane\", $AR140=\"Ag Propane\", $AR140=\"Ag-Propane\"),$AC140,  $AB140),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR140=\"Agribusiness\", $AR140=\"Ag\",$AR140=\"Propane\", $AR140=\"Ag Propane\", $AR140=\"Ag-Propane\"),$AC140,  $AB140),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"HVAC",25]
["H2641","H2641","Not Eligible","Variable Torque VFD, Cooling Tower Fan","H2641: Variable Torque VFD, Cooling Tower Fan","Complete Table H of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load","Must operate ≥ 2,000 hours & be ≤ 500 hp. Speed must be automatically controlled by diff pressure, flow, temp (variable signal)","Use on chillers, kitchen ventilation, and air compressor DNQ.  Refer to \"Cooling Systems\" section if installing chiller w/VFD, Process Systems catalog for VFD air compressor, or apply for a custom incentive, if installing VFD elsewhere.","Staged air volume systems (using VFD to achieve two-speed fan control on RTU) not eligible, but maybe eligible for custom incentive.","See VFD section of Process Systems catalog for constant torque and variable torque VFD incentives for industrial and process uses.","For VFD for agribusiness equipment, see Agribusiness catalog.",null,null,"New Construction via core program, not BNC if process equipment. OK if VFD is sized larger than motor - question if VFD is smaller than motor.","VFD, VFD nameplate, equipment being controlled by VFD. 1 photo showing VFD & equipment controlled is OK if information is clearly visible.","VFDs will generally be located on the wall or a support column close (say 5-20 feet) to the fan or pump that it is controlling.","Locate some industrial process VFDs in motor control center away from equipment (large gray box on floor - dimensions will vary with # of motors).","On new air-handlers/RTUs, find VFDs installed on unit exterior or within control panel section. If not visible, take clear photo of equipment nameplate & model #.","Generally the VFD will be labeled with what it controls (AHU-1, Pump CW-2, etc.)…make sure that is visible in the picture.","Verify VFD is in \"auto\" mode with output display varying (% or Hz). If unit isn't displaying this or constantly shows 60Hz, inquire about functionality/system issues.",{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP","N/A","HP",2641,2641,2641,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2641: Variable Torque VFD, Cooling Tower Fan","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR141=\"Agribusiness\", $AR141=\"Ag\",$AR141=\"Propane\", $AR141=\"Ag Propane\", $AR141=\"Ag-Propane\"),$AC141,  $AB141),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR141=\"Agribusiness\", $AR141=\"Ag\",$AR141=\"Propane\", $AR141=\"Ag Propane\", $AR141=\"Ag-Propane\"),$AC141,  $AB141),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"HVAC",25]
["H2643","H2643","Not Eligible","Variable Torque VFD, HVAC Fan","H2643: Variable Torque VFD, HVAC Fan","Complete Table H of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load","Must operate ≥ 2,000 hours & be ≤ 500 hp. Speed must be automatically controlled by diff pressure, flow, temp (variable signal)","Use on chillers, kitchen ventilation, and air compressor DNQ.  Refer to \"Cooling Systems\" section if installing chiller w/VFD, Process Systems catalog for VFD air compressor, or apply for a custom incentive, if installing VFD elsewhere.","Staged air volume systems (using VFD to achieve two-speed fan control on RTU) not eligible, but maybe eligible for custom incentive.","See VFD section of Process Systems catalog for constant torque and variable torque VFD incentives for industrial and process uses.","For VFD for agribusiness equipment, see Agribusiness catalog.",null,null,"Use individual itemized VFD project costs. OK if VFD is sized larger than motor - question if VFD is smaller than motor.","VFD, VFD nameplate, equipment being controlled by VFD. 1 photo showing VFD & equipment controlled is OK if information is clearly visible.","VFDs will generally be located on the wall or a support column close (say 5-20 feet) to the fan or pump that it is controlling.","Locate some industrial process VFDs in motor control center away from equipment (large gray box on floor - dimensions will vary with # of motors).","On new air-handlers/RTUs, find VFDs installed on unit exterior or within control panel section. If not visible, take clear photo of equipment nameplate & model #.","Generally the VFD will be labeled with what it controls (AHU-1, Pump CW-2, etc.)…make sure that is visible in the picture.","Verify VFD is in \"auto\" mode with output display varying (% or Hz). If unit isn't displaying this or constantly shows 60Hz, inquire about functionality/system issues.",{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP","N/A","HP",2643,2643,2643,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2643: Variable Torque VFD, HVAC Fan","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR142=\"Agribusiness\", $AR142=\"Ag\",$AR142=\"Propane\", $AR142=\"Ag Propane\", $AR142=\"Ag-Propane\"),$AC142,  $AB142),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR142=\"Agribusiness\", $AR142=\"Ag\",$AR142=\"Propane\", $AR142=\"Ag Propane\", $AR142=\"Ag-Propane\"),$AC142,  $AB142),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"HVAC",25]
["H2726","H2726","Not Eligible","Variable Torque VFD, Chilled Water Distribution Pump","H2726: Variable Torque VFD, Chilled Water Distribution Pump","Complete Table H of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load","Must operate ≥ 2,000 hours & be ≤ 500 hp. Speed must be automatically controlled by diff pressure, flow, temp (variable signal)","Use on chillers, kitchen ventilation, and air compressor DNQ.  Refer to \"Cooling Systems\" section if installing chiller w/VFD, Process Systems catalog for VFD air compressor, or apply for a custom incentive, if installing VFD elsewhere.","Staged air volume systems (using VFD to achieve two-speed fan control on RTU) not eligible, but maybe eligible for custom incentive.","See VFD section of Process Systems catalog for constant torque and variable torque VFD incentives for industrial and process uses.","For VFD for agribusiness equipment, see Agribusiness catalog.",null,null,"New Construction via core program, not BNC if process equipment. OK if VFD is sized larger than motor - question if VFD is smaller than motor.","VFD, VFD nameplate, equipment being controlled by VFD. 1 photo showing VFD & equipment controlled is OK if information is clearly visible.","VFDs will generally be located on the wall or a support column close (say 5-20 feet) to the fan or pump that it is controlling.","Locate some industrial process VFDs in motor control center away from equipment (large gray box on floor - dimensions will vary with # of motors).","On new air-handlers/RTUs, find VFDs installed on unit exterior or within control panel section. If not visible, take clear photo of equipment nameplate & model #.","Generally the VFD will be labeled with what it controls (AHU-1, Pump CW-2, etc.)…make sure that is visible in the picture.","Verify VFD is in \"auto\" mode with output display varying (% or Hz). If unit isn't displaying this or constantly shows 60Hz, inquire about functionality/system issues.",{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP","N/A","HP",2726,2726,2726,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2726: Variable Torque VFD, Chilled Water Distribution Pump","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR143=\"Agribusiness\", $AR143=\"Ag\",$AR143=\"Propane\", $AR143=\"Ag Propane\", $AR143=\"Ag-Propane\"),$AC143,  $AB143),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR143=\"Agribusiness\", $AR143=\"Ag\",$AR143=\"Propane\", $AR143=\"Ag Propane\", $AR143=\"Ag-Propane\"),$AC143,  $AB143),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"HVAC",25]
["H2644","H2644","Not Eligible","Variable Torque VFD, HVAC Heating Pump","H2644: Variable Torque VFD, HVAC Heating Pump","Complete Table H of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load","Must operate ≥ 2,000 hours & be ≤ 500 hp. Speed must be automatically controlled by diff pressure, flow, temp (variable signal)","Use on chillers, kitchen ventilation, and air compressor DNQ.  Refer to \"Cooling Systems\" section if installing chiller w/VFD, Process Systems catalog for VFD air compressor, or apply for a custom incentive, if installing VFD elsewhere.","Staged air volume systems (using VFD to achieve two-speed fan control on RTU) not eligible, but maybe eligible for custom incentive.","See VFD section of Process Systems catalog for constant torque and variable torque VFD incentives for industrial and process uses.","For VFD for agribusiness equipment, see Agribusiness catalog.",null,null,"Use individual itemized VFD project costs. OK if VFD is sized larger than motor - question if VFD is smaller than motor.","VFD, VFD nameplate, equipment being controlled by VFD. 1 photo showing VFD & equipment controlled is OK if information is clearly visible.","VFDs will generally be located on the wall or a support column close (say 5-20 feet) to the fan or pump that it is controlling.","Locate some industrial process VFDs in motor control center away from equipment (large gray box on floor - dimensions will vary with # of motors).","On new air-handlers/RTUs, find VFDs installed on unit exterior or within control panel section. If not visible, take clear photo of equipment nameplate & model #.","Generally the VFD will be labeled with what it controls (AHU-1, Pump CW-2, etc.)…make sure that is visible in the picture.","Verify VFD is in \"auto\" mode with output display varying (% or Hz). If unit isn't displaying this or constantly shows 60Hz, inquire about functionality/system issues.",{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP","N/A","HP",2644,2644,2644,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2644: Variable Torque VFD, HVAC Heating Pump","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR144=\"Agribusiness\", $AR144=\"Ag\",$AR144=\"Propane\", $AR144=\"Ag Propane\", $AR144=\"Ag-Propane\"),$AC144,  $AB144),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR144=\"Agribusiness\", $AR144=\"Ag\",$AR144=\"Propane\", $AR144=\"Ag Propane\", $AR144=\"Ag-Propane\"),$AC144,  $AB144),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"HVAC",25]
["H2646","H2646","N-H2646","Variable Torque VFD, Pool Pump Motor","H2646: Variable Torque VFD, Pool Pump Motor","Complete Table H of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load","Must operate ≥ 2,000 hours & be ≤ 500 hp. Speed must be automatically controlled by diff pressure, flow, temp (variable signal)","Use on chillers, kitchen ventilation, and air compressor DNQ.  Refer to \"Cooling Systems\" section if installing chiller w/VFD, Process Systems catalog for VFD air compressor, or apply for a custom incentive, if installing VFD elsewhere.","Staged air volume systems (using VFD to achieve two-speed fan control on RTU) not eligible, but maybe eligible for custom incentive.","See VFD section of Process Systems catalog for constant torque and variable torque VFD incentives for industrial and process uses.","For VFD for agribusiness equipment, see Agribusiness catalog.",null,null,"Use individual itemized VFD project costs. OK if VFD is sized larger than motor - question if VFD is smaller than motor.","VFD, VFD nameplate, equipment being controlled by VFD. 1 photo showing VFD & equipment controlled is OK if information is clearly visible.","VFDs will generally be located on the wall or a support column close (say 5-20 feet) to the fan or pump that it is controlling.","Locate some industrial process VFDs in motor control center away from equipment (large gray box on floor - dimensions will vary with # of motors).","On new air-handlers/RTUs, find VFDs installed on unit exterior or within control panel section. If not visible, take clear photo of equipment nameplate & model #.","Generally the VFD will be labeled with what it controls (AHU-1, Pump CW-2, etc.)…make sure that is visible in the picture.","Verify VFD is in \"auto\" mode with output display varying (% or Hz). If unit isn't displaying this or constantly shows 60Hz, inquire about functionality/system issues.",{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP",{"v":45,"d":"$45.00"},"HP",2646,2646,2646,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2646: Variable Torque VFD, Pool Pump Motor","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR145=\"Agribusiness\", $AR145=\"Ag\",$AR145=\"Propane\", $AR145=\"Ag Propane\", $AR145=\"Ag-Propane\"),$AC145,  $AB145),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR145=\"Agribusiness\", $AR145=\"Ag\",$AR145=\"Propane\", $AR145=\"Ag Propane\", $AR145=\"Ag-Propane\"),$AC145,  $AB145),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":25,"d":"25.00"}},"HVAC",25]
["H3494","H3494","N-H3494","Variable Speed ECM Pump, < 100 Watts Max Input, Domestic Hot Water Recirculation","H3494: Variable Speed ECM Pump, < 100 Watts Max Input, Domestic Hot Water Recirculation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":80,"d":"$80.00"},"Pump",{"v":80,"d":"$80.00"},"Pump",{"$f":"V146","v":{"v":80,"d":"$80.00"}},"Pump",3494,{"$f":"AB146","v":3494},{"$f":"AB146","v":3494},"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3494: Variable Speed ECM Pump, < 100 Watts Max Input, Domestic Hot Water Recirculation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR146=\"Agribusiness\", $AR146=\"Ag\",$AR146=\"Propane\", $AR146=\"Ag Propane\", $AR146=\"Ag-Propane\"),$AC146,  $AB146),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR146=\"Agribusiness\", $AR146=\"Ag\",$AR146=\"Propane\", $AR146=\"Ag Propane\", $AR146=\"Ag-Propane\"),$AC146,  $AB146),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3495","H3495","N-H3495","Variable Speed ECM Pump, 100 - 500 Watts Max Input, Domestic Hot Water Recirculation","H3495: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Domestic Hot Water Recirculation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":200,"d":"$200.00"},"Pump",{"$f":"V147","v":{"v":200,"d":"$200.00"}},"Pump",{"$f":"V147","v":{"v":200,"d":"$200.00"}},"Pump",3495,{"$f":"AB147","v":3495},{"$f":"AB147","v":3495},"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3495: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Domestic Hot Water Recirculation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR147=\"Agribusiness\", $AR147=\"Ag\",$AR147=\"Propane\", $AR147=\"Ag Propane\", $AR147=\"Ag-Propane\"),$AC147,  $AB147),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR147=\"Agribusiness\", $AR147=\"Ag\",$AR147=\"Propane\", $AR147=\"Ag Propane\", $AR147=\"Ag-Propane\"),$AC147,  $AB147),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3496","H3496","N-H3496","Variable Speed ECM Pump, > 500 Watts Max Input, Domestic Hot Water Recirculation","H3496: Variable Speed ECM Pump, > 500 Watts Max Input, Domestic Hot Water Recirculation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":400,"d":"$400.00"},"Pump",{"v":400,"d":"$400.00"},"Pump",{"v":400,"d":"$400.00"},"Pump",3496,3496,3496,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3496: Variable Speed ECM Pump, > 500 Watts Max Input, Domestic Hot Water Recirculation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR148=\"Agribusiness\", $AR148=\"Ag\",$AR148=\"Propane\", $AR148=\"Ag Propane\", $AR148=\"Ag-Propane\"),$AC148,  $AB148),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR148=\"Agribusiness\", $AR148=\"Ag\",$AR148=\"Propane\", $AR148=\"Ag Propane\", $AR148=\"Ag-Propane\"),$AC148,  $AB148),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3497","H3497","N-H3497","Variable Speed ECM Pump, < 100 Watts Max Input, Heating Water Circulation","H3497: Variable Speed ECM Pump, < 100 Watts Max Input, Heating Water Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":80,"d":"$80.00"},"Pump",{"v":80,"d":"$80.00"},"Pump",{"v":80,"d":"$80.00"},"Pump",3497,3497,3497,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3497: Variable Speed ECM Pump, < 100 Watts Max Input, Heating Water Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR149=\"Agribusiness\", $AR149=\"Ag\",$AR149=\"Propane\", $AR149=\"Ag Propane\", $AR149=\"Ag-Propane\"),$AC149,  $AB149),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR149=\"Agribusiness\", $AR149=\"Ag\",$AR149=\"Propane\", $AR149=\"Ag Propane\", $AR149=\"Ag-Propane\"),$AC149,  $AB149),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3498","H3498","N-H3498","Variable Speed ECM Pump, 100 - 500 Watts Max Input, Heating Water Circulation","H3498: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Heating Water Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":200,"d":"$200.00"},"Pump",{"v":200,"d":"$200.00"},"Pump",{"v":200,"d":"$200.00"},"Pump",3498,3498,3498,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3498: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Heating Water Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR150=\"Agribusiness\", $AR150=\"Ag\",$AR150=\"Propane\", $AR150=\"Ag Propane\", $AR150=\"Ag-Propane\"),$AC150,  $AB150),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR150=\"Agribusiness\", $AR150=\"Ag\",$AR150=\"Propane\", $AR150=\"Ag Propane\", $AR150=\"Ag-Propane\"),$AC150,  $AB150),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3499","H3499","N-H3499","Variable Speed ECM Pump, > 500 Watts Max Input, Heating Water Circulation","H3499: Variable Speed ECM Pump, > 500 Watts Max Input, Heating Water Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":400,"d":"$400.00"},"Pump",{"v":400,"d":"$400.00"},"Pump",{"v":400,"d":"$400.00"},"Pump",3499,3499,3499,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3499: Variable Speed ECM Pump, > 500 Watts Max Input, Heating Water Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR151=\"Agribusiness\", $AR151=\"Ag\",$AR151=\"Propane\", $AR151=\"Ag Propane\", $AR151=\"Ag-Propane\"),$AC151,  $AB151),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR151=\"Agribusiness\", $AR151=\"Ag\",$AR151=\"Propane\", $AR151=\"Ag Propane\", $AR151=\"Ag-Propane\"),$AC151,  $AB151),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3500","H3500","N-H3500","Variable Speed ECM Pump, < 100 Watts Max Input, Cooling Water Circulation","H3500: Variable Speed ECM Pump, < 100 Watts Max Input, Cooling Water Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":80,"d":"$80.00"},"Pump",{"v":80,"d":"$80.00"},"Pump",{"v":80,"d":"$80.00"},"Pump",3500,3500,3500,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3500: Variable Speed ECM Pump, < 100 Watts Max Input, Cooling Water Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR152=\"Agribusiness\", $AR152=\"Ag\",$AR152=\"Propane\", $AR152=\"Ag Propane\", $AR152=\"Ag-Propane\"),$AC152,  $AB152),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR152=\"Agribusiness\", $AR152=\"Ag\",$AR152=\"Propane\", $AR152=\"Ag Propane\", $AR152=\"Ag-Propane\"),$AC152,  $AB152),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3501","H3501","N-H3501","Variable Speed ECM Pump, 100 - 500 Watts Max Input, Cooling Water Circulation","H3501: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Cooling Water Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":200,"d":"$200.00"},"Pump",{"v":200,"d":"$200.00"},"Pump",{"v":200,"d":"$200.00"},"Pump",3501,3501,3501,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3501: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Cooling Water Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR153=\"Agribusiness\", $AR153=\"Ag\",$AR153=\"Propane\", $AR153=\"Ag Propane\", $AR153=\"Ag-Propane\"),$AC153,  $AB153),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR153=\"Agribusiness\", $AR153=\"Ag\",$AR153=\"Propane\", $AR153=\"Ag Propane\", $AR153=\"Ag-Propane\"),$AC153,  $AB153),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3502","H3502","N-H3502","Variable Speed ECM Pump, > 500 Watts Max Input, Cooling Water Circulation","H3502: Variable Speed ECM Pump, > 500 Watts Max Input, Cooling Water Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":400,"d":"$400.00"},"Pump",{"v":400,"d":"$400.00"},"Pump",{"v":400,"d":"$400.00"},"Pump",3502,3502,3502,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3502: Variable Speed ECM Pump, > 500 Watts Max Input, Cooling Water Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR154=\"Agribusiness\", $AR154=\"Ag\",$AR154=\"Propane\", $AR154=\"Ag Propane\", $AR154=\"Ag-Propane\"),$AC154,  $AB154),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR154=\"Agribusiness\", $AR154=\"Ag\",$AR154=\"Propane\", $AR154=\"Ag Propane\", $AR154=\"Ag-Propane\"),$AC154,  $AB154),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3503","H3503","N-H3503","Variable Speed ECM Pump, < 100 Watts Max Input, Water Loop Heat Pump Circulation","H3503: Variable Speed ECM Pump, < 100 Watts Max Input, Water Loop Heat Pump Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":80,"d":"$80.00"},"Pump",{"v":80,"d":"$80.00"},"Pump",{"v":80,"d":"$80.00"},"Pump",3503,3503,3503,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3503: Variable Speed ECM Pump, < 100 Watts Max Input, Water Loop Heat Pump Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR155=\"Agribusiness\", $AR155=\"Ag\",$AR155=\"Propane\", $AR155=\"Ag Propane\", $AR155=\"Ag-Propane\"),$AC155,  $AB155),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR155=\"Agribusiness\", $AR155=\"Ag\",$AR155=\"Propane\", $AR155=\"Ag Propane\", $AR155=\"Ag-Propane\"),$AC155,  $AB155),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3504","H3504","N-H3504","Variable Speed ECM Pump, 100 - 500 Watts Max Input, Water Loop Heat Pump Circulation","H3504: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Water Loop Heat Pump Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":200,"d":"$200.00"},"Pump",{"v":200,"d":"$200.00"},"Pump",{"v":200,"d":"$200.00"},"Pump",3504,3504,3504,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3504: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Water Loop Heat Pump Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR156=\"Agribusiness\", $AR156=\"Ag\",$AR156=\"Propane\", $AR156=\"Ag Propane\", $AR156=\"Ag-Propane\"),$AC156,  $AB156),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR156=\"Agribusiness\", $AR156=\"Ag\",$AR156=\"Propane\", $AR156=\"Ag Propane\", $AR156=\"Ag-Propane\"),$AC156,  $AB156),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
["H3505","H3505","N-H3505","Variable Speed ECM Pump, > 500 Watts Max Input, Water Loop Heat Pump Circulation","H3505: Variable Speed ECM Pump, > 500 Watts Max Input, Water Loop Heat Pump Circulation","Replacement of PSC motor pumps either continuous run, timer controlled, or controlled by temp sensor.","New pump speed must be automatically controlled by differential pressure, flow, temp, or other variable signal.","Ineligible for NC if HVAC hydronic system is >=300MBh.",{"$nulls":7},"Pump and components of respective measure, e.g. water heater if on DHW.",{"$nulls":5},{"v":400,"d":"$400.00"},"Pump",{"v":400,"d":"$400.00"},"Pump",{"v":400,"d":"$400.00"},"Pump",3505,3505,3505,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3505: Variable Speed ECM Pump, > 500 Watts Max Input, Water Loop Heat Pump Circulation","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR157=\"Agribusiness\", $AR157=\"Ag\",$AR157=\"Propane\", $AR157=\"Ag Propane\", $AR157=\"Ag-Propane\"),$AC157,  $AB157),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR157=\"Agribusiness\", $AR157=\"Ag\",$AR157=\"Propane\", $AR157=\"Ag Propane\", $AR157=\"Ag-Propane\"),$AC157,  $AB157),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",26]
[{"$nulls":3},"-----------------------HVAC CATALOG: BUILDING ENVELOPE ----------------------","-----------------------HVAC CATALOG: BUILDING ENVELOPE ----------------------",{"$nulls":32},"-----------------------HVAC CATALOG: BUILDING ENVELOPE ----------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR158=\"Agribusiness\", $AR158=\"Ag\",$AR158=\"Propane\", $AR158=\"Ag Propane\", $AR158=\"Ag-Propane\"),$AC158,  $AB158),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR158=\"Agribusiness\", $AR158=\"Ag\",$AR158=\"Propane\", $AR158=\"Ag Propane\", $AR158=\"Ag-Propane\"),$AC158,  $AB158),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["B2300","B2300","Not Eligible","Dock Door Infiltration Reduction, New Install","B2300: Dock Door Infiltration Reduction, New Install","Intended to reduce air infiltration at truck loading docks. Seals must effectively close all gaps between building & semitrailer.","To qualify, building interior space must be heated with natural gas during winter. ","Refrigerated interior spaces are not eligible but may qualify for a custom incentive.","Dock door seals extend out to fill gap between dock door & trailer, including “hinge gap” for outwardly swinging trailer doors.","Air seals may be attached to exterior of building or around edge of ramp and must maintain effective seal both when ramp is in use or out of use.","Brush-type or whisker-type perimeter/edge seals may be used with air seals but do not qualify for incentive",{"$nulls":10},{"v":250,"d":"$250.00"},"Door Sealed",{"$f":"V159","v":{"v":250,"d":"$250.00"}},"Door Sealed","N/A",{"$f":"W159","v":"Door Sealed"},2300,2300,2300,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","B2300: Dock Door Infiltration Reduction, New Install","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR159=\"Agribusiness\", $AR159=\"Ag\",$AR159=\"Propane\", $AR159=\"Ag Propane\", $AR159=\"Ag-Propane\"),$AC159,  $AB159),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR159=\"Agribusiness\", $AR159=\"Ag\",$AR159=\"Propane\", $AR159=\"Ag Propane\", $AR159=\"Ag-Propane\"),$AC159,  $AB159),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",27]
["B2301","B2301","Not Eligible","Dock Door Infiltration Reduction, Replace Existing","B2301: Dock Door Infiltration Reduction, Replace Existing","Intended to reduce air infiltration at truck loading docks. Seals must effectively close all gaps between building & semitrailer.","To qualify, building interior space must be heated with natural gas during winter. ","Refrigerated interior spaces are not eligible but may qualify for a custom incentive.","Dock door seals extend out to fill gap between dock door & trailer, including “hinge gap” for outwardly swinging trailer doors.","Air seals may be attached to exterior of building or around edge of ramp and must maintain effective seal both when ramp is in use or out of use.","Brush-type or whisker-type perimeter/edge seals may be used with air seals but do not qualify for incentive",{"$nulls":10},{"v":250,"d":"$250.00"},"Door Sealed",{"v":250,"d":"$250.00"},"Door Sealed","N/A","Door Sealed",2301,2301,2301,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","B2301: Dock Door Infiltration Reduction, Replace Existing","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR160=\"Agribusiness\", $AR160=\"Ag\",$AR160=\"Propane\", $AR160=\"Ag Propane\", $AR160=\"Ag-Propane\"),$AC160,  $AB160),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR160=\"Agribusiness\", $AR160=\"Ag\",$AR160=\"Propane\", $AR160=\"Ag Propane\", $AR160=\"Ag-Propane\"),$AC160,  $AB160),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",27]
["B2302","B2302","Not Eligible","Dock Pit/Ramp External Seal, Added to Existing \"Brush\" Barrier","B2302: Dock Pit/Ramp External Seal, Added to Existing \"Brush\" Barrier","Intended to reduce air infiltration at truck loading docks. Seals must effectively close all gaps between building & semitrailer.","Building interior must be heated w/ natural gas. Refrigerated space not eligible but may qualify for custom incentive.","Leveler ramp air seals reduce air infiltration from around the loading dock leveler ramp. ","Air seals may be attached to building exterior or edge of ramp & must maintain effective seal when ramp is in use or out of use. ","Brush-type or whisker-type perimeter/edge seals may be used in conjunction with air seals but do not qualify for incentive.",{"$nulls":11},{"v":125,"d":"$125.00"},"Pit sealed",{"v":125,"d":"$125.00"},"Pit sealed","N/A","Pit sealed",2302,2302,2302,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","B2302: Dock Pit/Ramp External Seal, Added to Existing \"Brush\" Barrier","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR161=\"Agribusiness\", $AR161=\"Ag\",$AR161=\"Propane\", $AR161=\"Ag Propane\", $AR161=\"Ag-Propane\"),$AC161,  $AB161),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR161=\"Agribusiness\", $AR161=\"Ag\",$AR161=\"Propane\", $AR161=\"Ag Propane\", $AR161=\"Ag-Propane\"),$AC161,  $AB161),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",27]
["B2303","B2303","N-B2303","Dock Pit/Ramp External Seal, No Brush Barrier Present","B2303: Dock Pit/Ramp External Seal, No Brush Barrier Present","Intended to reduce air infiltration at truck loading docks. Seals must effectively close all gaps between building & semitrailer.","Building interior must be heated w/ natural gas. Refrigerated space not eligible but may qualify for custom incentive.","Leveler ramp air seals reduce air infiltration from around the loading dock leveler ramp. ","Air seals may be attached to building exterior or edge of ramp & must maintain effective seal when ramp is in use or out of use. ","Brush-type or whisker-type perimeter/edge seals may be used in conjunction with air seals but do not qualify for incentive.",{"$nulls":11},{"v":125,"d":"$125.00"},"Pit sealed",{"v":125,"d":"$125.00"},"Pit sealed",{"v":125,"d":"$125.00"},"Pit sealed",2303,2303,2303,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","B2303: Dock Pit/Ramp External Seal, No Brush Barrier Present","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR162=\"Agribusiness\", $AR162=\"Ag\",$AR162=\"Propane\", $AR162=\"Ag Propane\", $AR162=\"Ag-Propane\"),$AC162,  $AB162),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR162=\"Agribusiness\", $AR162=\"Ag\",$AR162=\"Propane\", $AR162=\"Ag Propane\", $AR162=\"Ag-Propane\"),$AC162,  $AB162),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",27]
["B5438","B5438","N-B5438","Spring-loaded Overhead Door Hinge","B5438: Spring-loaded Overhead Door Hinge","Reduces air infiltration by using spring-loaded hinges that keep overhead door sections pressed tightly against the seals","Must be heated with only natural gas during winter. Waste oil burners, propane, or otherfuel sources are not eligible.","Rreplacement of existing spring-loaded overhead door hinges do not qualify.",{"$nulls":7},"Close up of spring loaded door hinge, overhead door from inside showing all hinges.",{"$nulls":5},{"v":170,"d":"$170.00"},"Per Door",{"v":170,"d":"$170.00"},"Per Door",{"v":130,"d":"$130.00"},"Per Door",5438,5438,5438,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","B5438: Spring-loaded Overhead Door Hinge","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR163=\"Agribusiness\", $AR163=\"Ag\",$AR163=\"Propane\", $AR163=\"Ag Propane\", $AR163=\"Ag-Propane\"),$AC163,  $AB163),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR163=\"Agribusiness\", $AR163=\"Ag\",$AR163=\"Propane\", $AR163=\"Ag Propane\", $AR163=\"Ag-Propane\"),$AC163,  $AB163),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"HVAC",27]
["B10219","B10219","Not Eligible","Roof Insulation, Existing Insulation <R-20","B10219: Roof Insulation, Existing Insulation <R-20","Non-res building heated via NG.  May be cooled, but not required.","Minimum of R-10 must be added.  May be a combination of various insulation types.","Complete Table I of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.",{"$nulls":7},"Documentation of existing and new insulation type and thickness if possible.",{"$nulls":5},{"v":0.3,"d":"$0.30"},"Sq Ft",{"v":0.3,"d":"$0.30"},"Sq Ft","N/A","Sq Ft",10219,10219,10219,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A164),\"\",IF(A164<>\"Not Eligible\",A164,IF(B164<>\"Not Eligible\",B164,C164))&\": \") &D164","v":"B10219: Roof Insulation, Existing Insulation <R-20"},"Yes","Yes","Sq Ft",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR164=\"Agribusiness\", $AR164=\"Ag\",$AR164=\"Propane\", $AR164=\"Ag Propane\", $AR164=\"Ag-Propane\"),$AC164,  $AB164),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR164=\"Agribusiness\", $AR164=\"Ag\",$AR164=\"Propane\", $AR164=\"Ag Propane\", $AR164=\"Ag-Propane\"),$AC164,  $AB164),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"HVAC",27]
["B10220","B10220","Not Eligible","Roof Insulation, Existing Insulation ≥R-20","B10220: Roof Insulation, Existing Insulation ≥R-20","Non-res building heated via NG.  May be cooled, but not required.","Minimum of R-10 must be added.  May be a combination of various insulation types.","Complete Table I of the \"HVAC/Plumbing Incentive Catalog Supplemental Data Sheet\" for this measure.",{"$nulls":7},"Documentation of existing and new insulation type and thickness if possible.",{"$nulls":5},{"v":0.15,"d":"$0.15"},"Sq Ft",{"v":0.15,"d":"$0.15"},"Sq Ft","N/A","Sq Ft",10220,10220,10220,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","B10220: Roof Insulation, Existing Insulation ≥R-20","Yes","Yes","Sq Ft",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR165=\"Agribusiness\", $AR165=\"Ag\",$AR165=\"Propane\", $AR165=\"Ag Propane\", $AR165=\"Ag-Propane\"),$AC165,  $AB165),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR165=\"Agribusiness\", $AR165=\"Ag\",$AR165=\"Propane\", $AR165=\"Ag Propane\", $AR165=\"Ag-Propane\"),$AC165,  $AB165),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"HVAC",27]
[{"$nulls":3},"-----------------------COMMERCIAL REFRIGERATION CATALOG: NON-SELF CONTAINED-----------------------","-----------------------COMMERCIAL REFRIGERATION CATALOG: NON-SELF CONTAINED-----------------------",{"$nulls":32},"-----------------------COMMERCIAL REFRIGERATION CATALOG: NON-SELF CONTAINED-----------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR166=\"Agribusiness\", $AR166=\"Ag\",$AR166=\"Propane\", $AR166=\"Ag Propane\", $AR166=\"Ag-Propane\"),$AC166,  $AB166),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR166=\"Agribusiness\", $AR166=\"Ag\",$AR166=\"Propane\", $AR166=\"Ag Propane\", $AR166=\"Ag-Propane\"),$AC166,  $AB166),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["R2308","R2308","Not Eligible","ECM Evaporator Fan Motor, Walk-in Cooler, < 1/20 HP",{"$f":"IF(ISBLANK(A167),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C167,IF(FOEIncentCodeType=IncentCodeTypeAg,B167,A167))&\": \") &D167","v":"R2308: ECM Evaporator Fan Motor, Walk-in Cooler, < 1/20 HP"},"Incentives are for ECMs or brushless direct current (DC) fan motors replacing shaded pole (SP) or permanent split capacitor (PSC) motors.","For retrofit of existing walk-in evaporators & replacing existing functional walk-ins with new walk-ins.","Incentive is not available when replacing non-operational walk-ins or for new construction","New motors must be designed specifically for use in evaporators",{"$nulls":6},"Nameplate of walk-in/reach-in case, walk-in evaporator, reach-in case.","Reach-in nameplates are located in the top corner of vertical cases, and along the back wall of island/\"coffin\" cases.","Walk-in nameplates are located on the evaporator box - which is not always accessible.","Walk-in evaporator will be located at the top of the walk-in space, typically near a wall.",null,null,{"v":50,"d":"$50.00"},"Motor",{"v":50,"d":"$50.00"},"Motor","N/A",{"$f":"W167","v":"Motor"},2308,2308,2308,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2308: ECM Evaporator Fan Motor, Walk-in Cooler, < 1/20 HP","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR167=\"Agribusiness\", $AR167=\"Ag\",$AR167=\"Propane\", $AR167=\"Ag Propane\", $AR167=\"Ag-Propane\"),$AC167,  $AB167),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR167=\"Agribusiness\", $AR167=\"Ag\",$AR167=\"Propane\", $AR167=\"Ag Propane\", $AR167=\"Ag-Propane\"),$AC167,  $AB167),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",8]
["R2309","R2309","Not Eligible","ECM Evaporator Fan Motor, Walk-in Cooler, 1/20 - 1 HP","R2309: ECM Evaporator Fan Motor, Walk-in Cooler, 1/20 - 1 HP","Incentives are for ECMs or brushless direct current (DC) fan motors replacing shaded pole (SP) or permanent split capacitor (PSC) motors.","For retrofit of existing walk-in evaporators & replacing existing functional walk-ins with new walk-ins.","Incentive is not available when replacing non-operational walk-ins or for new construction","New motors must be designed specifically for use in evaporators",{"$nulls":6},"Nameplate of walk-in/reach-in case, walk-in evaporator, reach-in case.","Reach-in nameplates are located in the top corner of vertical cases, and along the back wall of island/\"coffin\" cases.","Walk-in nameplates are located on the evaporator box - which is not always accessible.","Walk-in evaporator will be located at the top of the walk-in space, typically near a wall.",null,null,{"v":100,"d":"$100.00"},"Motor",{"v":100,"d":"$100.00"},"Motor","N/A","Motor",2309,2309,2309,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2309: ECM Evaporator Fan Motor, Walk-in Cooler, 1/20 - 1 HP","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR168=\"Agribusiness\", $AR168=\"Ag\",$AR168=\"Propane\", $AR168=\"Ag Propane\", $AR168=\"Ag-Propane\"),$AC168,  $AB168),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR168=\"Agribusiness\", $AR168=\"Ag\",$AR168=\"Propane\", $AR168=\"Ag Propane\", $AR168=\"Ag-Propane\"),$AC168,  $AB168),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",8]
["R2310","R2310","Not Eligible","ECM Evaporator Fan Motor, Walk-in Freezer, < 1/20 HP","R2310: ECM Evaporator Fan Motor, Walk-in Freezer, < 1/20 HP","Incentives are for ECMs or brushless direct current (DC) fan motors replacing shaded pole (SP) or permanent split capacitor (PSC) motors.","For retrofit of existing walk-in evaporators & replacing existing functional walk-ins with new walk-ins.","Incentive is not available when replacing non-operational walk-ins or for new construction","New motors must be designed specifically for use in evaporators",{"$nulls":6},"Nameplate of walk-in/reach-in case, walk-in evaporator, reach-in case.","Reach-in nameplates are located in the top corner of vertical cases, and along the back wall of island/\"coffin\" cases.","Walk-in nameplates are located on the evaporator box - which is not always accessible.","Walk-in evaporator will be located at the top of the walk-in space, typically near a wall.",null,null,{"v":50,"d":"$50.00"},"Motor",{"v":50,"d":"$50.00"},"Motor","N/A","Motor",2310,2310,2310,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2310: ECM Evaporator Fan Motor, Walk-in Freezer, < 1/20 HP","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR169=\"Agribusiness\", $AR169=\"Ag\",$AR169=\"Propane\", $AR169=\"Ag Propane\", $AR169=\"Ag-Propane\"),$AC169,  $AB169),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR169=\"Agribusiness\", $AR169=\"Ag\",$AR169=\"Propane\", $AR169=\"Ag Propane\", $AR169=\"Ag-Propane\"),$AC169,  $AB169),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",8]
["R2311","R2311","Not Eligible","ECM Evaporator Fan Motor, Walk-in Freezer, 1/20 - 1 HP","R2311: ECM Evaporator Fan Motor, Walk-in Freezer, 1/20 - 1 HP","Incentives are for ECMs or brushless direct current (DC) fan motors replacing shaded pole (SP) or permanent split capacitor (PSC) motors.","For retrofit of existing walk-in evaporators & replacing existing functional walk-ins with new walk-ins.","Incentive is not available when replacing non-operational walk-ins or for new construction","New motors must be designed specifically for use in evaporators",{"$nulls":6},"Nameplate of walk-in/reach-in case, walk-in evaporator, reach-in case.","Reach-in nameplates are located in the top corner of vertical cases, and along the back wall of island/\"coffin\" cases.","Walk-in nameplates are located on the evaporator box - which is not always accessible.","Walk-in evaporator will be located at the top of the walk-in space, typically near a wall.",null,null,{"v":100,"d":"$100.00"},"Motor",{"v":100,"d":"$100.00"},"Motor","N/A","Motor",2311,2311,2311,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2311: ECM Evaporator Fan Motor, Walk-in Freezer, 1/20 - 1 HP","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR170=\"Agribusiness\", $AR170=\"Ag\",$AR170=\"Propane\", $AR170=\"Ag Propane\", $AR170=\"Ag-Propane\"),$AC170,  $AB170),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR170=\"Agribusiness\", $AR170=\"Ag\",$AR170=\"Propane\", $AR170=\"Ag Propane\", $AR170=\"Ag-Propane\"),$AC170,  $AB170),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",8]
["R2312","R2312","Not Eligible","ECM Evaporator Fan Motor, Cooler/Freezer Case","R2312: ECM Evaporator Fan Motor, Cooler/Freezer Case","Incentives are for ECMs or brushless direct current (DC) fan motors replacing shaded pole (SP) or permanent split capacitor (PSC) motors.","For retrofit of existing display cases & replacing existing functional display cases with new display cases.","Incentive is not available when replacing non-operational reach-in coolers/freezers or for new construction","New motors must be designed specifically for use in evaporators",{"$nulls":6},"Nameplate of walk-in/reach-in case, walk-in evaporator, reach-in case.","Reach-in nameplates are located in the top corner of vertical cases, and along the back wall of island/\"coffin\" cases.","Walk-in nameplates are located on the evaporator box - which is not always accessible.","Walk-in evaporator will be located at the top of the walk-in space, typically near a wall.",null,null,{"v":70,"d":"$70.00"},"Motor",{"v":70,"d":"$70.00"},"Motor","N/A","Motor",2312,2312,2312,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2312: ECM Evaporator Fan Motor, Cooler/Freezer Case","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR171=\"Agribusiness\", $AR171=\"Ag\",$AR171=\"Propane\", $AR171=\"Ag Propane\", $AR171=\"Ag-Propane\"),$AC171,  $AB171),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR171=\"Agribusiness\", $AR171=\"Ag\",$AR171=\"Propane\", $AR171=\"Ag Propane\", $AR171=\"Ag-Propane\"),$AC171,  $AB171),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",8]
["R4284","R4284","Not Eligible","PMS Evaporator Fan Motor, Cooler/Freezer Case","R4284: PMS Evaporator Fan Motor, Cooler/Freezer Case","Incentives are for Permanent Magnet Synchronous Motor, replacing shaded pole (SP) or permanent split capacitor (PSC) motors.","For retrofit of existing display cases & replacing existing functional display cases with new display cases.","Incentive is not available when replacing non-operational reach-in coolers/freezers or for new construction","New motors must be designed specifically for use in evaporators",{"$nulls":12},{"v":70,"d":"$70.00"},"Motor",{"v":70,"d":"$70.00"},"Motor","N/A","Motor",4284,4284,4284,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R4284: PMS Evaporator Fan Motor, Cooler/Freezer Case","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR172=\"Agribusiness\", $AR172=\"Ag\",$AR172=\"Propane\", $AR172=\"Ag Propane\", $AR172=\"Ag-Propane\"),$AC172,  $AB172),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR172=\"Agribusiness\", $AR172=\"Ag\",$AR172=\"Propane\", $AR172=\"Ag Propane\", $AR172=\"Ag-Propane\"),$AC172,  $AB172),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",8]
["R2306","R2306","Not Eligible","ECM Compressor Head Fan Motor","R2306: ECM Compressor Head Fan Motor","Incentives are for ECMs or brushless direct current (DC) fan motors replacing shaded pole (SP) or permanent split capacitor (PSC) motors.","Must be used in conjunction with air-cooled condensers and compressors","Not eligible for installation in redundant or backup equipment",{"$nulls":5},"Incentive must be ≤100% project cost.",null,"Compressor/condenser nameplate, and fan layout on compressor/condenser","Compressor/condenser will be located in a non-conditioned part of the facility (back room, basement, etc.) or outside (behind building, on roof, etc.)","Nameplates are typically located on the side or front of the units",{"$nulls":3},{"v":50,"d":"$50.00"},"Motor",{"v":50,"d":"$50.00"},"Motor","N/A","Motor",2306,2306,2306,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2306: ECM Compressor Head Fan Motor","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR173=\"Agribusiness\", $AR173=\"Ag\",$AR173=\"Propane\", $AR173=\"Ag Propane\", $AR173=\"Ag-Propane\"),$AC173,  $AB173),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR173=\"Agribusiness\", $AR173=\"Ag\",$AR173=\"Propane\", $AR173=\"Ag Propane\", $AR173=\"Ag-Propane\"),$AC173,  $AB173),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",8]
["R2307","R2307","Not Eligible","ECM Condenser / Condensing Unit Fan Motor","R2307: ECM Condenser / Condensing Unit Fan Motor","Incentives are for ECMs or brushless direct current (DC) fan motors replacing shaded pole (SP) or permanent split capacitor (PSC) motors.","Must be used in conjunction with air-cooled condensers and compressors","Not eligible for installation in redundant or backup equipment",{"$nulls":5},"Incentive must be ≤100% project cost.",null,"Compressor/condenser nameplate, and fan layout on compressor/condenser","Compressor/condenser will be located in a non-conditioned part of the facility (back room, basement, etc.) or outside (behind building, on roof, etc.)","Nameplates are typically located on the side or front of the units",{"$nulls":3},{"v":50,"d":"$50.00"},"Motor",{"v":50,"d":"$50.00"},"Motor","N/A","Motor",2307,2307,2307,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2307: ECM Condenser / Condensing Unit Fan Motor","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR174=\"Agribusiness\", $AR174=\"Ag\",$AR174=\"Propane\", $AR174=\"Ag Propane\", $AR174=\"Ag-Propane\"),$AC174,  $AB174),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR174=\"Agribusiness\", $AR174=\"Ag\",$AR174=\"Propane\", $AR174=\"Ag Propane\", $AR174=\"Ag-Propane\"),$AC174,  $AB174),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",8]
["R2509","R2509","N-R2509","Reach-In Refrigerated Case with Doors replacing Open Multideck Case","R2509: Reach-In Refrigerated Case with Doors replacing Open Multideck Case","For existing buildings, existing cases must be open multideck-style, ≥ 6' tall w/o doors, and be functional / in active use prior to replacement. ","Both cooler and freezer qualify. Island, floral and specialty cases DNQ. New Cases only, refurbished cases DNQ.","Case width of open multideck-style and case with doors must be within 3 linear ft of each other. Customer must provide…","...case footprint details (case model #, quantities, and store floor plan w/ location of cases) to prove cases within 3 linear ft.","If installing new cases, must provide documents to confirm an alternate case is being considered.","Requires both an eligible electric and natural gas utility to qualify. Customers with only an eligible electrical or natural gas utility may qualify for custom incentives.",{"$nulls":3},"This is to replace an open multideck case with a completely new case with doors. These cases with doors are considerably more expensive than open multideck cases, and have a stricter DOE energy usage per foot requirement compared to open cases.","Case line-up and case nameplate.","Reach-in nameplates are located in the top corner of vertical cases.",{"$nulls":4},{"v":200,"d":"$200.00"},"Linear Foot",{"v":200,"d":"$200.00"},"Linear Foot",{"v":100,"d":"$100.00"},"Linear Foot",2509,2509,2509,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2509: Reach-In Refrigerated Case with Doors replacing Open Multideck Case","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR175=\"Agribusiness\", $AR175=\"Ag\",$AR175=\"Propane\", $AR175=\"Ag Propane\", $AR175=\"Ag-Propane\"),$AC175,  $AB175),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR175=\"Agribusiness\", $AR175=\"Ag\",$AR175=\"Propane\", $AR175=\"Ag Propane\", $AR175=\"Ag-Propane\"),$AC175,  $AB175),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",9]
["R3409","R3409","N-R3409","Install doors on open Multideck-Style Cases","R3409: Install doors on open Multideck-Style Cases","For addition of doors to existing open multideck-style cases or installation of multideck-style cases w/ doors in new construction applications.","Existing cases must be open multideck-style and 6 feet or taller without doors and may either be cooler or freezer.","Island, floral and specialty cases do not qualify.","Enter linear feet of doors added to case (Linear foot measurement is the side-to-side measured width of the case)","Anti-sweat heater controls, no-energy doors, LED lighting and ECM fan motors are also eligible on these cases (if installed)","Requires both an eligible electric and natural gas utility to qualify. Customers with only an eligible electrical or natural gas utility may qualify for custom incentives.",{"$nulls":3},"This is to purchase a set of doors to enclose an existing (or new for NC) open multideck case. Typically includes new sheet metal for the front in addition to the doors so the case appears to be new. ","Case line-up, case nameplate and door nameplate (if available)","Door nameplate should be located on an end of one of the door frames.","Reach-in nameplates are located in the top corner of vertical cases.",{"$nulls":3},{"v":100,"d":"$100.00"},"Linear Foot",{"v":100,"d":"$100.00"},"Linear Foot",{"v":65,"d":"$65.00"},"Linear Foot",3409,3409,3409,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R3409: Install doors on open Multideck-Style Cases","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR176=\"Agribusiness\", $AR176=\"Ag\",$AR176=\"Propane\", $AR176=\"Ag Propane\", $AR176=\"Ag-Propane\"),$AC176,  $AB176),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR176=\"Agribusiness\", $AR176=\"Ag\",$AR176=\"Propane\", $AR176=\"Ag Propane\", $AR176=\"Ag-Propane\"),$AC176,  $AB176),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",9]
["R2236","R2236","Not Eligible","Case Door,Cooler,No-Heat",{"$f":"IF(ISBLANK(A177),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C177,IF(FOEIncentCodeType=IncentCodeTypeAg,B177,A177))&\": \") &D177","v":"R2236: Case Door,Cooler,No-Heat"},"Doors for self-contained refrigerated cases are not eligible.","For cooler applications, only no-heat doors qualify; low-heat doors are not eligible.","No-heat doors are doors with anti-sweat heaters w/ < 52W per cooler door.....","...these heaters can be found on the glass, frame and/or rail (mullion).",{"$nulls":6},"Door nameplate, lineup of doors, case nameplate (if no door nameplate)","Door nameplate should be located on an end of one of the door frames","If a nameplate is not easily accessible on an end of the case lineup, look for end of case in line up (seams between cases; cases are 1-, 2-, 3-, 4- or 5- door)",{"$nulls":3},{"v":11,"d":"$11.00"},"Door",{"v":11,"d":"$11.00"},"Door","N/A",{"$f":"W177","v":"Door"},2236,{"$f":"AB177","v":2236},2236,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A177),\"\",IF(A177<>\"Not Eligible\",A177,IF(B177<>\"Not Eligible\",B177,C177))&\": \") &D177","v":"R2236: Case Door,Cooler,No-Heat"},"No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR177=\"Agribusiness\", $AR177=\"Ag\",$AR177=\"Propane\", $AR177=\"Ag Propane\", $AR177=\"Ag-Propane\"),$AC177,  $AB177),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR177=\"Agribusiness\", $AR177=\"Ag\",$AR177=\"Propane\", $AR177=\"Ag Propane\", $AR177=\"Ag-Propane\"),$AC177,  $AB177),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",9]
["R2234","R2234","Not Eligible","Case Door,Freezer,Low-Heat",{"$f":"IF(ISBLANK(A178),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C178,IF(FOEIncentCodeType=IncentCodeTypeAg,B178,A178))&\": \") &D178","v":"R2234: Case Door,Freezer,Low-Heat"},"Doors for self-contained refrigerated cases are not eligible.","Must be a Low-heat type door","Low-heat doors are doors w/ anti-sweat heaters with a wattage <63W per cooler door and <133W per freezer door…","...these heaters can be found on the glass, frame and/or rail (mullion).","For freezer applications, both low-heat and no-heat doors qualify.",{"$nulls":5},"Door nameplate, lineup of doors, case nameplate (if no door nameplate)","Door nameplate should be located on an end of one of the door frames","If a nameplate is not easily accessible on an end of the case lineup, look for end of case in line up (seams between cases; cases are 1-, 2-, 3-, 4- or 5- door)",{"$nulls":3},{"v":60,"d":"$60.00"},"Door",{"v":60,"d":"$60.00"},"Door","N/A",{"$f":"W178","v":"Door"},2234,{"$f":"AB178","v":2234},2234,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A178),\"\",IF(A178<>\"Not Eligible\",A178,IF(B178<>\"Not Eligible\",B178,C178))&\": \") &D178","v":"R2234: Case Door,Freezer,Low-Heat"},"No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR178=\"Agribusiness\", $AR178=\"Ag\",$AR178=\"Propane\", $AR178=\"Ag Propane\", $AR178=\"Ag-Propane\"),$AC178,  $AB178),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR178=\"Agribusiness\", $AR178=\"Ag\",$AR178=\"Propane\", $AR178=\"Ag Propane\", $AR178=\"Ag-Propane\"),$AC178,  $AB178),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",9]
["R2235","R2235","Not Eligible","Case Door,Freezer,No-Heat",{"$f":"IF(ISBLANK(A179),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C179,IF(FOEIncentCodeType=IncentCodeTypeAg,B179,A179))&\": \") &D179","v":"R2235: Case Door,Freezer,No-Heat"},"Doors for self-contained refrigerated cases are not eligible.","Must be a No-heat type door","No-heat doors are doors with anti-sweat heaters w/ < 54 W per freezer door…","…these heaters can be found on the glass, frame and/or rail (mullion).","For freezer applications, both low-heat and no-heat doors qualify.",{"$nulls":5},"Door nameplate, lineup of doors, case nameplate (if no door nameplate)","Door nameplate should be located on an end of one of the door frames","If a nameplate is not easily accessible on an end of the case lineup, look for end of case in line up (seams between cases; cases are 1-, 2-, 3-, 4- or 5- door)",{"$nulls":3},{"v":130,"d":"$130.00"},"Door",{"v":130,"d":"$130.00"},"Door","N/A",{"$f":"W179","v":"Door"},2235,{"$f":"AB179","v":2235},2235,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A179),\"\",IF(A179<>\"Not Eligible\",A179,IF(B179<>\"Not Eligible\",B179,C179))&\": \") &D179","v":"R2235: Case Door,Freezer,No-Heat"},"No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR179=\"Agribusiness\", $AR179=\"Ag\",$AR179=\"Propane\", $AR179=\"Ag Propane\", $AR179=\"Ag-Propane\"),$AC179,  $AB179),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR179=\"Agribusiness\", $AR179=\"Ag\",$AR179=\"Propane\", $AR179=\"Ag Propane\", $AR179=\"Ag-Propane\"),$AC179,  $AB179),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",9]
["R3114","R3114","Not Eligible","LED, Horizontal Case Lighting, replacing Linear Fluorescent",{"$f":"IF(ISBLANK(A180),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C180,IF(FOEIncentCodeType=IncentCodeTypeAg,B180,A180))&\": \") &D180","v":"R3114: LED, Horizontal Case Lighting, replacing Linear Fluorescent"},"DLC TRT V5.0 or higher listed under Display Case Luminaires, Horizontal Refrigerated Case Luminaires (horiz LED incentives only), …","…  or Vertical Refrigerated Case Luminaires (vert LED incentives only) primary use category","Limited to LED fixtures on reach-in refrigerated cases; self-contained refrigerated merchandisers qualify if over 5 ft in length.","Complete make and model numbers must be included on invoicing in order to be eligible for an incentive","Incentives available for LED retrofits in existing refrigerated display cases & new installation on refrigerated display cases w/qualifying LED case lights.",{"$nulls":5},"Close-up of case lighting, nameplate (if possible) & case lighting \"run.\"","Verification of make and model number may depend upon method case lighting is mounted within the case.","For canopy lighting… There may be a mirror to help reflect light within the case, there may display enough of the back of the fixture to obtain the make and model information.","For horizontal case lighting… fixtures will be attached via magnet to the shelves, which means easy removal (do not force off) to capture a photo of make and model information.","For vertical case lighting… the make and model information may be visible if you check between the mullion and the fixture.","If make and model information is not visible, several photos of the fixture close up and throughout the case are recommended.",{"v":5,"d":"$5.00"},"Linear Foot of Lamps",{"v":5,"d":"$5.00"},"Linear Foot of Lamps","N/A",{"$f":"W180","v":"Linear Foot of Lamps"},3114,{"$f":"AB180","v":3114},3114,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A180),\"\",IF(A180<>\"Not Eligible\",A180,IF(B180<>\"Not Eligible\",B180,C180))&\": \") &D180","v":"R3114: LED, Horizontal Case Lighting, replacing Linear Fluorescent"},"No","Yes","Linear Feet",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR180=\"Agribusiness\", $AR180=\"Ag\",$AR180=\"Propane\", $AR180=\"Ag Propane\", $AR180=\"Ag-Propane\"),$AC180,  $AB180),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR180=\"Agribusiness\", $AR180=\"Ag\",$AR180=\"Propane\", $AR180=\"Ag Propane\", $AR180=\"Ag-Propane\"),$AC180,  $AB180),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Refrigeration",10]
["R2456","R2456","Not Eligible","LED, Vertical Case Lighting, replacing Linear Fluorescent",{"$f":"IF(ISBLANK(A181),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C181,IF(FOEIncentCodeType=IncentCodeTypeAg,B181,A181))&\": \") &D181","v":"R2456: LED, Vertical Case Lighting, replacing Linear Fluorescent"},"DLC TRT V5.0 or higher listed under Display Case Luminaires, Horizontal Refrigerated Case Luminaires (horiz only), …","…  or Vertical Refrigerated Case Luminaires (vert only) primary use category","Limited to LED fixtures on reach-in refrigerated cases; self-contained refrigerated merchandisers qualify if over 5 ft in length.","Complete make and model numbers must be included on invoicing in order to be eligible for an incentive","Incentives available for LED retrofits in existing refrigerated display cases & new installation on refrigerated display cases w/qualifying LED case lights.",{"$nulls":5},"Close-up of case lighting, nameplate (if possible) & case lighting \"run.\"","Verification of make and model number may depend upon method case lighting is mounted within the case.","For canopy lighting… There may be a mirror to help reflect light within the case, there may display enough of the back of the fixture to obtain the make and model information.","For horizontal case lighting… fixtures will be attached via magnet to the shelves, which means easy removal (do not force off) to capture a photo of make and model information.","For vertical case lighting… the make and model information may be visible if you check between the mullion and the fixture.","If make and model information is not visible, several photos of the fixture close up and throughout the case are recommended.",{"v":25,"d":"$25.00"},"Fixture",{"v":25,"d":"$25.00"},"Fixture","N/A",{"$f":"W181","v":"Fixture"},2456,{"$f":"AB181","v":2456},2456,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A181),\"\",IF(A181<>\"Not Eligible\",A181,IF(B181<>\"Not Eligible\",B181,C181))&\": \") &D181","v":"R2456: LED, Vertical Case Lighting, replacing Linear Fluorescent"},"No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR181=\"Agribusiness\", $AR181=\"Ag\",$AR181=\"Propane\", $AR181=\"Ag Propane\", $AR181=\"Ag-Propane\"),$AC181,  $AB181),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR181=\"Agribusiness\", $AR181=\"Ag\",$AR181=\"Propane\", $AR181=\"Ag Propane\", $AR181=\"Ag-Propane\"),$AC181,  $AB181),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",10]
["R2271","R2271","N-R2271","Night Curtains for Open Multideck-Style Cases","R2271: Night Curtains for Open Multideck-Style Cases","Applies to professionally installed, permanent night curtain products only.","Curtain must be manufactured with low-emissivity perforations or use breathable woven aluminum fabric.","Both motorized and pull-down versions are eligible.","Linear foot measurement is the side-to-side (not top to bottom) measured width of all installed night curtains","Existing cases must be open multideck-style and 6 feet or taller without doors and may be cooler or freezer.",{"$nulls":5},"Night curtain and manufacturer","Night curtains are either mounted inside the canopy by the lighting or outside the canopy on the front of the case.","Often, night curtains do not have nameplate/model number information on them, if there is specific model information obtain a photo of that.","Night curtain handles or bottom section usually contain manufacturer information.",null,null,{"v":10,"d":"$10.00"},"Linear Foot",{"v":10,"d":"$10.00"},"Linear Foot",{"v":7,"d":"$7.00"},"Linear Foot",2271,2271,2271,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2271: Night Curtains for Open Multideck-Style Cases","No","No","Linear Feet",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR182=\"Agribusiness\", $AR182=\"Ag\",$AR182=\"Propane\", $AR182=\"Ag Propane\", $AR182=\"Ag-Propane\"),$AC182,  $AB182),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR182=\"Agribusiness\", $AR182=\"Ag\",$AR182=\"Propane\", $AR182=\"Ag Propane\", $AR182=\"Ag-Propane\"),$AC182,  $AB182),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Refrigeration",10]
["R3183","R3183","Not Eligible","Strip Curtain for Walk-In Freezers and Coolers","R3183: Strip Curtain for Walk-In Freezers and Coolers","Applies to professionally installed, permanent strip curtain products only. Strip curtains must be at least 0.06 inches thick.","For walk-in coolers & freezers w/o strip curtains installed or replacement of old, ineffective (worn out, broken, missing strips) strip curtains.","Linear foot measurement is the side-to-side (not top to bottom) measured width of the access door opening for the walk-in cooler or freezer.","Incentive is only for strip curtains installed on access doors to walk-in cooler or freezer. If strip curtains are being added or …","… replaced to open product display areas of the walk-ins, contact Focus on Energy, as a custom incentive may be available.",{"$nulls":11},{"v":8,"d":"$8.00"},"Linear Foot",{"v":8,"d":"$8.00"},"Linear Foot","N/A","Linear Foot",3183,3183,3183,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R3183: Strip Curtain for Walk-In Freezers and Coolers","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR183=\"Agribusiness\", $AR183=\"Ag\",$AR183=\"Propane\", $AR183=\"Ag Propane\", $AR183=\"Ag-Propane\"),$AC183,  $AB183),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR183=\"Agribusiness\", $AR183=\"Ag\",$AR183=\"Propane\", $AR183=\"Ag Propane\", $AR183=\"Ag-Propane\"),$AC183,  $AB183),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",10]
[{"$nulls":3},"-----------------------COMMERCIAL REFRIGERATION CATALOG: CONTROLS-----------------------","-----------------------COMMERCIAL REFRIGERATION CATALOG: CONTROLS-----------------------",{"$nulls":32},"-----------------------COMMERCIAL REFRIGERATION CATALOG: CONTROLS-----------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR184=\"Agribusiness\", $AR184=\"Ag\",$AR184=\"Propane\", $AR184=\"Ag Propane\", $AR184=\"Ag-Propane\"),$AC184,  $AB184),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR184=\"Agribusiness\", $AR184=\"Ag\",$AR184=\"Propane\", $AR184=\"Ag Propane\", $AR184=\"Ag-Propane\"),$AC184,  $AB184),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration"]
["R5439","R5439","Not Eligible","Anti-Sweat Heater Controls, Freezer Case","R5439: Anti-Sweat Heater Controls, Freezer Case","Must sense the relative humidity in the air outside of the display case and turn off the anti-sweat heaters at low humidity conditions","Must control heaters on rail (mullion) and door, if equipped with heater","Invoice must include make and model number of controls. Controls costs must be itemized separately on invoice.","Controls may be part of larger store system, such as PMAC, Energy Mgmt System, etc. (include system info w/ options for ASHC)",{"$nulls":6},"Control module, door/humidity sensor","Often, the control module for the entire refrigeration system is shared for the anti-sweat heater controls. Unless customer or trade ally servicing the equipment is with you, do NOT press any buttons on the control module.","Control modules will be located in the back room, typically close to the refrigeration system.","Door sensors are traditionally a flat gold disk (similar to a coin in size) that is mounted along the case frame or door.","Humidity sensors will be mounted outside of the cases and are traditionally a small black box above the doors with a red and green light.",null,{"v":40,"d":"$40.00"},"Door",{"v":40,"d":"$40.00"},"Door","N/A",{"$f":"W185","v":"Door"},2197,2197,2197,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R5439: Anti-Sweat Heater Controls, Freezer Case","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR185=\"Agribusiness\", $AR185=\"Ag\",$AR185=\"Propane\", $AR185=\"Ag Propane\", $AR185=\"Ag-Propane\"),$AC185,  $AB185),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR185=\"Agribusiness\", $AR185=\"Ag\",$AR185=\"Propane\", $AR185=\"Ag Propane\", $AR185=\"Ag-Propane\"),$AC185,  $AB185),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",11]
["R5440","R5440","Not Eligible","Anti-Sweat Heater Controls, Refrigerated Case","R5440: Anti-Sweat Heater Controls, Refrigerated Case","Must sense the relative humidity in the air outside of the display case and turn off the anti-sweat heaters at low humidity conditions","Must control heaters on rail (mullion) and door, if equipped with heater","Invoice must include make and model number of controls. Controls costs must be itemized separately on invoice.","Controls may be part of larger store system, such as PMAC, Energy Mgmt System, etc. (include system info w/ options for ASHC)",{"$nulls":6},"Control module, door/humidity sensor","Often, the control module for the entire refrigeration system is shared for the anti-sweat heater controls. Unless customer or trade ally servicing the equipment is with you, do NOT press any buttons on the control module.","Control modules will be located in the back room, typically close to the refrigeration system.","Door sensors are traditionally a flat gold disk (similar to a coin in size) that is mounted along the case frame or door.","Humidity sensors will be mounted outside of the cases and are traditionally a small black box above the doors with a red and green light.",null,{"v":40,"d":"$40.00"},"Door",{"v":40,"d":"$40.00"},"Door","N/A","Door",2200,2200,2200,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R5440: Anti-Sweat Heater Controls, Refrigerated Case","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR186=\"Agribusiness\", $AR186=\"Ag\",$AR186=\"Propane\", $AR186=\"Ag Propane\", $AR186=\"Ag-Propane\"),$AC186,  $AB186),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR186=\"Agribusiness\", $AR186=\"Ag\",$AR186=\"Propane\", $AR186=\"Ag Propane\", $AR186=\"Ag-Propane\"),$AC186,  $AB186),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",11]
["R2269","R2269","N-R2269","Evaporator Fan Control for Walk-in Cooler/Freezer","R2269: Evaporator Fan Control for Walk-in Cooler/Freezer","For '# of Units' on the application, use the quantity of evaporator fan motors controlled, not the # of controllers installed.","Eligible for controls used in conjunction with SP, PSC and/or ECM evaporator fan motors in walk-in coolers and freezers","By signing the application, customer agrees the cooler/freezer space has been properly tested to avoid hot spots away from thermostat during low-speed fan operation.",{"$nulls":7},"Control module on evaporator(s) and shot of evaporators which shows the number of fans.","Control module can be located on bottom, face or side of walk-in evaporator.",{"$nulls":4},{"v":25,"d":"$25.00"},"Motor",{"v":25,"d":"$25.00"},"Motor",{"v":15,"d":"$15.00"},"Motor",2269,2269,2269,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R2269: Evaporator Fan Control for Walk-in Cooler/Freezer","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR187=\"Agribusiness\", $AR187=\"Ag\",$AR187=\"Propane\", $AR187=\"Ag Propane\", $AR187=\"Ag-Propane\"),$AC187,  $AB187),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR187=\"Agribusiness\", $AR187=\"Ag\",$AR187=\"Propane\", $AR187=\"Ag Propane\", $AR187=\"Ag-Propane\"),$AC187,  $AB187),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",11]
["R4759","R4759","N-R4759","Evaporator Fan Control Reach-in Cooler/Freezer","R4759: Evaporator Fan Control Reach-in Cooler/Freezer","For '# of Units' on the application, use the quantity of evaporator fan motors controlled, not the # of controllers installed.","Eligible for controls used in conjunction with SP, PSC and/or ECM evaporator fan motors in reach-in coolers and freezers","By signing the application, customer agrees the cooler/freezer space has been properly tested to avoid hot spots away from thermostat during low-speed fan operation.",{"$nulls":13},{"v":30,"d":"$30.00"},"Motor",{"v":30,"d":"$30.00"},"Motor",{"v":16,"d":"$16.00"},"Motor",4759,4759,4759,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R4759: Evaporator Fan Control Reach-in Cooler/Freezer","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR188=\"Agribusiness\", $AR188=\"Ag\",$AR188=\"Propane\", $AR188=\"Ag Propane\", $AR188=\"Ag-Propane\"),$AC188,  $AB188),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR188=\"Agribusiness\", $AR188=\"Ag\",$AR188=\"Propane\", $AR188=\"Ag Propane\", $AR188=\"Ag-Propane\"),$AC188,  $AB188),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Refrigeration",11]
["R4758","R4758","N-R4758","Freezer Demand Defrost","R4758: Freezer Demand Defrost","Incentive is based on kW of electric defrost controlled.","Include evaporator make and model information, along with the defrost controls make and model information","Incentive is for freezer electric defrost heaters only. Cooler electric defrost heaters may be eligible for a custom incentive. ","Control costs are itemized separately","For existing buildings, incentives are not available for replacing existing controls",{"$nulls":11},{"v":20,"d":"$20.00"},"kW Controlled",{"v":20,"d":"$20.00"},"kW Controlled",{"v":15,"d":"$15.00"},"kW Controlled",4758,4758,4758,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R4758: Freezer Demand Defrost","No","Yes","kW Controlled",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR189=\"Agribusiness\", $AR189=\"Ag\",$AR189=\"Propane\", $AR189=\"Ag Propane\", $AR189=\"Ag-Propane\"),$AC189,  $AB189),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR189=\"Agribusiness\", $AR189=\"Ag\",$AR189=\"Propane\", $AR189=\"Ag Propane\", $AR189=\"Ag-Propane\"),$AC189,  $AB189),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":250,"d":"250.00"}},"Refrigeration",11]
["R4360","R4360","Not Eligible","Refrigeration Controls, Floating Head Pressure","R4360: Refrigeration Controls, Floating Head Pressure","Controls must monitor & modulate refrigerant line pressure based on ambient temperature and/or atmospheric conditions.","Controls for both air-cooled condensing unit and central refrigeration systems are eligible.","Heating, ventilation and air conditioning (HVAC) and ammonia systems are not eligible.","Enter refrigeration system horsepower controlled with floating head pressure controls.  If hp is unavailable convert by:","LT hp = LT compressor capacity (Btu/h)/6,000","MT hp = MT compressor capacity (Btu/h)/8,700",{"$nulls":4},"Control module, refrigeration system information or compressor nameplates.","Often, the control module for the entire refrigeration system is shared for the floating head pressure controls. Unless customer or trade ally servicing the equipment is with you, do NOT press any buttons on the control module.","The refrigeration system information is a sticker on/near the entire refrigeration system that lists out the compressor(s) and system BTUh (used to verify total system tonnage)","Another method of verifying the size is by obtaining all of the compressor nameplates - typically on the side or face of the compressor.",null,null,{"v":25,"d":"$25.00"},"HP",{"v":25,"d":"$25.00"},"HP","N/A","HP",4360,{"$f":"AB190","v":4360},4360,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","R4360: Refrigeration Controls, Floating Head Pressure","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR190=\"Agribusiness\", $AR190=\"Ag\",$AR190=\"Propane\", $AR190=\"Ag Propane\", $AR190=\"Ag-Propane\"),$AC190,  $AB190),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":10,"d":"10.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR190=\"Agribusiness\", $AR190=\"Ag\",$AR190=\"Propane\", $AR190=\"Ag Propane\", $AR190=\"Ag-Propane\"),$AC190,  $AB190),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},"Refrigeration",11]
[{"$nulls":3},"----------------------PROCESS SYSTEMS CATALOG: COMPRESSED AIR AND VACUUM-------------------------","----------------------PROCESS SYSTEMS CATALOG: COMPRESSED AIR AND VACUUM-------------------------",{"$nulls":32},"----------------------PROCESS SYSTEMS CATALOG: COMPRESSED AIR AND VACUUM-------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR191=\"Agribusiness\", $AR191=\"Ag\",$AR191=\"Propane\", $AR191=\"Ag Propane\", $AR191=\"Ag-Propane\"),$AC191,  $AB191),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR191=\"Agribusiness\", $AR191=\"Ag\",$AR191=\"Propane\", $AR191=\"Ag Propane\", $AR191=\"Ag-Propane\"),$AC191,  $AB191),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["PS4766","PS4766","Not Eligible","Compressed Air Leak Survey and Repair","PS4766: Compressed Air Leak Survey and Repair","Complete Table A of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentive is per HP of connected air compressors in system, not per CFM of leak identified.  HP for backup air compressors DNQ.","Must repair 1 leak per 5 hp. If < 1 leak per 5 hp found, all leaks must be repaired (unless explanation provided & Focus approves).","Eligible once per customer site per 12 month period per customer site with a maximum incentive of $5,000/year and up to 100% of survey and repair costs.","A leak log must be included with application","Leaks must be repaired before app is submitted & Focus must receive the app within 120 days of  leak survey completion date.",{"$nulls":10},{"v":6,"d":"$6"},"Connected HP",{"v":6,"d":"$6.00"},"Connected HP","N/A",{"$f":"W192","v":"Connected HP"},4766,4766,4766,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4766: Compressed Air Leak Survey and Repair","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR192=\"Agribusiness\", $AR192=\"Ag\",$AR192=\"Propane\", $AR192=\"Ag Propane\", $AR192=\"Ag-Propane\"),$AC192,  $AB192),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR192=\"Agribusiness\", $AR192=\"Ag\",$AR192=\"Propane\", $AR192=\"Ag Propane\", $AR192=\"Ag-Propane\"),$AC192,  $AB192),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":3000,"d":"3,000.00"}},"Process Systems",12]
["PS2196","PS2196","N-PS2196","Variable Speed Drive Air Compressors","PS2196: Variable Speed Drive Air Compressors","Complete Tables B1 & B2 of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Must have CAGI sheet at intended operating pressure…or mfg spec sheet if mfg doesn't participate in CAGI. ","New VSD air compressors only; Must be variable speed rotary vane or variable speed screw compressor type to be eligible.","Retrofits & redundant/backup units DNQ. Replacing an old VSD compressor with a new VSD compressor DNQ. Min. 2,000 hours of op/year. ","Adding a VSD to existing compressor DNQ. Adding a VSD compressor to system that already includes one DNQ (unless intent is to pay incremental hp).","Limit 1 VSD compressor per CA system (connected network of piping) unless variance granted by Focus in advance.",{"$nulls":10},{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",2196,2196,2196,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2196: Variable Speed Drive Air Compressors","Yes","Yes","Compressor HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR193=\"Agribusiness\", $AR193=\"Ag\",$AR193=\"Propane\", $AR193=\"Ag Propane\", $AR193=\"Ag-Propane\"),$AC193,  $AB193),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR193=\"Agribusiness\", $AR193=\"Ag\",$AR193=\"Propane\", $AR193=\"Ag Propane\", $AR193=\"Ag-Propane\"),$AC193,  $AB193),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Process Systems",12]
["PS4361","PS4361","N-PS4361","Variable Speed Drive Vacuum Pump, ≤ 30 hp, Variable Torque","PS4361: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Variable Torque","Complete Table I1 of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Vacuum pumps must operate a minimum of 2,000 hours annually.","Variable torque vacuum pumps are non-positive displacement pumps, including, centrifugal blowers…","… and regenerative blowers.","Vacuum pumps purchased or installed for backup or redundant systems DNQ.","Submit manufacturer specification sheet showing the type vacuum pump installed.",{"$nulls":10},{"v":65,"d":"$65.00"},"HP",{"v":65,"d":"$65.00"},"HP",{"v":60,"d":"$60.00"},"HP",4361,4361,4361,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4361: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Variable Torque","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR194=\"Agribusiness\", $AR194=\"Ag\",$AR194=\"Propane\", $AR194=\"Ag Propane\", $AR194=\"Ag-Propane\"),$AC194,  $AB194),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR194=\"Agribusiness\", $AR194=\"Ag\",$AR194=\"Propane\", $AR194=\"Ag Propane\", $AR194=\"Ag-Propane\"),$AC194,  $AB194),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":30,"d":"30.00"}},"Process Systems",13]
["PS4362","PS4362","N-PS4362","Variable Speed Drive Vacuum Pump, ≤ 30 hp, Constant Torque","PS4362: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Constant Torque","Complete Table I1 of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Vacuum pumps must operate a minimum of 2,000 hours annually.","Constant torque vacuum pumps are positive displacement pumps, including reciprocating piston, diaphragm,…","…rocking piston, rotary vane, liquid ring, rotary screw, and lobed rotor pumps.","Vacuum pumps purchased or installed for backup or redundant systems DNQ.","Submit manufacturer specification sheet showing the type vacuum pump installed.",{"$nulls":10},{"v":65,"d":"$65.00"},"HP",{"v":65,"d":"$65.00"},"HP",{"v":60,"d":"$60.00"},"HP",4362,4362,4362,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4362: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Constant Torque","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR195=\"Agribusiness\", $AR195=\"Ag\",$AR195=\"Propane\", $AR195=\"Ag Propane\", $AR195=\"Ag-Propane\"),$AC195,  $AB195),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR195=\"Agribusiness\", $AR195=\"Ag\",$AR195=\"Propane\", $AR195=\"Ag Propane\", $AR195=\"Ag-Propane\"),$AC195,  $AB195),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":30,"d":"30.00"}},"Process Systems",13]
["PS2264","PS2264","N-PS2264","Cycling or VFD-Controlled Refrigerated Air Dryer","PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer","Must be properly sized to meet the needs of the compressed air system","Must be cycling or VFD-controlled refrigerated dryers replacing non-cycling refrigeration air dryers","Replacement of desiccant, deliquescent, heat of compression, membrane, or other types of dryers DNQ","If air dryer is integral to antoher piece of equipment (i.e., part of the air compressor, provide a Mfg spec sheet for that piece of equip. to confirm that it includes a cycling or VFD controlled air dryer","Installation of controls to an existing air dryer is not eligible","Controls-based efficiency projects and/or replacement other dryer types may qualify custom incentive.","Use dryer's CFM to calculate incentive",{"$nulls":9},{"v":2,"d":"$2.00"},"CFM",{"v":2,"d":"$2.00"},"CFM",{"v":2,"d":"$2.00"},"CFM",2264,2264,2264,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer","No","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR196=\"Agribusiness\", $AR196=\"Ag\",$AR196=\"Propane\", $AR196=\"Ag Propane\", $AR196=\"Ag-Propane\"),$AC196,  $AB196),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":50,"d":"50.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR196=\"Agribusiness\", $AR196=\"Ag\",$AR196=\"Propane\", $AR196=\"Ag Propane\", $AR196=\"Ag-Propane\"),$AC196,  $AB196),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":3000,"d":"3,000.00"}},"Process Systems",14]
["PS4363","PS4363","N-PS4363","Dewpoint Demand Controls for Desiccant Dryers","PS4363: Dewpoint Demand Controls for Desiccant Dryers","Complete Table C of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Dryer controls are only for use on heatless, heated, or blower purge desiccant dryers.","Dryer must have a dew point sensor at discharge to monitor demand.","Dryer controls must control the regeneration process based on actual dewpoint instead of regenerating based on time alone.","Dryer controls are not eligible for back/redundant desiccant dryers.","Use dryer's CFM to calculate incentive",{"$nulls":10},{"v":4,"d":"$4.00"},"CFM",{"v":4,"d":"$4.00"},"CFM",{"v":4,"d":"$4.00"},"CFM",4363,4363,4363,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4363: Dewpoint Demand Controls for Desiccant Dryers","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR197=\"Agribusiness\", $AR197=\"Ag\",$AR197=\"Propane\", $AR197=\"Ag Propane\", $AR197=\"Ag-Propane\"),$AC197,  $AB197),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR197=\"Agribusiness\", $AR197=\"Ag\",$AR197=\"Propane\", $AR197=\"Ag Propane\", $AR197=\"Ag-Propane\"),$AC197,  $AB197),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",14]
["PS5441","PS5441","N-PS5441","Desiccant Compressed Air Dryer, Heated","PS5441: Desiccant Compressed Air Dryer, Heated","Complete Table D of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Must replace a heatless desiccant dryer that uses compressed air to regenerate the desiccant.","Backup and redundant desiccant dryers are not eligible.","Use dryer's CFM to calculate incentive","Efficient desiccant dryers which also have dewpoint controls may apply for this incentive and for PS4363, … ","… provided the dryer being replaced did not have dewpoint controls or this is a new installation and there was not an existing dryer.",{"$nulls":4},"Dryer, dryer nameplate, dryer control panel display if present",{"$nulls":5},{"v":4,"d":"$4.00"},"CFM",{"v":4,"d":"$4.00"},"CFM",{"v":4,"d":"$4.00"},"CFM",5441,5441,5441,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS5441: Desiccant Compressed Air Dryer, Heated","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR198=\"Agribusiness\", $AR198=\"Ag\",$AR198=\"Propane\", $AR198=\"Ag Propane\", $AR198=\"Ag-Propane\"),$AC198,  $AB198),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR198=\"Agribusiness\", $AR198=\"Ag\",$AR198=\"Propane\", $AR198=\"Ag Propane\", $AR198=\"Ag-Propane\"),$AC198,  $AB198),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",14]
["PS5442","PS5442","N-PS5442","Desiccant Compressed Air Dryer, Blower Purge","PS5442: Desiccant Compressed Air Dryer, Blower Purge","Complete Table D of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Must replace a heatless desiccant dryer that uses compressed air to regenerate the desiccant.","Backup and redundant desiccant dryers are not eligible.","Use dryer's CFM to calculate incentive","Efficient desiccant dryers which also have dewpoint controls may apply for this incentive and for PS4363, … ","… provided the dryer being replaced did not have dewpoint controls or this is a new installation and there was not an existing dryer.",{"$nulls":4},"Dryer, dryer nameplate, dryer control panel display if present",{"$nulls":5},{"v":4.25,"d":"$4.25"},"CFM",{"v":4.25,"d":"$4.25"},"CFM",{"v":4.25,"d":"$4.25"},"CFM",5442,5442,5442,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS5442: Desiccant Compressed Air Dryer, Blower Purge","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR199=\"Agribusiness\", $AR199=\"Ag\",$AR199=\"Propane\", $AR199=\"Ag Propane\", $AR199=\"Ag-Propane\"),$AC199,  $AB199),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR199=\"Agribusiness\", $AR199=\"Ag\",$AR199=\"Propane\", $AR199=\"Ag Propane\", $AR199=\"Ag-Propane\"),$AC199,  $AB199),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",14]
["PS5443","PS5443","N-PS5443","Desiccant Compressed Air Dryer, Zero Purge","PS5443: Desiccant Compressed Air Dryer, Zero Purge","Complete Table D of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Must replace a heatless desiccant dryer that uses compressed air to regenerate the desiccant.","Backup and redundant desiccant dryers are not eligible.","Use dryer's CFM to calculate incentive","Efficient desiccant dryers which also have dewpoint controls may apply for this incentive and for PS4363, … ","… provided the dryer being replaced did not have dewpoint controls or this is a new installation and there was not an existing dryer.",{"$nulls":4},"Dryer, dryer nameplate, dryer control panel display if present",{"$nulls":5},{"v":4.75,"d":"$4.75"},"CFM",{"v":4.75,"d":"$4.75"},"CFM",{"v":4.75,"d":"$4.75"},"CFM",5443,5443,5443,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS5443: Desiccant Compressed Air Dryer, Zero Purge","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR200=\"Agribusiness\", $AR200=\"Ag\",$AR200=\"Propane\", $AR200=\"Ag Propane\", $AR200=\"Ag-Propane\"),$AC200,  $AB200),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR200=\"Agribusiness\", $AR200=\"Ag\",$AR200=\"Propane\", $AR200=\"Ag Propane\", $AR200=\"Ag-Propane\"),$AC200,  $AB200),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",14]
["PS2254","PS2254","N-PS2254","No Air-Loss Condensate Drains","PS2254: No Air-Loss Condensate Drains","Must be used with load/no-load, variable speed, variable displacement, or centrifugal compressors. ","Manual, lever operated mechanical or solenoid drains DNQ","Must be \"no-loss\" (continuously measure presence of condensate, purge only when needed, and prevent purging of comp. air)","If no-loss drain is integral to another piece of equipment, provide a mfg's spec sheet to confirm","Load/no-load system must have adequate storage for drains to be eligible.","Replacement of existing no air-loss condensate drains DNQ",{"$nulls":10},{"v":130,"d":"$130.00"},"Drain",{"v":130,"d":"$130.00"},"Drain",{"v":130,"d":"$130.00"},"Drain",2254,2254,2254,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2254: No Air-Loss Condensate Drains","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR201=\"Agribusiness\", $AR201=\"Ag\",$AR201=\"Propane\", $AR201=\"Ag Propane\", $AR201=\"Ag-Propane\"),$AC201,  $AB201),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR201=\"Agribusiness\", $AR201=\"Ag\",$AR201=\"Propane\", $AR201=\"Ag Propane\", $AR201=\"Ag-Propane\"),$AC201,  $AB201),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",15]
["PS2255","PS2255","N-PS2255","Pressure/Flow Controllers","PS2255: Pressure/Flow Controllers","Limit one controller per system","The pressure/flow controller must be installed on the main pressure header","Not to replace drop line regulators or filter-regulator lubricators","Check past projects or request info from TA/Customer to confirm # and size of compressors.",{"$nulls":12},{"v":20,"d":"$20.00"},"HP",{"v":20,"d":"$20.00"},"HP",{"v":20,"d":"$20.00"},"HP",2255,2255,2255,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2255: Pressure/Flow Controllers","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR202=\"Agribusiness\", $AR202=\"Ag\",$AR202=\"Propane\", $AR202=\"Ag Propane\", $AR202=\"Ag-Propane\"),$AC202,  $AB202),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR202=\"Agribusiness\", $AR202=\"Ag\",$AR202=\"Propane\", $AR202=\"Ag Propane\", $AR202=\"Ag-Propane\"),$AC202,  $AB202),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",15]
["PS2258","PS2258","N-PS2258","Compressed Air Mist Eliminators","PS2258: Compressed Air Mist Eliminators","Must have an initial pressure drop ≤ 1 psig (include spec sheet to confirm)","Must replace (or for NC be installed instead of) a standard coalescing filter (small inline disposable filter)","Some mfg. may refer to mist eliminator as \"coalescing type filter\"…but it is still eligible. ","Check past projects or request info from TA/Customer to confirm # and size of compressors.",{"$nulls":12},{"v":6,"d":"$6.00"},"HP",{"v":6,"d":"$6.00"},"HP",{"v":6,"d":"$6.00"},"HP",2258,2258,2258,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2258: Compressed Air Mist Eliminators","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR203=\"Agribusiness\", $AR203=\"Ag\",$AR203=\"Propane\", $AR203=\"Ag Propane\", $AR203=\"Ag-Propane\"),$AC203,  $AB203),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR203=\"Agribusiness\", $AR203=\"Ag\",$AR203=\"Propane\", $AR203=\"Ag Propane\", $AR203=\"Ag-Propane\"),$AC203,  $AB203),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",15]
["PS5444","PS5444","N-PS5444","Compressed Air Storage, Increase from ≤ 1 Gal/CFM to ≥ 3 Gal/CFM","PS5444: Compressed Air Storage, Increase from ≤ 1 Gal/CFM to ≥ 3 Gal/CFM","Complete Table E of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Compressed air storage is only available for air compressors with load/no load and modulating controls with blowdown. ","This measure is intended for storage used at the air compressor plant level, not for distributed storage serving only a portion of the facility.","The existing system must have ≤ 1 gal/CFM of storage to qualify.","The upgraded system must have ≥ 3 gal/CFM of storage to qualify.","The additional storage can be added on the dry side (after air dryer) or wet side (before air dryer).",{"$nulls":10},{"v":35,"d":"$35.00"},"HP",{"$f":"V204","v":{"v":35,"d":"$35.00"}},{"$f":"W204","v":"HP"},{"v":35,"d":"$35.00"},"HP",5444,{"$f":"AB204","v":5444},5444,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A204),\"\",IF(A204<>\"Not Eligible\",A204,IF(B204<>\"Not Eligible\",B204,C204))&\": \") &D204","v":"PS5444: Compressed Air Storage, Increase from ≤ 1 Gal/CFM to ≥ 3 Gal/CFM"},"Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR204=\"Agribusiness\", $AR204=\"Ag\",$AR204=\"Propane\", $AR204=\"Ag Propane\", $AR204=\"Ag-Propane\"),$AC204,  $AB204),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR204=\"Agribusiness\", $AR204=\"Ag\",$AR204=\"Propane\", $AR204=\"Ag Propane\", $AR204=\"Ag-Propane\"),$AC204,  $AB204),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",15]
["PS2259","PS2259","N-PS2259","Air Entraining Nozzles","PS2259: Air Entraining Nozzles","Nozzle must be engineered. ","Nozzles must be rated at or less than 10 SCFM (1/8\"), 17 SCFM (1/4\"), 18 SCFM (3/8\"), and 18 SCFM (1/2\") at 80 PSIG","Compressed air system must operate ≥ 2,000 hours per year",{"$nulls":13},{"v":50,"d":"$50.00"},"Nozzle",{"v":50,"d":"$50.00"},"Nozzle",{"v":50,"d":"$50.00"},"Nozzle",2259,2259,2259,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2259: Air Entraining Nozzles","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR205=\"Agribusiness\", $AR205=\"Ag\",$AR205=\"Propane\", $AR205=\"Ag Propane\", $AR205=\"Ag-Propane\"),$AC205,  $AB205),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR205=\"Agribusiness\", $AR205=\"Ag\",$AR205=\"Propane\", $AR205=\"Ag Propane\", $AR205=\"Ag-Propane\"),$AC205,  $AB205),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",16]
["PS2257","PS2257","N-PS2257","Compressed Air Heat Recovery","PS2257: Compressed Air Heat Recovery","For heat recovery to offset space heating from natural gas fired heating equip. Heat recovery to offset process heating DNQ (custom possible).","Heat recovery for redundant/backup air compressors DNQ. Replacing existing heat recovery and upgrading from manual control DNQ.","System must include automatic controls to switch from winter to summer operation. Systems w/ manual damper controls DNQ.","Invoice is sufficiently detailed to confirm installation of heat recovery system.","Incentive must be ≤ 50% of project cost. ","Project must result in est. net reduction BTUs consumed in facility to be eligible.","Static pressure in area where compressor/vacuum pump is enclosed must remain same.","If outside air is used in system, antifreeze protection must be considered.",{"$nulls":8},{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",2257,2257,2257,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS2257: Compressed Air Heat Recovery","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR206=\"Agribusiness\", $AR206=\"Ag\",$AR206=\"Propane\", $AR206=\"Ag Propane\", $AR206=\"Ag-Propane\"),$AC206,  $AB206),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR206=\"Agribusiness\", $AR206=\"Ag\",$AR206=\"Propane\", $AR206=\"Ag Propane\", $AR206=\"Ag-Propane\"),$AC206,  $AB206),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",16]
["PS3928","PS3928","N-PS3928","Vacuum Pump Heat Recovery","PS3928: Vacuum Pump Heat Recovery","For heat recovery to offset space heating from natural gas fired heating equip. Heat recovery to offset process heating DNQ (custom possible).","Heat recovery for redundant/backup vacuum pumps DNQ. Replacing existing heat recovery and upgrading from manual control DNQ.","System must include automatic controls to switch from winter to summer operation. Systems w/ manual damper controls DNQ.","Invoice is sufficiently detailed to confirm installation of heat recovery system.","Incentive must be ≤ 50% of project cost. ","Project must result in est. net reduction BTUs consumed in facility to be eligible.","Static pressure in area where compressor/vacuum pump is enclosed must remain same.","If outside air is used in system, antifreeze protection must be considered.",{"$nulls":8},{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",3928,3928,3928,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS3928: Vacuum Pump Heat Recovery","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR207=\"Agribusiness\", $AR207=\"Ag\",$AR207=\"Propane\", $AR207=\"Ag Propane\", $AR207=\"Ag-Propane\"),$AC207,  $AB207),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR207=\"Agribusiness\", $AR207=\"Ag\",$AR207=\"Propane\", $AR207=\"Ag Propane\", $AR207=\"Ag-Propane\"),$AC207,  $AB207),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Process Systems",16]
["PS2848","PS2848","Not Eligible","Compressed Air Process Load Shifting","PS2848: Compressed Air Process Load Shifting","Complete Table F of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Replace inappropriate uses of compressed air (blow off, cooling, air motors, etc.) with blower or electric motor.","Compressed air load shifting incentive is for existing compressed air systems only.","Inappropriate use must have an annual runtime of at least 2,000 hours.","Pre-approval is recommended.","Incentive must be ≤ 50% of project cost. ",{"$nulls":3},"Incentive = (Comp Air Inappropriate HP - HP of Replacement Technology) * $200/hp.",{"$nulls":6},{"v":300,"d":"$300.00"},"HP Shifted",{"v":300,"d":"$300.00"},"HP Shifted","N/A","HP Shifted",2848,2848,2848,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS2848: Compressed Air Process Load Shifting","Yes","Yes","HP Shifted",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR208=\"Agribusiness\", $AR208=\"Ag\",$AR208=\"Propane\", $AR208=\"Ag Propane\", $AR208=\"Ag-Propane\"),$AC208,  $AB208),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR208=\"Agribusiness\", $AR208=\"Ag\",$AR208=\"Propane\", $AR208=\"Ag Propane\", $AR208=\"Ag-Propane\"),$AC208,  $AB208),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":400,"d":"400.00"}},"Process Systems",16]
[{"$nulls":3},"----------------------PROCESS SYSTEMS CATALOG: STEAM SYSTEMS-------------------------","----------------------PROCESS SYSTEMS CATALOG: STEAM SYSTEMS-------------------------",{"$nulls":9},"",{"$nulls":22},"----------------------PROCESS SYSTEMS CATALOG: STEAM SYSTEMS-------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR209=\"Agribusiness\", $AR209=\"Ag\",$AR209=\"Propane\", $AR209=\"Ag Propane\", $AR209=\"Ag-Propane\"),$AC209,  $AB209),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR209=\"Agribusiness\", $AR209=\"Ag\",$AR209=\"Propane\", $AR209=\"Ag Propane\", $AR209=\"Ag-Propane\"),$AC209,  $AB209),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["PS4041","PS4041","Not Eligible","Steam Trap Survey (Process)","PS4041: Steam Trap Survey (Process)","Survey log must include all necessary fields.","For natural gas fired steam systems only. Electric, propane, oil, and municipal steam systems DNQ","At least 20% of surveyed traps must be replaced. If < 20% of traps are failed, all leaking traps must be repaired/replaced","If all identified failed traps must be repaired/replaced, customer may provide written explanation for a trap that can't be repaired or replaced & may still qualify.","Survey incentive only available once per year per steam system",{"$nulls":4},"...provide written explanation for a trap that cannot be repaired or replaced and may still qualify for a custom incentive.  Note that 2225 is now only for HVAC steam traps.","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":8,"d":"$8.00"},"Steam Trap",{"v":8,"d":"$8.00"},"Steam Trap","N/A",{"$f":"W210","v":"Steam Trap"},4041,4041,4041,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4041: Steam Trap Survey (Process)","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR210=\"Agribusiness\", $AR210=\"Ag\",$AR210=\"Propane\", $AR210=\"Ag Propane\", $AR210=\"Ag-Propane\"),$AC210,  $AB210),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR210=\"Agribusiness\", $AR210=\"Ag\",$AR210=\"Propane\", $AR210=\"Ag Propane\", $AR210=\"Ag-Propane\"),$AC210,  $AB210),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",17]
["PS3999","PS3999","Not Eligible","Steam Trap Repair/Replacement, Industrial, < 10 psig","PS3999: Steam Trap Repair/Replacement, Industrial, < 10 psig","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. Process traps only; use separate measures for HVAC traps.","Only natural gas based steam systems are eligible. Can't apply for both prescriptive & RCx steam trap offer.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, if possible, that the actual system steam pressure is < 10 PSI. Do not use rated PSI of the steam trap.",{"$nulls":4},"...provide written explanation for a trap that cannot be repaired or replaced and may still qualify for a custom incentive.","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":60,"d":"$60.00"},"Steam Trap",{"$f":"V211","v":{"v":60,"d":"$60.00"}},"Steam Trap","N/A","Steam Trap",3999,3999,3999,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS3999: Steam Trap Repair/Replacement, Industrial, < 10 psig","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR211=\"Agribusiness\", $AR211=\"Ag\",$AR211=\"Propane\", $AR211=\"Ag Propane\", $AR211=\"Ag-Propane\"),$AC211,  $AB211),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR211=\"Agribusiness\", $AR211=\"Ag\",$AR211=\"Propane\", $AR211=\"Ag Propane\", $AR211=\"Ag-Propane\"),$AC211,  $AB211),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",17]
["PS4000","PS4000","Not Eligible","Steam Trap Repair/Replacement, Industrial, 10-49 psig","PS4000: Steam Trap Repair/Replacement, Industrial, 10-49 psig","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. Process traps only; use separate measures for HVAC traps.","Only natural gas based steam systems are eligible. Can't apply for both prescriptive & RCx steam trap offer.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, that UOM in SPECTRUM is the actual system steam pressure + 14.7 PSI. Do not use rated PSI of the steam trap as steam pressure.",{"$nulls":4},"...provide written explanation for a trap that cannot be repaired or replaced and may still qualify for a custom incentive.","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":100,"d":"$100.00"},"Steam Trap",{"v":100,"d":"$100.00"},"Steam Trap","N/A","Steam Trap",4000,4000,4000,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4000: Steam Trap Repair/Replacement, Industrial, 10-49 psig","No","Yes","PSIA (PSIG + 14.7)",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR212=\"Agribusiness\", $AR212=\"Ag\",$AR212=\"Propane\", $AR212=\"Ag Propane\", $AR212=\"Ag-Propane\"),$AC212,  $AB212),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":24.7,"d":"24.70"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR212=\"Agribusiness\", $AR212=\"Ag\",$AR212=\"Propane\", $AR212=\"Ag Propane\", $AR212=\"Ag-Propane\"),$AC212,  $AB212),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":63.7,"d":"63.70"}},"Process Systems",17]
["PS4001","PS4001","Not Eligible","Steam Trap Repair/Replacement, Industrial, 50-124 psig","PS4001: Steam Trap Repair/Replacement, Industrial, 50-124 psig","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. Process traps only; use separate measures for HVAC traps.","Only natural gas based steam systems are eligible. Can't apply for both prescriptive & RCx steam trap offer.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, that UOM in SPECTRUM is the actual system steam pressure + 14.7 PSI. Do not use rated PSI of the steam trap as steam pressure.",{"$nulls":4},"...provide written explanation for a trap that cannot be repaired or replaced and may still qualify for a custom incentive.","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":150,"d":"$150.00"},"Steam Trap",{"v":150,"d":"$150.00"},"Steam Trap","N/A","Steam Trap",4001,4001,4001,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4001: Steam Trap Repair/Replacement, Industrial, 50-124 psig","No","Yes","PSIA (PSIG + 14.7)",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR213=\"Agribusiness\", $AR213=\"Ag\",$AR213=\"Propane\", $AR213=\"Ag Propane\", $AR213=\"Ag-Propane\"),$AC213,  $AB213),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":64.7,"d":"64.70"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR213=\"Agribusiness\", $AR213=\"Ag\",$AR213=\"Propane\", $AR213=\"Ag Propane\", $AR213=\"Ag-Propane\"),$AC213,  $AB213),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":138.7,"d":"138.70"}},"Process Systems",17]
["PS4002","PS4002","Not Eligible","Steam Trap Repair/Replacement, Industrial, 125-225 psig","PS4002: Steam Trap Repair/Replacement, Industrial, 125-225 psig","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. Process traps only; use separate measures for HVAC traps.","Only natural gas based steam systems are eligible. Can't apply for both prescriptive & RCx steam trap offer.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, that UOM in SPECTRUM is the actual system steam pressure + 14.7 PSI. Do not use rated PSI of the steam trap as steam pressure.",{"$nulls":4},"...provide written explanation for a trap that cannot be repaired or replaced and may still qualify for a custom incentive.","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":250,"d":"$250.00"},"Steam Trap",{"v":250,"d":"$250.00"},"Steam Trap","N/A","Steam Trap",4002,4002,4002,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4002: Steam Trap Repair/Replacement, Industrial, 125-225 psig","No","Yes","PSIA (PSIG + 14.7)",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR214=\"Agribusiness\", $AR214=\"Ag\",$AR214=\"Propane\", $AR214=\"Ag Propane\", $AR214=\"Ag-Propane\"),$AC214,  $AB214),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":139.7,"d":"139.70"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR214=\"Agribusiness\", $AR214=\"Ag\",$AR214=\"Propane\", $AR214=\"Ag Propane\", $AR214=\"Ag-Propane\"),$AC214,  $AB214),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":239.7,"d":"239.70"}},"Process Systems",17]
["PS4003","PS4003","Not Eligible","Steam Trap Repair/Replacement, Industrial, > 225 psig","PS4003: Steam Trap Repair/Replacement, Industrial, > 225 psig","Only leaking traps are eligible; failed closed or plugged traps aren't eligible. Process traps only; use separate measures for HVAC traps.","Only natural gas based steam systems are eligible. Can't apply for both prescriptive & RCx steam trap offer.","For mass replacement of steam traps, incentive is only available for 20% of repaired traps","Repairs do not need to be made at one time, but only one repair incentive per trap can be applied for in a year.","Confirm, that UOM in SPECTRUM is the actual system steam pressure + 14.7 PSI. Do not use rated PSI of the steam trap as steam pressure.",{"$nulls":4},"...provide written explanation for a trap that cannot be repaired or replaced and may still qualify for a custom incentive.","Close-up of steam trap (with tag number in sight)",{"$nulls":5},{"v":420,"d":"$420.00"},"Steam Trap",{"v":420,"d":"$420.00"},"Steam Trap","N/A","Steam Trap",4003,4003,4003,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4003: Steam Trap Repair/Replacement, Industrial, > 225 psig","No","Yes","PSIA (PSIG + 14.7)",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR215=\"Agribusiness\", $AR215=\"Ag\",$AR215=\"Propane\", $AR215=\"Ag Propane\", $AR215=\"Ag-Propane\"),$AC215,  $AB215),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":239.7,"d":"239.70"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR215=\"Agribusiness\", $AR215=\"Ag\",$AR215=\"Propane\", $AR215=\"Ag Propane\", $AR215=\"Ag-Propane\"),$AC215,  $AB215),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":314.7,"d":"314.70"}},"Process Systems",17]
["PS4761","PS4761","Not Eligible","Process Boiler Combustion Upgrades, Linkageless Controls","PS4761: Process Boiler Combustion Upgrades, Linkageless Controls","Complete Table G of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentives are for existing natural gas-fired, force-draft boilers only","Must operate ≥ 2,000 hours/year","Installation on redundant or backup boiler does not qualify","Boiler input is entered in boiler horsepower (1 BHP = 33.476 MBh)","Incentive must be ≤ 50% of project cost","Invoices must be attached and include the manufacturer name and model number of linkageless controls.",{"$nulls":9},{"v":35,"d":"$35"},"BHP",{"v":35,"d":"$35.00"},"BHP","N/A","BHP",4761,4761,4761,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS4761: Process Boiler Combustion Upgrades, Linkageless Controls","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR216=\"Agribusiness\", $AR216=\"Ag\",$AR216=\"Propane\", $AR216=\"Ag Propane\", $AR216=\"Ag-Propane\"),$AC216,  $AB216),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":10,"d":"10.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR216=\"Agribusiness\", $AR216=\"Ag\",$AR216=\"Propane\", $AR216=\"Ag Propane\", $AR216=\"Ag-Propane\"),$AC216,  $AB216),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",17]
["PS4762","PS4762","N-PS4762","Process Boiler Combustion Upgrades, O2 Trim Controls","PS4762: Process Boiler Combustion Upgrades, O2 Trim Controls","Complete Table G of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentives are for existing natural gas-fired, force-draft boilers only","Must operate ≥ 2,000 hours/year","Installation on redundant or backup boiler does not qualify","Boiler input is entered in boiler horsepower (1 BHP = 33.476 MBh)","Incentive must be ≤ 50% of project cost","Invoices must be attached and include the manufacturer name and model number of O2 trim equipment.",{"$nulls":9},{"v":10,"d":"$10"},"BHP",{"v":10,"d":"$10.00"},"BHP",{"v":10,"d":"$10.00"},"BHP",4762,4762,4762,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS4762: Process Boiler Combustion Upgrades, O2 Trim Controls","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR217=\"Agribusiness\", $AR217=\"Ag\",$AR217=\"Propane\", $AR217=\"Ag Propane\", $AR217=\"Ag-Propane\"),$AC217,  $AB217),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":10,"d":"10.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR217=\"Agribusiness\", $AR217=\"Ag\",$AR217=\"Propane\", $AR217=\"Ag Propane\", $AR217=\"Ag-Propane\"),$AC217,  $AB217),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",17]
["PS4760","PS4760","Not Eligible","Process Boiler Combustion Upgrades, High Turndown Burner, Retrofit on Existing Boiler","PS4760: Process Boiler Combustion Upgrades, High Turndown Burner, Retrofit on Existing Boiler","Complete Table G of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentives are for existing natural gas-fired, force-draft boilers only","Must operate ≥ 2,000 hours/year","Installation on redundant or backup boiler does not qualify","Boiler input is entered in boiler horsepower (1 BHP = 33.476 MBh)","High turndown boiler must be able to provide efficient combustion at a 10:1 turndown ratio","Incentive must be ≤ 50% of project cost","Invoices must be attached and include the manufacturer name and model number of high turndown burner equipment.",{"$nulls":8},{"v":20,"d":"$20"},"BHP",{"v":20,"d":"$20.00"},"BHP","N/A","BHP",4760,4760,4760,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS4760: Process Boiler Combustion Upgrades, High Turndown Burner, Retrofit on Existing Boiler","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR218=\"Agribusiness\", $AR218=\"Ag\",$AR218=\"Propane\", $AR218=\"Ag Propane\", $AR218=\"Ag-Propane\"),$AC218,  $AB218),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":10,"d":"10.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR218=\"Agribusiness\", $AR218=\"Ag\",$AR218=\"Propane\", $AR218=\"Ag Propane\", $AR218=\"Ag-Propane\"),$AC218,  $AB218),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",17]
["PS5238","PS5238","N-PS5238","High Turndown Burner, New Boiler Replacement","PS5238: High Turndown Burner, New Boiler Replacement","Complete Table G of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentives are for existing natural gas-fired, force-draft boilers only","Must operate ≥ 2,000 hours/year","Installation on redundant or backup boiler does not qualify","Boiler input is entered in boiler horsepower (1 BHP = 33.476 MBh)","High turndown boiler must be able to provide efficient combustion at a 10:1 turndown ratio","Incentive must be ≤ 50% of project cost","Invoices must be attached and include the manufacturer name and model number of high turndown burner equipment.",{"$nulls":8},{"v":20,"d":"$20"},"BHP",{"v":20,"d":"$20.00"},"BHP",{"v":20,"d":"$20.00"},"BHP",5238,5238,5238,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS5238: High Turndown Burner, New Boiler Replacement","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR219=\"Agribusiness\", $AR219=\"Ag\",$AR219=\"Propane\", $AR219=\"Ag Propane\", $AR219=\"Ag-Propane\"),$AC219,  $AB219),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR219=\"Agribusiness\", $AR219=\"Ag\",$AR219=\"Propane\", $AR219=\"Ag Propane\", $AR219=\"Ag-Propane\"),$AC219,  $AB219),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",17]
[{"$nulls":3},"----------------------PROCESS SYSTEMS CATALOG: VFDs-------------------------","----------------------PROCESS SYSTEMS CATALOG: VFDs-------------------------",{"$nulls":32},"----------------------PROCESS SYSTEMS CATALOG: VFDs-------------------------",null,null,"HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR220=\"Agribusiness\", $AR220=\"Ag\",$AR220=\"Propane\", $AR220=\"Ag Propane\", $AR220=\"Ag-Propane\"),$AC220,  $AB220),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR220=\"Agribusiness\", $AR220=\"Ag\",$AR220=\"Propane\", $AR220=\"Ag Propane\", $AR220=\"Ag-Propane\"),$AC220,  $AB220),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["PS2726","PS2726","N-PS2726","Variable Frequency Drives, Variable Torque, CW Distribution Pump","PS2726: Variable Frequency Drives, Variable Torque, CW Distribution Pump","Complete Table H1 (and H2 if >500hp) of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure","Must be used in a pumping or air handling application, must operate ≥ 2,000 hours","Chillers, kitchen ventilation, and air compressor applications DNQ. VFD installed only to allow soft start DNQ.","Redundant or back-up units DNQ. Routine replacement of existing VFD DNQ. Staged air volume systems (Carrier RTUs) DNQ.","For VSD vacuum pumps, see separate VSD vacuum pump incentive (PS4361). See Dairy/Livestock app for dairy VSD vacuum pumps.","VFD speed must to automatically controlled by differential pressure, flow, temp or other variable signal.","VFD must be installed on centrifugal or axial flow pump or fan",null,null,"OK if VFD is sized larger than motor (incentive based on motor hp) - question if VFD is smaller than motor.","VFD itself, VFD nameplate if visible, nameplate of equipment being controlled (pump/fan motor). ",{"$nulls":5},{"v":55,"d":"$55.00"},"HP",{"$f":"V221","v":{"v":55,"d":"$55.00"}},"HP",{"v":45,"d":"$45.00"},"HP",2726,2726,2726,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2726: Variable Frequency Drives, Variable Torque, CW Distribution Pump","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR221=\"Agribusiness\", $AR221=\"Ag\",$AR221=\"Propane\", $AR221=\"Ag Propane\", $AR221=\"Ag-Propane\"),$AC221,  $AB221),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR221=\"Agribusiness\", $AR221=\"Ag\",$AR221=\"Propane\", $AR221=\"Ag Propane\", $AR221=\"Ag-Propane\"),$AC221,  $AB221),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"Process Systems",18]
["PS2640","PS2640","N-PS2640","Variable Frequency Drives, Variable Torque, Boiler Draft Fan","PS2640: Variable Frequency Drives, Variable Torque, Boiler Draft Fan","Complete Table H1 (and H2 if >500hp) of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure","Must be used in a pumping or air handling application, must operate ≥ 2,000 hours","Chillers, kitchen ventilation, and air compressor applications DNQ. VFD installed only to allow soft start DNQ.","Redundant or back-up units DNQ. Routine replacement of existing VFD DNQ. Staged air volume systems (Carrier RTUs) DNQ.","For VSD vacuum pumps, see separate VSD vacuum pump incentive (PS4361). See Dairy/Livestock app for dairy VSD vacuum pumps.","VFD speed must to automatically controlled by differential pressure, flow, temp or other variable signal.","VFD must be installed on centrifugal or axial flow pump or fan",null,null,"OK if VFD is sized larger than motor (incentive based on motor hp) - question if VFD is smaller than motor.","VFD itself, VFD nameplate if visible, nameplate of equipment being controlled (pump/fan motor). ",{"$nulls":5},{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP",{"v":45,"d":"$45.00"},"HP",2640,2640,2640,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2640: Variable Frequency Drives, Variable Torque, Boiler Draft Fan","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR222=\"Agribusiness\", $AR222=\"Ag\",$AR222=\"Propane\", $AR222=\"Ag Propane\", $AR222=\"Ag-Propane\"),$AC222,  $AB222),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR222=\"Agribusiness\", $AR222=\"Ag\",$AR222=\"Propane\", $AR222=\"Ag Propane\", $AR222=\"Ag-Propane\"),$AC222,  $AB222),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"Process Systems",18]
["PS2641","PS2641","N-PS2641","Variable Frequency Drives, Variable Torque, Cooling Tower Fan","PS2641: Variable Frequency Drives, Variable Torque, Cooling Tower Fan","Complete Table H1 (and H2 if >500hp) of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure","Must be used in a pumping or air handling application, must operate ≥ 2,000 hours","Chillers, kitchen ventilation, and air compressor applications DNQ. VFD installed only to allow soft start DNQ.","Redundant or back-up units DNQ. Routine replacement of existing VFD DNQ. Staged air volume systems (Carrier RTUs) DNQ.","For VSD vacuum pumps, see separate VSD vacuum pump incentive (PS4361). See Dairy/Livestock app for dairy VSD vacuum pumps.","VFD speed must to automatically controlled by differential pressure, flow, temp or other variable signal.","VFD must be installed on centrifugal or axial flow pump or fan",null,null,"OK if VFD is sized larger than motor (incentive based on motor hp) - question if VFD is smaller than motor.","VFD itself, VFD nameplate if visible, nameplate of equipment being controlled (pump/fan motor). ",{"$nulls":5},{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP",{"v":45,"d":"$45.00"},"HP",2641,2641,2641,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2641: Variable Frequency Drives, Variable Torque, Cooling Tower Fan","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR223=\"Agribusiness\", $AR223=\"Ag\",$AR223=\"Propane\", $AR223=\"Ag Propane\", $AR223=\"Ag-Propane\"),$AC223,  $AB223),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR223=\"Agribusiness\", $AR223=\"Ag\",$AR223=\"Propane\", $AR223=\"Ag Propane\", $AR223=\"Ag-Propane\"),$AC223,  $AB223),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"Process Systems",18]
["PS2647","PS2647","N-PS2647","Variable Frequency Drives, Variable Torque, Process Fan","PS2647: Variable Frequency Drives, Variable Torque, Process Fan","Complete Table H1 (and H2 if >500hp) of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure","Must be used in a pumping or air handling application, must operate ≥ 2,000 hours","Chillers, kitchen ventilation, and air compressor applications DNQ. VFD installed only to allow soft start DNQ.","Redundant or back-up units DNQ. Routine replacement of existing VFD DNQ. Staged air volume systems (Carrier RTUs) DNQ.","For VSD vacuum pumps, see separate VSD vacuum pump incentive (PS4361). See Dairy/Livestock app for dairy VSD vacuum pumps.","VFD speed must to automatically controlled by differential pressure, flow, temp or other variable signal.","VFD must be installed on centrifugal or axial flow pump or fan",null,null,"OK if VFD is sized larger than motor (incentive based on motor hp) - question if VFD is smaller than motor.","VFD itself, VFD nameplate if visible, nameplate of equipment being controlled (pump/fan motor). ",{"$nulls":5},{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP",{"v":45,"d":"$45.00"},"HP",2647,2647,2647,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2647: Variable Frequency Drives, Variable Torque, Process Fan","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR224=\"Agribusiness\", $AR224=\"Ag\",$AR224=\"Propane\", $AR224=\"Ag Propane\", $AR224=\"Ag-Propane\"),$AC224,  $AB224),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR224=\"Agribusiness\", $AR224=\"Ag\",$AR224=\"Propane\", $AR224=\"Ag Propane\", $AR224=\"Ag-Propane\"),$AC224,  $AB224),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Process Systems",18]
["PS2648","PS2648","N-PS2648","Variable Frequency Drives, Variable Torque, Process Pump","PS2648: Variable Frequency Drives, Variable Torque, Process Pump","Complete Table H1 (and H2 if >500hp) of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure","Must be used in a pumping or air handling application, must operate ≥ 2,000 hours","Chillers, kitchen ventilation, and air compressor applications DNQ. VFD installed only to allow soft start DNQ.","Redundant or back-up units DNQ. Routine replacement of existing VFD DNQ. Staged air volume systems (Carrier RTUs) DNQ.","For VSD vacuum pumps, see separate VSD vacuum pump incentive (PS4361). See Dairy/Livestock app for dairy VSD vacuum pumps.","VFD speed must to automatically controlled by differential pressure, flow, temp or other variable signal.","VFD must be installed on centrifugal or axial flow pump or fan",null,null,"OK if VFD is sized larger than motor (incentive based on motor hp) - question if VFD is smaller than motor.","VFD itself, VFD nameplate if visible, nameplate of equipment being controlled (pump/fan motor). ",{"$nulls":5},{"v":55,"d":"$55.00"},"HP",{"v":55,"d":"$55.00"},"HP",{"v":45,"d":"$45.00"},"HP",2648,2648,2648,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2648: Variable Frequency Drives, Variable Torque, Process Pump","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR225=\"Agribusiness\", $AR225=\"Ag\",$AR225=\"Propane\", $AR225=\"Ag Propane\", $AR225=\"Ag-Propane\"),$AC225,  $AB225),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR225=\"Agribusiness\", $AR225=\"Ag\",$AR225=\"Propane\", $AR225=\"Ag Propane\", $AR225=\"Ag-Propane\"),$AC225,  $AB225),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Process Systems",18]
["PS10436","PS10436","N-PS10436","Variable Frequency Drives, Variable Torque, Process Pump (500-1,999 HOU)",{"$f":"IF(ISBLANK(A226),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C226,IF(FOEIncentCodeType=IncentCodeTypeAg,B226,A226))&\": \") &D226","v":"PS10436: Variable Frequency Drives, Variable Torque, Process Pump (500-1,999 HOU)"},"Complete Table H1 (and H2 if >500hp) of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure","Must be used in a pumping or air handling application, must operate 500-1,999 hours","Chillers, kitchen ventilation, and air compressor applications DNQ. VFD installed only to allow soft start DNQ.","Redundant or back-up units DNQ. Routine replacement of existing VFD DNQ. Staged air volume systems (Carrier RTUs) DNQ.","For VSD vacuum pumps, see separate VSD vacuum pump incentive (PS4361). See Dairy/Livestock app for dairy VSD vacuum pumps.","VFD speed must to automatically controlled by differential pressure, flow, temp or other variable signal.","VFD must be installed on centrifugal or axial flow pump or fan",null,null,"OK if VFD is sized larger than motor (incentive based on motor hp) - question if VFD is smaller than motor.","VFD itself, VFD nameplate if visible, nameplate of equipment being controlled (pump/fan motor). ",{"$nulls":5},{"v":20,"d":"$20.00"},"HP",{"v":20,"d":"$20.00"},"HP",{"v":15,"d":"$15.00"},"HP",10436,10436,10436,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS10436: Variable Frequency Drives, Variable Torque, Process Pump (500-1,999 HOU)","Yes","Yes","HP",{"v":0.1,"d":"0.10"},{"v":500,"d":"500.00"},"Process Systems",18]
["PS10434","PS10434","N-PS10434","Variable Frequency Drives, Variable Torque, Process Fan (500-1,999 HOU)","PS10434: Variable Frequency Drives, Variable Torque, Process Fan (500-1,999 HOU)","Complete Table H1 (and H2 if >500hp) of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure","Must be used in a pumping or air handling application, must operate 500-1,999 hours","Chillers, kitchen ventilation, and air compressor applications DNQ. VFD installed only to allow soft start DNQ.","Redundant or back-up units DNQ. Routine replacement of existing VFD DNQ. Staged air volume systems (Carrier RTUs) DNQ.","For VSD vacuum pumps, see separate VSD vacuum pump incentive (PS4361). See Dairy/Livestock app for dairy VSD vacuum pumps.","VFD speed must to automatically controlled by differential pressure, flow, temp or other variable signal.","VFD must be installed on centrifugal or axial flow pump or fan",null,null,"OK if VFD is sized larger than motor (incentive based on motor hp) - question if VFD is smaller than motor.","VFD itself, VFD nameplate if visible, nameplate of equipment being controlled (pump/fan motor). ",{"$nulls":5},{"v":20,"d":"$20.00"},"HP",{"v":20,"d":"$20.00"},"HP",{"v":15,"d":"$15.00"},"HP",10434,10434,10434,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS10434: Variable Frequency Drives, Variable Torque, Process Fan (500-1,999 HOU)","Yes","Yes","HP",{"v":0.1,"d":"0.10"},{"v":500,"d":"500.00"},"Process Systems",18]
["PS3280","PS3280","N-PS3280","Variable Frequency Drives, Constant Torque, All Types","PS3280: Variable Frequency Drives, Constant Torque, All Types","Complete Table I1 (and I2 if >500hp) of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure","Must be used in constant torque equip. (conveyor, positive displacement pump, refrig. compressor, crusher/shredder, mixer, etc.)","Must operate ≥ 2,000 hours. VFD installed only to allow soft start do not qualify. ","For air compressors, see separate VSD air compressor incentive (PS2196). For VSD vacuum pumps, see separate VSD vacuum pump incentive (PS4362). ","Redundant or back-up units DNQ. Routine replacement of existing VFD DNQ.","VFD speed can be automatically controlled by differential pressure, flow, temp or other variable signal, or be manually controlled.",{"$nulls":3},"Use individual itemized VFD project costs. OK if VFD is sized larger than motor - question if VFD is smaller than motor.","VFD itself, VFD nameplate if visible, nameplate of motor being controlled.",{"$nulls":5},{"v":50,"d":"$50.00"},"HP",{"v":50,"d":"$50.00"},"HP",{"v":40,"d":"$40.00"},"HP",3280,3280,3280,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A228),\"\",IF(A228<>\"Not Eligible\",A228,IF(B228<>\"Not Eligible\",B228,C228))&\": \") &D228","v":"PS3280: Variable Frequency Drives, Constant Torque, All Types"},"Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR228=\"Agribusiness\", $AR228=\"Ag\",$AR228=\"Propane\", $AR228=\"Ag Propane\", $AR228=\"Ag-Propane\"),$AC228,  $AB228),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR228=\"Agribusiness\", $AR228=\"Ag\",$AR228=\"Propane\", $AR228=\"Ag Propane\", $AR228=\"Ag-Propane\"),$AC228,  $AB228),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Process Systems",18]
[{"$nulls":3},"----------------------PROCESS SYSTEMS CATALOG: DATA CENTER AND TELECOM FACILITIES-------------------------","----------------------PROCESS SYSTEMS CATALOG: DATA CENTER AND TELECOM FACILITIES-------------------------",{"$nulls":32},"----------------------PROCESS SYSTEMS CATALOG: DATA CENTER AND TELECOM FACILITIES-------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR229=\"Agribusiness\", $AR229=\"Ag\",$AR229=\"Propane\", $AR229=\"Ag Propane\", $AR229=\"Ag-Propane\"),$AC229,  $AB229),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR229=\"Agribusiness\", $AR229=\"Ag\",$AR229=\"Propane\", $AR229=\"Ag Propane\", $AR229=\"Ag-Propane\"),$AC229,  $AB229),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems"]
["PS4776","PS4776","Not Eligible","Air Side Economizer, Data Center/Telecom","PS4776: Air Side Economizer, Data Center/Telecom","Complete Table J of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Cannot replace existing air side economizer","Air side economizer must be automatically controlled based on outside air temperature or enthalpy","Redundant or back-up units DNQ. ","Process loads in manufacturing facilities are not eligible","Air side economizer limited to offsetting ≤100 tons of mechanical cooling. ",{"$nulls":10},{"v":170,"d":"$170"},"Ton",{"$f":"V230","v":{"v":170,"d":"$170.00"}},"Ton","N/A",{"$f":"W230","v":"Ton"},4776,{"$f":"AB230","v":4776},4776,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4776: Air Side Economizer, Data Center/Telecom","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR230=\"Agribusiness\", $AR230=\"Ag\",$AR230=\"Propane\", $AR230=\"Ag Propane\", $AR230=\"Ag-Propane\"),$AC230,  $AB230),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR230=\"Agribusiness\", $AR230=\"Ag\",$AR230=\"Propane\", $AR230=\"Ag Propane\", $AR230=\"Ag-Propane\"),$AC230,  $AB230),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},"Process Systems",19]
["PS2305","PS2305","Not Eligible","Energy-Efficient Drycooler, Data Center/Telecom","PS2305: Energy-Efficient Drycooler, Data Center/Telecom","Complete Table K of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Must install a water-side economizer and must not replace an existing water-side economizer","Air side economizer must be automatically controlled based on outside air temperature or enthalpy","Only for data centers and telecom facilities with DX CRAC units. (Drycoolers for chilled water systems may be eligible for custom incentives","Must provide documentation of CRAC cooling performance data","Redundant or non-operational CRAC units do not count toward the total capacity",{"$nulls":3},"Provide documentation of total rated capacity of data center cooling system. Documentation should include an inventory of CRAC units with quantity, capacity, manufacturer and model number of each unit.",{"$nulls":6},{"v":130,"d":"$130"},"Ton",{"v":130,"d":"$130.00"},"Ton","N/A","Ton",2305,2305,2305,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2305: Energy-Efficient Drycooler, Data Center/Telecom","Yes","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR231=\"Agribusiness\", $AR231=\"Ag\",$AR231=\"Propane\", $AR231=\"Ag Propane\", $AR231=\"Ag-Propane\"),$AC231,  $AB231),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR231=\"Agribusiness\", $AR231=\"Ag\",$AR231=\"Propane\", $AR231=\"Ag Propane\", $AR231=\"Ag-Propane\"),$AC231,  $AB231),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",19]
["PS4777","PS4777","Not Eligible","Efficient UPS","PS4777: Efficient UPS","Complete Table L of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentive is based on kW of IT equipment load (output of the UPS)","Efficiency of the new UPS should be based on tests done in accordance with DOE 10 CFR 430","Efficient UPS must be ≥ 94% full load efficiency. (Confirm with spec sheet)","The existing UPS must be ≤ 90% efficient at the current IT load. (Must provide spec sheets, pictures, or metered data of UPS controls to confirm existing UPS efficiency)",{"$nulls":11},{"v":35,"d":"$35"},"kW",{"v":35,"d":"$35.00"},"kW","N/A","kW",4777,4777,4777,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4777: Efficient UPS","Yes","Yes","kW Capacity",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR232=\"Agribusiness\", $AR232=\"Ag\",$AR232=\"Propane\", $AR232=\"Ag Propane\", $AR232=\"Ag-Propane\"),$AC232,  $AB232),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR232=\"Agribusiness\", $AR232=\"Ag\",$AR232=\"Propane\", $AR232=\"Ag Propane\", $AR232=\"Ag-Propane\"),$AC232,  $AB232),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",19]
["PS4778","PS4778","Not Eligible","Efficient Rectifier","PS4778: Efficient Rectifier","Complete Table L of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentive is based on kW of IT equipment load (output of the rectifier)","Efficiency of the new rectifier should be based on tests done in accordance with DOE 10 CFR 430","Efficient rectifier must be ≥ 94% full load efficiency. (Confirm with spec sheet or other clear documentation)","The existing UPS must be ≤ 90% efficient at the current IT load. (Must provide spec sheets, pictures, or metered data of UPS controls to confirm existing rectifier efficiency)",{"$nulls":11},{"v":35,"d":"$35"},"kW",{"v":35,"d":"$35.00"},"kW","N/A","kW",4778,4778,4778,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4778: Efficient Rectifier","Yes","Yes","kW Capacity",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR233=\"Agribusiness\", $AR233=\"Ag\",$AR233=\"Propane\", $AR233=\"Ag Propane\", $AR233=\"Ag-Propane\"),$AC233,  $AB233),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR233=\"Agribusiness\", $AR233=\"Ag\",$AR233=\"Propane\", $AR233=\"Ag Propane\", $AR233=\"Ag-Propane\"),$AC233,  $AB233),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50,"d":"50.00"}},"Process Systems",19]
[{"$nulls":3},"----------------------PROCESS SYSTEMS CATALOG: PROCESS SPECIALTY EQUIPMENT-------------------------",{"$f":"IF(ISBLANK(A234),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C234,IF(FOEIncentCodeType=IncentCodeTypeAg,B234,A234))&\": \") &D234","v":"----------------------PROCESS SYSTEMS CATALOG: PROCESS SPECIALTY EQUIPMENT-------------------------"},{"$nulls":9},"",{"$nulls":22},"----------------------PROCESS SYSTEMS CATALOG: PROCESS SPECIALTY EQUIPMENT-------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR234=\"Agribusiness\", $AR234=\"Ag\",$AR234=\"Propane\", $AR234=\"Ag Propane\", $AR234=\"Ag-Propane\"),$AC234,  $AB234),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR234=\"Agribusiness\", $AR234=\"Ag\",$AR234=\"Propane\", $AR234=\"Ag Propane\", $AR234=\"Ag-Propane\"),$AC234,  $AB234),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems"]
["PS2490","PS2490","N-PS2490","Radiant Heater Band","PS2490: Radiant Heater Band","Complete Table M of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Available for installation of efficient radiant heater bands used in plastics equipment","Must be used on plastics equipment including injection molding, profile and sheet extrusion and blow molding.","Provide metered data if available","lncentlve Is limited to 50% of the project cost, Including equipment and external labor (Internal labor eligible for schools and government customers).",{"$nulls":11},{"v":100,"d":"$100.00"},"kW of existing heater bands",{"$f":"V235","v":{"v":100,"d":"$100.00"}},"kW of existing heater bands",{"$f":"V235","v":{"v":100,"d":"$100.00"}},{"$f":"W235","v":"kW of existing heater bands"},2490,2490,2490,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS2490: Radiant Heater Band","Yes","Yes","Existing kW",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR235=\"Agribusiness\", $AR235=\"Ag\",$AR235=\"Propane\", $AR235=\"Ag Propane\", $AR235=\"Ag-Propane\"),$AC235,  $AB235),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR235=\"Agribusiness\", $AR235=\"Ag\",$AR235=\"Propane\", $AR235=\"Ag Propane\", $AR235=\"Ag-Propane\"),$AC235,  $AB235),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":10,"d":"10.00"}},"Process Systems",20]
["PS2496","PS2496","N-PS2496","Pressure Screen Rotor","PS2496: Pressure Screen Rotor","Complete Table N of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","lncenllve Is limited to 50% of the project cost, Including equipment and external labor (Internal labor eligible for schools and government customers).","Provide metered data if available",{"$nulls":13},{"v":70,"d":"$70.00"},"HP",{"v":70,"d":"$70.00"},"HP",{"$f":"V236","v":{"v":70,"d":"$70.00"}},"HP",2496,2496,2496,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS2496: Pressure Screen Rotor","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR236=\"Agribusiness\", $AR236=\"Ag\",$AR236=\"Propane\", $AR236=\"Ag Propane\", $AR236=\"Ag-Propane\"),$AC236,  $AB236),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR236=\"Agribusiness\", $AR236=\"Ag\",$AR236=\"Propane\", $AR236=\"Ag Propane\", $AR236=\"Ag-Propane\"),$AC236,  $AB236),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":250,"d":"250.00"}},"Process Systems",20]
["PS2538","PS2538","N-PS2538","Repulper Rotor without Extraction Plate","PS2538: Repulper Rotor without Extraction Plate","Complete Table O of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Only for rotor applications that run at least 4,000 hours per year","Provide metered data if available","Incentive Is limited to 50% of the project cost, Including equipment and external labor (Internal labor eligible for schools and government customers).",{"$nulls":12},{"v":60,"d":"$60.00"},"HP",{"v":60,"d":"$60.00"},"HP",{"v":60,"d":"$60.00"},"HP",2538,2538,2538,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS2538: Repulper Rotor without Extraction Plate","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR237=\"Agribusiness\", $AR237=\"Ag\",$AR237=\"Propane\", $AR237=\"Ag Propane\", $AR237=\"Ag-Propane\"),$AC237,  $AB237),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR237=\"Agribusiness\", $AR237=\"Ag\",$AR237=\"Propane\", $AR237=\"Ag Propane\", $AR237=\"Ag-Propane\"),$AC237,  $AB237),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1250,"d":"1,250.00"}},"Process Systems",20]
["PS5210","PS5210","N-PS5210","Repulper Rotor with Extraction Plate","PS5210: Repulper Rotor with Extraction Plate","Complete Table O of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Only for rotor applications that run at least 4,000 hours per year","Provide metered data if available","Incentive Is limited to 50% of the project cost, Including equipment and external labor (Internal labor eligible for schools and government customers).",{"$nulls":12},{"v":70,"d":"$70.00"},"HP",{"v":70,"d":"$70.00"},"HP",{"v":70,"d":"$70.00"},"HP",5210,5210,5210,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS5210: Repulper Rotor with Extraction Plate","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR238=\"Agribusiness\", $AR238=\"Ag\",$AR238=\"Propane\", $AR238=\"Ag Propane\", $AR238=\"Ag-Propane\"),$AC238,  $AB238),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR238=\"Agribusiness\", $AR238=\"Ag\",$AR238=\"Propane\", $AR238=\"Ag Propane\", $AR238=\"Ag-Propane\"),$AC238,  $AB238),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Process Systems",20]
["PS4764","PS4764","N-PS4764","Spline Rotor Upgrade","PS4764: Spline Rotor Upgrade","Complete Table P of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentive is per refiner HP","Refiner must operate ≥ 4,000 hours/year","Incentive Is limited to 50% of the project cost, Including equipment and external labor (Internal labor eligible for schools and government customers).",{"$nulls":12},{"v":40,"d":"$40"},"HP",{"v":40,"d":"$40.00"},"HP",{"v":40,"d":"$40.00"},"HP",4764,4764,4764,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS4764: Spline Rotor Upgrade","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR239=\"Agribusiness\", $AR239=\"Ag\",$AR239=\"Propane\", $AR239=\"Ag Propane\", $AR239=\"Ag-Propane\"),$AC239,  $AB239),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":10,"d":"10.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR239=\"Agribusiness\", $AR239=\"Ag\",$AR239=\"Propane\", $AR239=\"Ag Propane\", $AR239=\"Ag-Propane\"),$AC239,  $AB239),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Process Systems",20]
["PS4763","PS4763","N-PS4763","HE Side Entry Agitator","PS4763: HE Side Entry Agitator","Complete Table Q of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Incentive is per agitator motor HP","Side entry agitator must install new engineered impeller","Refiner must operate ≥ 4,000 hours/year","Incentive Is limited to 50% of the project cost, Including equipment and external labor (Internal labor eligible for schools and government customers).",{"$nulls":11},{"v":60,"d":"$60"},"HP",{"v":60,"d":"$60.00"},"HP",{"v":60,"d":"$60.00"},"HP",4763,4763,4763,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS4763: HE Side Entry Agitator","Yes","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR240=\"Agribusiness\", $AR240=\"Ag\",$AR240=\"Propane\", $AR240=\"Ag Propane\", $AR240=\"Ag-Propane\"),$AC240,  $AB240),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":25,"d":"25.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR240=\"Agribusiness\", $AR240=\"Ag\",$AR240=\"Propane\", $AR240=\"Ag Propane\", $AR240=\"Ag-Propane\"),$AC240,  $AB240),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":250,"d":"250.00"}},"Process Systems",21]
["PS4765","PS4765","N-PS4765","Industrial High Frequency Battery Charger","PS4765: Industrial High Frequency Battery Charger","Complete Table R of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Charger must meet the California Energy Commission's 2016 Appliance Efficiency Regulations for Large Battery Chargers.","Incentive is per kW-hour (1,000 watt-hours) of battery charger capacity.","The charger must operate ≥ 1,000 hours/year","Charger must replace a ferroresonant, silicon controlled rectifier (SCR)or hybrid ferroresonant/SCR battery charger","Measure is not intended for electric/hybrid vehicles driven on public roads/highways","Use battery capacity in kW-hour from qualified products list, unless actual battery capacity (kW-hour or watt-hours) is significantly different. Refer to catalog for details on formula to use if significantly different.",{"$nulls":9},{"v":7,"d":"$7.00"},"kWh Capacity",{"v":7,"d":"$7.00"},"kWh Capacity",{"v":7,"d":"$7.00"},"kWh Capacity",4765,4765,4765,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS4765: Industrial High Frequency Battery Charger","Yes","Yes","kWh of charger capacity",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR241=\"Agribusiness\", $AR241=\"Ag\",$AR241=\"Propane\", $AR241=\"Ag Propane\", $AR241=\"Ag-Propane\"),$AC241,  $AB241),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR241=\"Agribusiness\", $AR241=\"Ag\",$AR241=\"Propane\", $AR241=\"Ag Propane\", $AR241=\"Ag-Propane\"),$AC241,  $AB241),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},"Process Systems",21]
["PS3244","PS3244","N-PS3244","Process Exhaust Filtration","PS3244: Process Exhaust Filtration","Complete Table S of the \"Process Systems Incentive Catalog Supplemental Data Sheet\" for this measure.","Must reduce/eliminate process exhaust by filtering/recirculating air & reducing/eliminating make-up air & assoc. heating energy.","Hours of operation must be ≥ 2,000 hours/year","Filtration must be applied to a manufacturing process. Commercial HVAC applications are not eligible.","Incentive Is limited to 50% of the project cost, Including equipment and external labor (Internal labor eligible for schools and government customers).","Make-up air systems that provide cooling or projects that offset the need for additional make-up air should go custom.",{"$nulls":10},{"v":1,"d":"$1.00"},"CFM Reduced",{"v":1,"d":"$1.00"},"CFM Reduced",{"$f":"V242","v":{"v":1,"d":"$1.00"}},"CFM Reduced",3244,3244,3244,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS3244: Process Exhaust Filtration","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR242=\"Agribusiness\", $AR242=\"Ag\",$AR242=\"Propane\", $AR242=\"Ag Propane\", $AR242=\"Ag-Propane\"),$AC242,  $AB242),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR242=\"Agribusiness\", $AR242=\"Ag\",$AR242=\"Propane\", $AR242=\"Ag Propane\", $AR242=\"Ag-Propane\"),$AC242,  $AB242),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Process Systems",21]
[{"$nulls":3},"----------------------AGRIBUSINESS CATALOG: MILKING EQUIPMENT -----------------------------","----------------------AGRIBUSINESS CATALOG: MILKING EQUIPMENT -----------------------------",{"$nulls":9},"",{"$nulls":22},"----------------------AGRIBUSINESS CATALOG: MILKING EQUIPMENT -----------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR243=\"Agribusiness\", $AR243=\"Ag\",$AR243=\"Propane\", $AR243=\"Ag Propane\", $AR243=\"Ag-Propane\"),$AC243,  $AB243),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR243=\"Agribusiness\", $AR243=\"Ag\",$AR243=\"Propane\", $AR243=\"Ag Propane\", $AR243=\"Ag-Propane\"),$AC243,  $AB243),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG3982","Eligible Under AgV2","Well Water Plate Heat Exchanger (<135 milking cows)","AG3982: Well Water Plate Heat Exchanger (<135 milking cows)","Select the appropriate plate cooler measure listed in the catalog depending on your number of milking cows. Enter number of milking cows in Units column on the Incentive Application for <135 milking cows.","Limit one incentive per milking operation.","New plate cooler installations only.","Milking cows includes dry cows, excludes heifers not yet fresh.",{"$nulls":4},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":600,"d":"$600.00"},"Plate Cooler",{"$f":"X244","v":{"v":600,"d":"$600.00"}},{"$f":"Y244","v":"Plate Cooler"},"N/A",3982,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG3982: Well Water Plate Heat Exchanger (<135 milking cows)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR244=\"Agribusiness\", $AR244=\"Ag\",$AR244=\"Propane\", $AR244=\"Ag Propane\", $AR244=\"Ag-Propane\"),$AC244,  $AB244),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR244=\"Agribusiness\", $AR244=\"Ag\",$AR244=\"Propane\", $AR244=\"Ag Propane\", $AR244=\"Ag-Propane\"),$AC244,  $AB244),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":135,"d":"135.00"}},"Agribusiness",12]
["Not Eligible","AG3983","Eligible Under AgV2","Well Water Plate Heat Exchanger (≥135 milking cows)","AG3983: Well Water Plate Heat Exchanger (≥135 milking cows)","Select the appropriate plate cooler measure listed in the catalog depending on your number of milking cows. Enter number of milking cows in Units column on the Incentive Application for ≥135 milking cows.","Limit one incentive per milking operation.","New plate cooler installations only.","Milking cows includes dry cows, excludes heifers not yet fresh.",{"$nulls":4},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":5,"d":"$5.00"},"Milking Cow",{"$f":"X245","v":{"v":5,"d":"$5.00"}},"Milking Cow","N/A",3983,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG3983: Well Water Plate Heat Exchanger (≥135 milking cows)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR245=\"Agribusiness\", $AR245=\"Ag\",$AR245=\"Propane\", $AR245=\"Ag Propane\", $AR245=\"Ag-Propane\"),$AC245,  $AB245),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":135,"d":"135.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR245=\"Agribusiness\", $AR245=\"Ag\",$AR245=\"Propane\", $AR245=\"Ag Propane\", $AR245=\"Ag-Propane\"),$AC245,  $AB245),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",12]
["Not Eligible","N-AG3982","Eligible Under AgV2","Well Water Plate Heat Exchanger (<135 milking cows)","N-AG3982: Well Water Plate Heat Exchanger (<135 milking cows)","Select the appropriate plate cooler measure listed in the catalog depending on your number of milking cows. Enter number of milking cows in the Units column on the Incentive Application for <135 milking cows.","Limit one incentive per milking operation.","New plate cooler installations only.","Milking cows includes dry cows, excludes heifers not yet fresh.",{"$nulls":4},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":600,"d":"$600.00"},"Plate Cooler",{"v":600,"d":"$600.00"},"Plate Cooler","N/A",3982,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG3982: Well Water Plate Heat Exchanger (<135 milking cows)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR246=\"Agribusiness\", $AR246=\"Ag\",$AR246=\"Propane\", $AR246=\"Ag Propane\", $AR246=\"Ag-Propane\"),$AC246,  $AB246),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR246=\"Agribusiness\", $AR246=\"Ag\",$AR246=\"Propane\", $AR246=\"Ag Propane\", $AR246=\"Ag-Propane\"),$AC246,  $AB246),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":135,"d":"135.00"}},"Agribusiness",12]
["Not Eligible","N-AG3983","Eligible Under AgV2","Well Water Plate Heat Exchanger (≥135 milking cows)","N-AG3983: Well Water Plate Heat Exchanger (≥135 milking cows)","Select the appropriate plate cooler measure listed in the catalog depending on your number of milking cows. Enter number of milking cows in Units column on the Incentive Application for ≥135 milking cows.","Limit one incentive per milking operation.","New plate cooler installations only.","Milking cows includes dry cows, excludes heifers not yet fresh.",{"$nulls":4},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":5,"d":"$5.00"},"Milking Cow",{"v":5,"d":"$5.00"},"Milking Cow","N/A",3983,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG3983: Well Water Plate Heat Exchanger (≥135 milking cows)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR247=\"Agribusiness\", $AR247=\"Ag\",$AR247=\"Propane\", $AR247=\"Ag Propane\", $AR247=\"Ag-Propane\"),$AC247,  $AB247),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":135,"d":"135.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR247=\"Agribusiness\", $AR247=\"Ag\",$AR247=\"Propane\", $AR247=\"Ag Propane\", $AR247=\"Ag-Propane\"),$AC247,  $AB247),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",12]
["Not Eligible","AG5231","Eligible Under AgV2","Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)","AG5231: Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)","Enter number of milking cows served by new equipment in Units column on the Incentive Application. For less than 500 milking cows.","For robotic milking operations, enter total number of milking cows served by new robot(s) with VSDs. Include quantity of VSDs on invoice if multiple are installed.","Limit one incentive per milking operation.","New variable speed control installations only. Redundant or backup units do not qualify.","See notes below if there are multiple VFDs","Milking cows includes dry cows, excludes heifers not yet fresh.",null,null,"Incentive must be ≤100% project cost.","To enter savings in Spectrum, enter number of VFDs in the \"units\" cell and enter total cows divided by number of VFDs in the cell asking for number of cows.  Example, if there are 300 cows total and 2 VFDs, enter 150 cows in the cell asking for number of cows. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":10,"d":"$10.00"},"Milking Cow",{"v":10,"d":"$10.00"},"Milking Cow","N/A",5231,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG5231: Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR248=\"Agribusiness\", $AR248=\"Ag\",$AR248=\"Propane\", $AR248=\"Ag Propane\", $AR248=\"Ag-Propane\"),$AC248,  $AB248),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR248=\"Agribusiness\", $AR248=\"Ag\",$AR248=\"Propane\", $AR248=\"Ag Propane\", $AR248=\"Ag-Propane\"),$AC248,  $AB248),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":499,"d":"499.00"}},"Agribusiness",12]
["Not Eligible","AG5232","Eligible Under AgV2","Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)","AG5232: Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)","Enter number of milking cows served by new equipment in Units column on the Incentive Application. For 500 to 2000 cows. ","For robotic milking operations, enter total number of milking cows served by new robot(s) with VSDs. Include quantity of VSDs on invoice if multiple are installed.","Limit one incentive per milking operation.","New variable speed control installations only. Redundant or backup units do not qualify.","See notes below if there are multiple VFDs","Milking cows includes dry cows, excludes heifers not yet fresh.",null,null,"Incentive must be ≤100% project cost.","To enter savings in Spectrum, enter number of VFDs in the \"units\" cell and enter total cows divided by number of VFDs in the cell asking for number of cows.  Example, if there are 300 cows total and 2 VFDs, enter 150 cows in the cell asking for number of cows. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":7,"d":"$7.00"},"Milking Cow",{"v":7,"d":"$7.00"},"Milking Cow","N/A",5232,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG5232: Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR249=\"Agribusiness\", $AR249=\"Ag\",$AR249=\"Propane\", $AR249=\"Ag Propane\", $AR249=\"Ag-Propane\"),$AC249,  $AB249),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR249=\"Agribusiness\", $AR249=\"Ag\",$AR249=\"Propane\", $AR249=\"Ag Propane\", $AR249=\"Ag-Propane\"),$AC249,  $AB249),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":2000,"d":"2,000.00"}},"Agribusiness",12]
["Not Eligible","AG10435","Eligible Under AgV3","Variable Speed Control Vacuum Pump, >2000 milking cows (Dairy Farm, Parlor, Milk House)",{"$f":"IF(ISBLANK(A250),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C250,IF(FOEIncentCodeType=IncentCodeTypeAg,B250,A250))&\": \") &D250","v":"AG10435: Variable Speed Control Vacuum Pump, >2000 milking cows (Dairy Farm, Parlor, Milk House)"},"Enter number of milking cows served by new equipment in Units column on the Incentive Application. For over 2000 cows.","For robotic milking operations, enter total number of milking cows served by new robot(s) with VSDs. Include quantity of VSDs on invoice if multiple are installed.","Limit one incentive per milking operation.","New variable speed control installations only. Redundant or backup units do not qualify.","See notes below if there are multiple VFDs","Milking cows includes dry cows, excludes heifers not yet fresh.",null,null,"Incentive must be ≤100% project cost.","To enter savings in Spectrum, enter number of VFDs in the \"units\" cell and enter total cows divided by number of VFDs in the cell asking for number of cows.  Example, if there are 300 cows total and 2 VFDs, enter 150 cows in the cell asking for number of cows. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":3,"d":"$3.00"},"Milking Cow",{"v":3,"d":"$3.00"},"Milking Cow","N/A",10435,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG10435: Variable Speed Control Vacuum Pump, >2000 milking cows (Dairy Farm, Parlor, Milk House)","No","No","",{"v":2000,"d":"2,000.00"},{"v":15000,"d":"15,000.00"},"Agribusiness",12]
["Not Eligible","AG3988","Eligible Under AgV2","Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)","AG3988: Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)","Enter number of milking cows served by new equipment in Units column on the Incentive Application.","For robotic milking operations, enter total number of milking cows served by new robot(s) with VSDs. Include quantity of VSDs on invoice if multiple are installed.","Limit one incentive per milking operation.","New variable speed control installations only. Redundant or backup units do not qualify.","See notes below if there are multiple VFDs","Milking cows includes dry cows, excludes heifers not yet fresh.",null,null,"Incentive must be ≤100% project cost.","To enter savings in Spectrum, enter number of VFDs in the \"units\" cell and enter total cows divided by number of VFDs in the cell asking for number of cows.  Example, if there are 300 cows total and 2 VFDs, enter 150 cows in the cell asking for number of cows. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":4,"d":"$4.00"},"Milking Cow",{"v":4,"d":"$4.00"},"Milking Cow","N/A",3988,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG3988: Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR251=\"Agribusiness\", $AR251=\"Ag\",$AR251=\"Propane\", $AR251=\"Ag Propane\", $AR251=\"Ag-Propane\"),$AC251,  $AB251),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR251=\"Agribusiness\", $AR251=\"Ag\",$AR251=\"Propane\", $AR251=\"Ag Propane\", $AR251=\"Ag-Propane\"),$AC251,  $AB251),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",12]
["Not Eligible","N-AG5231","Eligible Under AgV2","Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)","N-AG5231: Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)","Enter number of milking cows served by new equipment in Units column on the Incentive Application. For less than 500 milking cows.","For robotic milking operations, enter total number of milking cows served by new robot(s) with VSDs. Include quantity of VSDs on invoice if multiple are installed.","Limit one incentive per milking operation.","New variable speed control installations only. Redundant or backup units do not qualify.","See notes below if there are multiple VFDs","Milking cows includes dry cows, excludes heifers not yet fresh.",null,null,"Incentive must be ≤100% project cost.","To enter savings in Spectrum, enter number of VFDs in the \"units\" cell and enter total cows divided by number of VFDs in the cell asking for number of cows.  Example, if there are 300 cows total and 2 VFDs, enter 150 cows in the cell asking for number of cows. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":10,"d":"$10.00"},"Milking Cow",{"v":10,"d":"$10.00"},"Milking Cow","N/A",5231,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5231: Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR252=\"Agribusiness\", $AR252=\"Ag\",$AR252=\"Propane\", $AR252=\"Ag Propane\", $AR252=\"Ag-Propane\"),$AC252,  $AB252),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR252=\"Agribusiness\", $AR252=\"Ag\",$AR252=\"Propane\", $AR252=\"Ag Propane\", $AR252=\"Ag-Propane\"),$AC252,  $AB252),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":499,"d":"499.00"}},"Agribusiness",12]
["Not Eligible","N-AG5232","Eligible Under AgV2","Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)","N-AG5232: Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)","Enter number of milking cows served by new equipment in Units column on the Incentive Application. For 500 to 2000 cows. Over 2000 cows must go custom.","For robotic milking operations, enter total number of milking cows served by new robot(s) with VSDs. Include quantity of VSDs on invoice if multiple are installed.","Limit one incentive per milking operation.","New variable speed control installations only. Redundant or backup units do not qualify.","See notes below if there are multiple VFDs","Milking cows includes dry cows, excludes heifers not yet fresh.",null,null,"Incentive must be ≤100% project cost.","To enter savings in Spectrum, enter number of VFDs in the \"units\" cell and enter total cows divided by number of VFDs in the cell asking for number of cows.  Example, if there are 300 cows total and 2 VFDs, enter 150 cows in the cell asking for number of cows. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":7,"d":"$7.00"},"Milking Cow",{"v":7,"d":"$7.00"},"Milking Cow","N/A",5232,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5232: Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR253=\"Agribusiness\", $AR253=\"Ag\",$AR253=\"Propane\", $AR253=\"Ag Propane\", $AR253=\"Ag-Propane\"),$AC253,  $AB253),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR253=\"Agribusiness\", $AR253=\"Ag\",$AR253=\"Propane\", $AR253=\"Ag Propane\", $AR253=\"Ag-Propane\"),$AC253,  $AB253),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":2000,"d":"2,000.00"}},"Agribusiness",12]
["Not Eligible","N-AG10435","Eligible Under AgV3","Variable Speed Control Vacuum Pump, >2000 milking cows (Dairy Farm, Parlor, Milk House)","N-AG10435: Variable Speed Control Vacuum Pump, >2000 milking cows (Dairy Farm, Parlor, Milk House)","Enter number of milking cows served by new equipment in Units column on the Incentive Application. For over 2000 cows.","For robotic milking operations, enter total number of milking cows served by new robot(s) with VSDs. Include quantity of VSDs on invoice if multiple are installed.","Limit one incentive per milking operation.","New variable speed control installations only. Redundant or backup units do not qualify.","See notes below if there are multiple VFDs","Milking cows includes dry cows, excludes heifers not yet fresh.",null,null,"Incentive must be ≤100% project cost.","To enter savings in Spectrum, enter number of VFDs in the \"units\" cell and enter total cows divided by number of VFDs in the cell asking for number of cows.  Example, if there are 300 cows total and 2 VFDs, enter 150 cows in the cell asking for number of cows. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":3,"d":"$3.00"},"Milking Cow",{"v":3,"d":"$3.00"},"Milking Cow","N/A",10435,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10435: Variable Speed Control Vacuum Pump, >2000 milking cows (Dairy Farm, Parlor, Milk House)","No","No","",{"v":2000,"d":"2,000.00"},{"v":15000,"d":"15,000.00"},"Agribusiness",12]
["Not Eligible","N-AG3988","Eligible Under AgV2","Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)","N-AG3988: Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)","Enter number of milking cows served by new equipment in Units column on the Incentive Application.","For robotic milking operations, enter total number of milking cows served by new robot(s) with VSDs. Include quantity of VSDs on invoice if multiple are installed.","Limit one incentive per milking operation.","New variable speed control installations only. Redundant or backup units do not qualify.","See notes below if there are multiple VFDs","Milking cows includes dry cows, excludes heifers not yet fresh.",null,null,"Incentive must be ≤100% project cost.","To enter savings in Spectrum, enter number of VFDs in the \"units\" cell and enter total cows divided by number of VFDs in the cell asking for number of cows. Example, if there are 300 cows total and 2 VFDs, enter 150 cows in the cell asking for number of cows. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":4,"d":"$4.00"},"Milking Cow",{"v":4,"d":"$4.00"},"Milking Cow","N/A",3988,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG3988: Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR255=\"Agribusiness\", $AR255=\"Ag\",$AR255=\"Propane\", $AR255=\"Ag Propane\", $AR255=\"Ag-Propane\"),$AC255,  $AB255),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR255=\"Agribusiness\", $AR255=\"Ag\",$AR255=\"Propane\", $AR255=\"Ag Propane\", $AR255=\"Ag-Propane\"),$AC255,  $AB255),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",12]
[{"$nulls":3},"----------------------AGRIBUSINESS CATALOG: OTHER SPECIALTY EQUIPMENT -----------------------------",{"$f":"IF(ISBLANK(A256),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C256,IF(FOEIncentCodeType=IncentCodeTypeAg,B256,A256))&\": \") &D256","v":"----------------------AGRIBUSINESS CATALOG: OTHER SPECIALTY EQUIPMENT -----------------------------"},{"$nulls":9},"",{"$nulls":22},"----------------------AGRIBUSINESS CATALOG: OTHER SPECIALTY EQUIPMENT -----------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR256=\"Agribusiness\", $AR256=\"Ag\",$AR256=\"Propane\", $AR256=\"Ag Propane\", $AR256=\"Ag-Propane\"),$AC256,  $AB256),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR256=\"Agribusiness\", $AR256=\"Ag\",$AR256=\"Propane\", $AR256=\"Ag Propane\", $AR256=\"Ag-Propane\"),$AC256,  $AB256),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG2660","Not Eligible","Low-Energy Livestock Waterer (Heating Element Maximum of 250W)","AG2660: Low-Energy Livestock Waterer (Heating Element Maximum of 250W)","If replacing existing equipment, existing waterer must have heating elements.","Low-energy waterer must have a maximum combined heating element wattage of 250W.",null,"Verify insulation is adequate for the location waterer is installed.","Model number of waterer must be listed on the invoice.",{"$nulls":3},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":90,"d":"$90.00"},"Waterer","N/A","Waterer","N/A",2660,"N/A","N/A",{"$f":"IFERROR(IF(SEARCH(\"N-\",B257),\"Yes\",\"No\"),\"No\")","v":"No"},"N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG2660: Low-Energy Livestock Waterer (Heating Element Maximum of 250W)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR257=\"Agribusiness\", $AR257=\"Ag\",$AR257=\"Propane\", $AR257=\"Ag Propane\", $AR257=\"Ag-Propane\"),$AC257,  $AB257),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR257=\"Agribusiness\", $AR257=\"Ag\",$AR257=\"Propane\", $AR257=\"Ag Propane\", $AR257=\"Ag-Propane\"),$AC257,  $AB257),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",13]
["Not Eligible","AG3018","Eligible Under AgV2","Zero-Energy Livestock Waterer","AG3018: Zero-Energy Livestock Waterer","If replacing existing equipment, existing waterer must have heating elements.","Low-energy waterer must have a maximum combined heating element wattage of 250W.","Zero-energy waterer must contain no heating elements.","Verify insulation is adequate for the location waterer is installed.","Model number of waterer must be listed on the invoice.",{"$nulls":3},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":100,"d":"$100.00"},"Waterer",{"v":100,"d":"$100.00"},"Waterer","N/A",3018,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG3018: Zero-Energy Livestock Waterer","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR258=\"Agribusiness\", $AR258=\"Ag\",$AR258=\"Propane\", $AR258=\"Ag Propane\", $AR258=\"Ag-Propane\"),$AC258,  $AB258),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR258=\"Agribusiness\", $AR258=\"Ag\",$AR258=\"Propane\", $AR258=\"Ag Propane\", $AR258=\"Ag-Propane\"),$AC258,  $AB258),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",13]
["Not Eligible","N-AG3018","Eligible Under AgV2","Zero-Energy Livestock Waterer","N-AG3018: Zero-Energy Livestock Waterer","If replacing existing equipment, existing waterer must have heating elements.","Low-energy waterer must have a maximum combined heating element wattage of 250W.","Zero-energy waterer must contain no heating elements.","Verify insulation is adequate for the location waterer is installed.","Model number of waterer must be listed on the invoice.",{"$nulls":3},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":100,"d":"$100.00"},"Waterer",{"v":100,"d":"$100.00"},"Waterer","N/A",3018,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG3018: Zero-Energy Livestock Waterer","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR259=\"Agribusiness\", $AR259=\"Ag\",$AR259=\"Propane\", $AR259=\"Ag Propane\", $AR259=\"Ag-Propane\"),$AC259,  $AB259),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR259=\"Agribusiness\", $AR259=\"Ag\",$AR259=\"Propane\", $AR259=\"Ag Propane\", $AR259=\"Ag-Propane\"),$AC259,  $AB259),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",13]
["Not Eligible","AG4939","Eligible Under AgV2","Swine Farrowing Crate Heater, Single","AG4939: Swine Farrowing Crate Heater, Single","Heaters must be installed in the farrowing crates directly under or over the piglets","Heaters must have thermostatic controller that automatically varies the heat output according to the needs of the piglets","For replacement or instead of heat lamps or ceramic heaters",{"$nulls":5},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":30,"d":"$30.00"},"Heater",{"v":30,"d":"$30.00"},"Heater","N/A",4939,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4939: Swine Farrowing Crate Heater, Single","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR260=\"Agribusiness\", $AR260=\"Ag\",$AR260=\"Propane\", $AR260=\"Ag Propane\", $AR260=\"Ag-Propane\"),$AC260,  $AB260),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR260=\"Agribusiness\", $AR260=\"Ag\",$AR260=\"Propane\", $AR260=\"Ag Propane\", $AR260=\"Ag-Propane\"),$AC260,  $AB260),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",13]
["Not Eligible","AG4940","Eligible Under AgV2","Swine Farrowing Crate Heater, Double","AG4940: Swine Farrowing Crate Heater, Double","Heaters must be installed in the farrowing crates directly under or over the piglets","Heaters must have thermostatic controller that automatically varies the heat output according to the needs of the piglets","For replacement or instead of heat lamps or ceramic heaters",{"$nulls":5},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":60,"d":"$60.00"},"Heater",{"v":60,"d":"$60.00"},{"$f":"Y261","v":"Heater"},"N/A",4940,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4940: Swine Farrowing Crate Heater, Double","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR261=\"Agribusiness\", $AR261=\"Ag\",$AR261=\"Propane\", $AR261=\"Ag Propane\", $AR261=\"Ag-Propane\"),$AC261,  $AB261),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR261=\"Agribusiness\", $AR261=\"Ag\",$AR261=\"Propane\", $AR261=\"Ag Propane\", $AR261=\"Ag-Propane\"),$AC261,  $AB261),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",13]
["Not Eligible","N-AG4939","Eligible Under AgV2","Swine Farrowing Crate Heater, Single","N-AG4939: Swine Farrowing Crate Heater, Single","Heaters must be installed in the farrowing crates directly under or over the piglets","Heaters must have thermostatic controller that automatically varies the heat output according to the needs of the piglets","For replacement or instead of heat lamps or ceramic heaters",{"$nulls":5},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":30,"d":"$30.00"},"Heater",{"v":30,"d":"$30.00"},"Heater","N/A",4939,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4939: Swine Farrowing Crate Heater, Single","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR262=\"Agribusiness\", $AR262=\"Ag\",$AR262=\"Propane\", $AR262=\"Ag Propane\", $AR262=\"Ag-Propane\"),$AC262,  $AB262),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR262=\"Agribusiness\", $AR262=\"Ag\",$AR262=\"Propane\", $AR262=\"Ag Propane\", $AR262=\"Ag-Propane\"),$AC262,  $AB262),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",13]
["Not Eligible","N-AG4940","Eligible Under AgV2","Swine Farrowing Crate Heater, Double","N-AG4940: Swine Farrowing Crate Heater, Double","Heaters must be installed in the farrowing crates directly under or over the piglets","Heaters must have thermostatic controller that automatically varies the heat output according to the needs of the piglets","For replacement or instead of heat lamps or ceramic heaters",{"$nulls":5},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":60,"d":"$60.00"},"Heater",{"v":60,"d":"$60.00"},"Heater","N/A",4940,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4940: Swine Farrowing Crate Heater, Double","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR263=\"Agribusiness\", $AR263=\"Ag\",$AR263=\"Propane\", $AR263=\"Ag Propane\", $AR263=\"Ag-Propane\"),$AC263,  $AB263),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR263=\"Agribusiness\", $AR263=\"Ag\",$AR263=\"Propane\", $AR263=\"Ag Propane\", $AR263=\"Ag-Propane\"),$AC263,  $AB263),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",13]
["Not Eligible","AG3386","Not Eligible","Efficient Grain Dryer (Natural Gas or Propane)","AG3386: Efficient Grain Dryer (Natural Gas or Propane)","Complete Tables A1-A2 of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.  See catalog for specifics","All new grain dryers must be permanent installations that use natural gas or propane as the heating source. ONLY CORN DRYERS ARE ELIGIBLE.","Installed replacement grain dryer must be new. Used or rebuilt equipment is not eligible. For incentive purposes, 10% moisture content reduction bushels/hour rating in full heat mode of new grain dryer should be used.","New grain dryer must improve dryer efficiency by 250 BTU/lb H2O.","Equipment not eligible for prescriptive incentives may be eligible for custom incentives.","Manufacturer Specification Sheet of proposed grain dryer must be included with Grain Dryer Application.","Dryer must include at least one of these energy-efficient features - Staged Temperature (higher temperature for wettest grain), Grain Turners or Inverters (rotate dry grain away from plenum), Differential Grain Speed (drying column designed to move grain ","next to plenum faster), Varied Width of Drying Column (narrower at top where wet grain is located), Some type of grain heat recovery features, Advanced grain dryer operation controls.  Pre-qualification of proposed equipment is recommended.","Corresponding Propane MMID: AG4868","If electric utility is non-participating, make a note of that when creating activity for hybrid calc. Non-participating electric utility ok, do not claim any electric savings. Consult with PM if incentive should be adjusted.",{"$nulls":6},"N/A","N/A",{"v":20,"d":"$20.00"},"Bushel/hr drying capacity","N/A","Bushel/hr drying capacity","N/A",3386,"N/A","N/A",{"$f":"IFERROR(IF(SEARCH(\"N-\",B264),\"Yes\",\"No\"),\"No\")","v":"No"},"N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG3386: Efficient Grain Dryer (Natural Gas or Propane)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR264=\"Agribusiness\", $AR264=\"Ag\",$AR264=\"Propane\", $AR264=\"Ag Propane\", $AR264=\"Ag-Propane\"),$AC264,  $AB264),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR264=\"Agribusiness\", $AR264=\"Ag\",$AR264=\"Propane\", $AR264=\"Ag Propane\", $AR264=\"Ag-Propane\"),$AC264,  $AB264),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5000,"d":"5,000.00"}},"Agribusiness",14]
["Not Eligible","N-AG10421","N-AG10421","Efficient Grain Dryer, Mixed Flow Only (Natural Gas or Propane)",{"$f":"IF(ISBLANK(A265),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C265,IF(FOEIncentCodeType=IncentCodeTypeAg,B265,A265))&\": \") &D265","v":"N-AG10421: Efficient Grain Dryer, Mixed Flow Only (Natural Gas or Propane)"},"Complete Tables A1-A2 of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.  See catalog for specifics","All new grain dryers must be permanent installations that use natural gas or propane as the heating source. ONLY CORN DRYERS ARE ELIGIBLE.","Installed replacement grain dryer must be new. Used or rebuilt equipment is not eligible. For incentive purposes, 10% moisture content reduction bushels/hour rating in full heat mode of new grain dryer should be used.","New grain dryer must improve dryer efficiency by 250 BTU/lb H2O.","Equipment not eligible for prescriptive incentives may be eligible for custom incentives.","Manufacturer Specification Sheet of proposed grain dryer must be included with Grain Dryer Application.","Dryer must be Mixed Flow.  ","Pre-qualification of proposed equipment is recommended.","Corresponding Propane MMID: AG4868","If electric utility is non-participating, make a note of that when creating activity for hybrid calc. Non-participating electric utility ok, do not claim any electric savings. Consult with PM if incentive should be adjusted.",{"$nulls":6},"N/A","N/A",{"v":8,"d":"$8.00"},"Bushel/hr drying capacity",{"v":8,"d":"$8.00"},"Bushel/hr drying capacity","N/A",10421,10421,"Yes",{"$f":"IFERROR(IF(SEARCH(\"N-\",B265),\"Yes\",\"No\"),\"No\")","v":"Yes"},"N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10421: Efficient Grain Dryer, Mixed Flow Only (Natural Gas or Propane)","Yes","Yes","",{"v":500,"d":"500.00"},{"v":5000,"d":"5,000.00"},"Agribusiness",14]
["Not Eligible","AG2434","Not Eligible","Pump Motor Horsepower Reduction","AG2434: Pump Motor Horsepower Reduction","Complete Tables B1 and B2 of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure. See catalog for specifics","Project cost includes materials and labor to install new nozzle package and new motor.","To qualify, horsepower reduction projects must consist of both re-nozzling the existing irrigation system and reducing the well pump motor horsepower.","Must replace all the nozzles on the entire system.","Must install nozzles that require at least 10% less horsepower at the well pump than the original nozzle package.","Must replace pump motor and reduce motor horsepower by 10% or more.","Well pump must be electrically powered, with energy provided by a participating electricity provider.","This measure does not include the use of VFD control to reduce motor horsepower. See page 32 for VFD measures.",{"$nulls":8},"N/A","N/A",{"v":85,"d":"$85.00"},"Reduced HP","N/A","Reduced HP","N/A",2434,"N/A","N/A",{"$f":"IFERROR(IF(SEARCH(\"N-\",B266),\"Yes\",\"No\"),\"No\")","v":"No"},"N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG2434: Pump Motor Horsepower Reduction","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR266=\"Agribusiness\", $AR266=\"Ag\",$AR266=\"Propane\", $AR266=\"Ag Propane\", $AR266=\"Ag-Propane\"),$AC266,  $AB266),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR266=\"Agribusiness\", $AR266=\"Ag\",$AR266=\"Propane\", $AR266=\"Ag Propane\", $AR266=\"Ag-Propane\"),$AC266,  $AB266),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":75,"d":"75.00"}},"Agribusiness",15]
["Not Eligible","AG4949","Eligible Under AgV2","VFD, Irrigation Well Pump (≥500 Annual Operating Hours)","AG4949: VFD, Irrigation Well Pump (≥500 Annual Operating Hours)","Complete Tables C1 and C2 of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.  See catalog for specifics.","VFD must be installed on a centrifugal or axial flow pump i.e., a variable torque load used to control a process on your crop farm.","Equipment controlled by VFD must operate a min. of 500 hours annual & individual motors controlled by a VFD may not exceed 500 hp.  VFDs controlling motors larger than 500 HP or that run <500 hours annually may be eligible for a custom incentive.","Redundant or back-up units do not qualify. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD.","VFD speed must be automatically controlled by differential pressure, flow, temperature, or other variable signal. Units installed only to allow soft starts are not eligible.","The system controlled must have significant load diversity that will result in savings through motor speed variation.","VFDs may not be beneficial in pump systems where static head makes up a large portion of the total system head. It is also important that the load on the system vary over time to take advantage of the savings that a VFD can provide.","Be sure to understand these aspects of your system and discuss them with the equipment vendor in advance of applying VFD\ntechnology.","Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":70,"d":"$70.00"},"hp",{"v":70,"d":"$70.00"},{"$f":"Y267","v":"hp"},"N/A",4949,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4949: VFD, Irrigation Well Pump (≥500 Annual Operating Hours)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR267=\"Agribusiness\", $AR267=\"Ag\",$AR267=\"Propane\", $AR267=\"Ag Propane\", $AR267=\"Ag-Propane\"),$AC267,  $AB267),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":10,"d":"10.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR267=\"Agribusiness\", $AR267=\"Ag\",$AR267=\"Propane\", $AR267=\"Ag Propane\", $AR267=\"Ag-Propane\"),$AC267,  $AB267),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"Agribusiness","15 & 24"]
["Not Eligible","N-AG4949","Eligible Under AgV2","VFD, Irrigation Well Pump (≥500 Annual Operating Hours)","N-AG4949: VFD, Irrigation Well Pump (≥500 Annual Operating Hours)","Complete Tables C1 and C2 of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.  See catalog for specifics.","VFD must be installed on a centrifugal or axial flow pump i.e., a variable torque load used to control a process on your crop farm.","Equipment controlled by VFD must operate a min. of 500 hours annual & individual motors controlled by a VFD may not exceed 500 hp.  VFDs controlling motors larger than 500 HP or that run <500 hours annually may be eligible for a custom incentive.","Redundant or back-up units do not qualify. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD.","VFD speed must be automatically controlled by differential pressure, flow, temperature, or other variable signal. Units installed only to allow soft starts are not eligible.","The system controlled must have significant load diversity that will result in savings through motor speed variation.","VFDs may not be beneficial in pump systems where static head makes up a large portion of the total system head. It is also important that the load on the system vary over time to take advantage of the savings that a VFD can provide.","Be sure to understand these aspects of your system and discuss them with the equipment vendor in advance of applying VFD\ntechnology.","Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":40,"d":"$40.00"},"hp",{"v":40,"d":"$40.00"},{"$f":"Y268","v":"hp"},"N/A",4949,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4949: VFD, Irrigation Well Pump (≥500 Annual Operating Hours)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR268=\"Agribusiness\", $AR268=\"Ag\",$AR268=\"Propane\", $AR268=\"Ag Propane\", $AR268=\"Ag-Propane\"),$AC268,  $AB268),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":10,"d":"10.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR268=\"Agribusiness\", $AR268=\"Ag\",$AR268=\"Propane\", $AR268=\"Ag Propane\", $AR268=\"Ag-Propane\"),$AC268,  $AB268),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"Agribusiness","15 & 24"]
[{"$nulls":3},"----------------------AGRIBUSINESS CATALOG: GREENHOUSE ENVELOPE AND CONTROLS --------------------------------------------","----------------------AGRIBUSINESS CATALOG: GREENHOUSE ENVELOPE AND CONTROLS --------------------------------------------"]
["Not Eligible","AG10438","Not Eligible","Greenhouse Glazing (Natural Gas or Propane)","AG10438: Greenhouse Glazing (Natural Gas or Propane)","Complete the Greenhouse Supplemental Data Sheet","Installed glazing must have U value ≤0.60.  Manufacturer's spec sheet to confirm.","Installed glazing must be double poly with infrared treatment; 6mm, 8mm, or 16mm double poly; or triple poly.","Other glazings may be elgible for custom.",{"$nulls":12},"N/A","N/A",{"v":1.25,"d":"$1.25"},"square feet",{"v":1.25,"d":"$1.25"},{"$f":"Y270","v":"square feet"},"N/A",10438,"N/A","N/A","See NC MMID","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No",{"$f":"IF(ISBLANK(A270),\"\",IF(A270<>\"Not Eligible\",A270,IF(B270<>\"Not Eligible\",B270,C270))&\": \") &D270","v":"AG10438: Greenhouse Glazing (Natural Gas or Propane)"},"Yes","Yes","Sq Ft",{"v":500,"d":"500.00"},{"v":100000,"d":"100,000.00"},"Agribusiness",16]
["Not Eligible","N-AG10438","Eligible Under AgV2","Greenhouse Glazing (Natural Gas or Propane)","N-AG10438: Greenhouse Glazing (Natural Gas or Propane)","Complete the Greenhouse Supplemental Data Sheet","Installed glazing must have U value ≤0.60.  Manufacturer's spec sheet to confirm.","Installed glazing must be double poly with infrared treatment; 6mm, 8mm, or 16mm double poly; or triple poly.","Other glazings may be elgible for custom.",{"$nulls":12},"N/A","N/A",{"v":1.25,"d":"$1.25"},"square feet",{"v":1.25,"d":"$1.25"},"square feet","N/A",10438,"N/A","N/A","Yes","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-AG10438: Greenhouse Glazing (Natural Gas or Propane)","Yes","Yes","Sq Ft",{"v":500,"d":"500.00"},{"v":100000,"d":"100,000.00"},"Agribusiness",16]
["Not Eligible","AG10442","Not Eligible","Greenhouse Thermal Curtain (Natural Gas or Propane)","AG10442: Greenhouse Thermal Curtain (Natural Gas or Propane)","Complete the Greenhouse Supplemental Data Sheet","Installed thermal curtain must have energy savings rating of ≥50%.  Manufacturer's spec sheet to confirm.","Primary heating distribution location must be underneath the curtain.","Thermal curtain must be installed above the plants.  Curtains applied to sidewalls may be eligible for custom incentives.",{"$nulls":12},"N/A","N/A",{"v":1,"d":"$1.00"},"square feet",{"v":1,"d":"$1.00"},"square feet","N/A",10442,"N/A","N/A","See NC MMID","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","AG10442: Greenhouse Thermal Curtain (Natural Gas or Propane)","Yes","Yes","Sq Ft",{"v":500,"d":"500.00"},{"v":100000,"d":"100,000.00"},"Agribusiness",16]
["Not Eligible","N-AG10442","Eligible Under AgV2","Greenhouse Thermal Curtain (Natural Gas or Propane)","N-AG10442: Greenhouse Thermal Curtain (Natural Gas or Propane)","Complete the Greenhouse Supplemental Data Sheet","Installed thermal curtain must have energy savings rating of ≥50%.  Manufacturer's spec sheet to confirm.","Primary heating distribution location must be underneath the curtain.","Thermal curtain must be installed above the plants.  Curtains applied to sidewalls may be eligible for custom incentives.",{"$nulls":12},"N/A","N/A",{"v":1,"d":"$1.00"},"square feet",{"v":1,"d":"$1.00"},"square feet","N/A",10442,"N/A","N/A","Yes","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-AG10442: Greenhouse Thermal Curtain (Natural Gas or Propane)","Yes","Yes","Sq Ft",{"v":500,"d":"500.00"},{"v":100000,"d":"100,000.00"},"Agribusiness",16]
["Not Eligible","AG10444","Not Eligible","Greenhouse Climate Controls (Natural Gas or Propane)","AG10444: Greenhouse Climate Controls (Natural Gas or Propane)","Complete the Greenhouse Supplemental Data Sheet","Installed system must control heating and ventilation and have a min of two temp stages.  Manufacturer's spec sheet to confirm.","Daytime set points must be above 65F and active for at least 12 hours per day.","Nighttime set points must be above 60F (but cannot exceed daytime set point).","Must not have a climate control system already installed.",{"$nulls":11},"N/A","N/A",{"v":0.6,"d":"$0.60"},"square feet",{"v":0.6,"d":"$0.60"},"square feet","N/A",10444,"N/A","N/A","See NC MMID","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","AG10444: Greenhouse Climate Controls (Natural Gas or Propane)","Yes","Yes","Sq Ft",{"v":500,"d":"500.00"},{"v":100000,"d":"100,000.00"},"Agribusiness",16]
["Not Eligible","N-AG10444","Eligible Under AgV2","Greenhouse Climate Controls (Natural Gas or Propane)","N-AG10444: Greenhouse Climate Controls (Natural Gas or Propane)","Complete the Greenhouse Supplemental Data Sheet","Installed system must control heating and ventilation and have a min of two temp stages.  Manufacturer's spec sheet to confirm.","Daytime set points must be above 65F and active for at least 12 hours per day.","Nighttime set points must be above 60F (but cannot exceed daytime set point).","Baseline must be provided as if not installing a climate control system.",{"$nulls":11},"N/A","N/A",{"v":0.6,"d":"$0.60"},"square feet",{"v":0.6,"d":"$0.60"},"square feet","N/A",10444,"N/A","N/A","Yes","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-AG10444: Greenhouse Climate Controls (Natural Gas or Propane)","Yes","Yes","Sq Ft",{"v":500,"d":"500.00"},{"v":100000,"d":"100,000.00"},"Agribusiness",16]
[{"$nulls":3},"----------------------AGRIBUSINESS CATALOG: LIGHTING --------------------------------------------","----------------------AGRIBUSINESS CATALOG: LIGHTING --------------------------------------------","","","","","","","","","","",{"$nulls":22},"----------------------AGRIBUSINESS CATALOG: LIGHTING --------------------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR276=\"Agribusiness\", $AR276=\"Ag\",$AR276=\"Propane\", $AR276=\"Ag Propane\", $AR276=\"Ag-Propane\"),$AC276,  $AB276),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR276=\"Agribusiness\", $AR276=\"Ag\",$AR276=\"Propane\", $AR276=\"Ag Propane\", $AR276=\"Ag-Propane\"),$AC276,  $AB276),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["L5459","L5459","N-L5459","1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer","L5459: 1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer","For 1-for-1 replacement of T12 or standard T8 fluorescent fixtures","Must be DLC TRT V5.0 or higher listed in the \"Troffer\" general application.","New fixture must consume ≤ 43W.","Other LED configurations may qualify for a custom incentive.",{"$nulls":5},"Other LED configurations may qualify for custom incentive.","Provide clear photo(s) of: fixture layout and (if possible) fixture packaging label.","Verify fixture size by comparing to grid ceiling as reference.",{"$nulls":4},{"v":10,"d":"$10.00"},"Fixture",{"v":10,"d":"$10.00"},"Fixture",{"v":7,"d":"$7.00"},{"$f":"Y277","v":"Fixture"},"N/A",5459,5459,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L5459: 1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR277=\"Agribusiness\", $AR277=\"Ag\",$AR277=\"Propane\", $AR277=\"Ag Propane\", $AR277=\"Ag-Propane\"),$AC277,  $AB277),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR277=\"Agribusiness\", $AR277=\"Ag\",$AR277=\"Propane\", $AR277=\"Ag Propane\", $AR277=\"Ag-Propane\"),$AC277,  $AB277),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",17]
["L3111","L3111","N-L3111","2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer","L3111: 2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer","For 1-for-1 replacement of T12 or standard T8 fluorescent fixtures","Must be DLC TRT V5.0 or higher listed in the \"Troffer\" general application.","New fixture must consume ≤ 55W","Other LED configurations may qualify for a custom incentive.",{"$nulls":5},"Work paper is based on 3 and 4 lamp fixtures only. ","Provide clear photo(s) of: fixture layout and (if possible) fixture packaging label.","Verify fixture size by comparing to grid ceiling as reference.",{"$nulls":4},{"v":25,"d":"$25.00"},"Fixture",{"v":25,"d":"$25.00"},"Fixture",{"v":20,"d":"$20.00"},"Fixture","N/A",3111,3111,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3111: 2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR278=\"Agribusiness\", $AR278=\"Ag\",$AR278=\"Propane\", $AR278=\"Ag Propane\", $AR278=\"Ag-Propane\"),$AC278,  $AB278),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR278=\"Agribusiness\", $AR278=\"Ag\",$AR278=\"Propane\", $AR278=\"Ag Propane\", $AR278=\"Ag-Propane\"),$AC278,  $AB278),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",17]
["L3400","L3400","N-L3400","2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","For 1-for-1 replacement of T12 or standard T8 fluorescent fixtures","Must be DLC TRT V5.0 or higher listed in the \"Troffer\" general application.","New fixture must consume ≤ 39W.","Other LED configurations may qualify for a custom incentive.",{"$nulls":6},"Provide clear photo(s) of: fixture layout and (if possible) fixture packaging label.","Verify fixture size by comparing to grid ceiling as reference.",{"$nulls":4},{"v":15,"d":"$15.00"},"Fixture",{"v":15,"d":"$15.00"},"Fixture",{"v":10,"d":"$10.00"},"Fixture","N/A",3400,3400,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR279=\"Agribusiness\", $AR279=\"Ag\",$AR279=\"Propane\", $AR279=\"Ag Propane\", $AR279=\"Ag-Propane\"),$AC279,  $AB279),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR279=\"Agribusiness\", $AR279=\"Ag\",$AR279=\"Propane\", $AR279=\"Ag Propane\", $AR279=\"Ag-Propane\"),$AC279,  $AB279),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",17]
["L3401","L3401","N-L3401","2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","For 1-for-1 replacement of T12 or standard T8 fluorescent fixtures","Must be DLC TRT V5.0 or higher listed in the \"Troffer\" general application.","New fixture must consume ≤ 85W.","2G11 base lamps replaced must have a nominal lamp wattage between 40-55 watts.","Other LED configurations may qualify for a custom incentive.",{"$nulls":5},"Provide clear photo(s) of: fixture layout and (if possible) fixture packaging label.","Verify fixture size by comparing to grid ceiling as reference.",{"$nulls":4},{"v":30,"d":"$30.00"},"Fixture",{"v":30,"d":"$30.00"},"Fixture",{"v":20,"d":"$20.00"},"Fixture","N/A",3401,3401,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR280=\"Agribusiness\", $AR280=\"Ag\",$AR280=\"Propane\", $AR280=\"Ag Propane\", $AR280=\"Ag-Propane\"),$AC280,  $AB280),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR280=\"Agribusiness\", $AR280=\"Ag\",$AR280=\"Propane\", $AR280=\"Ag Propane\", $AR280=\"Ag-Propane\"),$AC280,  $AB280),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",17]
["L10028","L10028","N-L10028","LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture",{"$f":"IF(ISBLANK(A281),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C281,IF(FOEIncentCodeType=IncentCodeTypeAg,B281,A281))&\": \") &D281","v":"L10028: LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture"},"Fixture must be listed on ENERGY STAR as a “Downlight Recessed,” “Downlight Solid State Retrofit,” “Downlight Surface Mount,” \"Ceiling Mount\" or \"LED Surface Mount Ceiling Retrofit\" fixture type and be intended for commercial use. ","For replacement of incandescent, CFL or HID fixtures in interior applications.","Low voltage or decorative LED fixtures that do not meet the criteria below may be eligible for custom incentives",{"$nulls":13},{"v":13,"d":"$13.00"},"Fixture",{"v":13,"d":"$13.00"},"Fixture",{"v":7,"d":"$7.00"},{"$f":"Y281","v":"Fixture"},"N/A",10028,10028,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A281),\"\",IF(A281<>\"Not Eligible\",A281,IF(B281<>\"Not Eligible\",B281,C281))&\": \") &D281","v":"L10028: LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture"},"No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR281=\"Agribusiness\", $AR281=\"Ag\",$AR281=\"Propane\", $AR281=\"Ag Propane\", $AR281=\"Ag-Propane\"),$AC281,  $AB281),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR281=\"Agribusiness\", $AR281=\"Ag\",$AR281=\"Propane\", $AR281=\"Ag Propane\", $AR281=\"Ag-Propane\"),$AC281,  $AB281),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",17]
["L10029","L10029","N-L10029","LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior",{"$f":"IF(ISBLANK(A282),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C282,IF(FOEIncentCodeType=IncentCodeTypeAg,B282,A282))&\": \") &D282","v":"L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"},"Fixture must be listed on Energy Star as a Downlight Recessed, Downlight Solid State Retrofit or Downlight Surface Mount fixture type and be intended for commercial use.","For replacement of incandescent, CFL or HID fixtures in exterior applications.",{"$nulls":14},{"v":20,"d":"$20"},"Fixture",{"v":20,"d":"$20.00"},"Fixture",{"v":10,"d":"$10.00"},{"$f":"Y282","v":"Fixture"},"N/A",10029,10029,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A282),\"\",IF(A282<>\"Not Eligible\",A282,IF(B282<>\"Not Eligible\",B282,C282))&\": \") &D282","v":"L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"},"No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR282=\"Agribusiness\", $AR282=\"Ag\",$AR282=\"Propane\", $AR282=\"Ag Propane\", $AR282=\"Ag-Propane\"),$AC282,  $AB282),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR282=\"Agribusiness\", $AR282=\"Ag\",$AR282=\"Propane\", $AR282=\"Ag Propane\", $AR282=\"Ag-Propane\"),$AC282,  $AB282),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",17]
["L10281","L10281","N-L10281","1’ to 3’ LED Linear Ambient Fixture, Interior",{"$f":"IF(ISBLANK(A283),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C283,IF(FOEIncentCodeType=IncentCodeTypeAg,B283,A283))&\": \") &D283","v":"L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"},"Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":6,"d":"$6.00"},"Fixture",{"v":6,"d":"$6.00"},"Fixture",{"v":4,"d":"$4.00"},{"$f":"Y283","v":"Fixture"},"N/A",10281,10281,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A283),\"\",IF(A283<>\"Not Eligible\",A283,IF(B283<>\"Not Eligible\",B283,C283))&\": \") &D283","v":"L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"},"No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR283=\"Agribusiness\", $AR283=\"Ag\",$AR283=\"Propane\", $AR283=\"Ag Propane\", $AR283=\"Ag-Propane\"),$AC283,  $AB283),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR283=\"Agribusiness\", $AR283=\"Ag\",$AR283=\"Propane\", $AR283=\"Ag Propane\", $AR283=\"Ag-Propane\"),$AC283,  $AB283),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["L10282","L10282","N-L10282","4' LED Linear Ambient Fixture, Interior","L10282: 4' LED Linear Ambient Fixture, Interior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":12,"d":"$12.00"},"Fixture",{"v":12,"d":"$12.00"},"Fixture",{"v":8,"d":"$8.00"},"Fixture","N/A",10282,10282,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10282: 4' LED Linear Ambient Fixture, Interior","No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR284=\"Agribusiness\", $AR284=\"Ag\",$AR284=\"Propane\", $AR284=\"Ag Propane\", $AR284=\"Ag-Propane\"),$AC284,  $AB284),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR284=\"Agribusiness\", $AR284=\"Ag\",$AR284=\"Propane\", $AR284=\"Ag Propane\", $AR284=\"Ag-Propane\"),$AC284,  $AB284),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["L10283","L10283","N-L10283","8' LED Linear Ambient Fixture, Interior","L10283: 8' LED Linear Ambient Fixture, Interior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":24,"d":"$24.00"},"Fixture",{"v":24,"d":"$24.00"},"Fixture",{"v":16,"d":"$16.00"},"Fixture","N/A",10283,10283,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10283: 8' LED Linear Ambient Fixture, Interior","No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR285=\"Agribusiness\", $AR285=\"Ag\",$AR285=\"Propane\", $AR285=\"Ag Propane\", $AR285=\"Ag-Propane\"),$AC285,  $AB285),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR285=\"Agribusiness\", $AR285=\"Ag\",$AR285=\"Propane\", $AR285=\"Ag Propane\", $AR285=\"Ag-Propane\"),$AC285,  $AB285),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["L10284","L10284","N-L10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":6,"d":"$6.00"},"Fixture",{"v":6,"d":"$6.00"},"Fixture",{"v":4,"d":"$4.00"},"Fixture","N/A",10284,10284,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior","No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR286=\"Agribusiness\", $AR286=\"Ag\",$AR286=\"Propane\", $AR286=\"Ag Propane\", $AR286=\"Ag-Propane\"),$AC286,  $AB286),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR286=\"Agribusiness\", $AR286=\"Ag\",$AR286=\"Propane\", $AR286=\"Ag Propane\", $AR286=\"Ag-Propane\"),$AC286,  $AB286),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["L10285","L10285","N-L10285","4' LED Linear Ambient Fixture, Exterior","L10285: 4' LED Linear Ambient Fixture, Exterior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":12,"d":"$12.00"},"Fixture",{"v":12,"d":"$12.00"},"Fixture",{"v":8,"d":"$8.00"},"Fixture","N/A",10285,10285,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10285: 4' LED Linear Ambient Fixture, Exterior","No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR287=\"Agribusiness\", $AR287=\"Ag\",$AR287=\"Propane\", $AR287=\"Ag Propane\", $AR287=\"Ag-Propane\"),$AC287,  $AB287),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR287=\"Agribusiness\", $AR287=\"Ag\",$AR287=\"Propane\", $AR287=\"Ag Propane\", $AR287=\"Ag-Propane\"),$AC287,  $AB287),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["L10286","L10286","N-L10286","8' LED Linear Ambient Fixture, Exterior","L10286: 8' LED Linear Ambient Fixture, Exterior","Must be DLC SSL QPL listed (TRT V5.0 or higher) in the \"Linear Ambient\" general application.","Fixtures that are DLC SSL QPL listed (TRT V5.0 or higher listed) in the Low-Bay General Application or the “Stairwell & Passageway Luminaires” primary use category are also eligible, if they have a linear profile.","Stairwell & Passageway Luminaires may also apply for bi-level occupancy controls.","Unique length fixtures not offered, such as 6', may combine or mix'n'match multiple Linear Ambient measures to equal total length.",{"$nulls":6},"Provide clear photo(s) of: fixture and/or example linear run, fixture packaging label (if possible) .","Verify fixture size by comparing to grid ceiling/ under cabinet/ structure as reference.",{"$nulls":4},{"v":24,"d":"$24.00"},"Fixture",{"v":24,"d":"$24.00"},"Fixture",{"v":16,"d":"$16.00"},"Fixture","N/A",10286,10286,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10286: 8' LED Linear Ambient Fixture, Exterior","No","No","Fixture",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR288=\"Agribusiness\", $AR288=\"Ag\",$AR288=\"Propane\", $AR288=\"Ag Propane\", $AR288=\"Ag-Propane\"),$AC288,  $AB288),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR288=\"Agribusiness\", $AR288=\"Ag\",$AR288=\"Propane\", $AR288=\"Ag Propane\", $AR288=\"Ag-Propane\"),$AC288,  $AB288),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["Not Eligible","AG4695","N-AG4695","LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture","AG4695: LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture","LED fixtures must be ≤155W and replace a 250W HID light","Retrofit products must be DLC SSL QPL listed (TRT V5.0 or higher) under the High-Bay or Low-Bay General Application category and be permanently wired or applicable cord and plug.","New fixtures must be DLC SSL QPL (TRT V5.0 or higher) listed under High-Bay or Low-Bay General Application category.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) under the \"Linear Ambient\" General Application category, \"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" Primary Use Designation, if they provide sufficient lighting levels and meet the wattage limitations in the table below.","Must be 1-for-1 replacement. Incentive is per fixture replaced","Integral ballast screw-based lamp retrofit products are not eligible for this incentive. Refer to page 16 for High/Low-Bay Mogul Screw-base (E39) LED lamps","Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","LEDs replacing existing HID fixtures less than 250W may qualify for a custom incentive",{"$nulls":8},"N/A","N/A",{"v":80,"d":"$80.00"},"Fixture",{"v":80,"d":"$80.00"},"Fixture","N/A",4695,4695,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4695: LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR289=\"Agribusiness\", $AR289=\"Ag\",$AR289=\"Propane\", $AR289=\"Ag Propane\", $AR289=\"Ag-Propane\"),$AC289,  $AB289),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR289=\"Agribusiness\", $AR289=\"Ag\",$AR289=\"Propane\", $AR289=\"Ag Propane\", $AR289=\"Ag-Propane\"),$AC289,  $AB289),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["Not Eligible","AG4696","N-AG4696","LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture","AG4696: LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture","LED fixtures must be ≤250W and replace a 320-399W HID light","Retrofit products must be DLC SSL QPL listed (TRT V5.0 or higher) under the High-Bay or Low-Bay General Application category and be permanently wired or applicable cord and plug.","New fixtures must be DLC SSL QPL (TRT V5.0 or higher) listed under High-Bay or Low-Bay General Application category.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) under the \"Linear Ambient\" General Application category, \"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" Primary Use Designation, if they provide sufficient lighting levels and meet the wattage limitations in the table below.","Must be 1-for-1 replacement. Incentive is per fixture replaced","Integral ballast screw-based lamp retrofit products are not eligible for this incentive. Refer to page 16 for High/Low-Bay Mogul Screw-base (E39) LED lamps","Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","LEDs replacing existing HID fixtures less than 250W may qualify for a custom incentive",{"$nulls":8},"N/A","N/A",{"v":80,"d":"$80.00"},"Fixture",{"v":80,"d":"$80.00"},"Fixture","N/A",4696,4696,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4696: LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR290=\"Agribusiness\", $AR290=\"Ag\",$AR290=\"Propane\", $AR290=\"Ag Propane\", $AR290=\"Ag-Propane\"),$AC290,  $AB290),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR290=\"Agribusiness\", $AR290=\"Ag\",$AR290=\"Propane\", $AR290=\"Ag Propane\", $AR290=\"Ag-Propane\"),$AC290,  $AB290),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["Not Eligible","AG4697","Not Eligible","LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture","AG4697: LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture","LED fixtures must be ≤250W and replace a 400W HID light","Retrofit products must be DLC SSL QPL listed (TRT V5.0 or higher) under the High-Bay or Low-Bay General Application category and be permanently wired or applicable cord and plug.","New fixtures must be DLC SSL QPL (TRT V5.0 or higher) listed under High-Bay or Low-Bay General Application category.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) under the \"Linear Ambient\" General Application category, \"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" Primary Use Designation, if they provide sufficient lighting levels and meet the wattage limitations in the table below.","Must be 1-for-1 replacement. Incentive is per fixture replaced","Integral ballast screw-based lamp retrofit products are not eligible for this incentive. Refer to page 16 for High/Low-Bay Mogul Screw-base (E39) LED lamps","Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","LEDs replacing existing HID fixtures less than 250W may qualify for a custom incentive",{"$nulls":8},"N/A","N/A",{"v":120,"d":"$120.00"},"Fixture","N/A","Fixture","N/A",4697,"N/A","N/A","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4697: LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR291=\"Agribusiness\", $AR291=\"Ag\",$AR291=\"Propane\", $AR291=\"Ag Propane\", $AR291=\"Ag-Propane\"),$AC291,  $AB291),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR291=\"Agribusiness\", $AR291=\"Ag\",$AR291=\"Propane\", $AR291=\"Ag Propane\", $AR291=\"Ag-Propane\"),$AC291,  $AB291),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["Not Eligible","AG4698","Not Eligible","LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture","AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture","LED fixtures must be ≤365W and replace a 400W HID light","Retrofit products must be DLC SSL QPL listed (TRT V5.0 or higher) under the High-Bay or Low-Bay General Application category and be permanently wired or applicable cord and plug.","New fixtures must be DLC SSL QPL (TRT V5.0 or higher) listed under High-Bay or Low-Bay General Application category.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) under the \"Linear Ambient\" General Application category, \"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" Primary Use Designation, if they provide sufficient lighting levels and meet the wattage limitations in the table below.","Must be 1-for-1 replacement. Incentive is per fixture replaced","Integral ballast screw-based lamp retrofit products are not eligible for this incentive. Refer to page 16 for High/Low-Bay Mogul Screw-base (E39) LED lamps","Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","LEDs replacing existing HID fixtures less than 250W may qualify for a custom incentive",{"$nulls":8},"N/A","N/A",{"v":80,"d":"$80.00"},"Fixture","N/A","Fixture","N/A",4698,"N/A","N/A","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A292),\"\",IF(A292<>\"Not Eligible\",A292,IF(B292<>\"Not Eligible\",B292,C292))&\": \") &D292","v":"AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture"},"No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR292=\"Agribusiness\", $AR292=\"Ag\",$AR292=\"Propane\", $AR292=\"Ag Propane\", $AR292=\"Ag-Propane\"),$AC292,  $AB292),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR292=\"Agribusiness\", $AR292=\"Ag\",$AR292=\"Propane\", $AR292=\"Ag Propane\", $AR292=\"Ag-Propane\"),$AC292,  $AB292),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["Not Eligible","AG4701","N-AG4701","LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture","AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture","LED fixtures must be ≤180W and replace a 6L T8 or 4L T5HO","Retrofit products must be DLC SSL QPL listed (TRT V5.0 or higher) under the High-Bay or Low-Bay General Application category and be permanently wired or applicable cord and plug.","New fixtures must be DLC SSL QPL (TRT V5.0 or higher) listed under High-Bay or Low-Bay General Application category.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) under the \"Linear Ambient\" General Application category, \"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" Primary Use Designation, if they provide sufficient lighting levels and meet the wattage limitations in the table below.","Must be 1-for-1 replacement. Incentive is per fixture replaced","Integral ballast screw-based lamp retrofit products are not eligible for this incentive. Refer to page 16 for High/Low-Bay Mogul Screw-base (E39) LED lamps","Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","LEDs replacing existing HID fixtures less than 250W may qualify for a custom incentive",{"$nulls":8},"N/A","N/A",{"v":70,"d":"$70.00"},"Fixture",{"v":70,"d":"$70.00"},"Fixture","N/A",4701,4701,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR293=\"Agribusiness\", $AR293=\"Ag\",$AR293=\"Propane\", $AR293=\"Ag Propane\", $AR293=\"Ag-Propane\"),$AC293,  $AB293),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR293=\"Agribusiness\", $AR293=\"Ag\",$AR293=\"Propane\", $AR293=\"Ag Propane\", $AR293=\"Ag-Propane\"),$AC293,  $AB293),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["Not Eligible","AG4702","N-AG4702","LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture","AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture","LED fixtures must be ≤250W and replace a 8LT8 or 6LT5HO","Retrofit products must be DLC SSL QPL listed (TRT V5.0 or higher) under the High-Bay or Low-Bay General Application category and be permanently wired or applicable cord and plug.","New fixtures must be DLC SSL QPL (TRT V5.0 or higher) listed under High-Bay or Low-Bay General Application category.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) under the \"Linear Ambient\" General Application category, \"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" Primary Use Designation, if they provide sufficient lighting levels and meet the wattage limitations in the table below.","Must be 1-for-1 replacement. Incentive is per fixture replaced","Integral ballast screw-based lamp retrofit products are not eligible for this incentive. Refer to page 16 for High/Low-Bay Mogul Screw-base (E39) LED lamps","Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","LEDs replacing existing HID fixtures less than 250W may qualify for a custom incentive",{"$nulls":8},"N/A","N/A",{"v":80,"d":"$80.00"},"Fixture",{"v":80,"d":"$80.00"},"Fixture","N/A",4702,"N/A","N/A","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR294=\"Agribusiness\", $AR294=\"Ag\",$AR294=\"Propane\", $AR294=\"Ag Propane\", $AR294=\"Ag-Propane\"),$AC294,  $AB294),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR294=\"Agribusiness\", $AR294=\"Ag\",$AR294=\"Propane\", $AR294=\"Ag Propane\", $AR294=\"Ag-Propane\"),$AC294,  $AB294),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["Not Eligible","AG4699","Not Eligible","LED Fixture, ≤500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture",{"$f":"IF(ISBLANK(A295),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C295,IF(FOEIncentCodeType=IncentCodeTypeAg,B295,A295))&\": \") &D295","v":"AG4699: LED Fixture, ≤500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture"},"LED fixtures must be ≤500W and replace a 1000W HID light","Retrofit products must be DLC SSL QPL listed (TRT V5.0 or higher) under the High-Bay or Low-Bay General Application category and be permanently wired or applicable cord and plug.","New fixtures must be DLC SSL QPL (TRT V5.0 or higher) listed under High-Bay or Low-Bay General Application category.","Fixtures for low-bay applications may use products that are DLC SSL QPL listed (TRT V5.0 or higher) under the \"Linear Ambient\" General Application category, \"Fuel Pump Canopy Luminaires\", or \"Parking Garage Luminaires\" Primary Use Designation, if they provide sufficient lighting levels and meet the wattage limitations in the table below.","Must be 1-for-1 replacement. Incentive is per fixture replaced","Integral ballast screw-based lamp retrofit products are not eligible for this incentive. Refer to page 16 for High/Low-Bay Mogul Screw-base (E39) LED lamps","Long-Day Lighting fixtures for dairy applications are eligible for this incentive.","LEDs replacing existing HID fixtures less than 250W may qualify for a custom incentive",{"$nulls":8},"N/A","N/A",{"v":200,"d":"$200.00"},"Fixture","N/A","Fixture","N/A",4699,"N/A","N/A","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4699: LED Fixture, ≤500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR295=\"Agribusiness\", $AR295=\"Ag\",$AR295=\"Propane\", $AR295=\"Ag Propane\", $AR295=\"Ag-Propane\"),$AC295,  $AB295),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR295=\"Agribusiness\", $AR295=\"Ag\",$AR295=\"Propane\", $AR295=\"Ag Propane\", $AR295=\"Ag-Propane\"),$AC295,  $AB295),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",18]
["L4280","L4280","Not Eligible","Outdoor LED Fixture or Retrofit Kit – Low Output",{"$f":"IF(ISBLANK(A296),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C296,IF(FOEIncentCodeType=IncentCodeTypeAg,B296,A296))&\": \") &D296","v":"L4280: Outdoor LED Fixture or Retrofit Kit – Low Output"},"Must be on DLC SSL QPL (TRT V5.0 or higher) listed in the \"Outdoor\" category ","For stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","Must be permanently wired","For fixtures with field adjustable lighting output, refer to Field Adjustable Lighting Output Guidance on page 7 for additional requirements.","Fixtures equipped with light shields to prevent light from leaving the property can be considered eligible, even if not DLC listed, if the equivalent fixture without the shield is DLC listed.",{"$nulls":11},{"v":30,"d":"$30"},"Fixture",{"v":30,"d":"$30"},"Fixture",{"v":20,"d":"$20.00"},"Fixture",4280,4280,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR296=\"Agribusiness\", $AR296=\"Ag\",$AR296=\"Propane\", $AR296=\"Ag Propane\", $AR296=\"Ag-Propane\"),$AC296,  $AB296),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR296=\"Agribusiness\", $AR296=\"Ag\",$AR296=\"Propane\", $AR296=\"Ag Propane\", $AR296=\"Ag-Propane\"),$AC296,  $AB296),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",19]
["L4281","L4281","Not Eligible","Outdoor LED Fixture or Retrofit Kit – Mid Output","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output","Must be on DLC SSL QPL (TRT V5.0 or higher) listed in the \"Outdoor\" category ","For stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","Must be permanently wired","For fixtures with field adjustable lighting output, refer to Field Adjustable Lighting Output Guidance on page 7 for additional requirements.","Fixtures equipped with light shields to prevent light from leaving the property can be considered eligible, even if not DLC listed, if the equivalent fixture without the shield is DLC listed.",{"$nulls":11},{"v":55,"d":"$55"},"Fixture",{"v":55,"d":"$55"},"Fixture",{"v":35,"d":"$35.00"},"Fixture",4281,4281,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR297=\"Agribusiness\", $AR297=\"Ag\",$AR297=\"Propane\", $AR297=\"Ag Propane\", $AR297=\"Ag-Propane\"),$AC297,  $AB297),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR297=\"Agribusiness\", $AR297=\"Ag\",$AR297=\"Propane\", $AR297=\"Ag Propane\", $AR297=\"Ag-Propane\"),$AC297,  $AB297),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",19]
["L4282","L4282","Not Eligible","Outdoor LED Fixture or Retrofit Kit – High Output ","L4282: Outdoor LED Fixture or Retrofit Kit – High Output ","Must be on DLC SSL QPL (TRT V5.0 or higher) listed in the \"Outdoor\" category ","For stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","Must be permanently wired","For fixtures with field adjustable lighting output, refer to Field Adjustable Lighting Output Guidance on page 7 for additional requirements.","Fixtures equipped with light shields to prevent light from leaving the property can be considered eligible, even if not DLC listed, if the equivalent fixture without the shield is DLC listed.",{"$nulls":11},{"v":100,"d":"$100"},"Fixture",{"v":100,"d":"$100"},"Fixture",{"v":90,"d":"$90.00"},"Fixture",4282,4282,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L4282: Outdoor LED Fixture or Retrofit Kit – High Output ","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR298=\"Agribusiness\", $AR298=\"Ag\",$AR298=\"Propane\", $AR298=\"Ag Propane\", $AR298=\"Ag-Propane\"),$AC298,  $AB298),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR298=\"Agribusiness\", $AR298=\"Ag\",$AR298=\"Propane\", $AR298=\"Ag Propane\", $AR298=\"Ag-Propane\"),$AC298,  $AB298),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",19]
["L4283","L4283","Not Eligible","Outdoor LED Fixture or Retrofit Kit – Very High Output","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output","Must be on DLC SSL QPL (TRT V5.0 or higher) listed in the \"Outdoor\" category ","For stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","Must be permanently wired","For fixtures with field adjustable lighting output, refer to Field Adjustable Lighting Output Guidance on page 7 for additional requirements.","Fixtures equipped with light shields to prevent light from leaving the property can be considered eligible, even if not DLC listed, if the equivalent fixture without the shield is DLC listed.",{"$nulls":11},{"v":250,"d":"$250"},"Fixture",{"v":250,"d":"$250"},"Fixture",{"v":200,"d":"$200.00"},"Fixture",4283,4283,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR299=\"Agribusiness\", $AR299=\"Ag\",$AR299=\"Propane\", $AR299=\"Ag Propane\", $AR299=\"Ag-Propane\"),$AC299,  $AB299),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR299=\"Agribusiness\", $AR299=\"Ag\",$AR299=\"Propane\", $AR299=\"Ag Propane\", $AR299=\"Ag-Propane\"),$AC299,  $AB299),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",19]
["N-L4280","N-L4280","N-L4280","Outdoor LED Fixture or Retrofit Kit – Low Output","N-L4280: Outdoor LED Fixture or Retrofit Kit – Low Output","Must be DLC SSL QPL listed (TRT V5.0 or higher) in an “Outdoor” General Application Category.","Must be permanently wired. Integral ballast screw-based lamp retrofit products of any technology are not eligible. Refer to page 25 for Exterior Mogul Screw-base (E39) LED lamps.","Stadium lighting is not eligible for prescriptive incentives.  Contact your Energy Advisor to determine eligibility for a custom incentive.","Area Fixtures & Retrofit Kits can be any of the following: Exterior Outdoor Pole-Mounted, Outdoor Decorative Area & Post-Top,…","...Parking Garage & Canopy/Soffit, Outdoor Wall-Mounted, Outdoor Flood & Spot, and Bollards.","Customers applying for municipal roadway lighting MUST submit a copy of utililty bill verifying customer is on a utility rate for customer owned street lights. Utility owned street lights are not eligible for incentives.","For stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","**Ignore lumen levels in measure name.  Use DLC category to qualify equipment**","Fixtures equipped with light shields are eligible if the equivalent shieldless fixture is DLC listed.",{"$nulls":7},{"v":20,"d":"$20.00"},"Fixture",{"v":20,"d":"$20.00"},"Fixture",{"v":20,"d":"$20.00"},{"$f":"W300","v":"Fixture"},4280,{"$f":"AB300","v":4280},4280,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-L4280: Outdoor LED Fixture or Retrofit Kit – Low Output","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR300=\"Agribusiness\", $AR300=\"Ag\",$AR300=\"Propane\", $AR300=\"Ag Propane\", $AR300=\"Ag-Propane\"),$AC300,  $AB300),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR300=\"Agribusiness\", $AR300=\"Ag\",$AR300=\"Propane\", $AR300=\"Ag Propane\", $AR300=\"Ag-Propane\"),$AC300,  $AB300),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",19]
["N-L4281","N-L4281","N-L4281","Outdoor LED Fixture or Retrofit Kit – Mid Output","N-L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output","Must be DLC SSL QPL listed (TRT V5.0 or higher) in an “Outdoor” General Application Category.","Must be permanently wired. Integral ballast screw-based lamp retrofit products of any technology are not eligible. Refer to page 25 for Exterior Mogul Screw-base (E39) LED lamps.","Stadium lighting is not eligible for prescriptive incentives.  Contact your Energy Advisor to determine eligibility for a custom incentive.","Area Fixtures & Retrofit Kits can be any of the following: Exterior Outdoor Pole-Mounted, Outdoor Decorative Area & Post-Top,…","...Parking Garage & Canopy/Soffit, Outdoor Wall-Mounted, Outdoor Flood & Spot, and Bollards.","Customers applying for municipal roadway lighting MUST submit a copy of utililty bill verifying customer is on a utility rate for customer owned street lights. Utility owned street lights are not eligible for incentives.","For stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","**Ignore lumen levels in measure name.  Use DLC category to qualify equipment**","Fixtures equipped with light shields are eligible if the equivalent shieldless fixture is DLC listed.",{"$nulls":7},{"v":35,"d":"$35.00"},"Fixture",{"v":35,"d":"$35.00"},"Fixture",{"v":35,"d":"$35.00"},{"$f":"W301","v":"Fixture"},4281,4281,4281,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR301=\"Agribusiness\", $AR301=\"Ag\",$AR301=\"Propane\", $AR301=\"Ag Propane\", $AR301=\"Ag-Propane\"),$AC301,  $AB301),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR301=\"Agribusiness\", $AR301=\"Ag\",$AR301=\"Propane\", $AR301=\"Ag Propane\", $AR301=\"Ag-Propane\"),$AC301,  $AB301),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",19]
["N-L4282","N-L4282","N-L4282","Outdoor LED Fixture or Retrofit Kit – High Output ","N-L4282: Outdoor LED Fixture or Retrofit Kit – High Output ","Must be DLC SSL QPL listed (TRT V5.0 or higher) in an “Outdoor” General Application Category.","Must be permanently wired. Integral ballast screw-based lamp retrofit products of any technology are not eligible. Refer to page 25 for Exterior Mogul Screw-base (E39) LED lamps.","Stadium lighting is not eligible for prescriptive incentives.  Contact your Energy Advisor to determine eligibility for a custom incentive.","Area Fixtures & Retrofit Kits can be any of the following: Exterior Outdoor Pole-Mounted, Outdoor Decorative Area & Post-Top,…","...Parking Garage & Canopy/Soffit, Outdoor Wall-Mounted, Outdoor Flood & Spot, and Bollards.","Customers applying for municipal roadway lighting MUST submit a copy of utililty bill verifying customer is on a utility rate for customer owned street lights. Utility owned street lights are not eligible for incentives.","For stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","**Ignore lumen levels in measure name.  Use DLC category to qualify equipment**","Fixtures equipped with light shields are eligible if the equivalent shieldless fixture is DLC listed.",{"$nulls":7},{"v":90,"d":"$90.00"},"Fixture",{"v":90,"d":"$90.00"},"Fixture",{"v":90,"d":"$90.00"},"Fixture",4282,4282,4282,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-L4282: Outdoor LED Fixture or Retrofit Kit – High Output ","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR302=\"Agribusiness\", $AR302=\"Ag\",$AR302=\"Propane\", $AR302=\"Ag Propane\", $AR302=\"Ag-Propane\"),$AC302,  $AB302),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR302=\"Agribusiness\", $AR302=\"Ag\",$AR302=\"Propane\", $AR302=\"Ag Propane\", $AR302=\"Ag-Propane\"),$AC302,  $AB302),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",19]
["N-L4283","N-L4283","N-L4283","Outdoor LED Fixture or Retrofit Kit – Very High Output","N-L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output","Must be DLC SSL QPL listed (TRT V5.0 or higher) in an “Outdoor” General Application Category.","Must be permanently wired. Integral ballast screw-based lamp retrofit products of any technology are not eligible. Refer to page 25 for Exterior Mogul Screw-base (E39) LED lamps.","Stadium lighting is not eligible for prescriptive incentives.  Contact your Energy Advisor to determine eligibility for a custom incentive.","Area Fixtures & Retrofit Kits can be any of the following: Exterior Outdoor Pole-Mounted, Outdoor Decorative Area & Post-Top,…","...Parking Garage & Canopy/Soffit, Outdoor Wall-Mounted, Outdoor Flood & Spot, and Bollards.","Customers applying for municipal roadway lighting MUST submit a copy of utililty bill verifying customer is on a utility rate for customer owned street lights. Utility owned street lights are not eligible for incentives.","For stairwell/passageway fixtures, see Linear Ambient fixtures and combine with Bi-Level Controls.","**Ignore lumen levels in measure name.  Use DLC category to qualify equipment**","Fixtures equipped with light shields are eligible if the equivalent shieldless fixture is DLC listed.",{"$nulls":7},{"v":200,"d":"$200.00"},"Fixture",{"v":200,"d":"$200.00"},"Fixture",{"v":200,"d":"$200.00"},"Fixture",4283,4283,4283,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR303=\"Agribusiness\", $AR303=\"Ag\",$AR303=\"Propane\", $AR303=\"Ag Propane\", $AR303=\"Ag-Propane\"),$AC303,  $AB303),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR303=\"Agribusiness\", $AR303=\"Ag\",$AR303=\"Propane\", $AR303=\"Ag Propane\", $AR303=\"Ag-Propane\"),$AC303,  $AB303),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",19]
["L10042","L10042","Not Eligible","DLC listed, Mogul Screw-Base (E39) LED lamp replacing existing E39 base lamp","L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing existing E39 base lamp","Must be DLC TRT V5.0 or higher in the \"Mogul (E39) Screw-Base Reaplcements for HID Lamps\" category.","Interior medium screw-base (E26) lamps may be eligible if E39 option is DLC listed. Contact Focus on Energy for assistance.","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":7},"lighting layout, close-up of lamp, lamp model number (if available)","Provide clear photo(s) of: lamp(s) and lamp packaging label (if possible).","Verify lamp is installed in high/low-bay fixture.",{"$nulls":3},{"v":30,"d":"$30.00"},"Lamp",{"$f":"V304","v":{"v":30,"d":"$30.00"}},{"$f":"W304","v":"Lamp"},"N/A",{"$f":"W304","v":"Lamp"},"N/A",10042,"N/A","N/A","No","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No",{"$f":"IF(ISBLANK(A304),\"\",IF(A304<>\"Not Eligible\",A304,IF(B304<>\"Not Eligible\",B304,C304))&\": \") &D304","v":"L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing existing E39 base lamp"},"No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR304=\"Agribusiness\", $AR304=\"Ag\",$AR304=\"Propane\", $AR304=\"Ag Propane\", $AR304=\"Ag-Propane\"),$AC304,  $AB304),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR304=\"Agribusiness\", $AR304=\"Ag\",$AR304=\"Propane\", $AR304=\"Ag Propane\", $AR304=\"Ag-Propane\"),$AC304,  $AB304),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",20]
["L10043","L10043","Not Eligible","Mogul Screw-in Base (E39) replacing existing E39 base lamp, Exterior",{"$f":"IF(ISBLANK(A305),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C305,IF(FOEIncentCodeType=IncentCodeTypeAg,B305,A305))&\": \") &D305","v":"L10043: Mogul Screw-in Base (E39) replacing existing E39 base lamp, Exterior"},"Must be DLC TRT V5.0 or higher in the \"Mogul (E39) Screw-Base Reaplcements for HID Lamps\" category.","Interior medium screw-base (E26) lamps may be eligible if E39 option is DLC listed. Contact Focus on Energy for assistance.","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":7},"Provide photo(s) of: lamp, lamp packaging label (if possible).","Verify lamp is installed in DLC-listed application.",{"$nulls":4},{"v":30,"d":"$30"},"N/A",{"v":30,"d":"$30.00"},"Lamp","N/A",{"$f":"Y305","v":"Lamp"},"N/A",10043,"N/A","N/A",{"$f":"IFERROR(IF(SEARCH(\"N-\",B305),\"Yes\",\"No\"),\"No\")","v":"No"},"N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No",{"$f":"IF(ISBLANK(A305),\"\",IF(A305<>\"Not Eligible\",A305,IF(B305<>\"Not Eligible\",B305,C305))&\": \") &D305","v":"L10043: Mogul Screw-in Base (E39) replacing existing E39 base lamp, Exterior"},"No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR305=\"Agribusiness\", $AR305=\"Ag\",$AR305=\"Propane\", $AR305=\"Ag Propane\", $AR305=\"Ag-Propane\"),$AC305,  $AB305),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR305=\"Agribusiness\", $AR305=\"Ag\",$AR305=\"Propane\", $AR305=\"Ag Propane\", $AR305=\"Ag-Propane\"),$AC305,  $AB305),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",20]
["L5451","L5451","Not Eligible","4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp","L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)","Measures can be used for 8' retrofit products.  Apply for the corresponding quantity installed.",{"$nulls":5},"Provide clear photo(s): of lamp, lamp packaging label (if possible).","Verify lamp is 4ft in length or is a U-Bend",null,"Verify lamp installed matches spec sheets, invoicing, and QPL provided.",null,null,{"v":3.25,"d":"$3.25"},"Lamp",{"v":3.25,"d":"$3.25"},{"$f":"W306","v":"Lamp"},"N/A",{"$f":"W306","v":"Lamp"},5451,{"$f":"AB306","v":5451},5451,"No",{"$f":"AE306","v":"No"},"No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No",{"$f":"IF(ISBLANK(A306),\"\",IF(A306<>\"Not Eligible\",A306,IF(B306<>\"Not Eligible\",B306,C306))&\": \") &D306","v":"L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR306=\"Agribusiness\", $AR306=\"Ag\",$AR306=\"Propane\", $AR306=\"Ag Propane\", $AR306=\"Ag-Propane\"),$AC306,  $AB306),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR306=\"Agribusiness\", $AR306=\"Ag\",$AR306=\"Propane\", $AR306=\"Ag Propane\", $AR306=\"Ag-Propane\"),$AC306,  $AB306),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",20]
["L5452","L5452","Not Eligible","4' TLED, replacing 4' T5HO Lamp","L5452: 4' TLED, replacing 4' T5HO Lamp","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)","Measures can be used for 8' retrofit products.  Apply for the corresponding quantity installed.",{"$nulls":5},"Provide clear photo(s): of lamp, lamp packaging label (if possible).",{"$nulls":5},{"v":7,"d":"$7.00"},"Lamp",{"v":7,"d":"$7.00"},"Lamp","N/A","Lamp",5452,5452,5452,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5452: 4' TLED, replacing 4' T5HO Lamp","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR307=\"Agribusiness\", $AR307=\"Ag\",$AR307=\"Propane\", $AR307=\"Ag Propane\", $AR307=\"Ag-Propane\"),$AC307,  $AB307),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR307=\"Agribusiness\", $AR307=\"Ag\",$AR307=\"Propane\", $AR307=\"Ag Propane\", $AR307=\"Ag-Propane\"),$AC307,  $AB307),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",20]
["L5453","L5453","Not Eligible","2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp","L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":6},"Provide clear photo(s): of lamp, lamp packaging label (if possible).","Verify lamp is 2ft in length.",{"$nulls":4},{"v":2.75,"d":"$2.75"},"Lamp",{"v":2.75,"d":"$2.75"},"Lamp","N/A","Lamp",5453,5453,5453,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR308=\"Agribusiness\", $AR308=\"Ag\",$AR308=\"Propane\", $AR308=\"Ag Propane\", $AR308=\"Ag-Propane\"),$AC308,  $AB308),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR308=\"Agribusiness\", $AR308=\"Ag\",$AR308=\"Propane\", $AR308=\"Ag Propane\", $AR308=\"Ag-Propane\"),$AC308,  $AB308),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",20]
["L5454","L5454","Not Eligible","8' TLED, replacing 8' T8 or T12 Lamp","L5454: 8' TLED, replacing 8' T8 or T12 Lamp","Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":6},"Provide clear photo(s): of lamp, lamp packaging label (if possible).","Verify lamp is 8ft in length.",{"$nulls":4},{"v":7,"d":"$7.00"},"Lamp",{"v":7,"d":"$7.00"},"Lamp","N/A","Lamp",5454,5454,5454,"No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","L5454: 8' TLED, replacing 8' T8 or T12 Lamp","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR309=\"Agribusiness\", $AR309=\"Ag\",$AR309=\"Propane\", $AR309=\"Ag Propane\", $AR309=\"Ag-Propane\"),$AC309,  $AB309),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR309=\"Agribusiness\", $AR309=\"Ag\",$AR309=\"Propane\", $AR309=\"Ag Propane\", $AR309=\"Ag-Propane\"),$AC309,  $AB309),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",20]
["L5456","L5456","Not Eligible","4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior",{"$f":"IF(ISBLANK(A310),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C310,IF(FOEIncentCodeType=IncentCodeTypeAg,B310,A310))&\": \") &D310","v":"L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"},"Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)","Measures can be used for 8' retrofit products.  Apply for the corresponding quantity installed.",{"$nulls":11},{"v":3.25,"d":"$3.25"},"Lamp",{"v":3.25,"d":"$3.25"},"Lamp","N/A","Lamp",5456,{"$f":"AB310","v":5456},"N/A","No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No",{"$f":"IF(ISBLANK(A310),\"\",IF(A310<>\"Not Eligible\",A310,IF(B310<>\"Not Eligible\",B310,C310))&\": \") &D310","v":"L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR310=\"Agribusiness\", $AR310=\"Ag\",$AR310=\"Propane\", $AR310=\"Ag Propane\", $AR310=\"Ag-Propane\"),$AC310,  $AB310),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR310=\"Agribusiness\", $AR310=\"Ag\",$AR310=\"Propane\", $AR310=\"Ag Propane\", $AR310=\"Ag-Propane\"),$AC310,  $AB310),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",20]
["L5458","L5458","Not Eligible","8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior",{"$f":"IF(ISBLANK(A311),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C311,IF(FOEIncentCodeType=IncentCodeTypeAg,B311,A311))&\": \") &D311","v":"L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"},"Must be DLC TRT V5.0 or higher listed in the respective \"Linear Replacement Lamps\" category.","Measures MAY NOT be combined with fixture incentives.","Measures are not intended for refrigerated display case applications","Limited to 50% of the retail product cost (cost excluding incentive, shipping, and sales tax)",{"$nulls":12},{"v":7,"d":"$7.00"},"Lamp",{"v":7,"d":"$7.00"},"Lamp","N/A","Lamp",5458,{"$f":"AB311","v":5458},"N/A","No","No","No",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No",{"$f":"IF(ISBLANK(A311),\"\",IF(A311<>\"Not Eligible\",A311,IF(B311<>\"Not Eligible\",B311,C311))&\": \") &D311","v":"L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR311=\"Agribusiness\", $AR311=\"Ag\",$AR311=\"Propane\", $AR311=\"Ag Propane\", $AR311=\"Ag-Propane\"),$AC311,  $AB311),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR311=\"Agribusiness\", $AR311=\"Ag\",$AR311=\"Propane\", $AR311=\"Ag Propane\", $AR311=\"Ag-Propane\"),$AC311,  $AB311),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",20]
["Not Eligible","AG5024","Not Eligible","Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture",{"$f":"IF(ISBLANK(A312),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C312,IF(FOEIncentCodeType=IncentCodeTypeAg,B312,A312))&\": \") &D312","v":"AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture"},"Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <700W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":210,"d":"$210.00"},"Fixture",{"v":210,"d":"$210.00"},"Fixture","N/A",5024,5024,"N/A","See NC MMID","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A312),\"\",IF(A312<>\"Not Eligible\",A312,IF(B312<>\"Not Eligible\",B312,C312))&\": \") &D312","v":"AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR312=\"Agribusiness\", $AR312=\"Ag\",$AR312=\"Propane\", $AR312=\"Ag Propane\", $AR312=\"Ag-Propane\"),$AC312,  $AB312),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR312=\"Agribusiness\", $AR312=\"Ag\",$AR312=\"Propane\", $AR312=\"Ag Propane\", $AR312=\"Ag-Propane\"),$AC312,  $AB312),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","AG5025","Not Eligible","Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture","AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture","Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <400W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":130,"d":"$130.00"},"Fixture",{"v":130,"d":"$130.00"},"Fixture","N/A",5025,5025,"N/A","See NC MMID","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR313=\"Agribusiness\", $AR313=\"Ag\",$AR313=\"Propane\", $AR313=\"Ag Propane\", $AR313=\"Ag-Propane\"),$AC313,  $AB313),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR313=\"Agribusiness\", $AR313=\"Ag\",$AR313=\"Propane\", $AR313=\"Ag Propane\", $AR313=\"Ag-Propane\"),$AC313,  $AB313),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","AG5026","Not Eligible","Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture","AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture","Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <700W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":140,"d":"$140.00"},"Fixture",{"v":140,"d":"$140.00"},"Fixture","N/A",5026,5026,"N/A","See NC MMID","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR314=\"Agribusiness\", $AR314=\"Ag\",$AR314=\"Propane\", $AR314=\"Ag Propane\", $AR314=\"Ag-Propane\"),$AC314,  $AB314),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR314=\"Agribusiness\", $AR314=\"Ag\",$AR314=\"Propane\", $AR314=\"Ag Propane\", $AR314=\"Ag-Propane\"),$AC314,  $AB314),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","AG5027","Not Eligible","Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture","AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture","Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <400W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":100,"d":"$100.00"},"Fixture",{"v":100,"d":"$100.00"},"Fixture","N/A",5027,5027,"N/A","See NC MMID","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR315=\"Agribusiness\", $AR315=\"Ag\",$AR315=\"Propane\", $AR315=\"Ag Propane\", $AR315=\"Ag-Propane\"),$AC315,  $AB315),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR315=\"Agribusiness\", $AR315=\"Ag\",$AR315=\"Propane\", $AR315=\"Ag Propane\", $AR315=\"Ag-Propane\"),$AC315,  $AB315),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","AG5028","Not Eligible","Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture","AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture","Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <250W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":90,"d":"$90.00"},"Fixture",{"v":90,"d":"$90.00"},"Fixture","N/A",5028,5028,"N/A","See NC MMID","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR316=\"Agribusiness\", $AR316=\"Ag\",$AR316=\"Propane\", $AR316=\"Ag Propane\", $AR316=\"Ag-Propane\"),$AC316,  $AB316),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR316=\"Agribusiness\", $AR316=\"Ag\",$AR316=\"Propane\", $AR316=\"Ag Propane\", $AR316=\"Ag-Propane\"),$AC316,  $AB316),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","N-AG5024","N-AG5024","Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture",{"$f":"IF(ISBLANK(A317),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C317,IF(FOEIncentCodeType=IncentCodeTypeAg,B317,A317))&\": \") &D317","v":"N-AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture"},"Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <700W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":210,"d":"$210.00"},"Fixture",{"v":210,"d":"$210.00"},"Fixture","N/A",5024,5024,"N/A","Yes","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR317=\"Agribusiness\", $AR317=\"Ag\",$AR317=\"Propane\", $AR317=\"Ag Propane\", $AR317=\"Ag-Propane\"),$AC317,  $AB317),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR317=\"Agribusiness\", $AR317=\"Ag\",$AR317=\"Propane\", $AR317=\"Ag Propane\", $AR317=\"Ag-Propane\"),$AC317,  $AB317),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","N-AG5025","N-AG5025","Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture","N-AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture","Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <400W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":130,"d":"$130.00"},"Fixture",{"v":130,"d":"$130.00"},"Fixture","N/A",5025,5025,"N/A","Yes","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR318=\"Agribusiness\", $AR318=\"Ag\",$AR318=\"Propane\", $AR318=\"Ag Propane\", $AR318=\"Ag-Propane\"),$AC318,  $AB318),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR318=\"Agribusiness\", $AR318=\"Ag\",$AR318=\"Propane\", $AR318=\"Ag Propane\", $AR318=\"Ag-Propane\"),$AC318,  $AB318),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","N-AG5026","N-AG5026","Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture","N-AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture","Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <700W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":140,"d":"$140.00"},"Fixture",{"v":140,"d":"$140.00"},"Fixture","N/A",5026,5026,"N/A","Yes","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR319=\"Agribusiness\", $AR319=\"Ag\",$AR319=\"Propane\", $AR319=\"Ag Propane\", $AR319=\"Ag-Propane\"),$AC319,  $AB319),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR319=\"Agribusiness\", $AR319=\"Ag\",$AR319=\"Propane\", $AR319=\"Ag Propane\", $AR319=\"Ag-Propane\"),$AC319,  $AB319),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","N-AG5027","N-AG5027","Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture","N-AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture","Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <400W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":100,"d":"$100.00"},"Fixture",{"v":100,"d":"$100.00"},"Fixture","N/A",5027,5027,"N/A","Yes","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR320=\"Agribusiness\", $AR320=\"Ag\",$AR320=\"Propane\", $AR320=\"Ag Propane\", $AR320=\"Ag-Propane\"),$AC320,  $AB320),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR320=\"Agribusiness\", $AR320=\"Ag\",$AR320=\"Propane\", $AR320=\"Ag Propane\", $AR320=\"Ag-Propane\"),$AC320,  $AB320),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","N-AG5028","N-AG5028","Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture","N-AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture","Non-stacked indoor farms and supplemented greenhouses are eligible for incentives. Vertical farming may qualify for custom incentive.","LED fixture must be <250W","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","One-for-one fixture replacements at existing buildings only",{"$nulls":3},"Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":90,"d":"$90.00"},"Fixture",{"v":90,"d":"$90.00"},"Fixture","N/A",5028,5028,"N/A","Yes","No","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR321=\"Agribusiness\", $AR321=\"Ag\",$AR321=\"Propane\", $AR321=\"Ag Propane\", $AR321=\"Ag-Propane\"),$AC321,  $AB321),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR321=\"Agribusiness\", $AR321=\"Ag\",$AR321=\"Propane\", $AR321=\"Ag Propane\", $AR321=\"Ag-Propane\"),$AC321,  $AB321),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",21]
["Not Eligible","AG5032","Not Eligible","Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture","AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture","Must be a non-stacked indoor farm. Vertical farming may qualify for custom incentive.","Requires pre-approval. Need two lighting design options (non-LED and LED) with equivalent PPFD","See catalog for pre-approval required documentation.","Must complete a Horticultural Lighting Workbook","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","Incentive is limited to 50% of project cost, including equipment and external labor","Enter annual kWh savings as unit of measure question","Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":0.15,"d":"$0.15"},"kWh saved",{"v":0.15,"d":"$0.15"},"kWh saved","N/A",5032,5032,"N/A","See NC MMID","No","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture","Yes","Yes","kWh saved",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR322=\"Agribusiness\", $AR322=\"Ag\",$AR322=\"Propane\", $AR322=\"Ag Propane\", $AR322=\"Ag-Propane\"),$AC322,  $AB322),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR322=\"Agribusiness\", $AR322=\"Ag\",$AR322=\"Propane\", $AR322=\"Ag Propane\", $AR322=\"Ag-Propane\"),$AC322,  $AB322),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":25000,"d":"25,000.00"}},"Agribusiness",21]
["Not Eligible","AG5033","Not Eligible","Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture","AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture","Must be a supplemented greenhouse. Vertical farming may qualify for custom incentive.","Requires pre-approval. Need two lighting design options (non-LED and LED) with equivalent PPFD","See catalog for pre-approval required documentation.","Must complete a Horticultural Lighting Workbook","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","Incentive is limited to 50% of project cost, including equipment and external labor","Enter annual kWh savings as unit of measure question","Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":0.15,"d":"$0.15"},"kWh saved",{"v":0.15,"d":"$0.15"},"kWh saved","N/A",5033,5033,"N/A","See NC MMID","No","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture","Yes","Yes","kWh saved",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR323=\"Agribusiness\", $AR323=\"Ag\",$AR323=\"Propane\", $AR323=\"Ag Propane\", $AR323=\"Ag-Propane\"),$AC323,  $AB323),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR323=\"Agribusiness\", $AR323=\"Ag\",$AR323=\"Propane\", $AR323=\"Ag Propane\", $AR323=\"Ag-Propane\"),$AC323,  $AB323),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":25000,"d":"25,000.00"}},"Agribusiness",21]
["Not Eligible","N-AG5032","N-AG5032","Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture",{"$f":"IF(ISBLANK(A324),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C324,IF(FOEIncentCodeType=IncentCodeTypeAg,B324,A324))&\": \") &D324","v":"N-AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture"},"Must be a non-stacked indoor farm. Vertical farming may qualify for custom incentive.","Requires pre-approval. Need two lighting design options (non-LED and LED) with equivalent PPFD","See catalog for pre-approval required documentation.","Must complete a Horticultural Lighting Workbook","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","Incentive is limited to 50% of project cost, including equipment and external labor","Enter annual kWh savings as unit of measure question","Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":0.15,"d":"$0.15"},"kWh saved",{"v":0.15,"d":"$0.15"},"kWh saved","N/A",5032,5032,"N/A","Yes","No","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture","Yes","Yes","kWh saved",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR324=\"Agribusiness\", $AR324=\"Ag\",$AR324=\"Propane\", $AR324=\"Ag Propane\", $AR324=\"Ag-Propane\"),$AC324,  $AB324),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR324=\"Agribusiness\", $AR324=\"Ag\",$AR324=\"Propane\", $AR324=\"Ag Propane\", $AR324=\"Ag-Propane\"),$AC324,  $AB324),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":25000,"d":"25,000.00"}},"Agribusiness",21]
["Not Eligible","N-AG5033","N-AG5033","Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture","N-AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture","Must be a supplemented greenhouse. Vertical farming may qualify for custom incentive.","Requires pre-approval. Need two lighting design options (non-LED and LED) with equivalent PPFD","See catalog for pre-approval required documentation.","Must complete a Horticultural Lighting Workbook","Customer must receive their electricity from participating utility","New fixtures must be DLC listed under Horticultural Lighting Category or meet the following requirements:","PPE ≥2.2 µmol/J, min 5 year warranty, and appropriate horticultural lighting designation by OSHA or Safety Compliance and Consulting Corporation","Incentive is limited to 50% of project cost, including equipment and external labor","Enter annual kWh savings as unit of measure question","Eligible for products purchased and installed after April 15, 2020.",{"$nulls":6},"N/A","N/A",{"v":0.15,"d":"$0.15"},"kWh saved",{"v":0.15,"d":"$0.15"},"kWh saved","N/A",5033,5033,"N/A","Yes","No","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture","Yes","Yes","kWh saved",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR325=\"Agribusiness\", $AR325=\"Ag\",$AR325=\"Propane\", $AR325=\"Ag Propane\", $AR325=\"Ag-Propane\"),$AC325,  $AB325),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR325=\"Agribusiness\", $AR325=\"Ag\",$AR325=\"Propane\", $AR325=\"Ag Propane\", $AR325=\"Ag-Propane\"),$AC325,  $AB325),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":25000,"d":"25,000.00"}},"Agribusiness",21]
["L10287","L10287","Not Eligible","General Wattage Reduction, ≥1,500 Hours, Interior","L10287: General Wattage Reduction, ≥1,500 Hours, Interior","Complete Table D of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.  See catalog for specifics.","Intended for LED to LED upgrades, products installed outside of their intended end-use and/or products not ES or DLC listed.","Must operate at least 1,500 hours annually.","Pre-approval required if requesting >$10k of incentives.","Rebates limited to 50% of the retail product cost (cost to customer); excludes credit, shipping, and tax.","If project/area results in other prescriptive 1-for-1 fixtures, ok to treat measure as fixture elimination.  Ensure incentives (this and 1-for-1 measure) do not exceed project cost.","If Measure Cost cannot be determined; ok to assume same value as incentive as long as condition above is met.","Omnidirectional, directional, or decorative lamps are not eligible.",{"$nulls":8},{"v":0.2,"d":"$0.20"},"Watt Reduced",{"$f":"V326","v":{"v":0.2,"d":"$0.20"}},"Watt Reduced","N/A",{"$f":"W326","v":"Watt Reduced"},10287,{"$f":"AB326","v":10287},10287,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10287: General Wattage Reduction, ≥1,500 Hours, Interior","No","Optional","Watt Reduced",{"v":5,"d":"5.00"},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR326=\"Agribusiness\", $AR326=\"Ag\",$AR326=\"Propane\", $AR326=\"Ag Propane\", $AR326=\"Ag-Propane\"),$AC326,  $AB326),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness",22]
["L10433","L10433","Not Eligible","General Wattage Reduction, <1,500 Hours, Interior","L10433: General Wattage Reduction, <1,500 Hours, Interior","Complete Table D of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.  See catalog for specifics.","Intended for LED to LED upgrades, products installed outside of their intended end-use and/or products not ES or DLC listed.","Must operate less than 1,500 hours annually.","Pre-approval required if requesting >$10k of incentives.","Rebates limited to 50% of the retail product cost (cost to customer); excludes credit, shipping, and tax.","If project/area results in other prescriptive 1-for-1 fixtures, ok to treat measure as fixture elimination.  Ensure incentives (this and 1-for-1 measure) do not exceed project cost.","If Measure Cost cannot be determined; ok to assume same value as incentive as long as condition above is met.","Omnidirectional, directional, or decorative lamps are not eligible.",{"$nulls":8},{"v":0.05,"d":"$0.05"},"Watt Reduced",{"v":0.05,"d":"$0.05"},"Watt Reduced","N/A","Watt Reduced",10433,10433,10433,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10433: General Wattage Reduction, <1,500 Hours, Interior","No","Optional","Watt Reduced",{"v":5,"d":"5.00"},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR327=\"Agribusiness\", $AR327=\"Ag\",$AR327=\"Propane\", $AR327=\"Ag Propane\", $AR327=\"Ag-Propane\"),$AC327,  $AB327),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness",22]
["L10288","L10288","Not Eligible","General Wattage Reduction, ≥1,500 Hours, Exterior","L10288: General Wattage Reduction, ≥1,500 Hours, Exterior","Complete Table D of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.  See catalog for specifics.","Intended for LED to LED upgrades, products installed outside of their intended end-use and/or products not ES or DLC listed.","Must operate at least 1,500 hours annually.","Pre-approval required if requesting >$10k of incentives.","Rebates limited to 50% of the retail product cost (cost to customer); excludes credit, shipping, and tax.","If project/area results in other prescriptive 1-for-1 fixtures, ok to treat measure as fixture elimination.  Ensure incentives (this and 1-for-1 measure) do not exceed project cost.","If Measure Cost cannot be determined; ok to assume same value as incentive as long as condition above is met.","Omnidirectional, directional, or decorative lamps are not eligible.",{"$nulls":8},{"v":0.2,"d":"$0.20"},"Watt Reduced",{"v":0.2,"d":"$0.20"},"Watt Reduced","N/A","Watt Reduced",10288,10288,10288,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10288: General Wattage Reduction, ≥1,500 Hours, Exterior","No","Optional","Watt Reduced",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR328=\"Agribusiness\", $AR328=\"Ag\",$AR328=\"Propane\", $AR328=\"Ag Propane\", $AR328=\"Ag-Propane\"),$AC328,  $AB328),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR328=\"Agribusiness\", $AR328=\"Ag\",$AR328=\"Propane\", $AR328=\"Ag Propane\", $AR328=\"Ag-Propane\"),$AC328,  $AB328),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness",22]
["L10437","L10437","Not Eligible","General Wattage Reduction, <1,500 Hours, Exterior","L10437: General Wattage Reduction, <1,500 Hours, Exterior","Complete Table D of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.  See catalog for specifics.","Intended for LED to LED upgrades, products installed outside of their intended end-use and/or products not ES or DLC listed.","Must operate less than 1,500 hours annually.","Pre-approval required if requesting >$10k of incentives.","Rebates limited to 50% of the retail product cost (cost to customer); excludes credit, shipping, and tax.","If project/area results in other prescriptive 1-for-1 fixtures, ok to treat measure as fixture elimination.  Ensure incentives (this and 1-for-1 measure) do not exceed project cost.","If Measure Cost cannot be determined; ok to assume same value as incentive as long as condition above is met.","Omnidirectional, directional, or decorative lamps are not eligible.",{"$nulls":8},{"v":0.05,"d":"$0.05"},"Watt Reduced",{"v":0.05,"d":"$0.05"},"Watt Reduced","N/A","Watt Reduced",10437,10437,10437,"No","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","L10437: General Wattage Reduction, <1,500 Hours, Exterior","No","Optional","Watt Reduced",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR329=\"Agribusiness\", $AR329=\"Ag\",$AR329=\"Propane\", $AR329=\"Ag Propane\", $AR329=\"Ag-Propane\"),$AC329,  $AB329),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":5,"d":"5.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR329=\"Agribusiness\", $AR329=\"Ag\",$AR329=\"Propane\", $AR329=\"Ag Propane\", $AR329=\"Ag-Propane\"),$AC329,  $AB329),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness",22]
[{"$nulls":3},"----------------------AGRIBUSINESS CATALOG: VENTILATION  --------------------------------------------","----------------------AGRIBUSINESS CATALOG: VENTILATION  --------------------------------------------","","","","","","","","","","",{"$nulls":21},"No","----------------------AGRIBUSINESS CATALOG: VENTILATION  --------------------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR330=\"Agribusiness\", $AR330=\"Ag\",$AR330=\"Propane\", $AR330=\"Ag Propane\", $AR330=\"Ag-Propane\"),$AC330,  $AB330),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR330=\"Agribusiness\", $AR330=\"Ag\",$AR330=\"Propane\", $AR330=\"Ag Propane\", $AR330=\"Ag-Propane\"),$AC330,  $AB330),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG3998","Not Eligible","Fans, High Volume Low Speed (HVLS)","AG3998: Fans, High Volume Low Speed (HVLS)","Enter Diamter in feet in units column on the incentive application (i.e., 5 fans X 16 feet)","Minimum 16 feet fan diameter.","Submit fan specification sheet with application",{"$nulls":5},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":100,"d":"$100.00"},"Fan Diameter (feet)",{"v":100,"d":"$100.00"},{"$f":"Y331","v":"Fan Diameter (feet)"},"N/A",3998,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A331),\"\",IF(A331<>\"Not Eligible\",A331,IF(B331<>\"Not Eligible\",B331,C331))&\": \") &D331","v":"AG3998: Fans, High Volume Low Speed (HVLS)"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR331=\"Agribusiness\", $AR331=\"Ag\",$AR331=\"Propane\", $AR331=\"Ag Propane\", $AR331=\"Ag-Propane\"),$AC331,  $AB331),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":7,"d":"7.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR331=\"Agribusiness\", $AR331=\"Ag\",$AR331=\"Propane\", $AR331=\"Ag Propane\", $AR331=\"Ag-Propane\"),$AC331,  $AB331),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":25,"d":"25.00"}},"Agribusiness",23]
["Not Eligible","N-AG3998","Eligible Under AgV2","Fans, High Volume Low Speed (HVLS)","N-AG3998: Fans, High Volume Low Speed (HVLS)","Enter Diamter in feet in units column on the incentive application (i.e., 5 fans X 16 feet)","Minimum 16 feet fan diameter.","Submit fan specification sheet with application",{"$nulls":5},"Incentive must be ≤100% project cost.",{"$nulls":7},"N/A","N/A",{"v":100,"d":"$100.00"},"Fan Diameter (feet)",{"v":100,"d":"$100.00"},{"$f":"Y332","v":"Fan Diameter (feet)"},"N/A",3998,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A332),\"\",IF(A332<>\"Not Eligible\",A332,IF(B332<>\"Not Eligible\",B332,C332))&\": \") &D332","v":"N-AG3998: Fans, High Volume Low Speed (HVLS)"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR332=\"Agribusiness\", $AR332=\"Ag\",$AR332=\"Propane\", $AR332=\"Ag Propane\", $AR332=\"Ag-Propane\"),$AC332,  $AB332),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":7,"d":"7.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR332=\"Agribusiness\", $AR332=\"Ag\",$AR332=\"Propane\", $AR332=\"Ag Propane\", $AR332=\"Ag-Propane\"),$AC332,  $AB332),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":25,"d":"25.00"}},"Agribusiness",23]
["Not Eligible","AG5089","Not Eligible","Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed","AG5089: Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed","Product must be ≥ 48 inch fan with variable speed","Variable speed fans do not have a minimum performance requirement.","Variable speed must be automatically controlled by temperature.","Variable speed fans are not eligible for other variable frequency drive incentives.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":11},"N/A","N/A",{"v":425,"d":"$425.00"},"Fan",{"v":425,"d":"$425.00"},{"$f":"Y333","v":"Fan"},"N/A",5089,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A333),\"\",IF(A333<>\"Not Eligible\",A333,IF(B333<>\"Not Eligible\",B333,C333))&\": \") &D333","v":"AG5089: Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR333=\"Agribusiness\", $AR333=\"Ag\",$AR333=\"Propane\", $AR333=\"Ag Propane\", $AR333=\"Ag-Propane\"),$AC333,  $AB333),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR333=\"Agribusiness\", $AR333=\"Ag\",$AR333=\"Propane\", $AR333=\"Ag Propane\", $AR333=\"Ag-Propane\"),$AC333,  $AB333),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",23]
["Not Eligible","N-AG5089","Eligible Under AgV2","Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed","N-AG5089: Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed","Product must be ≥ 48 inch fan with variable speed","Variable speed fans do not have a minimum performance requirement.","Variable speed must be automatically controlled by temperature.","Variable speed fans are not eligible for other variable frequency drive incentives.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":11},"N/A","N/A",{"v":425,"d":"$425.00"},"Fan",{"v":425,"d":"$425.00"},"Fan","N/A",5089,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5089: Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR334=\"Agribusiness\", $AR334=\"Ag\",$AR334=\"Propane\", $AR334=\"Ag Propane\", $AR334=\"Ag-Propane\"),$AC334,  $AB334),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR334=\"Agribusiness\", $AR334=\"Ag\",$AR334=\"Propane\", $AR334=\"Ag Propane\", $AR334=\"Ag-Propane\"),$AC334,  $AB334),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",23]
["Not Eligible","AG5095","Not Eligible","Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed","AG5095: Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed","Product must be ≥ 48 inch fan with variable speed","Variable speed fans do not have a minimum performance requirement.","Must operate a minimum of 4,000 hours annually to be eligible.","Variable speed must be automatically controlled by temperature.","Variable speed fans are not eligible for other variable frequency drive incentives.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":10},"N/A","N/A",{"v":325,"d":"$325.00"},"Fan",{"v":325,"d":"$325.00"},"Fan","N/A",5095,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG5095: Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR335=\"Agribusiness\", $AR335=\"Ag\",$AR335=\"Propane\", $AR335=\"Ag Propane\", $AR335=\"Ag-Propane\"),$AC335,  $AB335),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR335=\"Agribusiness\", $AR335=\"Ag\",$AR335=\"Propane\", $AR335=\"Ag Propane\", $AR335=\"Ag-Propane\"),$AC335,  $AB335),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",23]
["Not Eligible","N-AG5095","Eligible Under AgV2","Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed","N-AG5095: Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed","Product must be ≥ 48 inch fan with variable speed","Variable speed fans do not have a minimum performance requirement.","Must operate a minimum of 4,000 hours annually to be eligible.","Variable speed must be automatically controlled by temperature.","Variable speed fans are not eligible for other variable frequency drive incentives.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":10},"N/A","N/A",{"v":325,"d":"$325.00"},"Fan",{"v":325,"d":"$325.00"},"Fan","N/A",5095,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5095: Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR336=\"Agribusiness\", $AR336=\"Ag\",$AR336=\"Propane\", $AR336=\"Ag Propane\", $AR336=\"Ag-Propane\"),$AC336,  $AB336),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR336=\"Agribusiness\", $AR336=\"Ag\",$AR336=\"Propane\", $AR336=\"Ag Propane\", $AR336=\"Ag-Propane\"),$AC336,  $AB336),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",23]
["Not Eligible","AG5086","Not Eligible","Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)","AG5086: Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)","36 to 47 inch fans must be greater than or equal to 20.0 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control Association","(AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.  ","Full fan model number and fan diameter must be included on invoice.",{"$nulls":12},"N/A","N/A",{"v":70,"d":"$70.00"},"Fan",{"v":70,"d":"$70.00"},"Fan","N/A",5086,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A337),\"\",IF(A337<>\"Not Eligible\",A337,IF(B337<>\"Not Eligible\",B337,C337))&\": \") &D337","v":"AG5086: Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR337=\"Agribusiness\", $AR337=\"Ag\",$AR337=\"Propane\", $AR337=\"Ag Propane\", $AR337=\"Ag-Propane\"),$AC337,  $AB337),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR337=\"Agribusiness\", $AR337=\"Ag\",$AR337=\"Propane\", $AR337=\"Ag Propane\", $AR337=\"Ag-Propane\"),$AC337,  $AB337),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",23]
["Not Eligible","AG5087","Not Eligible","Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)","AG5087: Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)","≥ 48 inch fans must be greater than or equal to 24.5 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control Association","(AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.  ","Full fan model number and fan diameter must be included on invoice.",{"$nulls":12},"N/A","N/A",{"v":90,"d":"$90.00"},"Fan",{"v":90,"d":"$90.00"},"Fan","N/A",5087,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A338),\"\",IF(A338<>\"Not Eligible\",A338,IF(B338<>\"Not Eligible\",B338,C338))&\": \") &D338","v":"AG5087: Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR338=\"Agribusiness\", $AR338=\"Ag\",$AR338=\"Propane\", $AR338=\"Ag Propane\", $AR338=\"Ag-Propane\"),$AC338,  $AB338),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR338=\"Agribusiness\", $AR338=\"Ag\",$AR338=\"Propane\", $AR338=\"Ag Propane\", $AR338=\"Ag-Propane\"),$AC338,  $AB338),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",23]
["Not Eligible","N-AG5086","Eligible Under AgV2","Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)","N-AG5086: Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)","36 to 47 inch fans must be greater than or equal to 20.0 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control Association","(AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.  ","Full fan model number and fan diameter must be included on invoice.",{"$nulls":12},"N/A","N/A",{"v":70,"d":"$70.00"},"Fan",{"v":70,"d":"$70.00"},"Fan","N/A",5086,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A339),\"\",IF(A339<>\"Not Eligible\",A339,IF(B339<>\"Not Eligible\",B339,C339))&\": \") &D339","v":"N-AG5086: Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR339=\"Agribusiness\", $AR339=\"Ag\",$AR339=\"Propane\", $AR339=\"Ag Propane\", $AR339=\"Ag-Propane\"),$AC339,  $AB339),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR339=\"Agribusiness\", $AR339=\"Ag\",$AR339=\"Propane\", $AR339=\"Ag Propane\", $AR339=\"Ag-Propane\"),$AC339,  $AB339),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",23]
["Not Eligible","N-AG5087","Eligible Under AgV2","Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)","N-AG5087: Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)","≥ 48 inch fans must be greater than or equal to 24.5 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control Association","(AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.  ","Full fan model number and fan diameter must be included on invoice.",{"$nulls":12},"N/A","N/A",{"v":90,"d":"$90.00"},"Fan",{"v":90,"d":"$90.00"},"Fan","N/A",5087,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5087: Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR340=\"Agribusiness\", $AR340=\"Ag\",$AR340=\"Propane\", $AR340=\"Ag Propane\", $AR340=\"Ag-Propane\"),$AC340,  $AB340),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR340=\"Agribusiness\", $AR340=\"Ag\",$AR340=\"Propane\", $AR340=\"Ag Propane\", $AR340=\"Ag-Propane\"),$AC340,  $AB340),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",23]
["Not Eligible","AG5090","Not Eligible","Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)","AG5090: Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)","24 to 35 inch fans must be greater than or equal to 15.8 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control","Association (AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.","Must operate a minimum of 4,000 hours annually to be eligible.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":11},"N/A","N/A",{"v":40,"d":"$40.00"},"Fan",{"v":40,"d":"$40.00"},"Fan","N/A",5090,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A341),\"\",IF(A341<>\"Not Eligible\",A341,IF(B341<>\"Not Eligible\",B341,C341))&\": \") &D341","v":"AG5090: Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR341=\"Agribusiness\", $AR341=\"Ag\",$AR341=\"Propane\", $AR341=\"Ag Propane\", $AR341=\"Ag-Propane\"),$AC341,  $AB341),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR341=\"Agribusiness\", $AR341=\"Ag\",$AR341=\"Propane\", $AR341=\"Ag Propane\", $AR341=\"Ag-Propane\"),$AC341,  $AB341),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",24]
["Not Eligible","AG5091","Not Eligible","Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)","AG5091: Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)","36 to 47 inch fans must be greater than or equal to 20.0 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control","Association (AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.","Must operate a minimum of 4,000 hours annually to be eligible.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":11},"N/A","N/A",{"v":70,"d":"$70.00"},"Fan",{"v":70,"d":"$70.00"},"Fan","N/A",5091,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A342),\"\",IF(A342<>\"Not Eligible\",A342,IF(B342<>\"Not Eligible\",B342,C342))&\": \") &D342","v":"AG5091: Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR342=\"Agribusiness\", $AR342=\"Ag\",$AR342=\"Propane\", $AR342=\"Ag Propane\", $AR342=\"Ag-Propane\"),$AC342,  $AB342),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR342=\"Agribusiness\", $AR342=\"Ag\",$AR342=\"Propane\", $AR342=\"Ag Propane\", $AR342=\"Ag-Propane\"),$AC342,  $AB342),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",24]
["Not Eligible","AG5092","Not Eligible","Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)","AG5092: Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)","≥ 48 inch fans must be greater than or equal to 24.5 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control","Association (AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.","Must operate a minimum of 4,000 hours annually to be eligible.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":11},"N/A","N/A",{"v":90,"d":"$90.00"},"Fan",{"v":90,"d":"$90.00"},"Fan","N/A",5092,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A343),\"\",IF(A343<>\"Not Eligible\",A343,IF(B343<>\"Not Eligible\",B343,C343))&\": \") &D343","v":"AG5092: Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)"},"No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR343=\"Agribusiness\", $AR343=\"Ag\",$AR343=\"Propane\", $AR343=\"Ag Propane\", $AR343=\"Ag-Propane\"),$AC343,  $AB343),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR343=\"Agribusiness\", $AR343=\"Ag\",$AR343=\"Propane\", $AR343=\"Ag Propane\", $AR343=\"Ag-Propane\"),$AC343,  $AB343),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",24]
["Not Eligible","N-AG5090","Eligible Under AgV2","Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)","N-AG5090: Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)","24 to 35 inch fans must be greater than or equal to 15.8 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control","Association (AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.","Must operate a minimum of 4,000 hours annually to be eligible.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":11},"N/A","N/A",{"v":40,"d":"$40.00"},"Fan",{"v":40,"d":"$40.00"},"Fan","N/A",5090,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5090: Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR344=\"Agribusiness\", $AR344=\"Ag\",$AR344=\"Propane\", $AR344=\"Ag Propane\", $AR344=\"Ag-Propane\"),$AC344,  $AB344),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR344=\"Agribusiness\", $AR344=\"Ag\",$AR344=\"Propane\", $AR344=\"Ag Propane\", $AR344=\"Ag-Propane\"),$AC344,  $AB344),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",24]
["Not Eligible","N-AG5091","Eligible Under AgV2","Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)","N-AG5091: Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)","36 to 47 inch fans must be greater than or equal to 20.0 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control","Association (AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.","Must operate a minimum of 4,000 hours annually to be eligible.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":11},"N/A","N/A",{"v":70,"d":"$70.00"},"Fan",{"v":70,"d":"$70.00"},"Fan","N/A",5091,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5091: Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR345=\"Agribusiness\", $AR345=\"Ag\",$AR345=\"Propane\", $AR345=\"Ag Propane\", $AR345=\"Ag-Propane\"),$AC345,  $AB345),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR345=\"Agribusiness\", $AR345=\"Ag\",$AR345=\"Propane\", $AR345=\"Ag Propane\", $AR345=\"Ag-Propane\"),$AC345,  $AB345),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",24]
["Not Eligible","N-AG5092","Eligible Under AgV2","Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)",{"$f":"IF(ISBLANK(A346),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C346,IF(FOEIncentCodeType=IncentCodeTypeAg,B346,A346))&\": \") &D346","v":"N-AG5092: Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)"},"≥ 48 inch fans must be greater than or equal to 24.5 lbf/kW.","Test report must be included with Fan Application to verify performance. Acceptable test report sources include Bio-Environmental and Structural Systems (BESS) labs, an accredited Air Movement and Control","Association (AMCA) testing facility or other third party lab in accordance with AMCA/ANSI 210 or 230 test procedures.","Must operate a minimum of 4,000 hours annually to be eligible.","Full fan model number and fan diameter must be included on invoice.",{"$nulls":11},"N/A","N/A",{"v":90,"d":"$90.00"},"Fan",{"v":90,"d":"$90.00"},"Fan","N/A",5092,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5092: Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)","No","No","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR346=\"Agribusiness\", $AR346=\"Ag\",$AR346=\"Propane\", $AR346=\"Ag Propane\", $AR346=\"Ag-Propane\"),$AC346,  $AB346),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR346=\"Agribusiness\", $AR346=\"Ag\",$AR346=\"Propane\", $AR346=\"Ag Propane\", $AR346=\"Ag-Propane\"),$AC346,  $AB346),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",24]
[{"$nulls":3},"----------------------AGRIBUSINESS CATALOG: VFD & COMPRESSED AIR  --------------------------------------------","----------------------AGRIBUSINESS CATALOG: VFD & COMPRESSED AIR  --------------------------------------------","","","","","","","","","","",{"$nulls":21},"No","----------------------AGRIBUSINESS CATALOG: VFD & COMPRESSED AIR  --------------------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR347=\"Agribusiness\", $AR347=\"Ag\",$AR347=\"Propane\", $AR347=\"Ag Propane\", $AR347=\"Ag-Propane\"),$AC347,  $AB347),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR347=\"Agribusiness\", $AR347=\"Ag\",$AR347=\"Propane\", $AR347=\"Ag Propane\", $AR347=\"Ag-Propane\"),$AC347,  $AB347),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG10209","Not Eligible","VFD, Ag Water System, ≥1000 hours","AG10209: VFD, Ag Water System, ≥1000 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures",null,"Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Primary use water system includes any direct well water pumping for waterer or cleaning needs. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":115,"d":"$115.00"},"hp",{"v":70,"d":"$70.00"},{"$f":"Y348","v":"hp"},"N/A",4043,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG10209: VFD, Ag Water System, ≥1000 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR348=\"Agribusiness\", $AR348=\"Ag\",$AR348=\"Propane\", $AR348=\"Ag Propane\", $AR348=\"Ag-Propane\"),$AC348,  $AB348),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR348=\"Agribusiness\", $AR348=\"Ag\",$AR348=\"Propane\", $AR348=\"Ag Propane\", $AR348=\"Ag-Propane\"),$AC348,  $AB348),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"Agribusiness",25]
["Not Eligible","AG10210","Not Eligible","VFD, Ag Water System, 500-999 hours","AG10210: VFD, Ag Water System, 500-999 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures",null,"Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Secondary use water system includes a pump distributing the warm water from the output of a well water plate-cooler for reuse purposes. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":70,"d":"$70.00"},"hp",{"v":40,"d":"$40.00"},"hp","N/A",4411,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG10210: VFD, Ag Water System, 500-999 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR349=\"Agribusiness\", $AR349=\"Ag\",$AR349=\"Propane\", $AR349=\"Ag Propane\", $AR349=\"Ag-Propane\"),$AC349,  $AB349),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR349=\"Agribusiness\", $AR349=\"Ag\",$AR349=\"Propane\", $AR349=\"Ag Propane\", $AR349=\"Ag-Propane\"),$AC349,  $AB349),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",25]
["Not Eligible","AG4949","Not Eligible","VFD, Irrigation Well Pump, ≥500 hours","AG4949: VFD, Irrigation Well Pump, ≥500 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures",null,"Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Secondary use water system includes a pump distributing the warm water from the output of a well water plate-cooler for reuse purposes. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":70,"d":"$70.00"},"hp",{"v":40,"d":"$40.00"},"hp","N/A",4412,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4949: VFD, Irrigation Well Pump, ≥500 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR350=\"Agribusiness\", $AR350=\"Ag\",$AR350=\"Propane\", $AR350=\"Ag Propane\", $AR350=\"Ag-Propane\"),$AC350,  $AB350),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR350=\"Agribusiness\", $AR350=\"Ag\",$AR350=\"Propane\", $AR350=\"Ag Propane\", $AR350=\"Ag-Propane\"),$AC350,  $AB350),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",25]
["Not Eligible","AG3777","Not Eligible","VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours","AG3777: VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures",null,"Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs. **TECH REVIEW - Use Non-HVAC Fans VFD Hybrid Calc**",{"$nulls":6},"N/A","N/A",{"v":125,"d":"$125.00"},"hp",{"v":100,"d":"$100.00"},"hp","N/A",3777,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A351),\"\",IF(A351<>\"Not Eligible\",A351,IF(B351<>\"Not Eligible\",B351,C351))&\": \") &D351","v":"AG3777: VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours"},"Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR351=\"Agribusiness\", $AR351=\"Ag\",$AR351=\"Propane\", $AR351=\"Ag Propane\", $AR351=\"Ag-Propane\"),$AC351,  $AB351),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR351=\"Agribusiness\", $AR351=\"Ag\",$AR351=\"Propane\", $AR351=\"Ag Propane\", $AR351=\"Ag-Propane\"),$AC351,  $AB351),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},"Agribusiness",25]
["Not Eligible","AG3835","Not Eligible","VFD, Process Pump, Agriculture, ≥ 1000 hours","AG3835: VFD, Process Pump, Agriculture, ≥ 1000 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures","Process Pump category can include a slurry pump or other process driven pump needs on a farm","Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Process pump can include a slurry pump or other process driven pump needs on a dairy farm. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":95,"d":"$95.00"},"hp",{"v":60,"d":"$60.00"},"hp","N/A",3835,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG3835: VFD, Process Pump, Agriculture, ≥ 1000 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR352=\"Agribusiness\", $AR352=\"Ag\",$AR352=\"Propane\", $AR352=\"Ag Propane\", $AR352=\"Ag-Propane\"),$AC352,  $AB352),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR352=\"Agribusiness\", $AR352=\"Ag\",$AR352=\"Propane\", $AR352=\"Ag Propane\", $AR352=\"Ag-Propane\"),$AC352,  $AB352),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"Agribusiness",25]
["Not Eligible","AG4414","Not Eligible","VFD, Process Pump, Agriculture, 500-999 hours","AG4414: VFD, Process Pump, Agriculture, 500-999 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures","Process Pump category can include a slurry pump or other process driven pump needs on a farm","Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Process pump can include a slurry pump or other process driven pump needs on a dairy farm. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":70,"d":"$70.00"},"hp",{"v":40,"d":"$40.00"},"hp","N/A",4414,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4414: VFD, Process Pump, Agriculture, 500-999 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR353=\"Agribusiness\", $AR353=\"Ag\",$AR353=\"Propane\", $AR353=\"Ag Propane\", $AR353=\"Ag-Propane\"),$AC353,  $AB353),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR353=\"Agribusiness\", $AR353=\"Ag\",$AR353=\"Propane\", $AR353=\"Ag Propane\", $AR353=\"Ag-Propane\"),$AC353,  $AB353),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",25]
["Not Eligible","N-AG10209","Eligible Under AgV2","VFD, Ag Water System, ≥1000 hours","N-AG10209: VFD, Ag Water System, ≥1000 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures",null,"Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Primary use water system includes any direct well water pumping for waterer or cleaning needs. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":115,"d":"$115.00"},"hp",{"v":70,"d":"$70.00"},"hp","N/A",4043,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10209: VFD, Ag Water System, ≥1000 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR354=\"Agribusiness\", $AR354=\"Ag\",$AR354=\"Propane\", $AR354=\"Ag Propane\", $AR354=\"Ag-Propane\"),$AC354,  $AB354),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR354=\"Agribusiness\", $AR354=\"Ag\",$AR354=\"Propane\", $AR354=\"Ag Propane\", $AR354=\"Ag-Propane\"),$AC354,  $AB354),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":200,"d":"200.00"}},"Agribusiness",25]
["Not Eligible","N-AG10210","Eligible Under AgV2","VFD, Ag Water System, 500-999 hours","N-AG10210: VFD, Ag Water System, 500-999 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures",null,"Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Secondary use water system includes a pump distributing the warm water from the output of a well water plate-cooler for reuse purposes. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other assoc",{"$nulls":6},"N/A","N/A",{"v":70,"d":"$70.00"},"hp",{"v":40,"d":"$40.00"},"hp","N/A",4411,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10210: VFD, Ag Water System, 500-999 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR355=\"Agribusiness\", $AR355=\"Ag\",$AR355=\"Propane\", $AR355=\"Ag Propane\", $AR355=\"Ag-Propane\"),$AC355,  $AB355),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR355=\"Agribusiness\", $AR355=\"Ag\",$AR355=\"Propane\", $AR355=\"Ag Propane\", $AR355=\"Ag-Propane\"),$AC355,  $AB355),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",25]
["Not Eligible","N-AG4949","Eligible Under AgV2","VFD, Irrigation Well Pump, ≥500 hours",{"$f":"IF(ISBLANK(A356),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C356,IF(FOEIncentCodeType=IncentCodeTypeAg,B356,A356))&\": \") &D356","v":"N-AG4949: VFD, Irrigation Well Pump, ≥500 hours"},"Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures",null,"Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Secondary use water system includes a pump distributing the warm water from the output of a well water plate-cooler for reuse purposes. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":70,"d":"$70.00"},"hp",{"v":40,"d":"$40.00"},"hp","N/A",4949,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4949: VFD, Irrigation Well Pump, ≥500 hours","Yes","Yes","",{"v":1,"d":"1.00"},{"v":500,"d":"500.00"},"Agribusiness",25]
["Not Eligible","N-AG3777","Eligible Under AgV2","VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours","N-AG3777: VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures",null,"Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs. **TECH REVIEW - Use Non-HVAC Fans VFD Hybrid Calc**",{"$nulls":6},"N/A","N/A",{"v":125,"d":"$125.00"},"hp",{"v":100,"d":"$100.00"},"hp","N/A",3777,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A357),\"\",IF(A357<>\"Not Eligible\",A357,IF(B357<>\"Not Eligible\",B357,C357))&\": \") &D357","v":"N-AG3777: VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours"},"Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR357=\"Agribusiness\", $AR357=\"Ag\",$AR357=\"Propane\", $AR357=\"Ag Propane\", $AR357=\"Ag-Propane\"),$AC357,  $AB357),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR357=\"Agribusiness\", $AR357=\"Ag\",$AR357=\"Propane\", $AR357=\"Ag Propane\", $AR357=\"Ag-Propane\"),$AC357,  $AB357),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},"Agribusiness",25]
["Not Eligible","N-AG3835","Eligible Under AgV2","VFD, Process Pump, Agriculture, ≥ 1000 hours","N-AG3835: VFD, Process Pump, Agriculture, ≥ 1000 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures","Process Pump category can include a slurry pump or other process driven pump needs on a farm","Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Process pump can include a slurry pump or other process driven pump needs on a dairy farm. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":95,"d":"$95.00"},"hp",{"v":60,"d":"$60.00"},"hp","N/A",3835,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG3835: VFD, Process Pump, Agriculture, ≥ 1000 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR358=\"Agribusiness\", $AR358=\"Ag\",$AR358=\"Propane\", $AR358=\"Ag Propane\", $AR358=\"Ag-Propane\"),$AC358,  $AB358),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR358=\"Agribusiness\", $AR358=\"Ag\",$AR358=\"Propane\", $AR358=\"Ag Propane\", $AR358=\"Ag-Propane\"),$AC358,  $AB358),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"Agribusiness",25]
["Not Eligible","N-AG4414","Eligible Under AgV2","VFD, Process Pump, Agriculture, 500-999 hours","N-AG4414: VFD, Process Pump, Agriculture, 500-999 hours","Must complete Table C1 (and C2 for Irrigation Well Pump) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures","Process Pump category can include a slurry pump or other process driven pump needs on a farm","Verify correct measure is being used for annual operating hours","VFD must be installed on a centrifugal or axial flow pump or fan, i.e., a variable torque load used to control a process on your dairy farm","The pump or fan may not exceed 500 hp.","Redundant/back-up units DNQ. Routine replacement of existing VFDs do not qualify.","Incentive is based on motor HP controlled by VFD","VFD speed must be automatically controlled by differential pressure, flow, temperature, or orther variable signal. Units installed only to allow soft starts are not eligible","see catalog for more","Process pump can include a slurry pump or other process driven pump needs on a dairy farm. OK if VFD is sized larger than motor - question if VFD is smaller than motor. Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":70,"d":"$70.00"},"hp",{"v":40,"d":"$40.00"},"hp","N/A",4414,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4414: VFD, Process Pump, Agriculture, 500-999 hours","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR359=\"Agribusiness\", $AR359=\"Ag\",$AR359=\"Propane\", $AR359=\"Ag Propane\", $AR359=\"Ag-Propane\"),$AC359,  $AB359),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR359=\"Agribusiness\", $AR359=\"Ag\",$AR359=\"Propane\", $AR359=\"Ag Propane\", $AR359=\"Ag-Propane\"),$AC359,  $AB359),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",25]
["Not Eligible","AG3836","Not Eligible","VFD, Constant Torque, ≥1000 Annual Hours, Ag","AG3836: VFD, Constant Torque, ≥1000 Annual Hours, Ag","Must complete Table C1 (and C3 if manually controlled) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures","VFDs must be installed on constant torque equipment (e.g., conveyors, auger/mixers, extruders, hoist, crusher/shredders, positive displacement pump).","≥1000 Annual Hours","The system using the VFD may not exceed 500 HP","VFD speed can be automatically controlled by differential pressure, flow, temperature or other variable signal, or be manually controlled","VFDs on vacuum pumps or air compressors are not eligible for this particular measure. See pg 11 Process catalog.","Incentive is based on the motor HP controlled by VFD","Redundant or backup units do not qualify","For NC projects, VFDs that are required in accordance to Wisconsin Energy Code are not eligible","Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":55,"d":"$55.00"},"hp",{"v":50,"d":"$50.00"},"hp","N/A",3836,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG3836: VFD, Constant Torque, ≥1000 Annual Hours, Ag","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR360=\"Agribusiness\", $AR360=\"Ag\",$AR360=\"Propane\", $AR360=\"Ag Propane\", $AR360=\"Ag-Propane\"),$AC360,  $AB360),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR360=\"Agribusiness\", $AR360=\"Ag\",$AR360=\"Propane\", $AR360=\"Ag Propane\", $AR360=\"Ag-Propane\"),$AC360,  $AB360),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":250,"d":"250.00"}},"Agribusiness",25]
["Not Eligible","AG4412","Not Eligible","VFD, Constant Torque, 500-999 Hours, Ag","AG4412: VFD, Constant Torque, 500-999 Hours, Ag","Must complete Table C1 (and C3 if manually controlled) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures","VFDs must be installed on constant torque equipment (e.g., conveyors, auger/mixers, extruders, hoist, crusher/shredders, positive displacement pump).","500-999 Hours","The system using the VFD may not exceed 500 HP","VFD speed can be automatically controlled by differential pressure, flow, temperature or other variable signal, or be manually controlled","VFDs on vacuum pumps or air compressors are not eligible for this particular measure. See pg 11 Process catalog.","Incentive is based on the motor HP controlled by VFD","Redundant or backup units do not qualify","For NC projects, VFDs that are required in accordance to Wisconsin Energy Code are not eligible","Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":40,"d":"$40.00"},"hp",{"v":30,"d":"$30.00"},"hp","N/A",4412,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4412: VFD, Constant Torque, 500-999 Hours, Ag","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR361=\"Agribusiness\", $AR361=\"Ag\",$AR361=\"Propane\", $AR361=\"Ag Propane\", $AR361=\"Ag-Propane\"),$AC361,  $AB361),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR361=\"Agribusiness\", $AR361=\"Ag\",$AR361=\"Propane\", $AR361=\"Ag Propane\", $AR361=\"Ag-Propane\"),$AC361,  $AB361),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",25]
["Not Eligible","N-AG3836","Eligible Under AgV2","VFD, Constant Torque, ≥1000 Annual Hours, Ag","N-AG3836: VFD, Constant Torque, ≥1000 Annual Hours, Ag","Must complete Table C1 (and C3 if manually controlled) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures","VFDs must be installed on constant torque equipment (e.g., conveyors, auger/mixers, extruders, hoist, crusher/shredders, positive displacement pump).","≥1000 Annual Hours","The system using the VFD may not exceed 500 HP","VFD speed can be automatically controlled by differential pressure, flow, temperature or other variable signal, or be manually controlled","VFDs on vacuum pumps or air compressors are not eligible for this particular measure. See pg 11 Process catalog.","Incentive is based on the motor HP controlled by VFD","Redundant or backup units do not qualify","For NC projects, VFDs that are required in accordance to Wisconsin Energy Code are not eligible","Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":55,"d":"$55.00"},"hp",{"v":50,"d":"$50.00"},"hp","N/A",3836,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG3836: VFD, Constant Torque, ≥1000 Annual Hours, Ag","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR362=\"Agribusiness\", $AR362=\"Ag\",$AR362=\"Propane\", $AR362=\"Ag Propane\", $AR362=\"Ag-Propane\"),$AC362,  $AB362),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR362=\"Agribusiness\", $AR362=\"Ag\",$AR362=\"Propane\", $AR362=\"Ag Propane\", $AR362=\"Ag-Propane\"),$AC362,  $AB362),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":250,"d":"250.00"}},"Agribusiness",25]
["Not Eligible","N-AG4412","Eligible Under AgV2","VFD, Constant Torque, 500-999 Hours, Ag","N-AG4412: VFD, Constant Torque, 500-999 Hours, Ag","Must complete Table C1 (and C3 if manually controlled) of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for these measures","VFDs must be installed on constant torque equipment (e.g., conveyors, auger/mixers, extruders, hoist, crusher/shredders, positive displacement pump).","500-999 Hours","The system using the VFD may not exceed 500 HP","VFD speed can be automatically controlled by differential pressure, flow, temperature or other variable signal, or be manually controlled","VFDs on vacuum pumps or air compressors are not eligible for this particular measure. See pg 11 Process catalog.","Incentive is based on the motor HP controlled by VFD","Redundant or backup units do not qualify","For NC projects, VFDs that are required in accordance to Wisconsin Energy Code are not eligible","Project cost is VFD only - no other associated costs.",{"$nulls":6},"N/A","N/A",{"v":40,"d":"$40.00"},"hp",{"v":30,"d":"$30.00"},"hp","N/A",4412,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4412: VFD, Constant Torque, 500-999 Hours, Ag","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR363=\"Agribusiness\", $AR363=\"Ag\",$AR363=\"Propane\", $AR363=\"Ag Propane\", $AR363=\"Ag-Propane\"),$AC363,  $AB363),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR363=\"Agribusiness\", $AR363=\"Ag\",$AR363=\"Propane\", $AR363=\"Ag Propane\", $AR363=\"Ag-Propane\"),$AC363,  $AB363),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",25]
["Not Eligible","PS2196","Not Eligible","Variable Speed Drive Air Compressor replacing Non-VSD Compressor","PS2196: Variable Speed Drive Air Compressor replacing Non-VSD Compressor","Complete Table E1 and E2 of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.","Submit manufacturer specification sheets and/or a CAGI sheet at anticipated operating pressure for items installed. If available, include spec sheets for the removed compressor.","Backup or redundant systems DNQ","Must be variable speed rotary vane compressor or variable speed screw compressor and operate a min of 2,000 hours annually","Limited to one VSD compressor per compressor air system","Replacing an old VSD compressor with a new (same size) VSD compressor DNQ. Replacement of an old VSD compressor with a new, larger VSD compr. is eligible for the increase in hp over the old compressor.  For example, if a 50 hp VSD compressor is replaced with a 75 hp VSD compressor, the 25 hp increase in capacity would be eligible for incentives.","Replaced equipment must be removed, if kept it must be used for emergency backup only.","This is for new VSD compressors only; adding a VSD to an existing compressor does not qualify. Replacing an old VSD compressor with a new VSD compressor does not qualify. Adding a VSD compressor to a system that already includes a VSD compressor does not qualify.",{"$nulls":8},"N/A","N/A",{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP","N/A",2196,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2196: Variable Speed Drive Air Compressor replacing Non-VSD Compressor","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR364=\"Agribusiness\", $AR364=\"Ag\",$AR364=\"Propane\", $AR364=\"Ag Propane\", $AR364=\"Ag-Propane\"),$AC364,  $AB364),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR364=\"Agribusiness\", $AR364=\"Ag\",$AR364=\"Propane\", $AR364=\"Ag Propane\", $AR364=\"Ag-Propane\"),$AC364,  $AB364),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",26]
["Not Eligible","N-PS2196","Eligible Under AgV2","Variable Speed Drive Air Compressor replacing Non-VSD Compressor","N-PS2196: Variable Speed Drive Air Compressor replacing Non-VSD Compressor","Complete Table E1 and E2 of the \"Agribusiness Incentive Catalog Supplemental Data Sheet\" for this measure.","Submit manufacturer specification sheets and/or a CAGI sheet at anticipated operating pressure for items installed. ","Backup or redundant systems DNQ","Must be variable speed rotary vane compressor or variable speed screw compressor and operate a min of 2,000 hours annually","Limited to one VSD compressor per compressor air system","Replacing an old VSD compressor with a new (same size) VSD compressor DNQ. Replacement of an old VSD compressor with a new, larger VSD compr. is eligible for the increase in hp over the old compressor.  For example, if a 50 hp VSD compressor is replaced with a 75 hp VSD compressor, the 25 hp increase in capacity would be eligible for incentives.","Replaced equipment must be removed, if kept it must be used for emergency backup only.","This is for new VSD compressors only; adding a VSD to an existing compressor does not qualify. Replacing an old VSD compressor with a new VSD compressor does not qualify. Adding a VSD compressor to a system that already includes a VSD compressor does not qualify.",{"$nulls":8},"N/A","N/A",{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP","N/A",2196,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-PS2196: Variable Speed Drive Air Compressor replacing Non-VSD Compressor","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR365=\"Agribusiness\", $AR365=\"Ag\",$AR365=\"Propane\", $AR365=\"Ag Propane\", $AR365=\"Ag-Propane\"),$AC365,  $AB365),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR365=\"Agribusiness\", $AR365=\"Ag\",$AR365=\"Propane\", $AR365=\"Ag Propane\", $AR365=\"Ag-Propane\"),$AC365,  $AB365),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":500,"d":"500.00"}},"Agribusiness",26]
["Not Eligible","PS2254","Not Eligible","No Air-Loss Condensate Drains","PS2254: No Air-Loss Condensate Drains","Must be used in systems with load/no-load, variable speed, variable displacement or centrifugal compressors","Load/no-load system must have adequate storage for drains to be eligible.","Manual drains, lever-operated mechanical drains or solenoid drains are not eligible","The replacement drain must be “no air-loss,” meaning it must continuously measure the presence of condensate, purge it only when necessary and only long enough to prevent the unintentional purging of compressed air.","If no air-loss condensate drain is integral to another piece of equipment (i.e., is part of the air compressor, air dryer, mist eliminator, etc.), provide a manufacturer’s specification sheet to confirm.",{"$nulls":11},"N/A","N/A",{"v":130,"d":"$130.00"},"Drain",{"v":130,"d":"$130.00"},"Drain","N/A",2254,2254,"N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2254: No Air-Loss Condensate Drains","No","Yes","",{"v":1,"d":"1.00"},{"v":500,"d":"500.00"},"Agribusiness",26]
["Not Eligible","N-PS2254","Eligible Under AgV2","No Air-Loss Condensate Drains",{"$f":"IF(ISBLANK(A367),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C367,IF(FOEIncentCodeType=IncentCodeTypeAg,B367,A367))&\": \") &D367","v":"N-PS2254: No Air-Loss Condensate Drains"},"Must be used in systems with load/no-load, variable speed, variable displacement or centrifugal compressors","Load/no-load system must have adequate storage for drains to be eligible.","Manual drains, lever-operated mechanical drains or solenoid drains are not eligible","The replacement drain must be “no air-loss,” meaning it must continuously measure the presence of condensate, purge it only when necessary and only long enough to prevent the unintentional purging of compressed air.","If no air-loss condensate drain is integral to another piece of equipment (i.e., is part of the air compressor, air dryer, mist eliminator, etc.), provide a manufacturer’s specification sheet to confirm.",{"$nulls":11},"N/A","N/A",{"v":130,"d":"$130.00"},"Drain",{"v":130,"d":"$130.00"},"Drain","N/A",2254,2254,"N/A","yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-PS2254: No Air-Loss Condensate Drains","No","Yes","",{"v":1,"d":"1.00"},{"v":500,"d":"500.00"},"Agribusiness",26]
["Not Eligible","PS2257","Not Eligible","Compressed Air Heat Recovery","PS2257: Compressed Air Heat Recovery","For heat recovery to offset space heating from natural gas fired heating equip. Heat recovery to offset process heating DNQ (custom possible).","Heat recovery for redundant/backup air compressors DNQ. Replacing existing heat recovery and upgrading from manual control DNQ.","System must include automatic controls to switch from winter to summer operation. Systems w/ manual damper controls DNQ.","Invoice is sufficiently detailed to confirm installation of heat recovery system.","Incentive must be ≤ 50% of project cost, including equipment and external labor.","Project must result in est. net reduction BTUs consumed in facility to be eligible.","Static pressure in area where compressor/vacuum pump is enclosed must remain same.","If outside air is used in system, antifreeze protection must be considered.",{"$nulls":8},"N/A","N/A",{"v":75,"d":"$75.00"},"HP",{"$f":"X368","v":{"v":75,"d":"$75.00"}},"HP",2257,{"$f":"AB368","v":2257},2257,"Yes","See NC MMID","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS2257: Compressed Air Heat Recovery","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR368=\"Agribusiness\", $AR368=\"Ag\",$AR368=\"Propane\", $AR368=\"Ag Propane\", $AR368=\"Ag-Propane\"),$AC368,  $AB368),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR368=\"Agribusiness\", $AR368=\"Ag\",$AR368=\"Propane\", $AR368=\"Ag Propane\", $AR368=\"Ag-Propane\"),$AC368,  $AB368),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Agribusiness",26]
["Not Eligible","N-PS2257","Eligible Under AgV2","Compressed Air Heat Recovery","N-PS2257: Compressed Air Heat Recovery","For heat recovery to offset space heating from natural gas fired heating equip. Heat recovery to offset process heating DNQ (custom possible).","Heat recovery for redundant/backup air compressors DNQ. Replacing existing heat recovery and upgrading from manual control DNQ.","System must include automatic controls to switch from winter to summer operation. Systems w/ manual damper controls DNQ.","Invoice is sufficiently detailed to confirm installation of heat recovery system.","Incentive must be ≤ 50% of project cost, including equipment and external labor.","Project must result in est. net reduction BTUs consumed in facility to be eligible.","Static pressure in area where compressor/vacuum pump is enclosed must remain same.","If outside air is used in system, antifreeze protection must be considered.",{"$nulls":8},"N/A","N/A",{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",2257,2257,2257,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-PS2257: Compressed Air Heat Recovery","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR369=\"Agribusiness\", $AR369=\"Ag\",$AR369=\"Propane\", $AR369=\"Ag Propane\", $AR369=\"Ag-Propane\"),$AC369,  $AB369),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR369=\"Agribusiness\", $AR369=\"Ag\",$AR369=\"Propane\", $AR369=\"Ag Propane\", $AR369=\"Ag-Propane\"),$AC369,  $AB369),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Agribusiness",26]
["Not Eligible","PS3928","Not Eligible","Vacuum Pump Heat Recovery","PS3928: Vacuum Pump Heat Recovery","For heat recovery to offset space heating from natural gas fired heating equip. Heat recovery to offset process heating DNQ (custom possible).","Heat recovery for redundant/backup vacuum pumps DNQ. Replacing existing heat recovery and upgrading from manual control DNQ.","System must include automatic controls to switch from winter to summer operation. Systems w/ manual damper controls DNQ.","Invoice is sufficiently detailed to confirm installation of heat recovery system.","Incentive must be ≤ 50% of project cost, including equipment and external labor.","Project must result in est. net reduction BTUs consumed in facility to be eligible.","Static pressure in area where compressor/vacuum pump is enclosed must remain same.","If outside air is used in system, antifreeze protection must be considered.",{"$nulls":8},"N/A","N/A",{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",3928,3928,3928,"Yes","See NC MMID","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS3928: Vacuum Pump Heat Recovery","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR370=\"Agribusiness\", $AR370=\"Ag\",$AR370=\"Propane\", $AR370=\"Ag Propane\", $AR370=\"Ag-Propane\"),$AC370,  $AB370),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR370=\"Agribusiness\", $AR370=\"Ag\",$AR370=\"Propane\", $AR370=\"Ag Propane\", $AR370=\"Ag-Propane\"),$AC370,  $AB370),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Agribusiness",26]
["Not Eligible","N-PS3928","Eligible Under AgV2","Vacuum Pump Heat Recovery",{"$f":"IF(ISBLANK(A371),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C371,IF(FOEIncentCodeType=IncentCodeTypeAg,B371,A371))&\": \") &D371","v":"N-PS3928: Vacuum Pump Heat Recovery"},"For heat recovery to offset space heating from natural gas fired heating equip. Heat recovery to offset process heating DNQ (custom possible).","Heat recovery for redundant/backup vacuum pumps DNQ. Replacing existing heat recovery and upgrading from manual control DNQ.","System must include automatic controls to switch from winter to summer operation. Systems w/ manual damper controls DNQ.","Invoice is sufficiently detailed to confirm installation of heat recovery system.","Incentive must be ≤ 50% of project cost, including equipment and external labor.","Project must result in est. net reduction BTUs consumed in facility to be eligible.","Static pressure in area where compressor/vacuum pump is enclosed must remain same.","If outside air is used in system, antifreeze protection must be considered.",{"$nulls":8},"N/A","N/A",{"v":75,"d":"$75.00"},"HP",{"v":75,"d":"$75.00"},"HP",3928,3928,3928,"Yes","Yes","Yes",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-PS3928: Vacuum Pump Heat Recovery","No","Yes","HP",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR371=\"Agribusiness\", $AR371=\"Ag\",$AR371=\"Propane\", $AR371=\"Ag Propane\", $AR371=\"Ag-Propane\"),$AC371,  $AB371),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR371=\"Agribusiness\", $AR371=\"Ag\",$AR371=\"Propane\", $AR371=\"Ag Propane\", $AR371=\"Ag-Propane\"),$AC371,  $AB371),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Agribusiness",26]
["Not Eligible","PS2264","Not Eligible","Cycling or VFD-Controlled Refrigerated Air Dryer","PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer","Must be properly sized to meet the needs of the compressed air system","Must be cycling or VFD-controlled refrigerated dryers replacing non-cycling refrigeration air dryers","Replacement of desiccant, deliquescent, heat of compression, membrane, or other types of dryers DNQ","If air dryer is integral to antoher piece of equipment (i.e., part of the air compressor, provide a Mfg spec sheet for that piece of equip. to confirm that it includes a cycling or VFD controlled air dryer","Installation of controls to an existing air dryer is not eligible","Controls-based efficiency projects and/or replacement other dryer types may qualify custom incentive.",{"$nulls":10},"N/A","N/A",{"v":2,"d":"$2.00"},"CFM",{"v":2,"d":"$2.00"},"CFM",2264,2264,2264,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer","No","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR372=\"Agribusiness\", $AR372=\"Ag\",$AR372=\"Propane\", $AR372=\"Ag Propane\", $AR372=\"Ag-Propane\"),$AC372,  $AB372),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":50,"d":"50.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR372=\"Agribusiness\", $AR372=\"Ag\",$AR372=\"Propane\", $AR372=\"Ag Propane\", $AR372=\"Ag-Propane\"),$AC372,  $AB372),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":3000,"d":"3,000.00"}},"Agribusiness",27]
["Not Eligible","N-PS2264","Eligible Under AgV2","Cycling or VFD-Controlled Refrigerated Air Dryer",{"$f":"IF(ISBLANK(A373),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C373,IF(FOEIncentCodeType=IncentCodeTypeAg,B373,A373))&\": \") &D373","v":"N-PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer"},"Must be properly sized to meet the needs of the compressed air system","Must be cycling or VFD-controlled refrigerated dryers replacing non-cycling refrigeration air dryers","Replacement of desiccant, deliquescent, heat of compression, membrane, or other types of dryers DNQ","If air dryer is integral to antoher piece of equipment (i.e., part of the air compressor, provide a Mfg spec sheet for that piece of equip. to confirm that it includes a cycling or VFD controlled air dryer","Installation of controls to an existing air dryer is not eligible","Controls-based efficiency projects and/or replacement other dryer types may qualify custom incentive.",{"$nulls":10},"N/A","N/A",{"v":2,"d":"$2.00"},"CFM",{"v":2,"d":"$2.00"},"CFM",2264,2264,2264,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer","No","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR373=\"Agribusiness\", $AR373=\"Ag\",$AR373=\"Propane\", $AR373=\"Ag Propane\", $AR373=\"Ag-Propane\"),$AC373,  $AB373),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":50,"d":"50.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR373=\"Agribusiness\", $AR373=\"Ag\",$AR373=\"Propane\", $AR373=\"Ag Propane\", $AR373=\"Ag-Propane\"),$AC373,  $AB373),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":3000,"d":"3,000.00"}},"Agribusiness",27]
[{"$nulls":3},"----------------------AGRIBUSINESS CATALOG: COOLING & SPACE HEATING EQUIPMENT --------------------------------------------","----------------------AGRIBUSINESS CATALOG: COOLING & SPACE HEATING EQUIPMENT --------------------------------------------",null,"","","","","","","","Corresponding Propane MMID: AG4852","",{"$nulls":21},"No","----------------------AGRIBUSINESS CATALOG: COOLING & SPACE HEATING EQUIPMENT --------------------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR374=\"Agribusiness\", $AR374=\"Ag\",$AR374=\"Propane\", $AR374=\"Ag Propane\", $AR374=\"Ag-Propane\"),$AC374,  $AB374),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR374=\"Agribusiness\", $AR374=\"Ag\",$AR374=\"Propane\", $AR374=\"Ag Propane\", $AR374=\"Ag-Propane\"),$AC374,  $AB374),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","H5423","Eligible Under AgV2","16 SEER2 A/C Split System or Single Package, < 5.42 tons","H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 16 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":75,"d":"$75.00"},"A/C Unit",{"$f":"V375","v":{"v":75,"d":"$75.00"}},"A/C Unit",{"v":50,"d":"$50.00"},{"$f":"W375","v":"A/C Unit"},5423,{"$f":"AB375","v":5423},5423,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR375=\"Agribusiness\", $AR375=\"Ag\",$AR375=\"Propane\", $AR375=\"Ag Propane\", $AR375=\"Ag-Propane\"),$AC375,  $AB375),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR375=\"Agribusiness\", $AR375=\"Ag\",$AR375=\"Propane\", $AR375=\"Ag Propane\", $AR375=\"Ag-Propane\"),$AC375,  $AB375),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5424","Eligible Under AgV2","17 SEER2 A/C Split System or Single Package, < 5.42 tons","H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 17 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":100,"d":"$100.00"},"A/C Unit",{"v":100,"d":"$100.00"},"A/C Unit",{"v":75,"d":"$75.00"},"A/C Unit",5424,5424,5424,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR376=\"Agribusiness\", $AR376=\"Ag\",$AR376=\"Propane\", $AR376=\"Ag Propane\", $AR376=\"Ag-Propane\"),$AC376,  $AB376),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR376=\"Agribusiness\", $AR376=\"Ag\",$AR376=\"Propane\", $AR376=\"Ag Propane\", $AR376=\"Ag-Propane\"),$AC376,  $AB376),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5425","Eligible Under AgV2","18 SEER2 A/C Split System or Single Package, < 5.42 tons","H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 18 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":125,"d":"$125.00"},"A/C Unit",{"v":125,"d":"$125.00"},"A/C Unit",{"v":100,"d":"$100.00"},"A/C Unit",5425,5425,5425,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR377=\"Agribusiness\", $AR377=\"Ag\",$AR377=\"Propane\", $AR377=\"Ag Propane\", $AR377=\"Ag-Propane\"),$AC377,  $AB377),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR377=\"Agribusiness\", $AR377=\"Ag\",$AR377=\"Propane\", $AR377=\"Ag Propane\", $AR377=\"Ag-Propane\"),$AC377,  $AB377),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5426","Eligible Under AgV2","19 SEER2 A/C Split System or Single Package, < 5.42 tons","H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 19 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":175,"d":"$175.00"},"A/C Unit",{"v":175,"d":"$175.00"},"A/C Unit",{"v":125,"d":"$125.00"},"A/C Unit",5426,5426,5426,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR378=\"Agribusiness\", $AR378=\"Ag\",$AR378=\"Propane\", $AR378=\"Ag Propane\", $AR378=\"Ag-Propane\"),$AC378,  $AB378),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR378=\"Agribusiness\", $AR378=\"Ag\",$AR378=\"Propane\", $AR378=\"Ag Propane\", $AR378=\"Ag-Propane\"),$AC378,  $AB378),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5427","Eligible Under AgV2","20 SEER2 A/C Split System or Single Package, < 5.42 tons","H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 20 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":200,"d":"$200.00"},"A/C Unit",{"v":200,"d":"$200.00"},"A/C Unit",{"v":150,"d":"$150.00"},"A/C Unit",5427,5427,5427,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR379=\"Agribusiness\", $AR379=\"Ag\",$AR379=\"Propane\", $AR379=\"Ag Propane\", $AR379=\"Ag-Propane\"),$AC379,  $AB379),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR379=\"Agribusiness\", $AR379=\"Ag\",$AR379=\"Propane\", $AR379=\"Ag Propane\", $AR379=\"Ag-Propane\"),$AC379,  $AB379),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5428","Eligible Under AgV2","16 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons",{"$f":"IF(ISBLANK(A380),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C380,IF(FOEIncentCodeType=IncentCodeTypeAg,B380,A380))&\": \") &D380","v":"H5428: 16 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons"},"Must be ≥ 16 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":85,"d":"$85.00"},"A/C Unit",{"v":85,"d":"$85.00"},"A/C Unit",{"v":55,"d":"$55.00"},"A/C Unit",5423,5423,5423,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5428: 16 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR380=\"Agribusiness\", $AR380=\"Ag\",$AR380=\"Propane\", $AR380=\"Ag Propane\", $AR380=\"Ag-Propane\"),$AC380,  $AB380),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR380=\"Agribusiness\", $AR380=\"Ag\",$AR380=\"Propane\", $AR380=\"Ag Propane\", $AR380=\"Ag-Propane\"),$AC380,  $AB380),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5429","Eligible Under AgV2","17 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","H5429: 17 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 17 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":110,"d":"$110.00"},"A/C Unit",{"v":110,"d":"$110.00"},"A/C Unit",{"v":80,"d":"$80.00"},"A/C Unit",5424,5424,5424,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5429: 17 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR381=\"Agribusiness\", $AR381=\"Ag\",$AR381=\"Propane\", $AR381=\"Ag Propane\", $AR381=\"Ag-Propane\"),$AC381,  $AB381),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR381=\"Agribusiness\", $AR381=\"Ag\",$AR381=\"Propane\", $AR381=\"Ag Propane\", $AR381=\"Ag-Propane\"),$AC381,  $AB381),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5430","Eligible Under AgV2","18 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","H5430: 18 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 18 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":135,"d":"$135.00"},"A/C Unit",{"v":135,"d":"$135.00"},"A/C Unit",{"v":105,"d":"$105.00"},"A/C Unit",5425,5425,5425,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5430: 18 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR382=\"Agribusiness\", $AR382=\"Ag\",$AR382=\"Propane\", $AR382=\"Ag Propane\", $AR382=\"Ag-Propane\"),$AC382,  $AB382),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR382=\"Agribusiness\", $AR382=\"Ag\",$AR382=\"Propane\", $AR382=\"Ag Propane\", $AR382=\"Ag-Propane\"),$AC382,  $AB382),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5431","Eligible Under AgV2","19 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","H5431: 19 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 19 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":185,"d":"$185.00"},"A/C Unit",{"v":185,"d":"$185.00"},"A/C Unit",{"v":130,"d":"$130.00"},"A/C Unit",5426,5426,5426,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5431: 19 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR383=\"Agribusiness\", $AR383=\"Ag\",$AR383=\"Propane\", $AR383=\"Ag Propane\", $AR383=\"Ag-Propane\"),$AC383,  $AB383),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR383=\"Agribusiness\", $AR383=\"Ag\",$AR383=\"Propane\", $AR383=\"Ag Propane\", $AR383=\"Ag-Propane\"),$AC383,  $AB383),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H5432","Eligible Under AgV2","20 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","H5432: 20 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 20 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":210,"d":"$210.00"},"A/C Unit",{"v":210,"d":"$210.00"},"A/C Unit",{"v":155,"d":"$155.00"},"A/C Unit",5427,5427,5427,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","H5432: 20 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR384=\"Agribusiness\", $AR384=\"Ag\",$AR384=\"Propane\", $AR384=\"Ag Propane\", $AR384=\"Ag-Propane\"),$AC384,  $AB384),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR384=\"Agribusiness\", $AR384=\"Ag\",$AR384=\"Propane\", $AR384=\"Ag Propane\", $AR384=\"Ag-Propane\"),$AC384,  $AB384),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5423","N-H5423","16 SEER2 A/C Split System or Single Package, < 5.42 tons","N-H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 16 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":75,"d":"$75.00"},"A/C Unit",{"v":75,"d":"$75.00"},"A/C Unit",{"v":50,"d":"$50.00"},"A/C Unit",5423,5423,5423,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR385=\"Agribusiness\", $AR385=\"Ag\",$AR385=\"Propane\", $AR385=\"Ag Propane\", $AR385=\"Ag-Propane\"),$AC385,  $AB385),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR385=\"Agribusiness\", $AR385=\"Ag\",$AR385=\"Propane\", $AR385=\"Ag Propane\", $AR385=\"Ag-Propane\"),$AC385,  $AB385),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5424","N-H5424","17 SEER2 A/C Split System or Single Package, < 5.42 tons","N-H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 17 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":100,"d":"$100.00"},"A/C Unit",{"v":100,"d":"$100.00"},"A/C Unit",{"v":75,"d":"$75.00"},"A/C Unit",5424,5424,5424,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR386=\"Agribusiness\", $AR386=\"Ag\",$AR386=\"Propane\", $AR386=\"Ag Propane\", $AR386=\"Ag-Propane\"),$AC386,  $AB386),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR386=\"Agribusiness\", $AR386=\"Ag\",$AR386=\"Propane\", $AR386=\"Ag Propane\", $AR386=\"Ag-Propane\"),$AC386,  $AB386),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5425","N-H5425","18 SEER2 A/C Split System or Single Package, < 5.42 tons","N-H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 18 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":125,"d":"$125.00"},"A/C Unit",{"v":125,"d":"$125.00"},"A/C Unit",{"v":100,"d":"$100.00"},"A/C Unit",5425,5425,5425,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR387=\"Agribusiness\", $AR387=\"Ag\",$AR387=\"Propane\", $AR387=\"Ag Propane\", $AR387=\"Ag-Propane\"),$AC387,  $AB387),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR387=\"Agribusiness\", $AR387=\"Ag\",$AR387=\"Propane\", $AR387=\"Ag Propane\", $AR387=\"Ag-Propane\"),$AC387,  $AB387),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5426","N-H5426","19 SEER2 A/C Split System or Single Package, < 5.42 tons","N-H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 19 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":175,"d":"$175.00"},"A/C Unit",{"v":175,"d":"$175.00"},"A/C Unit",{"v":125,"d":"$125.00"},"A/C Unit",5426,5426,5426,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR388=\"Agribusiness\", $AR388=\"Ag\",$AR388=\"Propane\", $AR388=\"Ag Propane\", $AR388=\"Ag-Propane\"),$AC388,  $AB388),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR388=\"Agribusiness\", $AR388=\"Ag\",$AR388=\"Propane\", $AR388=\"Ag Propane\", $AR388=\"Ag-Propane\"),$AC388,  $AB388),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5427","N-H5427","20 SEER2 A/C Split System or Single Package, < 5.42 tons","N-H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 20 SEER2 and < 65 MBH (5.42 ton)","AHRI verified cooling capacity and SEER2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":200,"d":"$200.00"},"A/C Unit",{"v":200,"d":"$200.00"},"A/C Unit",{"v":150,"d":"$150.00"},"A/C Unit",5427,5427,5427,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR389=\"Agribusiness\", $AR389=\"Ag\",$AR389=\"Propane\", $AR389=\"Ag Propane\", $AR389=\"Ag-Propane\"),$AC389,  $AB389),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR389=\"Agribusiness\", $AR389=\"Ag\",$AR389=\"Propane\", $AR389=\"Ag Propane\", $AR389=\"Ag-Propane\"),$AC389,  $AB389),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5428","N-H5428","16 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons",{"$f":"IF(ISBLANK(A390),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C390,IF(FOEIncentCodeType=IncentCodeTypeAg,B390,A390))&\": \") &D390","v":"N-H5428: 16 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons"},"Must be ≥ 16 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":85,"d":"$85.00"},"A/C Unit",{"v":85,"d":"$85.00"},"A/C Unit",{"v":55,"d":"$55.00"},"A/C Unit",5423,5423,5423,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5428: 16 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR390=\"Agribusiness\", $AR390=\"Ag\",$AR390=\"Propane\", $AR390=\"Ag Propane\", $AR390=\"Ag-Propane\"),$AC390,  $AB390),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR390=\"Agribusiness\", $AR390=\"Ag\",$AR390=\"Propane\", $AR390=\"Ag Propane\", $AR390=\"Ag-Propane\"),$AC390,  $AB390),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5429","N-H5429","17 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","N-H5429: 17 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 17 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":110,"d":"$110.00"},"A/C Unit",{"$f":"V391","v":{"v":110,"d":"$110.00"}},"A/C Unit",{"v":80,"d":"$80.00"},"A/C Unit",5424,5424,5424,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5429: 17 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR391=\"Agribusiness\", $AR391=\"Ag\",$AR391=\"Propane\", $AR391=\"Ag Propane\", $AR391=\"Ag-Propane\"),$AC391,  $AB391),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR391=\"Agribusiness\", $AR391=\"Ag\",$AR391=\"Propane\", $AR391=\"Ag Propane\", $AR391=\"Ag-Propane\"),$AC391,  $AB391),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5430","N-H5430","18 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","N-H5430: 18 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 18 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":135,"d":"$135.00"},"A/C Unit",{"v":135,"d":"$135.00"},"A/C Unit",{"v":105,"d":"$105.00"},"A/C Unit",5425,5425,5425,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5430: 18 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR392=\"Agribusiness\", $AR392=\"Ag\",$AR392=\"Propane\", $AR392=\"Ag Propane\", $AR392=\"Ag-Propane\"),$AC392,  $AB392),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR392=\"Agribusiness\", $AR392=\"Ag\",$AR392=\"Propane\", $AR392=\"Ag Propane\", $AR392=\"Ag-Propane\"),$AC392,  $AB392),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5431","N-H5431","19 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","N-H5431: 19 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 19 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":185,"d":"$185.00"},"A/C Unit",{"v":185,"d":"$185.00"},"A/C Unit",{"v":130,"d":"$130.00"},"A/C Unit",5426,5426,5426,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5431: 19 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR393=\"Agribusiness\", $AR393=\"Ag\",$AR393=\"Propane\", $AR393=\"Ag Propane\", $AR393=\"Ag-Propane\"),$AC393,  $AB393),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR393=\"Agribusiness\", $AR393=\"Ag\",$AR393=\"Propane\", $AR393=\"Ag Propane\", $AR393=\"Ag-Propane\"),$AC393,  $AB393),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","N-H5432","N-H5432","20 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","N-H5432: 20 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","Must be ≥ 20 SEER2, < 65 MBH (5.42 ton), & ≥ 8.5 HSPF2","AHRI verified cooling capacity, SEER2, & HSPF2 will be used to calculate the incentive.","Systems qualified in the following AHRI Directories are eligible: 'Air Conditioners and Air Conditioner Coils', 'Heat Pumps', ‘Variable-Speed Mini-Split and Multi-Split Heat Pumps’ and 'Variable-Speed Mini-Split and Multi-Split Air Conditioners' (see ahridirectory.org)","Incentives are for standard HVAC applications only. Rooftop units and split sytem A/C used for industrial process cooling, ice rinks and refrigerated warehouses may qualify for a custom incentive","Unit of Measure question asks for # of Tons. Qty will be number of A/C units.","When used in data centers, rooftop units and split system air conditioners < 5.42 tons are eligible if they are AHRI listed.",{"$nulls":3},"AHRI will list the cooling capacity in Btuh. Need to divide by 12,000 to convert to tons. SHOW THIS CONVERSION RIGHT ON THE AHRI CERT. Do NOT round. If system wasn't tested as complete condensing unit and coil, EA/TR should request a model of the combined system at AHRI conditions to verify min efficiency requirements are met.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":210,"d":"$210.00"},"A/C Unit",{"v":210,"d":"$210.00"},"A/C Unit",{"v":155,"d":"$155.00"},"A/C Unit",5427,5427,5427,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"Yes","N-H5432: 20 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons","No","Yes","Tons",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR394=\"Agribusiness\", $AR394=\"Ag\",$AR394=\"Propane\", $AR394=\"Ag Propane\", $AR394=\"Ag-Propane\"),$AC394,  $AB394),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.5,"d":"0.50"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR394=\"Agribusiness\", $AR394=\"Ag\",$AR394=\"Propane\", $AR394=\"Ag Propane\", $AR394=\"Ag-Propane\"),$AC394,  $AB394),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":5.416666666666667,"d":"5.42"}},"Agribusiness",28]
["Not Eligible","H2422","Not Eligible","Infrared Heater (Retrofit Only)",{"$f":"IF(ISBLANK(A395),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C395,IF(FOEIncentCodeType=IncentCodeTypeAg,B395,A395))&\": \") &D395","v":"H2422: Infrared Heater (Retrofit Only)"},"Must have electronic ignition","Low-intensity and high-intensity units are eligible","Outdoor patio heating applications not eligible","Must be vented per manufacturer's specs","Low-intensity heaters must use outside non-conditioned combustion air","Replacement of existing infrared heater DNQ",null,null,"Corresponding Propane MMID: AG4854",null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":7.5,"d":"$7.50"},"MBh",{"v":7.5,"d":"$7.50"},{"$f":"Y395","v":"MBh"},"N/A",2422,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A395),\"\",IF(A395<>\"Not Eligible\",A395,IF(B395<>\"Not Eligible\",B395,C395))&\": \") &D395","v":"H2422: Infrared Heater (Retrofit Only)"},"No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR395=\"Agribusiness\", $AR395=\"Ag\",$AR395=\"Propane\", $AR395=\"Ag Propane\", $AR395=\"Ag-Propane\"),$AC395,  $AB395),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR395=\"Agribusiness\", $AR395=\"Ag\",$AR395=\"Propane\", $AR395=\"Ag Propane\", $AR395=\"Ag-Propane\"),$AC395,  $AB395),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Agribusiness",29]
["Not Eligible","N-H2422","Eligible Under AgV2","Infrared Heater (NC Only)",{"$f":"IF(ISBLANK(A396),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C396,IF(FOEIncentCodeType=IncentCodeTypeAg,B396,A396))&\": \") &D396","v":"N-H2422: Infrared Heater (NC Only)"},"Must have electronic ignition","Low-intensity and high-intensity units are eligible","Outdoor patio heating applications not eligible","Must be vented per manufacturer's specs","Low-intensity heaters must use outside non-conditioned combustion air","Replacement of existing infrared heater DNQ",null,null,"Corresponding Propane MMID: N-AG4854",null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":6,"d":"$6.00"},"MBh",{"v":6,"d":"$6.00"},{"$f":"Y396","v":"MBh"},"N/A",2422,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A396),\"\",IF(A396<>\"Not Eligible\",A396,IF(B396<>\"Not Eligible\",B396,C396))&\": \") &D396","v":"N-H2422: Infrared Heater (NC Only)"},"No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR396=\"Agribusiness\", $AR396=\"Ag\",$AR396=\"Propane\", $AR396=\"Ag Propane\", $AR396=\"Ag-Propane\"),$AC396,  $AB396),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR396=\"Agribusiness\", $AR396=\"Ag\",$AR396=\"Propane\", $AR396=\"Ag Propane\", $AR396=\"Ag-Propane\"),$AC396,  $AB396),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Agribusiness",29]
["Not Eligible","H2218","Not Eligible","Hot Water Boilers, < 300 MBh input, ≥90% AFUE","H2218: Hot Water Boilers, < 300 MBh input, ≥90% AFUE","Must be ≤ 300 MBh input and condensing boilers must modulate their firing rate and include outdoor-air reset control","Must be sealed combustion unit and ≥ 90% AFUE","Boiler incentives are only available for equipment used in space heating applications. Boilers used for only domestic hot water heating and industrial or process heating are not eligible for this incentive but may qualify for a Domestic Hot Water (DHW) or custom incentive. ","Space heating boilers also used for DHW may be eligible for indirect DHW incentives but are subject to requirments. In plant systems, boilers are eligible for incentives for their primary use only. A boiler replacing a space heating and indirect DHW system will use the capacity of the existing space heating and DHW systems to estimate the split of incentives. Boilers that only serve DHW are not eligible for the space heating incentives","≥90% AFUE or thermal efficiency boilers: If the heating system configuration is such that the boiler needs to operate at a high hot water temperature which prevents the flue gases from condensing, then the boiler is not eligible for H2218 or H3276.","Boiler efficiency will be verified using the AHRI database. If the boiler is not listed in the AHRI database, provide a boiler spec sheet with boiler input and output ratings and either AFUE or thermal efficiency as appropriate for boiler size",null,"Do not round AHRI capacity to a whole number.","Corresponding Propane MMID: AG4852",null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":7,"d":"$7.00"},"MBh",{"v":7,"d":"$7.00"},{"$f":"Y397","v":"MBh"},"N/A",2218,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H2218: Hot Water Boilers, < 300 MBh input, ≥90% AFUE","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR397=\"Agribusiness\", $AR397=\"Ag\",$AR397=\"Propane\", $AR397=\"Ag Propane\", $AR397=\"Ag-Propane\"),$AC397,  $AB397),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR397=\"Agribusiness\", $AR397=\"Ag\",$AR397=\"Propane\", $AR397=\"Ag Propane\", $AR397=\"Ag-Propane\"),$AC397,  $AB397),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Agribusiness",29]
["Not Eligible","H10222","Not Eligible","Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","Must be ≥ 90 and <95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,null,"See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","MBh",{"v":7,"d":"$7.00"},{"$f":"W398","v":"MBh"},{"v":7,"d":"$7.00"},{"$f":"W398","v":"MBh"},3276,{"$f":"AB398","v":3276},3276,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR398=\"Agribusiness\", $AR398=\"Ag\",$AR398=\"Propane\", $AR398=\"Ag Propane\", $AR398=\"Ag-Propane\"),$AC398,  $AB398),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR398=\"Agribusiness\", $AR398=\"Ag\",$AR398=\"Propane\", $AR398=\"Ag Propane\", $AR398=\"Ag-Propane\"),$AC398,  $AB398),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"Agribusiness",29]
["Not Eligible","H10207","Not Eligible","Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","Must be ≥ 95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,null,"See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","MBh",{"v":8,"d":"$8.00"},"MBh",{"v":8,"d":"$8.00"},"MBh",3276,3276,3276,"Yes","See NC MMID","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR399=\"Agribusiness\", $AR399=\"Ag\",$AR399=\"Propane\", $AR399=\"Ag Propane\", $AR399=\"Ag-Propane\"),$AC399,  $AB399),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR399=\"Agribusiness\", $AR399=\"Ag\",$AR399=\"Propane\", $AR399=\"Ag Propane\", $AR399=\"Ag-Propane\"),$AC399,  $AB399),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"Agribusiness",29]
["Not Eligible","N-H2218","Eligible Under AgV2","Hot Water Boilers, < 300 MBh input, ≥90% AFUE","N-H2218: Hot Water Boilers, < 300 MBh input, ≥90% AFUE","Must be ≤ 300 MBh input and condensing boilers must modulate their firing rate and include outdoor-air reset control","Must be sealed combustion unit and ≥ 90% AFUE","Boiler incentives are only available for equipment used in space heating applications. Boilers used for only domestic hot water heating and industrial or process heating are not eligible for this incentive but may qualify for a Domestic Hot Water (DHW) or custom incentive. ","Space heating boilers also used for DHW may be eligible for indirect DHW incentives but are subject to requirments. In plant systems, boilers are eligible for incentives for their primary use only. A boiler replacing a space heating and indirect DHW system will use the capacity of the existing space heating and DHW systems to estimate the split of incentives. Boilers that only serve DHW are not eligible for the space heating incentives","≥90% AFUE or thermal efficiency boilers: If the heating system configuration is such that the boiler needs to operate at a high hot water temperature which prevents the flue gases from condensing, then the boiler is not eligible for H2218 or H3276.","Boiler efficiency will be verified using the AHRI database. If the boiler is not listed in the AHRI database, provide a boiler spec sheet with boiler input and output ratings and either AFUE or thermal efficiency as appropriate for boiler size",null,"Do not round AHRI capacity to a whole number.","Corresponding Propane MMID: N-AG4852",null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":7,"d":"$7.00"},"MBh",{"v":7,"d":"$7.00"},"MBh","N/A",2218,2218,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H2218: Hot Water Boilers, < 300 MBh input, ≥90% AFUE","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR400=\"Agribusiness\", $AR400=\"Ag\",$AR400=\"Propane\", $AR400=\"Ag Propane\", $AR400=\"Ag-Propane\"),$AC400,  $AB400),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":15,"d":"15.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR400=\"Agribusiness\", $AR400=\"Ag\",$AR400=\"Propane\", $AR400=\"Ag Propane\", $AR400=\"Ag-Propane\"),$AC400,  $AB400),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Agribusiness",29]
["Not Eligible","N-H10222","Eligible Under AgV3","Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency",{"$f":"IF(ISBLANK(A401),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C401,IF(FOEIncentCodeType=IncentCodeTypeAg,B401,A401))&\": \") &D401","v":"N-H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency"},"Must be ≥ 90 and <95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,null,"See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","MBh",{"v":7,"d":"$7.00"},{"$f":"W401","v":"MBh"},{"v":7,"d":"$7.00"},{"$f":"W401","v":"MBh"},3276,{"$f":"AB401","v":3276},3276,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR401=\"Agribusiness\", $AR401=\"Ag\",$AR401=\"Propane\", $AR401=\"Ag Propane\", $AR401=\"Ag-Propane\"),$AC401,  $AB401),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR401=\"Agribusiness\", $AR401=\"Ag\",$AR401=\"Propane\", $AR401=\"Ag Propane\", $AR401=\"Ag-Propane\"),$AC401,  $AB401),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"Agribusiness",29]
["Not Eligible","N-H10207","Eligible Under AgV4","Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","N-H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","Must be ≥ 95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,null,"See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","MBh",{"v":8,"d":"$8.00"},"MBh",{"v":8,"d":"$8.00"},"MBh",3276,3276,3276,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR402=\"Agribusiness\", $AR402=\"Ag\",$AR402=\"Propane\", $AR402=\"Ag Propane\", $AR402=\"Ag-Propane\"),$AC402,  $AB402),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR402=\"Agribusiness\", $AR402=\"Ag\",$AR402=\"Propane\", $AR402=\"Ag Propane\", $AR402=\"Ag-Propane\"),$AC402,  $AB402),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"Agribusiness",29]
["Not Eligible","H3491","Not Eligible","Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG","H3491: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG","Must be ≥ 95% AFUE","Eligibility for furnace and single package vertical unit measures is based on customer having both an eligible electric and natural gas provider","Furnaces and single package vertical unit must meet the minimum efficiency requirements listed and be a sealed combustion unit. Efficiency ratings will be verified using the AHRI database.","Furnaces and single package vertical units must have a single speed, multi-speed, or variable speed electronically communicated motor (ECM). Permanent split capacitor (PSC) motors are not eligible. Air handlers with an ECM are not eligible.","Provide a manufacturer's spec sheet to document the required features","Must provide INPUT capacity of furnace or single package vertical units in MBh in Section 6 on the Incentive Application","Furnaces must have a multi-stage burner and have at least two firing stages","Furnaces listed on the Focus on Energy residential furnace qualified products list does not guarantee the furnace has all features required for agribusiness incentives","Corresponding Propane MMID: AG4870","Do not lump various sized furnaces when entering measure. Ok to lump same size (capacity in MBh) furnaces.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":420,"d":"$420.00"},"Furnace",{"v":420,"d":"$420.00"},"Furnace","N/A",3491,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3491: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR403=\"Agribusiness\", $AR403=\"Ag\",$AR403=\"Propane\", $AR403=\"Ag Propane\", $AR403=\"Ag-Propane\"),$AC403,  $AB403),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":40,"d":"40.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR403=\"Agribusiness\", $AR403=\"Ag\",$AR403=\"Propane\", $AR403=\"Ag Propane\", $AR403=\"Ag-Propane\"),$AC403,  $AB403),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"Agribusiness",30]
["Not Eligible","H3492","Not Eligible","Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG","H3492: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG","Must be ≥ 90% AFUE","Eligibility for furnace and single package vertical unit measures is based on customer having both an eligible electric and natural gas provider","Furnaces and single package vertical unit must meet the minimum efficiency requirements listed and be a sealed combustion unit. Efficiency ratings will be verified using the AHRI database.","Furnaces and single package vertical units must have a single speed, multi-speed, or variable speed electronically communicated motor (ECM). Permanent split capacitor (PSC) motors are not eligible. Air handlers with an ECM are not eligible.","Provide a manufacturer's spec sheet to document the required features","Must provide INPUT capacity of furnace or single package vertical units in MBh in Section 6 on the Incentive Application","Furnaces must have a multi-stage burner and have at least two firing stages","Furnaces listed on the Focus on Energy residential furnace qualified products list does not guarantee the furnace has all features required for agribusiness incentives","Corresponding Propane MMID: AG4869","Do not lump various sized furnaces when entering measure. Ok to lump same size (capacity in MBh) furnaces.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":200,"d":"$200.00"},"Furnace",{"v":200,"d":"$200.00"},"Furnace","N/A",3492,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H3492: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR404=\"Agribusiness\", $AR404=\"Ag\",$AR404=\"Propane\", $AR404=\"Ag Propane\", $AR404=\"Ag-Propane\"),$AC404,  $AB404),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":40,"d":"40.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR404=\"Agribusiness\", $AR404=\"Ag\",$AR404=\"Propane\", $AR404=\"Ag Propane\", $AR404=\"Ag-Propane\"),$AC404,  $AB404),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"Agribusiness",30]
["Not Eligible","N-H3491","Eligible Under AgV2","Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG","N-H3491: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG","Must be ≥ 95% AFUE","Eligibility for furnace and single package vertical unit measures is based on customer having both an eligible electric and natural gas provider","Furnaces and single package vertical unit must meet the minimum efficiency requirements listed and be a sealed combustion unit. Efficiency ratings will be verified using the AHRI database.","Furnaces and single package vertical units must have a single speed, multi-speed, or variable speed electronically communicated motor (ECM). Permanent split capacitor (PSC) motors are not eligible. Air handlers with an ECM are not eligible.","Provide a manufacturer's spec sheet to document the required features","Must provide INPUT capacity of furnace or single package vertical units in MBh in Section 6 on the Incentive Application","Furnaces must have a multi-stage burner and have at least two firing stages","Furnaces listed on the Focus on Energy residential furnace qualified products list does not guarantee the furnace has all features required for agribusiness incentives","Corresponding Propane MMID: N-AG4870","Do not lump various sized furnaces when entering measure. Ok to lump same size (capacity in MBh) furnaces.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":320,"d":"$320.00"},"Furnace",{"v":320,"d":"$320.00"},"Furnace","N/A",3491,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H3491: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR405=\"Agribusiness\", $AR405=\"Ag\",$AR405=\"Propane\", $AR405=\"Ag Propane\", $AR405=\"Ag-Propane\"),$AC405,  $AB405),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":40,"d":"40.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR405=\"Agribusiness\", $AR405=\"Ag\",$AR405=\"Propane\", $AR405=\"Ag Propane\", $AR405=\"Ag-Propane\"),$AC405,  $AB405),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"Agribusiness",30]
["Not Eligible","N-H3492","Eligible Under AgV2","Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG","N-H3492: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG","Must be ≥ 90% AFUE","Eligibility for furnace and single package vertical unit measures is based on customer having both an eligible electric and natural gas provider","Furnaces and single package vertical unit must meet the minimum efficiency requirements listed and be a sealed combustion unit. Efficiency ratings will be verified using the AHRI database.","Furnaces and single package vertical units must have a single speed, multi-speed, or variable speed electronically communicated motor (ECM). Permanent split capacitor (PSC) motors are not eligible. Air handlers with an ECM are not eligible.","Provide a manufacturer's spec sheet to document the required features","Must provide INPUT capacity of furnace or single package vertical units in MBh in Section 6 on the Incentive Application","Furnaces must have a multi-stage burner and have at least two firing stages","Furnaces listed on the Focus on Energy residential furnace qualified products list does not guarantee the furnace has all features required for agribusiness incentives","Corresponding Propane MMID: N-AG4869","Do not lump various sized furnaces when entering measure. Ok to lump same size (capacity in MBh) furnaces.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":150,"d":"$150.00"},"Furnace",{"v":150,"d":"$150.00"},"Furnace","N/A",3492,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H3492: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR406=\"Agribusiness\", $AR406=\"Ag\",$AR406=\"Propane\", $AR406=\"Ag Propane\", $AR406=\"Ag-Propane\"),$AC406,  $AB406),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":40,"d":"40.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR406=\"Agribusiness\", $AR406=\"Ag\",$AR406=\"Propane\", $AR406=\"Ag Propane\", $AR406=\"Ag-Propane\"),$AC406,  $AB406),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":150,"d":"150.00"}},"Agribusiness",30]
["Not Eligible","H5436","Not Eligible","Unit Heater, ≥90% Thermal Efficiency","H5436: Unit Heater, ≥90% Thermal Efficiency","Unit heater must be an upgrade from a standard efficiency (typically 80%-84% thermal efficiency) unit heater","Steam or hot water coils/systems are not eligible. Natural gas fired only.","Must be vented and condensate drained per manufacturer specifications","Direct fired rooftop units/make-up air units are not eligible for this incentive.","Must replace an existing non-condensing unit heater or be installed instead of a non-condensing unit heater.","Provide a manufacturer’s specification sheet to document the features and efficiency level of the unit heater, including input capacity in MBh.",null,null,"Corresponding Propane MMID: AG5437",{"$nulls":7},"N/A","N/A",{"v":4,"d":"$4.00"},"MBh",{"v":4,"d":"$4.00"},"MBh","N/A",5436,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A407),\"\",IF(A407<>\"Not Eligible\",A407,IF(B407<>\"Not Eligible\",B407,C407))&\": \") &D407","v":"H5436: Unit Heater, ≥90% Thermal Efficiency"},"No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR407=\"Agribusiness\", $AR407=\"Ag\",$AR407=\"Propane\", $AR407=\"Ag Propane\", $AR407=\"Ag-Propane\"),$AC407,  $AB407),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":50,"d":"50.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR407=\"Agribusiness\", $AR407=\"Ag\",$AR407=\"Propane\", $AR407=\"Ag Propane\", $AR407=\"Ag-Propane\"),$AC407,  $AB407),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":400,"d":"400.00"}},"Agribusiness",29]
["Not Eligible","N-H5436","Eligible Under AgV2","Unit Heater, ≥90% Thermal Efficiency","N-H5436: Unit Heater, ≥90% Thermal Efficiency","Unit heater must be an upgrade from a standard efficiency (typically 80%-84% thermal efficiency) unit heater","Steam or hot water coils/systems are not eligible. Natural gas fired only.","Must be vented and condensate drained per manufacturer specifications","Direct fired rooftop units/make-up air units are not eligible for this incentive.","Must replace an existing non-condensing unit heater or be installed instead of a non-condensing unit heater.","Provide a manufacturer’s specification sheet to document the features and efficiency level of the unit heater, including input capacity in MBh.",null,null,"Corresponding Propane MMID: N-AG5437",{"$nulls":7},"N/A","N/A",{"v":2.75,"d":"$2.75"},"MBh",{"v":2.75,"d":"$2.75"},"MBh","N/A",5436,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H5436: Unit Heater, ≥90% Thermal Efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR408=\"Agribusiness\", $AR408=\"Ag\",$AR408=\"Propane\", $AR408=\"Ag Propane\", $AR408=\"Ag-Propane\"),$AC408,  $AB408),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":50,"d":"50.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR408=\"Agribusiness\", $AR408=\"Ag\",$AR408=\"Propane\", $AR408=\"Ag Propane\", $AR408=\"Ag-Propane\"),$AC408,  $AB408),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":400,"d":"400.00"}},"Agribusiness",29]
["Not Eligible","H5081","Not Eligible","Direct Fired Make-up Air Unit, Constant Volume (NG or Propane)","H5081: Direct Fired Make-up Air Unit, Constant Volume (NG or Propane)","Complete Table F1 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","Incentive is available for upgrading (or installing instead of) indirect fired make-up air units or rooftop units which are approximately 80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible.","Replacement of electric or hydronically heated make-up air is not eligible.","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements.","Must serve an occupied space for at least 500 hours per year.",null,"Corresponding Propane MMID: AG5407",{"$nulls":7},"N/A","N/A",{"v":0.4,"d":"$0.40"},"CFM",{"v":0.4,"d":"$0.40"},"CFM","N/A",5081,5081,"N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H5081: Direct Fired Make-up Air Unit, Constant Volume (NG or Propane)","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR409=\"Agribusiness\", $AR409=\"Ag\",$AR409=\"Propane\", $AR409=\"Ag Propane\", $AR409=\"Ag-Propane\"),$AC409,  $AB409),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR409=\"Agribusiness\", $AR409=\"Ag\",$AR409=\"Propane\", $AR409=\"Ag Propane\", $AR409=\"Ag-Propane\"),$AC409,  $AB409),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness",30]
["Not Eligible","N-H5081","Eligible Under AgV2","Direct Fired Make-up Air Unit, Constant Volume (NG or Propane)","N-H5081: Direct Fired Make-up Air Unit, Constant Volume (NG or Propane)","Complete Table F1 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","Incentive is available for upgrading (or installing instead of) indirect fired make-up air units or rooftop units which are approximately 80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible.","Replacement of electric or hydronically heated make-up air is not eligible.","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements.","Must serve an occupied space for at least 500 hours per year.",null,"Corresponding Propane MMID: N-AG5407",{"$nulls":7},"N/A","N/A",{"v":0.3,"d":"$0.30"},"CFM",{"v":0.3,"d":"$0.30"},"CFM","N/A",5081,5081,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H5081: Direct Fired Make-up Air Unit, Constant Volume (NG or Propane)","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR410=\"Agribusiness\", $AR410=\"Ag\",$AR410=\"Propane\", $AR410=\"Ag Propane\", $AR410=\"Ag-Propane\"),$AC410,  $AB410),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":100,"d":"100.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR410=\"Agribusiness\", $AR410=\"Ag\",$AR410=\"Propane\", $AR410=\"Ag Propane\", $AR410=\"Ag-Propane\"),$AC410,  $AB410),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness",30]
["Not Eligible","H10030","Not Eligible","Direct Fired Make-up Air Unit, Variable Air Volume (NG or Propane)",{"$f":"IF(ISBLANK(A411),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C411,IF(FOEIncentCodeType=IncentCodeTypeAg,B411,A411))&\": \") &D411","v":"H10030: Direct Fired Make-up Air Unit, Variable Air Volume (NG or Propane)"},"Complete Table F2 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible. ","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":0.65,"d":"$0.65"},"CFM",{"v":0.65,"d":"$0.65"},"CFM","N/A",10030,10030,"N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10030: Direct Fired Make-up Air Unit, Variable Air Volume (NG or Propane)","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR411=\"Agribusiness\", $AR411=\"Ag\",$AR411=\"Propane\", $AR411=\"Ag Propane\", $AR411=\"Ag-Propane\"),$AC411,  $AB411),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":800,"d":"800.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR411=\"Agribusiness\", $AR411=\"Ag\",$AR411=\"Propane\", $AR411=\"Ag Propane\", $AR411=\"Ag-Propane\"),$AC411,  $AB411),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness",30]
["Not Eligible","N-H10030","Eligible Under AgV2","Direct Fired Make-up Air Unit, Variable Air Volume (NG or Propane)","N-H10030: Direct Fired Make-up Air Unit, Variable Air Volume (NG or Propane)","Complete Table F2 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible. ","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":0.4,"d":"$0.40"},"CFM",{"v":0.4,"d":"$0.40"},"CFM","N/A",10030,10030,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H10030: Direct Fired Make-up Air Unit, Variable Air Volume (NG or Propane)","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR412=\"Agribusiness\", $AR412=\"Ag\",$AR412=\"Propane\", $AR412=\"Ag Propane\", $AR412=\"Ag-Propane\"),$AC412,  $AB412),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":800,"d":"800.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR412=\"Agribusiness\", $AR412=\"Ag\",$AR412=\"Propane\", $AR412=\"Ag Propane\", $AR412=\"Ag-Propane\"),$AC412,  $AB412),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness",30]
["Not Eligible","H10445","Eligible Under AgV3","Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","H10445: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","Complete Table F2 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.","Cannot be combined with VFD incentives.",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":0.25,"d":"$0.25"},"CFM",{"v":0.25,"d":"$0.25"},"CFM","N/A",10445,10445,"N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10445: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","Yes","Yes","CFM",{"v":100,"d":"100.00"},{"v":50000,"d":"50,000.00"},"Agribusiness",30]
["Not Eligible","N-H10445","Eligible Under AgV2","Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)",{"$f":"IF(ISBLANK(A414),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C414,IF(FOEIncentCodeType=IncentCodeTypeAg,B414,A414))&\": \") &D414","v":"N-H10445: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)"},"Complete Table F2 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.","Cannot be combined with VFD incentives.",{"$nulls":3},"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":0.2,"d":"$0.20"},"CFM",{"v":0.2,"d":"$0.20"},"CFM","N/A",10445,10445,"N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H10445: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","Yes","Yes","CFM",{"v":100,"d":"100.00"},{"v":50000,"d":"50,000.00"},"Agribusiness",30]
[{"$nulls":3},"----------------------AGRIBUSINESS CATALOG: WATER HEATING EQUIPMENT  --------------------------------------------","----------------------AGRIBUSINESS CATALOG: WATER HEATING EQUIPMENT  --------------------------------------------","","","","","","","","","","",{"$nulls":21},"No","----------------------AGRIBUSINESS CATALOG: WATER HEATING EQUIPMENT  --------------------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR415=\"Agribusiness\", $AR415=\"Ag\",$AR415=\"Propane\", $AR415=\"Ag Propane\", $AR415=\"Ag-Propane\"),$AC415,  $AB415),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR415=\"Agribusiness\", $AR415=\"Ag\",$AR415=\"Propane\", $AR415=\"Ag Propane\", $AR415=\"Ag-Propane\"),$AC415,  $AB415),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG10032","Eligible Under AgV2","Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)","AG10032: Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)","Include the number of milking cows in Section 6 on the application.","RHR unit must be used to extract waste heat from the dairy's milk refrigeration system in order to preheat water to serve the dairy's water heater unit.","RHR units with heating element are NOT eligible","Facilities water heater(s) must be fueled by electricity or natural gas","Replacement, redundant or back-up units do not qualify.","Size (gallons) of RHR unit must be included on invoice","Incentive must be ≤100% project cost.",null,"Corresponding Propane MMID: AG10034","Create Calc Activity for Tech Review  to determine savings. VFD and/or plate cooler may be existing or installed at same time as RHR. If multiple RHRs installed, enter total # of cows for Unit of Measure Question. Do not divide the total # of cows by the number of RHRs.",{"$nulls":6},"N/A","N/A",{"v":1250,"d":"$1,250.00"},"RHR Unit",{"v":1250,"d":"$1,250.00"},{"$f":"Y416","v":"RHR Unit"},"N/A",10032,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG10032: Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR416=\"Agribusiness\", $AR416=\"Ag\",$AR416=\"Propane\", $AR416=\"Ag Propane\", $AR416=\"Ag-Propane\"),$AC416,  $AB416),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR416=\"Agribusiness\", $AR416=\"Ag\",$AR416=\"Propane\", $AR416=\"Ag Propane\", $AR416=\"Ag-Propane\"),$AC416,  $AB416),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",31]
["Not Eligible","AG10033","Eligible Under AgV2","Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)","AG10033: Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)","Include the number of milking cows in Section 6 on the application.","RHR unit must be used to extract waste heat from the dairy's milk refrigeration system in order to preheat water to serve the dairy's water heater unit.","RHR units with heating element are NOT eligible","Facilities water heater(s) must be fueled by electricity or natural gas","Replacement, redundant or back-up units do not qualify.","Size (gallons) of RHR unit must be included on invoice","Incentive must be ≤100% project cost.",null,null,"Create Calc Activity for Tech Review  to determine savings. VFD and/or plate cooler may be existing or installed at same time as RHR. If multiple RHRs installed, enter total # of cows for Unit of Measure Question. Do not divide the total # of cows by the number of RHRs.",{"$nulls":6},"N/A","N/A",{"v":1250,"d":"$1,250.00"},"RHR Unit",{"v":1250,"d":"$1,250.00"},"RHR Unit","N/A",10033,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG10033: Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR417=\"Agribusiness\", $AR417=\"Ag\",$AR417=\"Propane\", $AR417=\"Ag Propane\", $AR417=\"Ag-Propane\"),$AC417,  $AB417),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR417=\"Agribusiness\", $AR417=\"Ag\",$AR417=\"Propane\", $AR417=\"Ag Propane\", $AR417=\"Ag-Propane\"),$AC417,  $AB417),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",31]
["Not Eligible","N-AG10032","Eligible Under AgV2","Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)","N-AG10032: Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)","Include the number of milking cows in Section 6 on the application.","RHR unit must be used to extract waste heat from the dairy's milk refrigeration system in order to preheat water to serve the dairy's water heater unit.","RHR units with heating element are NOT eligible","Facilities water heater(s) must be fueled by electricity or natural gas","Replacement, redundant or back-up units do not qualify.","Size (gallons) of RHR unit must be included on invoice","Incentive must be ≤100% project cost.",null,"Corresponding Propane MMID: N-AG10034","Create Calc Activity for Tech Review  to determine savings. VFD and/or plate cooler may be existing or installed at same time as RHR. If multiple RHRs installed, enter total # of cows for Unit of Measure Question. Do not divide the total # of cows by the number of RHRs.",{"$nulls":6},"N/A","N/A",{"v":1250,"d":"$1,250.00"},"RHR Unit",{"v":1250,"d":"$1,250.00"},"RHR Unit","N/A",10032,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10032: Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR418=\"Agribusiness\", $AR418=\"Ag\",$AR418=\"Propane\", $AR418=\"Ag Propane\", $AR418=\"Ag-Propane\"),$AC418,  $AB418),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR418=\"Agribusiness\", $AR418=\"Ag\",$AR418=\"Propane\", $AR418=\"Ag Propane\", $AR418=\"Ag-Propane\"),$AC418,  $AB418),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",31]
["Not Eligible","N-AG10033","Eligible Under AgV2","Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)","N-AG10033: Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)","Include the number of milking cows in Section 6 on the application.","RHR unit must be used to extract waste heat from the dairy's milk refrigeration system in order to preheat water to serve the dairy's water heater unit.","RHR units with heating element are NOT eligible","Facilities water heater(s) must be fueled by electricity or natural gas","Replacement, redundant or back-up units do not qualify.","Size (gallons) of RHR unit must be included on invoice","Incentive must be ≤100% project cost.",null,null,"Create Calc Activity for Tech Review  to determine savings. VFD and/or plate cooler may be existing or installed at same time as RHR. If multiple RHRs installed, enter total # of cows for Unit of Measure Question. Do not divide the total # of cows by the number of RHRs.",{"$nulls":6},"N/A","N/A",{"v":1250,"d":"$1,250.00"},"RHR Unit",{"v":1250,"d":"$1,250.00"},"RHR Unit","N/A",10033,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10033: Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR419=\"Agribusiness\", $AR419=\"Ag\",$AR419=\"Propane\", $AR419=\"Ag Propane\", $AR419=\"Ag-Propane\"),$AC419,  $AB419),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR419=\"Agribusiness\", $AR419=\"Ag\",$AR419=\"Propane\", $AR419=\"Ag Propane\", $AR419=\"Ag-Propane\"),$AC419,  $AB419),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",31]
["Not Eligible","AG4937","Eligible Under AgV2","Water Heater, Ag, (Natural Gas or Propane)","AG4937: Water Heater, Ag, (Natural Gas or Propane)","Include the number of milking cows served by the water heater(s) in Section 6 on the application","Make, model number and size (gallons) must be included on the invoice","Water heater to supply hot water for dairy milk house use only","Thermal Efficiency must be ≥ 90% (as rated by AHRI)  Uniform Energy Factor must be 0.90 or greater for residential-type water heaters.","Redundant or back-up units do not qualify.",null,null,"Incentive must be ≤100% project cost.","Corresponding Propane MMID: AG4938","Create Calc Activity for Tech Review  to determine savings. ",{"$nulls":6},"N/A","N/A",{"v":1000,"d":"$1,000.00"},"Water Heater",{"v":1000,"d":"$1,000.00"},"Water Heater","N/A",4937,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4937: Water Heater, Ag, (Natural Gas or Propane)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR420=\"Agribusiness\", $AR420=\"Ag\",$AR420=\"Propane\", $AR420=\"Ag Propane\", $AR420=\"Ag-Propane\"),$AC420,  $AB420),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR420=\"Agribusiness\", $AR420=\"Ag\",$AR420=\"Propane\", $AR420=\"Ag Propane\", $AR420=\"Ag-Propane\"),$AC420,  $AB420),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",31]
["Not Eligible","N-AG4937","Eligible Under AgV2","Water Heater, Ag, (Natural Gas or Propane)","N-AG4937: Water Heater, Ag, (Natural Gas or Propane)","Include the number of milking cows served by the water heater(s) in Section 6 on the application","Make, model number and size (gallons) must be included on the invoice","Water heater to supply hot water for dairy milk house use only","Thermal Efficiency must be ≥ 90% (as rated by AHRI)  Uniform Energy Factor must be 0.90 or greater for residential-type water heaters.","Redundant or back-up units do not qualify.",null,null,"Incentive must be ≤100% project cost.","Corresponding Propane MMID: N-AG4938","Create Calc Activity for Tech Review  to determine savings. ",{"$nulls":6},"N/A","N/A",{"v":1000,"d":"$1,000.00"},"Water Heater",{"v":1000,"d":"$1,000.00"},"Water Heater","N/A",4937,"N/A","N/A","Yes","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4937: Water Heater, Ag, (Natural Gas or Propane)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR421=\"Agribusiness\", $AR421=\"Ag\",$AR421=\"Propane\", $AR421=\"Ag Propane\", $AR421=\"Ag-Propane\"),$AC421,  $AB421),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR421=\"Agribusiness\", $AR421=\"Ag\",$AR421=\"Propane\", $AR421=\"Ag Propane\", $AR421=\"Ag-Propane\"),$AC421,  $AB421),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",31]
[{"$nulls":3},"----------------------AG PROPANE CATALOG: SPECIALTY EQUIPMENT --------------------------------------------","----------------------AG PROPANE CATALOG: SPECIALTY EQUIPMENT --------------------------------------------",{"$nulls":32},{"$f":"IF(ISBLANK(A422),\"\",IF(A422<>\"Not Eligible\",A422,IF(B422<>\"Not Eligible\",IF(LEFT(B422,2)=\"S-\",RIGHT(B422,LEN(B422)-2),B422),IF(LEFT(C422,2)=\"M-\",RIGHT(C422,LEN(C422)-2),C422)))&\":  \") &D422","v":"----------------------AG PROPANE CATALOG: SPECIALTY EQUIPMENT --------------------------------------------"},null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR422=\"Agribusiness\", $AR422=\"Ag\",$AR422=\"Propane\", $AR422=\"Ag Propane\", $AR422=\"Ag-Propane\"),$AC422,  $AB422),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR422=\"Agribusiness\", $AR422=\"Ag\",$AR422=\"Propane\", $AR422=\"Ag Propane\", $AR422=\"Ag-Propane\"),$AC422,  $AB422),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG4868","Not Eligible","Grain Dryer, Energy Efficient, Propane","AG4868: Grain Dryer, Energy Efficient, Propane","Must complete Tables A1-A2 of the \"Propane and Electric Incentive Catalog Supplemental Data Sheet\" for this measure","Manufacturer's Spec Sheet must be submitted for proposed dryer with Grain Dryer Application","Must be permanent installations that use propane as heating source. Installed replacement grain dryer must be new. Used or rebuilt equipment is not eligible","New grain dryer must improve dryer efficiency (BTU/lb moisture removed) by 250 BTU/lb","Incentive calculated at 10% moisture content reduction bushels/hour rating of new grain dryer should be used","Equipment not eligible for prescriptive incentives may be eligible for custom incentives","Dryer must include at least one of these energy-efficient features: Staged Temperature, Grain Turners or Inverters, Differential Grain Speed, Varied Width of Drying Column, or Some type of grain heat recovery features. ","Pre-approval is recommended.","Corresponding NG MMID: AG3386","If electric utility is non-participating, make a note of that when creating activity for hybrid calc. Non-participating electric utility ok, do not claim any electric savings. Consult with PM if incentive should be adjusted.",{"$nulls":6},"N/A","N/A",{"v":20,"d":"$20.00"},"Bushel/hr drying capacity","N/A",{"$f":"Y423","v":"Bushel/hr drying capacity"},"N/A",4868,"N/A","N/A",{"$f":"IFERROR(IF(SEARCH(\"N-\",B423),\"Yes\",\"No\"),\"No\")","v":"No"},"N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A423),\"\",IF(A423<>\"Not Eligible\",A423,IF(B423<>\"Not Eligible\",B423,C423))&\": \") &D423","v":"AG4868: Grain Dryer, Energy Efficient, Propane"},"Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR423=\"Agribusiness\", $AR423=\"Ag\",$AR423=\"Propane\", $AR423=\"Ag Propane\", $AR423=\"Ag-Propane\"),$AC423,  $AB423),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR423=\"Agribusiness\", $AR423=\"Ag\",$AR423=\"Propane\", $AR423=\"Ag Propane\", $AR423=\"Ag-Propane\"),$AC423,  $AB423),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",14]
["Not Eligible","N-AG10423","Not Eligible","Efficient Grain Dryer, Mixed Flow Only (Natural Gas or Propane)",{"$f":"IF(ISBLANK(A424),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C424,IF(FOEIncentCodeType=IncentCodeTypeAg,B424,A424))&\": \") &D424","v":"N-AG10423: Efficient Grain Dryer, Mixed Flow Only (Natural Gas or Propane)"},"Only corn dryers are eligible","Only for Mixed Flow dryers","Must be permanent installations that use propane as heating source. Used or rebuilt equipment is not eligible","Incentive calculated at 10% moisture content reduction bushels/hour rating of new grain dryer should be used","Equipment not eligible for prescriptive incentives may be eligible for custom incentives",{"$nulls":3},"Corresponding NG MMID: AG10421","If electric utility is non-participating, make a note of that when creating activity for hybrid calc. Non-participating electric utility ok, do not claim any electric savings. Consult with PM if incentive should be adjusted.",{"$nulls":6},"N/A","N/A","N/A","Bushel/hr drying capacity",{"v":8,"d":"$8.00"},"Bushel/hr drying capacity","N/A","N/A",10423,"N/A",{"$f":"IFERROR(IF(SEARCH(\"N-\",B424),\"Yes\",\"No\"),\"No\")","v":"Yes"},"N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10423: Efficient Grain Dryer, Mixed Flow Only (Natural Gas or Propane)","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR424=\"Agribusiness\", $AR424=\"Ag\",$AR424=\"Propane\", $AR424=\"Ag Propane\", $AR424=\"Ag-Propane\"),$AC424,  $AB424),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR424=\"Agribusiness\", $AR424=\"Ag\",$AR424=\"Propane\", $AR424=\"Ag Propane\", $AR424=\"Ag-Propane\"),$AC424,  $AB424),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness",14]
[{"$nulls":3},"----------------------AG PROPANE CATALOG: VFDS AND COMPRESSED AIR --------------------------------------------","----------------------AG PROPANE CATALOG: VFDS AND COMPRESSED AIR --------------------------------------------",{"$nulls":32},{"$f":"IF(ISBLANK(A425),\"\",IF(A425<>\"Not Eligible\",A425,IF(B425<>\"Not Eligible\",IF(LEFT(B425,2)=\"S-\",RIGHT(B425,LEN(B425)-2),B425),IF(LEFT(C425,2)=\"M-\",RIGHT(C425,LEN(C425)-2),C425)))&\":  \") &D425","v":"----------------------AG PROPANE CATALOG: VFDS AND COMPRESSED AIR --------------------------------------------"},null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR425=\"Agribusiness\", $AR425=\"Ag\",$AR425=\"Propane\", $AR425=\"Ag Propane\", $AR425=\"Ag-Propane\"),$AC425,  $AB425),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR425=\"Agribusiness\", $AR425=\"Ag\",$AR425=\"Propane\", $AR425=\"Ag Propane\", $AR425=\"Ag-Propane\"),$AC425,  $AB425),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG4853","Not Eligible","Compressed Air Heat Recovery (Propane)","AG4853: Compressed Air Heat Recovery (Propane)","Heat recovery system must include automatic controls to switch from winter to summer operation. Systems with only manual damper controls are not eligible.","Heat recovery systems installed for backup or redundant air compressors or vacuum pumps do not qualify.","The project must result in an estimated net reduction of BTUs consumed in the facility to be eligible.","This incentive is for the installation of a new heat recovery system where one did not exist previously. Replacing an existing heat recovery system or upgrading an existing heat recovery system from manual to automatic controls does not qualify.","The static pressure in the area where the compressor or vacuum pump is enclosed must remain the same.","If outside air is used in the system, antifreeze protection must be considered.",null,null,"Incentive is limited to 50% of the project cost, including equipment and external labor. Corresponding NG MMID: PS2257",{"$nulls":7},"N/A","N/A",{"v":75,"d":"$75.00"},"hp","N/A",{"$f":"Y426","v":"hp"},"N/A",2257,"N/A","N/A","See NC MMID","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No",{"$f":"IF(ISBLANK(A426),\"\",IF(A426<>\"Not Eligible\",A426,IF(B426<>\"Not Eligible\",B426,C426))&\": \") &D426","v":"AG4853: Compressed Air Heat Recovery (Propane)"},"No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR426=\"Agribusiness\", $AR426=\"Ag\",$AR426=\"Propane\", $AR426=\"Ag Propane\", $AR426=\"Ag-Propane\"),$AC426,  $AB426),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR426=\"Agribusiness\", $AR426=\"Ag\",$AR426=\"Propane\", $AR426=\"Ag Propane\", $AR426=\"Ag-Propane\"),$AC426,  $AB426),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Agribusiness"]
["Not Eligible","N-AG4853","Eligible Under Ag Propane","Compressed Air Heat Recovery","N-AG4853: Compressed Air Heat Recovery","Heat recovery system must include automatic controls to switch from winter to summer operation. Systems with only manual damper controls are not eligible.","Heat recovery systems installed for backup or redundant air compressors or vacuum pumps do not qualify.","The project must result in an estimated net reduction of BTUs consumed in the facility to be eligible.","This incentive is for the installation of a new heat recovery system where one did not exist previously. Replacing an existing heat recovery system or upgrading an existing heat recovery system from manual to automatic controls does not qualify.","The static pressure in the area where the compressor or vacuum pump is enclosed must remain the same.","If outside air is used in the system, antifreeze protection must be considered.",null,null,"Incentive is limited to 50% of the project cost, including equipment and external labor. Corresponding NG MMID: PS2257",{"$nulls":7},"N/A","N/A",{"v":75,"d":"$75.00"},"hp",{"v":75,"d":"$75.00"},"hp","N/A",2257,2257,"N/A","Yes-to Ag Propane",{"$f":"IFERROR(IF(SEARCH(\"N-\",C427),\"Yes\",\"No\"),\"No\")","v":"No"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-AG4853: Compressed Air Heat Recovery","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR427=\"Agribusiness\", $AR427=\"Ag\",$AR427=\"Propane\", $AR427=\"Ag Propane\", $AR427=\"Ag-Propane\"),$AC427,  $AB427),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":1,"d":"1.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR427=\"Agribusiness\", $AR427=\"Ag\",$AR427=\"Propane\", $AR427=\"Ag Propane\", $AR427=\"Ag-Propane\"),$AC427,  $AB427),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":1000,"d":"1,000.00"}},"Agribusiness"]
["Not Eligible","PS3928","Not Eligible","Vacuum Pump Heat Recovery","PS3928: Vacuum Pump Heat Recovery","Heat recovery system must include automatic controls to switch from winter to summer operation. Systems with only manual damper controls are not eligible.","Heat recovery systems installed for backup or redundant air compressors or vacuum pumps do not qualify.","The project must result in an estimated net reduction of BTUs consumed in the facility to be eligible.","This incentive is for the installation of a new heat recovery system where one did not exist previously. Replacing an existing heat recovery system or upgrading an existing heat recovery system from manual to automatic controls does not qualify.","The static pressure in the area where the compressor or vacuum pump is enclosed must remain the same.","If outside air is used in the system, antifreeze protection must be considered.",null,null,"Incentive is limited to 50% of the project cost, including equipment and external labor.",{"$nulls":7},"N/A","N/A",{"v":75,"d":"$75.00"},"hp","N/A","hp","N/A",3928,"N/A","N/A","See NC MMID","N/A",{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","PS3928: Vacuum Pump Heat Recovery","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR428=\"Agribusiness\", $AR428=\"Ag\",$AR428=\"Propane\", $AR428=\"Ag Propane\", $AR428=\"Ag-Propane\"),$AC428,  $AB428),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR428=\"Agribusiness\", $AR428=\"Ag\",$AR428=\"Propane\", $AR428=\"Ag Propane\", $AR428=\"Ag-Propane\"),$AC428,  $AB428),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Agribusiness"]
["Not Eligible","N-PS3928","Eligible Under Ag Propane","Vacuum Pump Heat Recovery","N-PS3928: Vacuum Pump Heat Recovery","Heat recovery system must include automatic controls to switch from winter to summer operation. Systems with only manual damper controls are not eligible.","Heat recovery systems installed for backup or redundant air compressors or vacuum pumps do not qualify.","The project must result in an estimated net reduction of BTUs consumed in the facility to be eligible.","This incentive is for the installation of a new heat recovery system where one did not exist previously. Replacing an existing heat recovery system or upgrading an existing heat recovery system from manual to automatic controls does not qualify.","The static pressure in the area where the compressor or vacuum pump is enclosed must remain the same.","If outside air is used in the system, antifreeze protection must be considered.",null,null,"Incentive is limited to 50% of the project cost, including equipment and external labor.",{"$nulls":7},"N/A","N/A",{"v":75,"d":"$75.00"},"hp",{"v":75,"d":"$75.00"},"hp","N/A",3928,3928,"N/A","Yes-to Ag Propane",{"$f":"IFERROR(IF(SEARCH(\"N-\",C429),\"Yes\",\"No\"),\"No\")","v":"No"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},{"v":0.5,"d":"50.0%"},"No","N-PS3928: Vacuum Pump Heat Recovery","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR429=\"Agribusiness\", $AR429=\"Ag\",$AR429=\"Propane\", $AR429=\"Ag Propane\", $AR429=\"Ag-Propane\"),$AC429,  $AB429),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":0.1,"d":"0.10"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR429=\"Agribusiness\", $AR429=\"Ag\",$AR429=\"Propane\", $AR429=\"Ag Propane\", $AR429=\"Ag-Propane\"),$AC429,  $AB429),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},"Agribusiness"]
[{"$nulls":3},"----------------------AG PROPANE CATALOG: SPACE HEATING EQUIPMENT --------------------------------------------","----------------------AG PROPANE CATALOG: SPACE HEATING EQUIPMENT --------------------------------------------",{"$nulls":32},{"$f":"IF(ISBLANK(A430),\"\",IF(A430<>\"Not Eligible\",A430,IF(B430<>\"Not Eligible\",IF(LEFT(B430,2)=\"S-\",RIGHT(B430,LEN(B430)-2),B430),IF(LEFT(C430,2)=\"M-\",RIGHT(C430,LEN(C430)-2),C430)))&\":  \") &D430","v":"----------------------AG PROPANE CATALOG: SPACE HEATING EQUIPMENT --------------------------------------------"},null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR430=\"Agribusiness\", $AR430=\"Ag\",$AR430=\"Propane\", $AR430=\"Ag Propane\", $AR430=\"Ag-Propane\"),$AC430,  $AB430),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR430=\"Agribusiness\", $AR430=\"Ag\",$AR430=\"Propane\", $AR430=\"Ag Propane\", $AR430=\"Ag-Propane\"),$AC430,  $AB430),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG4852","Not Eligible","Hot Water Boilers, < 300 MBh input, ≥90% AFUE","AG4852: Hot Water Boilers, < 300 MBh input, ≥90% AFUE","Must be ≤ 300 MBh input and condensing boilers must modulate their firing rate and include outdoor-air reset control","Must be sealed combustion unit and ≥ 90% AFUE","Boiler incentives are only avaiable for equipment used in space heating applications.  Boilers used for only domestic hot water heating are not eligible for this incentives.","Space heating boilers also used for DHW may be eligible for indirect DHW incentives but are subject to requirments. In plant systems, boilers are eligible for incentives for their primary use only. A boiler replacing a space heating and indirect DHW system will use the capacity of the existing space heating and DHW systems to estimate the split of incentives. Boilers that only serve DHW are not eligible for the space heating incentives","Chimney liners must be installed where a high efficiency propane boiler replaces atmospherically drafted equipment that was vented through the same flue as a propane water heater.","Boiler efficiency will be verified using the AHRI database. If the boiler is not listed in the AHRI database, provide a boiler spec sheet with boiler input and output ratings and either AFUE or thermal efficiency as appropriate for boiler size","Steam boilers are not eligible for this incentive but may quality for a custom incentive","Incentive must be ≤100% project cost.","Corresponding NG MMID: H2218",{"$nulls":7},"N/A","N/A",{"v":7,"d":"$7.00"},"MBh",{"v":7,"d":"$7.00"},{"$f":"Y431","v":"MBh"},"N/A",4852,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A431),\"\",IF(A431<>\"Not Eligible\",A431,IF(B431<>\"Not Eligible\",B431,C431))&\": \") &D431","v":"AG4852: Hot Water Boilers, < 300 MBh input, ≥90% AFUE"},"No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR431=\"Agribusiness\", $AR431=\"Ag\",$AR431=\"Propane\", $AR431=\"Ag Propane\", $AR431=\"Ag-Propane\"),$AC431,  $AB431),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR431=\"Agribusiness\", $AR431=\"Ag\",$AR431=\"Propane\", $AR431=\"Ag Propane\", $AR431=\"Ag-Propane\"),$AC431,  $AB431),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","N-AG4852","Eligible Under Ag Propane","Hot Water Boilers, < 300 MBh input, ≥90% AFUE",{"$f":"IF(ISBLANK(A432),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C432,IF(FOEIncentCodeType=IncentCodeTypeAg,B432,A432))&\": \") &D432","v":"N-AG4852: Hot Water Boilers, < 300 MBh input, ≥90% AFUE"},"Must be ≤ 300 MBh input and condensing boilers must modulate their firing rate and include outdoor-air reset control","Must be sealed combustion unit and ≥ 90% AFUE","Boiler incentives are only avaiable for equipment used in space heating applications.  Boilers used for only domestic hot water heating are not eligible for this incentives.","Space heating boilers also used for DHW may be eligible for indirect DHW incentives but are subject to requirments. In plant systems, boilers are eligible for incentives for their primary use only. A boiler replacing a space heating and indirect DHW system will use the capacity of the existing space heating and DHW systems to estimate the split of incentives. Boilers that only serve DHW are not eligible for the space heating incentives","Chimney liners must be installed where a high efficiency propane boiler replaces atmospherically drafted equipment that was vented through the same flue as a propane water heater.","Boiler efficiency will be verified using the AHRI database. If the boiler is not listed in the AHRI database, provide a boiler spec sheet with boiler input and output ratings and either AFUE or thermal efficiency as appropriate for boiler size","Steam boilers are not eligible for this incentive but may quality for a custom incentive","Incentive must be ≤100% project cost.","Corresponding NG MMID: N-H2218",{"$nulls":7},"N/A","N/A",{"v":7,"d":"$7.00"},"MBh",{"v":7,"d":"$7.00"},"MBh","N/A",4852,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4852: Hot Water Boilers, < 300 MBh input, ≥90% AFUE","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR432=\"Agribusiness\", $AR432=\"Ag\",$AR432=\"Propane\", $AR432=\"Ag Propane\", $AR432=\"Ag-Propane\"),$AC432,  $AB432),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR432=\"Agribusiness\", $AR432=\"Ag\",$AR432=\"Propane\", $AR432=\"Ag Propane\", $AR432=\"Ag-Propane\"),$AC432,  $AB432),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","H10206","Not Eligible","Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","H10206: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","Must be ≥ 90 and <95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,"Corresponding NG MMID: H10222","See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":7,"d":"$7.00"},"MBh",{"v":7,"d":"$7.00"},{"$f":"W433","v":"MBh"},{"v":7,"d":"$7.00"},{"$f":"W433","v":"MBh"},3276,{"$f":"AB433","v":3276},3276,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10206: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR433=\"Agribusiness\", $AR433=\"Ag\",$AR433=\"Propane\", $AR433=\"Ag Propane\", $AR433=\"Ag-Propane\"),$AC433,  $AB433),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR433=\"Agribusiness\", $AR433=\"Ag\",$AR433=\"Propane\", $AR433=\"Ag Propane\", $AR433=\"Ag-Propane\"),$AC433,  $AB433),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"Agribusiness",29]
["Not Eligible","H10208","Not Eligible","Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","H10208: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","Must be ≥ 95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,"Corresponding NG MMID: H10207","See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":8,"d":"$8.00"},"MBh",{"v":8,"d":"$8.00"},"MBh",{"v":8,"d":"$8.00"},"MBh",3276,3276,3276,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10208: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR434=\"Agribusiness\", $AR434=\"Ag\",$AR434=\"Propane\", $AR434=\"Ag Propane\", $AR434=\"Ag-Propane\"),$AC434,  $AB434),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR434=\"Agribusiness\", $AR434=\"Ag\",$AR434=\"Propane\", $AR434=\"Ag Propane\", $AR434=\"Ag-Propane\"),$AC434,  $AB434),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"Agribusiness",29]
["Not Eligible","N-H10206","Eligible Under AgV3","Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","N-H10206: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","Must be ≥ 90 and <95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,"Corresponding NG MMID: N-H10222","See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":7,"d":"$7.00"},"MBh",{"v":7,"d":"$7.00"},"MBh",{"v":7,"d":"$7.00"},"MBh",3276,3276,3276,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H10206: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR435=\"Agribusiness\", $AR435=\"Ag\",$AR435=\"Propane\", $AR435=\"Ag Propane\", $AR435=\"Ag-Propane\"),$AC435,  $AB435),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR435=\"Agribusiness\", $AR435=\"Ag\",$AR435=\"Propane\", $AR435=\"Ag Propane\", $AR435=\"Ag-Propane\"),$AC435,  $AB435),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"Agribusiness",29]
["Not Eligible","N-H10208","Eligible Under AgV4","Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","N-H10208: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","Must be ≥ 95% thermal efficiency and be ≥300 MBh ","Boilers must be capable of capacity modulation","See AHRIdirectory.org to confirm efficiency %. Must provide mfg. spec sheet with boiler input  and output ratings and either AFUE or thermal efficiency as appropriate for boiler size.","Space heat only. Boilers for indirect domestic water heating only or for process loads DNQ.","Natural gas boilers only. Redundant or backup boilers do not qualify.","Steam boilers do not meet the efficiency requirements and aren't eligible (but may qualify for a custom incentive). Hot water boiler >=90% TE replacing a steam boiler is eligible.","Do not round AHRI capacity to a whole number.",null,"Corresponding NG MMID: N-H10207","See AHRIdirectory.org to confirm efficiency % - although not technically a requirement.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},{"v":8,"d":"$8.00"},"MBh",{"v":8,"d":"$8.00"},"MBh",{"v":8,"d":"$8.00"},"MBh",3276,3276,3276,"Yes","Yes","Yes",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H10208: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR436=\"Agribusiness\", $AR436=\"Ag\",$AR436=\"Propane\", $AR436=\"Ag Propane\", $AR436=\"Ag-Propane\"),$AC436,  $AB436),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":300,"d":"300.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR436=\"Agribusiness\", $AR436=\"Ag\",$AR436=\"Propane\", $AR436=\"Ag Propane\", $AR436=\"Ag-Propane\"),$AC436,  $AB436),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":6000,"d":"6,000.00"}},"Agribusiness",29]
["Not Eligible","AG4854","Not Eligible","Infrared Heater (Propane Only)","AG4854: Infrared Heater (Propane Only)","Must have electronic ignition","Low-intensity and high-intensity units are eligible","Must be vented per manufacturer's specs","Low-intensity heaters must use outside non-conditioned combustion air","Replacement of existing infrared heater DNQ",null,null,"Incentive must be ≤100% project cost.","Corresponding NG MMID: H2422",null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":7.5,"d":"$7.50"},"MBh","N/A","MBh","N/A",4854,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG4854: Infrared Heater (Propane Only)","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR437=\"Agribusiness\", $AR437=\"Ag\",$AR437=\"Propane\", $AR437=\"Ag Propane\", $AR437=\"Ag-Propane\"),$AC437,  $AB437),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR437=\"Agribusiness\", $AR437=\"Ag\",$AR437=\"Propane\", $AR437=\"Ag Propane\", $AR437=\"Ag-Propane\"),$AC437,  $AB437),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","N-AG4854","Eligible Under Ag Propane","Infrared Heater (Propane Only)","N-AG4854: Infrared Heater (Propane Only)","Must have electronic ignition","Low-intensity and high-intensity units are eligible","Must be vented per manufacturer's specs","Low-intensity heaters must use outside non-conditioned combustion air","Replacement of existing infrared heater DNQ",null,null,"Incentive must be ≤100% project cost.","Corresponding NG MMID: N-H2422",null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":6,"d":"$6.00"},"MBh",{"v":6,"d":"$6.00"},"MBh","N/A",4854,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4854: Infrared Heater (Propane Only)","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR438=\"Agribusiness\", $AR438=\"Ag\",$AR438=\"Propane\", $AR438=\"Ag Propane\", $AR438=\"Ag-Propane\"),$AC438,  $AB438),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR438=\"Agribusiness\", $AR438=\"Ag\",$AR438=\"Propane\", $AR438=\"Ag Propane\", $AR438=\"Ag-Propane\"),$AC438,  $AB438),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","AG4870","Not Eligible","Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane","AG4870: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane","Must be ≥ 90% AFUE","Furnaces and single package vertical unit must meet the minimum efficiency requirements listed and be a sealed combustion unit. Efficiency ratings will be verified using the AHRI database.","Furnaces and single package vertical units must have a single speed, multi-speed, or variable speed electronically communicated motor (ECM). Permanent split capacitor (PSC) motors are not eligible. Air handlers with an ECM are not eligible.","Provide a manufacturer's spec sheet to document the required features","Must provide INPUT capacity of furnace or single package vertical units in MBh in Section 7 on the Incentive Application","Furnaces must have a multi-stage burner and have at least two firing stages","Chimney liners must be installed if previously vented with water heater through chimney (more sealing guidelines)","Incentive must be ≤100% project cost.","Corresponding NG MMID: H3491","Do not lump various sized furnaces when entering measure. Ok to lump same size (capacity in MBh) furnaces.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":200,"d":"$200.00"},"Furnace",{"v":150,"d":"$150.00"},{"$f":"Y439","v":"Furnace"},"N/A",4870,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A439),\"\",IF(A439<>\"Not Eligible\",A439,IF(B439<>\"Not Eligible\",B439,C439))&\": \") &D439","v":"AG4870: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane"},"No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR439=\"Agribusiness\", $AR439=\"Ag\",$AR439=\"Propane\", $AR439=\"Ag Propane\", $AR439=\"Ag-Propane\"),$AC439,  $AB439),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR439=\"Agribusiness\", $AR439=\"Ag\",$AR439=\"Propane\", $AR439=\"Ag Propane\", $AR439=\"Ag-Propane\"),$AC439,  $AB439),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","AG4869","Not Eligible","Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane","AG4869: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane","Must be ≥ 95% AFUE","Furnaces and single package vertical unit must meet the minimum efficiency requirements listed and be a sealed combustion unit. Efficiency ratings will be verified using the AHRI database.","Furnaces and single package vertical units must have a single speed, multi-speed, or variable speed electronically communicated motor (ECM). Permanent split capacitor (PSC) motors are not eligible. Air handlers with an ECM are not eligible.","Provide a manufacturer's spec sheet to document the required features","Must provide INPUT capacity of furnace or single package vertical units in MBh in Section 7 on the Incentive Application","Furnaces must have a multi-stage burner and have at least two firing stages","Chimney liners must be installed if previously vented with water heater through chimney (more sealing guidelines)","Incentive must be ≤100% project cost.","Corresponding NG MMID: H3492","Do not lump various sized furnaces when entering measure. Ok to lump same size (capacity in MBh) furnaces.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":420,"d":"$420.00"},"Furnace",{"v":320,"d":"$320.00"},{"$f":"Y440","v":"Furnace"},"N/A",4869,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A440),\"\",IF(A440<>\"Not Eligible\",A440,IF(B440<>\"Not Eligible\",B440,C440))&\": \") &D440","v":"AG4869: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane"},"No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR440=\"Agribusiness\", $AR440=\"Ag\",$AR440=\"Propane\", $AR440=\"Ag Propane\", $AR440=\"Ag-Propane\"),$AC440,  $AB440),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR440=\"Agribusiness\", $AR440=\"Ag\",$AR440=\"Propane\", $AR440=\"Ag Propane\", $AR440=\"Ag-Propane\"),$AC440,  $AB440),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","N-AG4870","Eligible Under Ag Propane","Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane","N-AG4870: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane","Must be ≥ 90% AFUE","Furnaces and single package vertical unit must meet the minimum efficiency requirements listed and be a sealed combustion unit. Efficiency ratings will be verified using the AHRI database.","Furnaces and single package vertical units must have a single speed, multi-speed, or variable speed electronically communicated motor (ECM). Permanent split capacitor (PSC) motors are not eligible. Air handlers with an ECM are not eligible.","Provide a manufacturer's spec sheet to document the required features","Must provide INPUT capacity of furnace or single package vertical units in MBh in Section 7 on the Incentive Application","Furnaces must have a multi-stage burner and have at least two firing stages","Furnaces listed on the Focus on Energy residential furnace qualified products list does not guarantee the furnace has all features required for agribusiness incentives","Incentive must be ≤100% project cost.","Corresponding NG MMID: N-H3491","Do not lump various sized furnaces when entering measure. Ok to lump same size (capacity in MBh) furnaces.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":150,"d":"$150.00"},"Furnace",{"v":150,"d":"$150.00"},{"$f":"Y441","v":"Furnace"},"N/A",4870,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A441),\"\",IF(A441<>\"Not Eligible\",A441,IF(B441<>\"Not Eligible\",B441,C441))&\": \") &D441","v":"N-AG4870: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane"},"No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR441=\"Agribusiness\", $AR441=\"Ag\",$AR441=\"Propane\", $AR441=\"Ag Propane\", $AR441=\"Ag-Propane\"),$AC441,  $AB441),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR441=\"Agribusiness\", $AR441=\"Ag\",$AR441=\"Propane\", $AR441=\"Ag Propane\", $AR441=\"Ag-Propane\"),$AC441,  $AB441),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","N-AG4869","Eligible Under Ag Propane","Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane","N-AG4869: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane","Must be ≥ 95% AFUE","Furnaces and single package vertical unit must meet the minimum efficiency requirements listed and be a sealed combustion unit. Efficiency ratings will be verified using the AHRI database.","Furnaces and single package vertical units must have a single speed, multi-speed, or variable speed electronically communicated motor (ECM). Permanent split capacitor (PSC) motors are not eligible. Air handlers with an ECM are not eligible.","Provide a manufacturer's spec sheet to document the required features","Must provide INPUT capacity of furnace or single package vertical units in MBh in Section 7 on the Incentive Application","Furnaces must have a multi-stage burner and have at least two firing stages","Furnaces listed on the Focus on Energy residential furnace qualified products list does not guarantee the furnace has all features required for agribusiness incentives","Incentive must be ≤100% project cost.","Corresponding NG MMID: N-H3492","Do not lump various sized furnaces when entering measure. Ok to lump same size (capacity in MBh) furnaces.","equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":320,"d":"$320.00"},"Furnace",{"v":320,"d":"$320.00"},"Furnace","N/A",4869,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4869: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR442=\"Agribusiness\", $AR442=\"Ag\",$AR442=\"Propane\", $AR442=\"Ag Propane\", $AR442=\"Ag-Propane\"),$AC442,  $AB442),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR442=\"Agribusiness\", $AR442=\"Ag\",$AR442=\"Propane\", $AR442=\"Ag Propane\", $AR442=\"Ag-Propane\"),$AC442,  $AB442),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","AG5437","Not Eligible","Unit Heater, ≥ 90% Thermal Efficiency ","AG5437: Unit Heater, ≥ 90% Thermal Efficiency ","Unit heater must be an upgrade from a standard efficiency (typically 80%-84% thermal efficiency) unit heater","Steam or hot water coils/systems are not eligible. ","Must be vented and condensate drained per manufacturer specifications","Direct fired rooftop units/make-up air units are not eligible for this incentive.","Must replace an existing non-condensing unit heater or be installed instead of a non-condensing unit heater.","Provide a manufacturer’s specification sheet to document the features and efficiency level of the unit heater, including input capacity in MBh.","Incentive must be ≤100% project cost.",null,"Corresponding NG MMID: H5436",{"$nulls":7},"N/A","N/A",{"v":4,"d":"$4.00"},"MBh",{"v":2.75,"d":"$2.75"},"MBh","N/A",5437,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG5437: Unit Heater, ≥ 90% Thermal Efficiency ","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR443=\"Agribusiness\", $AR443=\"Ag\",$AR443=\"Propane\", $AR443=\"Ag Propane\", $AR443=\"Ag-Propane\"),$AC443,  $AB443),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR443=\"Agribusiness\", $AR443=\"Ag\",$AR443=\"Propane\", $AR443=\"Ag Propane\", $AR443=\"Ag-Propane\"),$AC443,  $AB443),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","N-AG5437","Not Eligible","Unit Heater, ≥ 90% Thermal Efficiency ","N-AG5437: Unit Heater, ≥ 90% Thermal Efficiency ","Unit heater must be an upgrade from a standard efficiency (typically 80%-84% thermal efficiency) unit heater","Steam or hot water coils/systems are not eligible. ","Must be vented and condensate drained per manufacturer specifications","Direct fired rooftop units/make-up air units are not eligible for this incentive.","Must replace an existing non-condensing unit heater or be installed instead of a non-condensing unit heater.","Provide a manufacturer’s specification sheet to document the features and efficiency level of the unit heater, including input capacity in MBh.","Incentive must be ≤100% project cost.",null,"Corresponding NG MMID: N-H5436",{"$nulls":7},"N/A","N/A",{"v":2.75,"d":"$2.75"},"MBh",{"v":2.75,"d":"$2.75"},"MBh","N/A",5437,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG5437: Unit Heater, ≥ 90% Thermal Efficiency ","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR444=\"Agribusiness\", $AR444=\"Ag\",$AR444=\"Propane\", $AR444=\"Ag Propane\", $AR444=\"Ag-Propane\"),$AC444,  $AB444),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR444=\"Agribusiness\", $AR444=\"Ag\",$AR444=\"Propane\", $AR444=\"Ag Propane\", $AR444=\"Ag-Propane\"),$AC444,  $AB444),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","AG5407","Not Eligible","Direct Fired Make-up Air Unit, Constant Volume","AG5407: Direct Fired Make-up Air Unit, Constant Volume","Complete Table F1 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","Incentive is available for upgrading (or installing instead of) indirect fired make-up air units or rooftop units which are approximately 80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible.","Replacement of electric or hydronically heated make-up air is not eligible.","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements.","Must serve an occupied space for at least 500 hours per year",null,"Corresponding NG MMID: H5081",{"$nulls":7},"N/A","N/A",{"v":0.4,"d":"$0.40"},"CFM",{"v":0.3,"d":"$0.30"},{"$f":"W445","v":"N/A"},"N/A",5407,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A445),\"\",IF(A445<>\"Not Eligible\",A445,IF(B445<>\"Not Eligible\",B445,C445))&\": \") &D445","v":"AG5407: Direct Fired Make-up Air Unit, Constant Volume"},"Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR445=\"Agribusiness\", $AR445=\"Ag\",$AR445=\"Propane\", $AR445=\"Ag Propane\", $AR445=\"Ag-Propane\"),$AC445,  $AB445),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR445=\"Agribusiness\", $AR445=\"Ag\",$AR445=\"Propane\", $AR445=\"Ag Propane\", $AR445=\"Ag-Propane\"),$AC445,  $AB445),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","N-AG5407","Eligible Under AgV2","Direct Fired Make-up Air Unit, Constant Volume","N-AG5407: Direct Fired Make-up Air Unit, Constant Volume","Complete Table F1 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","Incentive is available for upgrading (or installing instead of) indirect fired make-up air units or rooftop units which are approximately 80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible.","Replacement of electric or hydronically heated make-up air is not eligible.","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements.","Must serve an occupied space for at least 500 hours per year",null,"Corresponding NG MMID: N-H5081",{"$nulls":7},"N/A","N/A",{"v":0.3,"d":"$0.30"},"CFM",{"v":0.3,"d":"$0.30"},"N/A","N/A",5407,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A446),\"\",IF(A446<>\"Not Eligible\",A446,IF(B446<>\"Not Eligible\",B446,C446))&\": \") &D446","v":"N-AG5407: Direct Fired Make-up Air Unit, Constant Volume"},"Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR446=\"Agribusiness\", $AR446=\"Ag\",$AR446=\"Propane\", $AR446=\"Ag Propane\", $AR446=\"Ag-Propane\"),$AC446,  $AB446),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR446=\"Agribusiness\", $AR446=\"Ag\",$AR446=\"Propane\", $AR446=\"Ag Propane\", $AR446=\"Ag-Propane\"),$AC446,  $AB446),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","AG10031","Not Eligible","Direct Fired Make-up Air Unit, Variable Air Volume",{"$f":"IF(ISBLANK(A447),\"\",IF(FOEIncentCodeType=IncentCodeTypeNC,C447,IF(FOEIncentCodeType=IncentCodeTypeAg,B447,A447))&\": \") &D447","v":"AG10031: Direct Fired Make-up Air Unit, Variable Air Volume"},"Complete Table F2 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","Incentive is available for upgrading (or installing instead of) indirect fired make-up air units or rooftop units which are approximately 80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible.","Replacement of electric or hydronically heated make-up air is not eligible.","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements.","Must serve an occupied space for at least 500 hours per year",null,"Corresponding NG MMID: H10030",{"$nulls":7},"N/A","N/A",{"v":0.65,"d":"$0.65"},"CFM",{"v":0.4,"d":"$0.40"},"N/A","N/A",10031,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG10031: Direct Fired Make-up Air Unit, Variable Air Volume","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR447=\"Agribusiness\", $AR447=\"Ag\",$AR447=\"Propane\", $AR447=\"Ag Propane\", $AR447=\"Ag-Propane\"),$AC447,  $AB447),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":800,"d":"800.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR447=\"Agribusiness\", $AR447=\"Ag\",$AR447=\"Propane\", $AR447=\"Ag Propane\", $AR447=\"Ag-Propane\"),$AC447,  $AB447),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness"]
["Not Eligible","N-AG10031","Eligible Under AgV2","Direct Fired Make-up Air Unit, Variable Air Volume","N-AG10031: Direct Fired Make-up Air Unit, Variable Air Volume","Complete Table F2 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","Incentive is available for upgrading (or installing instead of) indirect fired make-up air units or rooftop units which are approximately 80% efficient.","Replacement of an existing direct-fired make-up air unit is not eligible.","Replacement of electric or hydronically heated make-up air is not eligible.","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements.","Must serve an occupied space for at least 500 hours per year",null,"Corresponding NG MMID: N-H10030",{"$nulls":7},"N/A","N/A",{"v":0.4,"d":"$0.40"},"CFM",{"v":0.4,"d":"$0.40"},"N/A","N/A",10031,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10031: Direct Fired Make-up Air Unit, Variable Air Volume","Yes","Yes","CFM",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR448=\"Agribusiness\", $AR448=\"Ag\",$AR448=\"Propane\", $AR448=\"Ag Propane\", $AR448=\"Ag-Propane\"),$AC448,  $AB448),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":{"v":800,"d":"800.00"}},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR448=\"Agribusiness\", $AR448=\"Ag\",$AR448=\"Propane\", $AR448=\"Ag Propane\", $AR448=\"Ag-Propane\"),$AC448,  $AB448),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":{"v":50000,"d":"50,000.00"}},"Agribusiness"]
["Not Eligible","H10439","Eligible Under AgV3","Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","H10439: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","Complete Table F2 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.","Cannot be combined with VFD incentives.",null,"Corresponding NG MMID: H10445",null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":0.25,"d":"$0.25"},"CFM",{"v":0.25,"d":"$0.25"},"CFM","N/A",10445,10445,"N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","H10439: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","Yes","Yes","CFM",{"v":100,"d":"100.00"},{"v":50000,"d":"50,000.00"},"Agribusiness",30]
["Not Eligible","N-H10439","Eligible Under AgV2","Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","N-H10439: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","Complete Table F2 of the “Agribusiness Incentive Catalog Supplemental Data Sheet”","For upgrading (or installing instead of) indirect fired make-up air units or rooftop units, which are ~80% efficient.","Replacement of electric or hydronically heated make-up air unit is not eligible. ","Intended for spaces with high ventilation or exhaust loads.","Installation and operation must follow all applicable building code requirements. ","Must serve an occupied space for at least 500 hours per year.","Cannot be combined with VFD incentives.",null,"Corresponding NG MMID: N-H10445",null,"equipment, location, equipment nameplate (if possible)",{"$nulls":5},"N/A","N/A",{"v":0.2,"d":"$0.20"},"CFM",{"v":0.2,"d":"$0.20"},"CFM","N/A",10445,10445,"N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-H10439: Direct Fired Make-up Air Unit, Variable Air Volume instead of Constant Volume (NG or Propane)","Yes","Yes","CFM",{"v":100,"d":"100.00"},{"v":50000,"d":"50,000.00"},"Agribusiness",30]
[{"$nulls":3},"----------------------AG PROPANE CATALOG: WATER HEATING EQUIPMENT --------------------------------------------","----------------------AG PROPANE CATALOG: WATER HEATING EQUIPMENT --------------------------------------------",{"$nulls":32},{"$f":"IF(ISBLANK(A451),\"\",IF(A451<>\"Not Eligible\",A451,IF(B451<>\"Not Eligible\",IF(LEFT(B451,2)=\"S-\",RIGHT(B451,LEN(B451)-2),B451),IF(LEFT(C451,2)=\"M-\",RIGHT(C451,LEN(C451)-2),C451)))&\":  \") &D451","v":"----------------------AG PROPANE CATALOG: WATER HEATING EQUIPMENT --------------------------------------------"},null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR451=\"Agribusiness\", $AR451=\"Ag\",$AR451=\"Propane\", $AR451=\"Ag Propane\", $AR451=\"Ag-Propane\"),$AC451,  $AB451),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR451=\"Agribusiness\", $AR451=\"Ag\",$AR451=\"Propane\", $AR451=\"Ag Propane\", $AR451=\"Ag-Propane\"),$AC451,  $AB451),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG10034","Not Eligible","RHR Unit (Propane Water Heater)","AG10034: RHR Unit (Propane Water Heater)","Include the number of milking cows in Section 6 on the application.","RHR unit must be used to extract waste heat from the dairy's milk refrigeration system in order to preheat water to serve the dairy's water heater unit.","RHR units with heating element are NOT eligible","Facilities water heater(s) must be fueled by propane","Redundant or back-up units do not qualify.","Size (gallons) of RHR unit must be included on invoice","Incentive must be ≤100% project cost.",null,"Corresponding NG MMID: AG10032","Create Calc Activity for Tech Review  to determine savings. VFD and/or plate cooler may be existing or installed at same time as RHR.",{"$nulls":6},"N/A","N/A",{"v":1250,"d":"$1,250.00"},"RHR Unit",{"v":1250,"d":"$1,250.00"},{"$f":"Y452","v":"RHR Unit"},"N/A",4874,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","AG10034:  RHR Unit (Propane Water Heater)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR452=\"Agribusiness\", $AR452=\"Ag\",$AR452=\"Propane\", $AR452=\"Ag Propane\", $AR452=\"Ag-Propane\"),$AC452,  $AB452),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR452=\"Agribusiness\", $AR452=\"Ag\",$AR452=\"Propane\", $AR452=\"Ag Propane\", $AR452=\"Ag-Propane\"),$AC452,  $AB452),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","N-AG10034","Eligible Under Ag Propane","RHR Unit (Propane Water Heater)","N-AG10034: RHR Unit (Propane Water Heater)","Include the number of milking cows in Section 6 on the application.","RHR unit must be used to extract waste heat from the dairy's milk refrigeration system in order to preheat water to serve the dairy's water heater unit.","RHR units with heating element are NOT eligible","Facilities water heater(s) must be fueled by propane","Redundant or back-up units do not qualify.","Size (gallons) of RHR unit must be included on invoice","Incentive must be ≤100% project cost.",null,"Corresponding NG MMID: N-AG10032","Create Calc Activity for Tech Review  to determine savings. VFD and/or plate cooler may be existing or installed at same time as RHR.",{"$nulls":6},"N/A","N/A",{"v":1250,"d":"$1,250.00"},"RHR Unit",{"v":1250,"d":"$1,250.00"},"RHR Unit","N/A",4874,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG10034:  RHR Unit (Propane Water Heater)","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR453=\"Agribusiness\", $AR453=\"Ag\",$AR453=\"Propane\", $AR453=\"Ag Propane\", $AR453=\"Ag-Propane\"),$AC453,  $AB453),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR453=\"Agribusiness\", $AR453=\"Ag\",$AR453=\"Propane\", $AR453=\"Ag Propane\", $AR453=\"Ag-Propane\"),$AC453,  $AB453),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","AG4938","Not Eligible","Propane Commercial Water Heater","AG4938: Propane Commercial Water Heater","Include the number of milking cows served by the water heater(s) in Section 6 on the application","Make, model number and size (gallons) must be included on the invoice","Water heater to supply hot water for dairy milk house use only","Thermal Efficiency must be >= 90% (as rated by AHRI)  Uniform Energy Factor must be 0.90 or greater for residential-type water heaters.","Redundant or back-up units do not qualify.",null,"For Propane water heaters only","Incentive must be ≤100% project cost.","Corresponding NG MMID: AG4937","Create Calc Activity for Tech Review  to determine savings. ",{"$nulls":6},"N/A","N/A",{"v":1000,"d":"$1,000.00"},"Water Heater",{"v":1000,"d":"$1,000.00"},"Water Heater","N/A",4938,"N/A","N/A","See NC MMID","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No",{"$f":"IF(ISBLANK(A454),\"\",IF(A454<>\"Not Eligible\",A454,IF(B454<>\"Not Eligible\",B454,C454))&\": \") &D454","v":"AG4938: Propane Commercial Water Heater"},"Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR454=\"Agribusiness\", $AR454=\"Ag\",$AR454=\"Propane\", $AR454=\"Ag Propane\", $AR454=\"Ag-Propane\"),$AC454,  $AB454),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR454=\"Agribusiness\", $AR454=\"Ag\",$AR454=\"Propane\", $AR454=\"Ag Propane\", $AR454=\"Ag-Propane\"),$AC454,  $AB454),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
["Not Eligible","N-AG4938","Eligible Under Ag Propane","Propane Commercial Water Heater","N-AG4938: Propane Commercial Water Heater","Include the number of milking cows served by the water heater(s) in Section 6 on the application","Make, model number and size (gallons) must be included on the invoice","Water heater to supply hot water for dairy milk house use only","Thermal Efficiency must be >= 90% (as rated by AHRI)  Uniform Energy Factor must be 0.90 or greater for residential-type water heaters.","Redundant or back-up units do not qualify.",null,"For Propane water heaters only","Incentive must be ≤100% project cost.","Corresponding NG MMID: N-AG4937","Create Calc Activity for Tech Review  to determine savings. ",{"$nulls":6},"N/A","N/A",{"v":1000,"d":"$1,000.00"},"Water Heater",{"v":1000,"d":"$1,000.00"},"Water Heater","N/A",4938,"N/A","N/A","Yes-to Ag Propane","N/A",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"No","N-AG4938: Propane Commercial Water Heater","Yes","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR455=\"Agribusiness\", $AR455=\"Ag\",$AR455=\"Propane\", $AR455=\"Ag Propane\", $AR455=\"Ag-Propane\"),$AC455,  $AB455),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR455=\"Agribusiness\", $AR455=\"Ag\",$AR455=\"Propane\", $AR455=\"Ag Propane\", $AR455=\"Ag-Propane\"),$AC455,  $AB455),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Agribusiness"]
[{"$nulls":3},"-------------------------------SPECIAL OFFERS AG-------------------------------","-------------------------------SPECIAL OFFERS AG-------------------------------",{"$nulls":32},"-------------------------------SPECIAL OFFERS AG-------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR456=\"Agribusiness\", $AR456=\"Ag\",$AR456=\"Propane\", $AR456=\"Ag Propane\", $AR456=\"Ag-Propane\"),$AC456,  $AB456),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR456=\"Agribusiness\", $AR456=\"Ag\",$AR456=\"Propane\", $AR456=\"Ag Propane\", $AR456=\"Ag-Propane\"),$AC456,  $AB456),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["Not Eligible","AG4403","Not Eligible","Refrigeration System Tune-Up, Agriculture","AG4403: Refrigeration System Tune-Up, Agriculture","Use TA Payment address listed on enrollment form found under TA Opportunity","Labor and travel costs only for project cost. Can also include refrigerent (R-22) and coil cleaner costs. No not include other supplies/part charges.","Ok to process if not all 'circles' are checked on checklist.","If a second credit invoice was created, we need to include a copy with application and original invoice.","Incentive capped at project cost.",{"$nulls":4},"For UOM question: If multiple compressors, divide total # of cows by # of compressors to get # of cows/compressor. Quantity is the number of compressors serviced.",{"$nulls":6},"N/A","N/A",{"v":40,"d":"$40.00"},"Compressor  ","N/A","N/A","N/A",4033,"N/A","N/A","No","No","N/A",{"v":1,"d":"100.0%"},"N/A","Yes","AG4403: Refrigeration System Tune-Up, Agriculture","No","No","Enter # of Milking Cows per Compressor",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR457=\"Agribusiness\", $AR457=\"Ag\",$AR457=\"Propane\", $AR457=\"Ag Propane\", $AR457=\"Ag-Propane\"),$AC457,  $AB457),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR457=\"Agribusiness\", $AR457=\"Ag\",$AR457=\"Propane\", $AR457=\"Ag Propane\", $AR457=\"Ag-Propane\"),$AC457,  $AB457),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]
["Not Eligible",5564,"Not Eligible","Grain Dryer, Tune-up","5564: Grain Dryer, Tune-up","Only corn dryers are eligible","Project cost includes tune-up labor cost and travel expenses. Replacement part costs are not included.","Eligible for natural gas dryers only","Unit of measure for savings is number of acres of corn planted",{"$nulls":5},"If electric utility is non-participating, notify TR. Non-participating electric utility OK, but we will need to adjust electric savings. Consult with PM if incentive should be adjusted. ",{"$nulls":6},"N/A","N/A",{"v":100,"d":"$100.00"},"Tune-up","N/A","N/A","N/A",5564,"N/A","N/A","No","No","N/A",{"v":1,"d":"100.0%"},"N/A","No","5564: Grain Dryer, Tune-up","No","No","Per acre corn planted",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR458=\"Agribusiness\", $AR458=\"Ag\",$AR458=\"Propane\", $AR458=\"Ag Propane\", $AR458=\"Ag-Propane\"),$AC458,  $AB458),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR458=\"Agribusiness\", $AR458=\"Ag\",$AR458=\"Propane\", $AR458=\"Ag Propane\", $AR458=\"Ag-Propane\"),$AC458,  $AB458),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]
["Not Eligible",5565,"Not Eligible","Grain Dryer, Tune-up, Propane-Fueled","5565: Grain Dryer, Tune-up, Propane-Fueled","Only corn dryers are eligible","Project cost includes tune-up labor cost and travel expenses. Replacement part costs are not included.","Eligible for propane dryers only","Unit of measure for savings is number of acres of corn planted","TR will enter savings in AgPropane workbook",{"$nulls":4},"If electric utility is non-participating, notify TR. Non-participating electric utility OK, but we will need to adjust electric savings. Consult with PM if incentive should be adjusted. ",{"$nulls":6},"N/A","N/A",{"v":100,"d":"$100.00"},"Tune-up","N/A","N/A","N/A",5565,"N/A","N/A","No","No","N/A",{"v":1,"d":"100.0%"},"N/A","No","5565: Grain Dryer, Tune-up, Propane-Fueled","No","Yes","Per acre corn planted",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR459=\"Agribusiness\", $AR459=\"Ag\",$AR459=\"Propane\", $AR459=\"Ag Propane\", $AR459=\"Ag-Propane\"),$AC459,  $AB459),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR459=\"Agribusiness\", $AR459=\"Ag\",$AR459=\"Propane\", $AR459=\"Ag Propane\", $AR459=\"Ag-Propane\"),$AC459,  $AB459),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]
[5190,5190,"Not Eligible","Pump Assessment","5190: Pump Assessment","Must complete a Pump Assessment Data Collection form for each unique pump assessed","Qualifying motors must be 40 HP or greater","Qualifying motors must operate a minimum of 500 hours per year","Incentive is capped at assessment cost.","See 'Guidance Resource Doc' for processing steps",{"$nulls":11},{"v":500,"d":"$500"},"Pump",{"v":500,"d":"$500.00"},"Pump","N/A","N/A",5190,5190,"N/A","N/A","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"N/A","No","5190: Pump Assessment","No","Yes","",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR460=\"Agribusiness\", $AR460=\"Ag\",$AR460=\"Propane\", $AR460=\"Ag Propane\", $AR460=\"Ag-Propane\"),$AC460,  $AB460),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR460=\"Agribusiness\", $AR460=\"Ag\",$AR460=\"Propane\", $AR460=\"Ag Propane\", $AR460=\"Ag-Propane\"),$AC460,  $AB460),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]
[5202,5202,"Not Eligible","Bonus, VSD after Pump Assessment","5202: Bonus, VSD after Pump Assessment","50% bonus up to $2000 for installing a VSD after completing a pump assessment","Project must be completed within 6 months of assessment","This bonus measure should be included on the application for the VSD incentive.",{"$nulls":13},"Varies","VSD","Varies","VSD","N/A","N/A",5202,5202,"N/A","N/A","No","No","N/A","N/A","N/A","No","5202: Bonus, VSD after Pump Assessment","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR461=\"Agribusiness\", $AR461=\"Ag\",$AR461=\"Propane\", $AR461=\"Ag Propane\", $AR461=\"Ag-Propane\"),$AC461,  $AB461),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR461=\"Agribusiness\", $AR461=\"Ag\",$AR461=\"Propane\", $AR461=\"Ag Propane\", $AR461=\"Ag-Propane\"),$AC461,  $AB461),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]
[{"$nulls":3},"-------------------------------SPECIAL OFFERS B&I-------------------------------","-------------------------------SPECIAL OFFERS B&I-------------------------------",{"$nulls":32},"-------------------------------SPECIAL OFFERS B&I-------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR462=\"Agribusiness\", $AR462=\"Ag\",$AR462=\"Propane\", $AR462=\"Ag Propane\", $AR462=\"Ag-Propane\"),$AC462,  $AB462),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR462=\"Agribusiness\", $AR462=\"Ag\",$AR462=\"Propane\", $AR462=\"Ag Propane\", $AR462=\"Ag-Propane\"),$AC462,  $AB462),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
[{"$nulls":4},"",{"$nulls":35},"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR463=\"Agribusiness\", $AR463=\"Ag\",$AR463=\"Propane\", $AR463=\"Ag Propane\", $AR463=\"Ag-Propane\"),$AC463,  $AB463),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR463=\"Agribusiness\", $AR463=\"Ag\",$AR463=\"Propane\", $AR463=\"Ag Propane\", $AR463=\"Ag-Propane\"),$AC463,  $AB463),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
[{"$nulls":4},"",{"$nulls":32},"",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR464=\"Agribusiness\", $AR464=\"Ag\",$AR464=\"Propane\", $AR464=\"Ag Propane\", $AR464=\"Ag-Propane\"),$AC464,  $AB464),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR464=\"Agribusiness\", $AR464=\"Ag\",$AR464=\"Propane\", $AR464=\"Ag Propane\", $AR464=\"Ag-Propane\"),$AC464,  $AB464),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]
[{"$nulls":3},"-------------------------------SPECIAL OFFERS LI-------------------------------","-------------------------------SPECIAL OFFERS LI-------------------------------",{"$nulls":32},"-------------------------------SPECIAL OFFERS LI-------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR465=\"Agribusiness\", $AR465=\"Ag\",$AR465=\"Propane\", $AR465=\"Ag Propane\", $AR465=\"Ag-Propane\"),$AC465,  $AB465),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR465=\"Agribusiness\", $AR465=\"Ag\",$AR465=\"Propane\", $AR465=\"Ag Propane\", $AR465=\"Ag-Propane\"),$AC465,  $AB465),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
[{"$nulls":4},"",{"$nulls":35},"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR466=\"Agribusiness\", $AR466=\"Ag\",$AR466=\"Propane\", $AR466=\"Ag Propane\", $AR466=\"Ag-Propane\"),$AC466,  $AB466),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR466=\"Agribusiness\", $AR466=\"Ag\",$AR466=\"Propane\", $AR466=\"Ag Propane\", $AR466=\"Ag-Propane\"),$AC466,  $AB466),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
[{"$nulls":4},"",{"$nulls":32},{"$f":"IF(ISBLANK(A467),\"\",IF(A467<>\"Not Eligible\",A467,IF(B467<>\"Not Eligible\",B467,C467))&\": \") &D467","v":""},null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR467=\"Agribusiness\", $AR467=\"Ag\",$AR467=\"Propane\", $AR467=\"Ag Propane\", $AR467=\"Ag-Propane\"),$AC467,  $AB467),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR467=\"Agribusiness\", $AR467=\"Ag\",$AR467=\"Propane\", $AR467=\"Ag Propane\", $AR467=\"Ag-Propane\"),$AC467,  $AB467),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]
[{"$nulls":3},"-------------------------------SPECIAL OFFERS S&G-------------------------------","-------------------------------SPECIAL OFFERS S&G-------------------------------",{"$nulls":32},"-------------------------------SPECIAL OFFERS S&G-------------------------------",null,null,"",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR468=\"Agribusiness\", $AR468=\"Ag\",$AR468=\"Propane\", $AR468=\"Ag Propane\", $AR468=\"Ag-Propane\"),$AC468,  $AB468),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR468=\"Agribusiness\", $AR468=\"Ag\",$AR468=\"Propane\", $AR468=\"Ag Propane\", $AR468=\"Ag-Propane\"),$AC468,  $AB468),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""}]
["H4419","Not Eligible","Not Eligible","Boiler Tune Up, Non-EBTU","Not Eligible: Boiler Tune Up, Non-EBTU","TA must perform a combustion efficiency test after tune-up and complete checklist on app","If multiple boilers serviced on same site, list number of boilers and total MBh","Use a separate application for each unique job site","Incentive is based on MBh Input value","Incentives are capped at 100% of tune-up cost",{"$nulls":4},"Ok to include interal labor costs for Schools and Government customers as long as proper documentation provided.",{"$nulls":6},{"v":0.05,"d":"$0.05"},"MBh Input","N/A","N/A","N/A","N/A",4419,"N/A","N/A","N/A","No","N/A",{"v":1,"d":"100.0%"},"N/A","N/A","Yes","H4419: Boiler Tune Up, Non-EBTU","No","No","MBh",{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR469=\"Agribusiness\", $AR469=\"Ag\",$AR469=\"Propane\", $AR469=\"Ag Propane\", $AR469=\"Ag-Propane\"),$AC469,  $AB469),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":0},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR469=\"Agribusiness\", $AR469=\"Ag\",$AR469=\"Propane\", $AR469=\"Ag Propane\", $AR469=\"Ag-Propane\"),$AC469,  $AB469),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":0},"Special Offer"]
[5190,5190,"Not Eligible","Pump Assessment","5190: Pump Assessment","Must complete a Pump Assessment Data Collection form for each unique pump assessed","Qualifying motors must be 40 HP or greater","Qualifying motors must operate a minimum of 500 hours per year","Incentive is capped at assessment cost.","See 'Guidance Resource Doc' for processing steps",{"$nulls":11},{"v":500,"d":"$500"},"Pump",{"v":500,"d":"$500.00"},"Pump","N/A","N/A",5190,5190,"N/A","N/A","No","No",{"v":1,"d":"100.0%"},{"v":1,"d":"100.0%"},"N/A","No","5190: Pump Assessment","No","Yes",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR470=\"Agribusiness\", $AR470=\"Ag\",$AR470=\"Propane\", $AR470=\"Ag Propane\", $AR470=\"Ag-Propane\"),$AC470,  $AB470),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR470=\"Agribusiness\", $AR470=\"Ag\",$AR470=\"Propane\", $AR470=\"Ag Propane\", $AR470=\"Ag-Propane\"),$AC470,  $AB470),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]
[5202,5202,"Not Eligible","Bonus, VSD after Pump Assessment","5202: Bonus, VSD after Pump Assessment","50% bonus up to $2000 for installing a VSD after completing a pump assessment","Project must be completed within 6 months of assessment","This bonus measure should be included on the application for the VSD incentive.",{"$nulls":13},"Varies","VSD","Varies","VSD","N/A","N/A",5202,5202,"N/A","N/A","No","No","N/A","N/A","N/A","No","5202: Bonus, VSD after Pump Assessment","No","No",null,{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR471=\"Agribusiness\", $AR471=\"Ag\",$AR471=\"Propane\", $AR471=\"Ag Propane\", $AR471=\"Ag-Propane\"),$AC471,  $AB471),'[4]UOM Range'!$A$4:$I$500,7,FALSE), \"\"),\"\")","v":""},{"$f":"IFERROR(_xlfn.IFNA(VLOOKUP(IF(OR($AR471=\"Agribusiness\", $AR471=\"Ag\",$AR471=\"Propane\", $AR471=\"Ag Propane\", $AR471=\"Ag-Propane\"),$AC471,  $AB471),'[4]UOM Range'!$A$4:$I$500,8,FALSE), \"\"),\"\")","v":""},"Special Offer"]

{"sheet":"Deemed Savings","index":5,"n_rows":940,"n_cols":7,"rows_kept":940,"hidden":true}
["MMID","Sector Savings Name","Sector","Measure Master","kW Savings Summer Peak Demand","kW Savings Winter Peak Demand","kWh Savings First Year"]
["L10028","LED Fixture, Downlights, Interior","Agribusiness","LED Fixture, Downlights, Interior",0.0281,0.0307,{"v":197,"d":"197.0000"}]
["L10029","LED Fixture, Downlights, Exterior","Agribusiness","LED Fixture, Downlights, Exterior",{"v":0,"d":"0.0000"},{"v":0.036,"d":"0.0360"},{"v":350,"d":"350.0000"}]
["L10039","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior","Agribusiness","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior",0.0181,0.0197,{"v":127,"d":"127.0000"}]
["L10040","Four Pin-Base Lamp Replacing CFL, DLC Listed, Exterior","Agribusiness","Four Pin-Base Lamp Replacing CFL, DLC Listed, Exterior",{"v":0,"d":"0.0000"},0.0122,{"v":118,"d":"118.0000"}]
["L10042","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)","Agribusiness","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)",0.2622,0.2856,{"v":1838,"d":"1838.0000"}]
["L10043","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior","Agribusiness","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior",{"v":0,"d":"0.0000"},{"v":0.772,"d":"0.7720"},{"v":751,"d":"751.0000"}]
["L10211","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC","Agribusiness","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC",0.0264,0.0287,{"v":172,"d":"172.0000"}]
["L10212","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC","Agribusiness","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC",0.0846,0.0922,{"v":540,"d":"540.0000"}]
["L10213","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC","Agribusiness","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC",0.0495,{"v":0.054,"d":"0.0540"},{"v":320,"d":"320.0000"}]
["L10214","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC","Agribusiness","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC",0.0174,0.0189,{"v":115,"d":"115.0000"}]
["L10215","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC","Agribusiness","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC",0.1557,0.1696,{"v":1216,"d":"1216.0000"}]
["L10216","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC","Agribusiness","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC",0.2411,0.2627,{"v":1552,"d":"1552.0000"}]
["L10217","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC","Agribusiness","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC",0.1015,0.1106,{"v":665,"d":"665.0000"}]
["L10218","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC","Agribusiness","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC",0.1488,0.1621,{"v":972,"d":"972.0000"}]
["L10281","1’ to 3’ LED Linear Ambient Fixture, Interior","Agribusiness","1’ to 3’ LED Linear Ambient Fixture, Interior",0.0061,{"v":6.6E-3,"d":"0.0066"},{"v":43,"d":"43.0000"}]
["L10282","4' LED Linear Ambient Fixture, Interior","Agribusiness","4' LED Linear Ambient Fixture, Interior",0.0122,0.0133,{"v":86,"d":"86.0000"}]
["L10283","8' LED Linear Ambient Fixture, Interior","Agribusiness","8' LED Linear Ambient Fixture, Interior",0.0244,0.0266,{"v":171,"d":"171.0000"}]
["L10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","Agribusiness","1’ to 3’ LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},{"v":0.003,"d":"0.0030"},{"v":30,"d":"30.0000"}]
["L10285","4' LED Linear Ambient Fixture, Exterior","Agribusiness","4' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0061,{"v":59,"d":"59.0000"}]
["L10286","8' LED Linear Ambient Fixture, Exterior","Agribusiness","8' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0121,{"v":118,"d":"118.0000"}]
["L10287","General Wattage Reduction, Interior","Agribusiness","General Wattage Reduction, Interior",0.0007,0.0007,{"v":4.7,"d":"4.7000"}]
["L10288","General Wattage Reduction, Exterior","Agribusiness","General Wattage Reduction, Exterior",{"v":0,"d":"0.0000"},0.0005,{"v":4.38,"d":"4.3800"}]
["L10289","Fixture Elimination, Interior","Agribusiness","Fixture Elimination, Interior",0.0007,0.0007,{"v":4.7,"d":"4.7000"}]
["L10290","Fixture Elimination, Exterior","Agribusiness","Fixture Elimination, Exterior",{"v":0,"d":"0.0000"},0.0005,{"v":4.38,"d":"4.3800"}]
["L2482","Occupancy Sensor, LED Refrigerated Case Lights","Agribusiness","Occupancy Sensor, LED Refrigerated Case Lights",0.0075,null,{"v":65,"d":"65.0000"}]
["L2768","LED, Exit Sign, Retrofit","Agribusiness","LED, Exit Sign, Retrofit",0.0213,0.0213,{"v":187,"d":"187.0000"}]
["L3093","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay","Agribusiness","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay",0.0013,{"v":1.5E-3,"d":"0.0015"},{"v":9.4,"d":"9.4000"}]
["L3094","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay","Agribusiness","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay",{"v":0,"d":"0.0000"},0.0009,{"v":8.76,"d":"8.7600"}]
["L3095","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay","Agribusiness","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay",0.5479,{"v":0.597,"d":"0.5970"},{"v":3842,"d":"3842.0000"}]
["L3096","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay","Agribusiness","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay",0.5282,0.5755,{"v":3704,"d":"3704.0000"}]
["L3097","LED Fixture, Bilevel, Stairwell and Passageway","Agribusiness","LED Fixture, Bilevel, Stairwell and Passageway",0.0228,0.0248,{"v":160,"d":"160.0000"}]
["L3111","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer","Agribusiness","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer",0.0386,0.0421,{"v":271,"d":"271.0000"}]
["L3114","LED, Horizontal Case Lighting","Agribusiness","LED, Horizontal Case Lighting",0.0174,0.0174,{"v":112,"d":"112.0000"}]
["L3393","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed","Agribusiness","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed",0.0664,null,{"v":465,"d":"465.0000"}]
["L3400","LED Fixture, 2x2, Low Output, DLC Listed","Agribusiness","LED Fixture, 2x2, Low Output, DLC Listed",0.0186,0.0203,{"v":131,"d":"131.0000"}]
["L3401","LED Fixture, 2x2, High Output, DLC Listed","Agribusiness","LED Fixture, 2x2, High Output, DLC Listed",0.0755,0.0822,{"v":529,"d":"529.0000"}]
["L3406","Daylighting Controls","Agribusiness","Daylighting Controls",0.0002,0.0002,{"v":1.32,"d":"1.3200"}]
["L3511","LED Replacement of 4’ T8 Lamps w/Integral or External Driver","Agribusiness","LED Replacement of 4’ T8 Lamps w/Integral or External Driver",{"v":6.6E-3,"d":"0.0066"},null,{"v":46,"d":"46.0000"}]
["L3512","LED Replacement of 4’ T8 Lamps utilizing existing ballast","Agribusiness","LED Replacement of 4’ T8 Lamps utilizing existing ballast",0.0072,null,{"v":50,"d":"50.0000"}]
["L3738","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section",{"v":1E-3,"d":"0.0010"},null,{"v":7,"d":"7.0000"}]
["L3739","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section",0.0106,null,{"v":74,"d":"74.0000"}]
["L3740","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section",0.0026,null,{"v":19,"d":"19.0000"}]
["L3741","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section",0.0082,null,{"v":58,"d":"58.0000"}]
["L3759","LED Replacement of 4’ T8 Lamps, Direct Wire","Agribusiness","LED Replacement of 4’ T8 Lamps, Direct Wire",0.0077,null,{"v":54,"d":"54.0000"}]
["L3760","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer","Agribusiness","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0109,null,{"v":76,"d":"76.0000"}]
["L3903","LED Signage Retrofit, Interior","Agribusiness","LED Signage Retrofit, Interior",0.0013,{"v":1.5E-3,"d":"0.0015"},{"v":9.4,"d":"9.4000"}]
["L3904","LED Signage Retrofit, Exterior","Agribusiness","LED Signage Retrofit, Exterior",{"v":0,"d":"0.0000"},0.0009,{"v":8.76,"d":"8.7600"}]
["L3929","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL",{"v":0,"d":"0.0000"},null,{"v":40,"d":"40.0000"}]
["L3930","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL",{"v":0,"d":"0.0000"},null,{"v":24,"d":"24.0000"}]
["L3931","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W",{"v":0,"d":"0.0000"},null,{"v":18,"d":"18.0000"}]
["L3932","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL",0.0062,null,{"v":43,"d":"43.0000"}]
["L3933","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL",0.0037,null,{"v":26,"d":"26.0000"}]
["L3934","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W",0.0027,null,{"v":19,"d":"19.0000"}]
["L3935","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent",{"v":0,"d":"0.0000"},null,{"v":499,"d":"499.0000"}]
["L3936","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent",{"v":0,"d":"0.0000"},null,{"v":364,"d":"364.0000"}]
["L3937","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent",{"v":0,"d":"0.0000"},null,{"v":284,"d":"284.0000"}]
["L3938","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent",{"v":0,"d":"0.0000"},null,{"v":237,"d":"237.0000"}]
["L3939","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 36W – 54W Incandescent","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 36W – 54W Incandescent",{"v":0,"d":"0.0000"},null,{"v":182,"d":"182.0000"}]
["L3940","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent","Agribusiness","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent",{"v":0,"d":"0.0000"},null,{"v":114,"d":"114.0000"}]
["L3941","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W",0.0763,null,{"v":535,"d":"535.0000"}]
["L3942","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W",0.0557,null,{"v":390,"d":"390.0000"}]
["L3943","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W",0.0434,null,{"v":305,"d":"305.0000"}]
["L3944","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W",0.0363,null,{"v":254,"d":"254.0000"}]
["L3945","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W",0.0279,null,{"v":195,"d":"195.0000"}]
["L3946","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W","Agribusiness","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W",0.0174,null,{"v":122,"d":"122.0000"}]
["L4280","LED, Exterior Fixture, Low Output, <= 4,999 lumens","Agribusiness","LED, Exterior Fixture, Low Output, <= 4,999 lumens",{"v":0,"d":"0.0000"},0.0122,{"v":389,"d":"389.0000"}]
["L4281","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens","Agribusiness","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens",{"v":0,"d":"0.0000"},{"v":0.027,"d":"0.0270"},{"v":731,"d":"731.0000"}]
["L4282","LED, Exterior Fixture, High Output, 10,000-29,999 lumens","Agribusiness","LED, Exterior Fixture, High Output, 10,000-29,999 lumens",{"v":0,"d":"0.0000"},0.0601,{"v":1806,"d":"1806.0000"}]
["L4283","LED, Exterior Fixture, Very High Output, >= 30,000 lumens","Agribusiness","LED, Exterior Fixture, Very High Output, >= 30,000 lumens",{"v":0,"d":"0.0000"},0.1486,{"v":3279,"d":"3279.0000"}]
["L4314","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12","Agribusiness","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12",0.0211,null,{"v":148,"d":"148.0000"}]
["L4315","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, Exterior","Agribusiness","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":138,"d":"138.0000"}]
["L4316","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, 24/7","Agribusiness","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, 24/7",0.0314,null,{"v":275,"d":"275.0000"}]
["L4317","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO","Agribusiness","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO",0.0468,null,{"v":328,"d":"328.0000"}]
["L4318","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, Exterior","Agribusiness","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":306,"d":"306.0000"}]
["L4319","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, 24/7","Agribusiness","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, 24/7",0.0699,null,{"v":612,"d":"612.0000"}]
["L4320","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12","Agribusiness","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12",0.0274,null,{"v":192,"d":"192.0000"}]
["L4321","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior","Agribusiness","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":179,"d":"179.0000"}]
["L4322","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, 24/7","Agribusiness","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, 24/7",0.0408,null,{"v":358,"d":"358.0000"}]
["L4323","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO","Agribusiness","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO",0.0783,null,{"v":549,"d":"549.0000"}]
["L4324","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior","Agribusiness","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":512,"d":"512.0000"}]
["L4325","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, 24/7","Agribusiness","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, 24/7",0.1168,null,{"v":1024,"d":"1024.0000"}]
["L4326","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12","Agribusiness","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12",0.0499,null,{"v":350,"d":"350.0000"}]
["L4327","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, Exterior","Agribusiness","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":326,"d":"326.0000"}]
["L4328","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, 24/7","Agribusiness","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, 24/7",0.0744,null,{"v":652,"d":"652.0000"}]
["L4329","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO","Agribusiness","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO",0.1008,null,{"v":707,"d":"707.0000"}]
["L4330","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, Exterior","Agribusiness","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":659,"d":"659.0000"}]
["L4331","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, 24/7","Agribusiness","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, 24/7",0.1504,null,{"v":1318,"d":"1318.0000"}]
["L4347","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay","Agribusiness","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay",0.1019,null,{"v":714,"d":"714.0000"}]
["L4348","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior","Agribusiness","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior",{"v":0,"d":"0.0000"},null,{"v":47,"d":"47.0000"}]
["L4349","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7","Agribusiness","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7",0.0107,null,{"v":94,"d":"94.0000"}]
["L4350","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior","Agribusiness","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior",{"v":0,"d":"0.0000"},null,{"v":50,"d":"50.0000"}]
["L4351","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7","Agribusiness","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7",0.0114,null,{"v":100,"d":"100.0000"}]
["L4352","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior","Agribusiness","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior",{"v":0,"d":"0.0000"},null,{"v":43,"d":"43.0000"}]
["L4353","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior, 24/7","Agribusiness","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior, 24/7",0.0098,null,{"v":86,"d":"86.0000"}]
["AG4695","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, Agriculture","Agribusiness","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, Agriculture",0.1274,0.1389,{"v":1084,"d":"1084.0000"}]
["AG4696","LED Fixture, <250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture","Agribusiness","LED Fixture, <250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture",{"v":0.135,"d":"0.1350"},0.1471,{"v":1227,"d":"1227.0000"}]
["AG4697","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, Agriculture","Agribusiness","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, Agriculture",0.1967,0.2144,{"v":1380,"d":"1380.0000"}]
["AG4698","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay, Agriculture","Agribusiness","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay, Agriculture",0.1356,null,{"v":1251,"d":"1251.0000"}]
["AG4699","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture","Agribusiness","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture",0.5479,{"v":0.597,"d":"0.5970"},{"v":3842,"d":"3842.0000"}]
["AG4701","<=180W LED, replacing or instead of 6L T8 or 4L T5HO, Agriculture","Agribusiness","<=180W LED, replacing or instead of 6L T8 or 4L T5HO, Agriculture",0.0664,null,{"v":465,"d":"465.0000"}]
["AG4702","<=250W LED, replacing or instead of 8LT8 or 6LT5HO, Agriculture","Agribusiness","<=250W LED, replacing or instead of 8LT8 or 6LT5HO, Agriculture",0.1019,null,{"v":714,"d":"714.0000"}]
["L4703","DLC Listed, Mogul Screw-Base (E39) lamp replacing HID (various), Agriculture","Agribusiness","DLC Listed, Mogul Screw-Base (E39) lamp replacing HID (various), Agriculture",0.0007,null,{"v":4.7,"d":"4.7000"}]
["L4781","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour",{"v":0.004,"d":"0.0040"},null,{"v":35,"d":"35.0000"}]
["L4782","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":17,"d":"17.0000"}]
["L4783","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour",0.0122,null,{"v":107,"d":"107.0000"}]
["L4784","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":54,"d":"54.0000"}]
["L4785","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour",{"v":1.5E-3,"d":"0.0015"},null,{"v":13,"d":"13.0000"}]
["L4786","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":7,"d":"7.0000"}]
["L4787","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour",0.0158,null,{"v":138,"d":"138.0000"}]
["L4788","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":69,"d":"69.0000"}]
["L4793","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer","Agribusiness","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0081,null,{"v":57,"d":"57.0000"}]
["L4795","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay","Agribusiness","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay",0.1385,null,{"v":971,"d":"971.0000"}]
["L4796","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay","Agribusiness","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay",0.1675,null,{"v":1175,"d":"1175.0000"}]
["L4797","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) ","Agribusiness","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) ",{"v":0.006,"d":"0.0060"},null,{"v":42,"d":"42.0000"}]
["L4798","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) ","Agribusiness","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) ",{"v":0.007,"d":"0.0070"},null,{"v":49,"d":"49.0000"}]
["L4799","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Agribusiness","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0069,null,{"v":48,"d":"48.0000"}]
["L4800","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) ","Agribusiness","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) ",0.0093,null,{"v":65,"d":"65.0000"}]
["L4801","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) ","Agribusiness","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) ",0.0087,null,{"v":61,"d":"61.0000"}]
["L4802","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Agribusiness","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0084,null,{"v":59,"d":"59.0000"}]
["L4803","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) ","Agribusiness","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) ",{"v":7.6E-3,"d":"0.0076"},null,{"v":53,"d":"53.0000"}]
["L4804","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) ","Agribusiness","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) ",0.0237,null,{"v":166,"d":"166.0000"}]
["L4805","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) ","Agribusiness","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) ",0.0106,null,{"v":75,"d":"75.0000"}]
["L4806","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) ","Agribusiness","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) ",0.0249,null,{"v":175,"d":"175.0000"}]
["L4807","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) ","Agribusiness","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) ",0.0091,null,{"v":64,"d":"64.0000"}]
["L4808","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) ","Agribusiness","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) ",0.0224,null,{"v":157,"d":"157.0000"}]
["L4809","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) ","Agribusiness","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) ",{"v":0.019,"d":"0.0190"},null,{"v":133,"d":"133.0000"}]
["L4810","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) ","Agribusiness","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) ",0.0147,null,{"v":103,"d":"103.0000"}]
["L4811","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Agribusiness","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0178,null,{"v":124,"d":"124.0000"}]
["L4812","Non-High Bay Occupancy/Vacancy Sensor","Agribusiness","Non-High Bay Occupancy/Vacancy Sensor",0.0002,0.0002,{"v":1.13,"d":"1.1300"}]
["L4813","LED Fixture, Track/Mono/Accent","Agribusiness","LED Fixture, Track/Mono/Accent",0.0007,0.0007,{"v":4.7,"d":"4.7000"}]
["L4830","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior","Agribusiness","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior",{"v":0,"d":"0.0000"},null,{"v":116,"d":"116.0000"}]
["L4831","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior","Agribusiness","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior",{"v":0,"d":"0.0000"},null,{"v":124,"d":"124.0000"}]
["L4832","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior","Agribusiness","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior",{"v":0,"d":"0.0000"},null,{"v":96,"d":"96.0000"}]
["L4833","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior 24/7","Agribusiness","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior 24/7",0.0265,null,{"v":232,"d":"232.0000"}]
["L4834","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior 24/7","Agribusiness","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior 24/7",0.0283,null,{"v":248,"d":"248.0000"}]
["L4835","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7","Agribusiness","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7",{"v":0.022,"d":"0.0220"},null,{"v":192,"d":"192.0000"}]
["AG5024","Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1,000W HID, Agriculture","Agribusiness","Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1,000W HID, Agriculture",{"v":0.454,"d":"0.4540"},{"v":0.454,"d":"0.4540"},{"v":2486,"d":"2486.0000"}]
["AG5025","Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture","Agribusiness","Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture",{"v":0.302,"d":"0.3020"},{"v":0.302,"d":"0.3020"},{"v":1653,"d":"1653.0000"}]
["AG5026","Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1,000W HID, Agriculture","Agribusiness","Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1,000W HID, Agriculture",{"v":0,"d":"0.0000"},{"v":0.2,"d":"0.2000"},{"v":962,"d":"962.0000"}]
["AG5027","Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture","Agribusiness","Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture",{"v":0,"d":"0.0000"},{"v":0.14,"d":"0.1400"},{"v":640,"d":"640.0000"}]
["AG5028","Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture","Agribusiness","Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture",{"v":0,"d":"0.0000"},{"v":0.12,"d":"0.1200"},{"v":575,"d":"575.0000"}]
["L5061","Occupancy Sensors, On/Off, High Bay","Agribusiness","Occupancy Sensors, On/Off, High Bay",0.0003,0.0003,{"v":1.97,"d":"1.9700"}]
["L5062","Bi-Level Controls, High Bay ","Agribusiness","Bi-Level Controls, High Bay ",{"v":1E-4,"d":"0.0001"},{"v":1E-4,"d":"0.0001"},{"v":0.82,"d":"0.8200"}]
["L5063","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn","Agribusiness","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn",{"v":0,"d":"0.0000"},0.0002,{"v":1.48,"d":"1.4800"}]
["L5064","Bi-level Controls, Parking Garage Fixtures, 24 Hour","Agribusiness","Bi-level Controls, Parking Garage Fixtures, 24 Hour",0.0003,0.0003,{"v":2.96,"d":"2.9600"}]
["L5211","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Agribusiness","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0.035,"d":"0.0350"},null,{"v":245,"d":"245.0000"}]
["L5212","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Agribusiness","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0.026,"d":"0.0260"},null,{"v":180,"d":"180.0000"}]
["L5213","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Agribusiness","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0.021,"d":"0.0210"},null,{"v":147,"d":"147.0000"}]
["L5214","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL","Agribusiness","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0.015,"d":"0.0150"},null,{"v":102,"d":"102.0000"}]
["L5215","Omnidirectional Interior LED with rated lumen output of 250-449 replacing incandescent or CFL","Agribusiness","Omnidirectional Interior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0.013,"d":"0.0130"},null,{"v":92,"d":"92.0000"}]
["L5216","Decorative Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Agribusiness","Decorative Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0.035,"d":"0.0350"},null,{"v":245,"d":"245.0000"}]
["L5217","Decorative Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Agribusiness","Decorative Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0.024,"d":"0.0240"},null,{"v":169,"d":"169.0000"}]
["L5218","Decorative Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Agribusiness","Decorative Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0.022,"d":"0.0220"},null,{"v":151,"d":"151.0000"}]
["L5219","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL","Agribusiness","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0.015,"d":"0.0150"},null,{"v":102,"d":"102.0000"}]
["L5220","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL","Agribusiness","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0.013,"d":"0.0130"},null,{"v":90,"d":"90.0000"}]
["L5221","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Agribusiness","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":228,"d":"228.0000"}]
["L5222","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Agribusiness","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":168,"d":"168.0000"}]
["L5223","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Agribusiness","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":137,"d":"137.0000"}]
["L5224","Omnidirectional Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL","Agribusiness","Omnidirectional Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":95,"d":"95.0000"}]
["L5226","Decorative Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Agribusiness","Decorative Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":228,"d":"228.0000"}]
["L5227","Decorative Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Agribusiness","Decorative Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":157,"d":"157.0000"}]
["L5228","Decorative Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Agribusiness","Decorative Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":141,"d":"141.0000"}]
["L5229","Decorative Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL","Agribusiness","Decorative Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":95,"d":"95.0000"}]
["L5230","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL","Agribusiness","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":84,"d":"84.0000"}]
["L5235","Refrigeration Savings for Lighting Upgrades in Freezers","Agribusiness","Refrigeration Savings for Lighting Upgrades in Freezers",0.0005,0.0005,{"v":3.36,"d":"3.3600"}]
["L5236","Refrigeration Savings for Lighting Upgrades in Coolers","Agribusiness","Refrigeration Savings for Lighting Upgrades in Coolers",0.0003,0.0003,{"v":2.04,"d":"2.0400"}]
["L5445","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section",{"v":2.3E-3,"d":"0.0023"},null,{"v":16,"d":"16.0000"}]
["L5446","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":15,"d":"15.0000"}]
["L5447","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7","Agribusiness","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7",0.0034,null,{"v":30,"d":"30.0000"}]
["L5448","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section",0.0044,null,{"v":31,"d":"31.0000"}]
["L5449","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":29,"d":"29.0000"}]
["L5450","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7","Agribusiness","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7",{"v":6.6E-3,"d":"0.0066"},null,{"v":58,"d":"58.0000"}]
["L5451","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior","Agribusiness","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior",{"v":0.008,"d":"0.0080"},0.0088,{"v":56,"d":"56.0000"}]
["L5452","4' TLED, Replacing 4' T5HO Lamp, Interior","Agribusiness","4' TLED, Replacing 4' T5HO Lamp, Interior",0.0246,0.0268,{"v":172,"d":"172.0000"}]
["L5453","2' TLED, Replacing 2' T8 or T12 Lamp, Interior","Agribusiness","2' TLED, Replacing 2' T8 or T12 Lamp, Interior",0.0069,0.0075,{"v":48,"d":"48.0000"}]
["L5454","8' TLED, Replacing 8' T8 or T12 Lamp, Interior","Agribusiness","8' TLED, Replacing 8' T8 or T12 Lamp, Interior",0.0133,0.0145,{"v":93,"d":"93.0000"}]
["L5455","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior 24/7","Agribusiness","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior 24/7",0.0118,null,{"v":104,"d":"104.0000"}]
["L5456","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior","Agribusiness","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior",{"v":0,"d":"0.0000"},0.0054,{"v":53,"d":"53.0000"}]
["L5457","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7","Agribusiness","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7",0.0198,null,{"v":174,"d":"174.0000"}]
["L5458","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior","Agribusiness","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior",{"v":0,"d":"0.0000"},null,{"v":87,"d":"87.0000"}]
["L5459","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer","Agribusiness","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer",0.0092,{"v":0.01,"d":"0.0100"},{"v":64,"d":"64.0000"}]
["L5460","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay","Agribusiness","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay",0.0221,0.0224,{"v":155,"d":"155.0000"}]
["L5461","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay","Agribusiness","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay",{"v":0.069,"d":"0.0690"},0.0752,{"v":484,"d":"484.0000"}]
["L10028","LED Fixture, Downlights, Interior","B&I","LED Fixture, Downlights, Interior",0.0319,0.0328,{"v":157,"d":"157.0000"}]
["L10029","LED Fixture, Downlights, Exterior","B&I","LED Fixture, Downlights, Exterior",{"v":0,"d":"0.0000"},{"v":0.036,"d":"0.0360"},{"v":350,"d":"350.0000"}]
["L10039","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior","B&I","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior",0.0205,0.0211,{"v":101,"d":"101.0000"}]
["L10040","Four Pin-Base Lamp Replacing CFL, DLC Listed, Exterior","B&I","Four Pin-Base Lamp Replacing CFL, DLC Listed, Exterior",{"v":0,"d":"0.0000"},0.0122,{"v":118,"d":"118.0000"}]
["L10042","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)","B&I","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)",0.1958,0.2009,{"v":961,"d":"961.0000"}]
["L10043","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior","B&I","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior",{"v":0,"d":"0.0000"},{"v":0.772,"d":"0.7720"},{"v":751,"d":"751.0000"}]
["L10211","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC","B&I","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC",0.0335,0.0222,{"v":149,"d":"149.0000"}]
["L10212","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC","B&I","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC",{"v":0.099,"d":"0.0990"},0.1016,{"v":444,"d":"444.0000"}]
["L10213","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC","B&I","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC",0.0598,0.0614,{"v":272,"d":"272.0000"}]
["L10214","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC","B&I","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC",0.0224,{"v":0.023,"d":"0.0230"},{"v":105,"d":"105.0000"}]
["L10215","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC","B&I","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC",{"v":0.186,"d":"0.1860"},0.1909,{"v":842,"d":"842.0000"}]
["L10216","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC","B&I","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC",0.2882,0.2957,{"v":1305,"d":"1305.0000"}]
["L10217","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC","B&I","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC",0.1268,0.1301,{"v":585,"d":"585.0000"}]
["L10218","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC","B&I","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC",0.1844,0.1893,{"v":848,"d":"848.0000"}]
["L10223","Advanced Lighting Controls, Interior","B&I","Advanced Lighting Controls, Interior",0.0004,0.0004,{"v":2.11,"d":"2.1100"}]
["L10224","Advanced Lighting Controls, Exterior","B&I","Advanced Lighting Controls, Exterior",{"v":0,"d":"0.0000"},0.0002,{"v":1.97,"d":"1.9700"}]
["L10281","1’ to 3’ LED Linear Ambient Fixture, Interior","B&I","1’ to 3’ LED Linear Ambient Fixture, Interior",0.0069,0.0071,{"v":34,"d":"34.0000"}]
["L10282","4' LED Linear Ambient Fixture, Interior","B&I","4' LED Linear Ambient Fixture, Interior",0.0138,0.0142,{"v":68,"d":"68.0000"}]
["L10283","8' LED Linear Ambient Fixture, Interior","B&I","8' LED Linear Ambient Fixture, Interior",0.0277,0.0284,{"v":136,"d":"136.0000"}]
["L10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","B&I","1’ to 3’ LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},{"v":0.003,"d":"0.0030"},{"v":30,"d":"30.0000"}]
["L10285","4' LED Linear Ambient Fixture, Exterior","B&I","4' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0061,{"v":59,"d":"59.0000"}]
["L10286","8' LED Linear Ambient Fixture, Exterior","B&I","8' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0121,{"v":118,"d":"118.0000"}]
["L10287","General Wattage Reduction, Interior","B&I","General Wattage Reduction, Interior",0.0008,0.0008,{"v":3.73,"d":"3.7300"}]
["L10288","General Wattage Reduction, Exterior","B&I","General Wattage Reduction, Exterior",{"v":0,"d":"0.0000"},0.0005,{"v":4.38,"d":"4.3800"}]
["L10289","Fixture Elimination, Interior","B&I","Fixture Elimination, Interior",0.0008,0.0008,{"v":3.73,"d":"3.7300"}]
["L10290","Fixture Elimination, Exterior","B&I","Fixture Elimination, Exterior",{"v":0,"d":"0.0000"},0.0005,{"v":4.38,"d":"4.3800"}]
["L2482","Occupancy Sensor, LED Refrigerated Case Lights","B&I","Occupancy Sensor, LED Refrigerated Case Lights",0.0075,null,{"v":65,"d":"65.0000"}]
["L2768","LED, Exit Sign, Retrofit","B&I","LED, Exit Sign, Retrofit",0.0213,0.0213,{"v":187,"d":"187.0000"}]
["L3091","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay","B&I","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay",0.1446,0.1484,{"v":710,"d":"710.0000"}]
["L3092","LED Fixture, <250 Watts, Replacing 320-400 Watt HID, High Bay","B&I","LED Fixture, <250 Watts, Replacing 320-400 Watt HID, High Bay",0.1531,0.1571,{"v":751,"d":"751.0000"}]
["L3093","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay","B&I","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay",0.2261,{"v":0.229,"d":"0.2290"},{"v":1095,"d":"1095.0000"}]
["L3094","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay","B&I","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay",{"v":0,"d":"0.0000"},0.0009,{"v":8.76,"d":"8.7600"}]
["L3095","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay","B&I","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay",0.6215,0.6379,{"v":3050,"d":"3050.0000"}]
["L3096","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay","B&I","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay",0.5991,0.6149,{"v":2941,"d":"2941.0000"}]
["L3097","LED Fixture, Bilevel, Stairwell and Passageway","B&I","LED Fixture, Bilevel, Stairwell and Passageway",0.0259,0.0265,{"v":127,"d":"127.0000"}]
["L3111","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer","B&I","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer",0.0438,{"v":0.045,"d":"0.0450"},{"v":215,"d":"215.0000"}]
["L3114","LED, Horizontal Case Lighting","B&I","LED, Horizontal Case Lighting",0.0174,0.0174,{"v":112,"d":"112.0000"}]
["L3393","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed","B&I","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed",0.0763,null,{"v":369,"d":"369.0000"}]
["L3400","LED Fixture, 2x2, Low Output, DLC Listed","B&I","LED Fixture, 2x2, Low Output, DLC Listed",0.0211,0.0217,{"v":104,"d":"104.0000"}]
["L3401","LED Fixture, 2x2, High Output, DLC Listed","B&I","LED Fixture, 2x2, High Output, DLC Listed",0.0856,0.0879,{"v":420,"d":"420.0000"}]
["L3406","Daylighting Controls","B&I","Daylighting Controls",0.0002,0.0002,{"v":1.04,"d":"1.0400"}]
["L3511","LED Replacement of 4’ T8 Lamps w/Integral or External Driver","B&I","LED Replacement of 4’ T8 Lamps w/Integral or External Driver",0.0075,null,{"v":36,"d":"36.0000"}]
["L3512","LED Replacement of 4’ T8 Lamps utilizing existing ballast","B&I","LED Replacement of 4’ T8 Lamps utilizing existing ballast",0.0083,null,{"v":40,"d":"40.0000"}]
["L3738","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section",0.0012,null,{"v":6,"d":"6.0000"}]
["L3739","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section",0.0121,null,{"v":59,"d":"59.0000"}]
["L3740","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section",{"v":0.003,"d":"0.0030"},null,{"v":15,"d":"15.0000"}]
["L3741","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section",0.0094,null,{"v":46,"d":"46.0000"}]
["L3759","LED Replacement of 4’ T8 Lamps, Direct Wire","B&I","LED Replacement of 4’ T8 Lamps, Direct Wire",0.0088,null,{"v":43,"d":"43.0000"}]
["L3760","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer","B&I","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0125,null,{"v":61,"d":"61.0000"}]
["L3903","LED Signage Retrofit, Interior","B&I","LED Signage Retrofit, Interior",{"v":1.5E-3,"d":"0.0015"},0.0016,{"v":7.46,"d":"7.4600"}]
["L3904","LED Signage Retrofit, Exterior","B&I","LED Signage Retrofit, Exterior",{"v":0,"d":"0.0000"},0.0009,{"v":8.76,"d":"8.7600"}]
["L3929","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL",{"v":0,"d":"0.0000"},null,{"v":40,"d":"40.0000"}]
["L3930","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL",{"v":0,"d":"0.0000"},null,{"v":24,"d":"24.0000"}]
["L3931","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W",{"v":0,"d":"0.0000"},null,{"v":18,"d":"18.0000"}]
["L3932","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL",0.0071,null,{"v":34,"d":"34.0000"}]
["L3933","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL",0.0042,null,{"v":21,"d":"21.0000"}]
["L3934","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W",0.0032,null,{"v":15,"d":"15.0000"}]
["L3935","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent",{"v":0,"d":"0.0000"},null,{"v":499,"d":"499.0000"}]
["L3936","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent",{"v":0,"d":"0.0000"},null,{"v":364,"d":"364.0000"}]
["L3937","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent",{"v":0,"d":"0.0000"},null,{"v":284,"d":"284.0000"}]
["L3938","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent",{"v":0,"d":"0.0000"},null,{"v":237,"d":"237.0000"}]
["L3939","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 36W – 54W Incandescent","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 36W – 54W Incandescent",{"v":0,"d":"0.0000"},null,{"v":182,"d":"182.0000"}]
["L3940","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent","B&I","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent",{"v":0,"d":"0.0000"},null,{"v":114,"d":"114.0000"}]
["L3941","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W",0.0877,null,{"v":425,"d":"425.0000"}]
["L3942","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W",{"v":0.064,"d":"0.0640"},null,{"v":310,"d":"310.0000"}]
["L3943","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W",0.0499,null,{"v":242,"d":"242.0000"}]
["L3944","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W",0.0417,null,{"v":202,"d":"202.0000"}]
["L3945","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W",{"v":0.032,"d":"0.0320"},null,{"v":155,"d":"155.0000"}]
["L3946","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W","B&I","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W",0.0201,null,{"v":97,"d":"97.0000"}]
["L4280","LED, Exterior Fixture, Low Output, <= 4,999 lumens","B&I","LED, Exterior Fixture, Low Output, <= 4,999 lumens",{"v":0,"d":"0.0000"},0.0122,{"v":389,"d":"389.0000"}]
["L4281","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens","B&I","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens",{"v":0,"d":"0.0000"},{"v":0.027,"d":"0.0270"},{"v":731,"d":"731.0000"}]
["L4282","LED, Exterior Fixture, High Output, 10,000-29,999 lumens","B&I","LED, Exterior Fixture, High Output, 10,000-29,999 lumens",{"v":0,"d":"0.0000"},0.0601,{"v":1806,"d":"1806.0000"}]
["L4283","LED, Exterior Fixture, Very High Output, >= 30,000 lumens","B&I","LED, Exterior Fixture, Very High Output, >= 30,000 lumens",{"v":0,"d":"0.0000"},0.1486,{"v":3279,"d":"3279.0000"}]
["L4314","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12","B&I","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12",0.0242,null,{"v":117,"d":"117.0000"}]
["L4315","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, Exterior","B&I","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":138,"d":"138.0000"}]
["L4316","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, 24/7","B&I","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, 24/7",0.0314,null,{"v":275,"d":"275.0000"}]
["L4317","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO","B&I","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO",0.0538,null,{"v":261,"d":"261.0000"}]
["L4318","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, Exterior","B&I","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":306,"d":"306.0000"}]
["L4319","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, 24/7","B&I","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, 24/7",0.0699,null,{"v":612,"d":"612.0000"}]
["L4320","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12","B&I","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12",0.0314,null,{"v":152,"d":"152.0000"}]
["L4321","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior","B&I","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":179,"d":"179.0000"}]
["L4322","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, 24/7","B&I","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, 24/7",0.0408,null,{"v":358,"d":"358.0000"}]
["L4323","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO","B&I","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO",{"v":0.09,"d":"0.0900"},null,{"v":436,"d":"436.0000"}]
["L4324","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior","B&I","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":512,"d":"512.0000"}]
["L4325","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, 24/7","B&I","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, 24/7",0.1168,null,{"v":1024,"d":"1024.0000"}]
["L4326","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12","B&I","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12",0.0573,null,{"v":278,"d":"278.0000"}]
["L4327","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, Exterior","B&I","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":326,"d":"326.0000"}]
["L4328","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, 24/7","B&I","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, 24/7",0.0744,null,{"v":652,"d":"652.0000"}]
["L4329","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO","B&I","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO",0.1158,null,{"v":561,"d":"561.0000"}]
["L4330","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, Exterior","B&I","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":659,"d":"659.0000"}]
["L4331","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, 24/7","B&I","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, 24/7",0.1504,null,{"v":1318,"d":"1318.0000"}]
["L4347","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay","B&I","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay",0.1171,null,{"v":567,"d":"567.0000"}]
["L4348","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior","B&I","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior",{"v":0,"d":"0.0000"},null,{"v":47,"d":"47.0000"}]
["L4349","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7","B&I","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7",0.0107,null,{"v":94,"d":"94.0000"}]
["L4350","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior","B&I","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior",{"v":0,"d":"0.0000"},null,{"v":50,"d":"50.0000"}]
["L4351","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7","B&I","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7",0.0114,null,{"v":100,"d":"100.0000"}]
["L4352","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior","B&I","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior",{"v":0,"d":"0.0000"},null,{"v":43,"d":"43.0000"}]
["L4353","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior, 24/7","B&I","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior, 24/7",0.0098,null,{"v":86,"d":"86.0000"}]
["L4781","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour",{"v":0.004,"d":"0.0040"},null,{"v":35,"d":"35.0000"}]
["L4782","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":17,"d":"17.0000"}]
["L4783","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour",0.0122,null,{"v":107,"d":"107.0000"}]
["L4784","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":54,"d":"54.0000"}]
["L4785","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour",{"v":1.5E-3,"d":"0.0015"},null,{"v":13,"d":"13.0000"}]
["L4786","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":7,"d":"7.0000"}]
["L4787","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour",0.0158,null,{"v":138,"d":"138.0000"}]
["L4788","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":69,"d":"69.0000"}]
["L4793","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer","B&I","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0093,null,{"v":45,"d":"45.0000"}]
["L4795","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay","B&I","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay",0.1592,null,{"v":771,"d":"771.0000"}]
["L4796","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay","B&I","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay",0.1925,null,{"v":933,"d":"933.0000"}]
["L4797","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) ","B&I","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) ",0.0069,null,{"v":33,"d":"33.0000"}]
["L4798","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) ","B&I","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) ",{"v":0.008,"d":"0.0080"},null,{"v":39,"d":"39.0000"}]
["L4799","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","B&I","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0079,null,{"v":38,"d":"38.0000"}]
["L4800","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) ","B&I","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) ",0.0106,null,{"v":52,"d":"52.0000"}]
["L4801","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) ","B&I","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) ",{"v":0.01,"d":"0.0100"},null,{"v":48,"d":"48.0000"}]
["L4802","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","B&I","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0097,null,{"v":47,"d":"47.0000"}]
["L4803","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) ","B&I","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) ",0.0087,null,{"v":42,"d":"42.0000"}]
["L4804","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) ","B&I","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) ",0.0272,null,{"v":132,"d":"132.0000"}]
["L4805","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) ","B&I","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) ",0.0122,null,{"v":59,"d":"59.0000"}]
["L4806","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) ","B&I","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) ",0.0286,null,{"v":139,"d":"139.0000"}]
["L4807","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) ","B&I","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) ",0.0104,null,{"v":50,"d":"50.0000"}]
["L4808","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) ","B&I","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) ",0.0258,null,{"v":125,"d":"125.0000"}]
["L4809","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) ","B&I","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) ",0.0218,null,{"v":106,"d":"106.0000"}]
["L4810","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) ","B&I","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) ",0.0169,null,{"v":82,"d":"82.0000"}]
["L4811","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","B&I","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0204,null,{"v":99,"d":"99.0000"}]
["L4812","Non-High Bay Occupancy/Vacancy Sensor","B&I","Non-High Bay Occupancy/Vacancy Sensor",0.0002,0.0002,{"v":0.9,"d":"0.9000"}]
["L4813","LED Fixture, Track/Mono/Accent","B&I","LED Fixture, Track/Mono/Accent",0.0008,0.0008,{"v":3.73,"d":"3.7300"}]
["L4830","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior","B&I","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior",{"v":0,"d":"0.0000"},null,{"v":116,"d":"116.0000"}]
["L4831","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior","B&I","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior",{"v":0,"d":"0.0000"},null,{"v":124,"d":"124.0000"}]
["L4832","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior","B&I","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior",{"v":0,"d":"0.0000"},null,{"v":96,"d":"96.0000"}]
["L4833","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior 24/7","B&I","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior 24/7",0.0265,null,{"v":232,"d":"232.0000"}]
["L4834","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior 24/7","B&I","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior 24/7",0.0283,null,{"v":248,"d":"248.0000"}]
["L4835","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7","B&I","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7",{"v":0.022,"d":"0.0220"},null,{"v":192,"d":"192.0000"}]
["L5061","Occupancy Sensors, On/Off, High Bay","B&I","Occupancy Sensors, On/Off, High Bay",0.0003,0.0003,{"v":1.27,"d":"1.2700"}]
["L5062","Bi-Level Controls, High Bay ","B&I","Bi-Level Controls, High Bay ",{"v":1E-4,"d":"0.0001"},{"v":1E-4,"d":"0.0001"},{"v":0.45,"d":"0.4500"}]
["L5063","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn","B&I","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn",{"v":0,"d":"0.0000"},0.0002,{"v":1.48,"d":"1.4800"}]
["L5064","Bi-level Controls, Parking Garage Fixtures, 24 Hour","B&I","Bi-level Controls, Parking Garage Fixtures, 24 Hour",0.0003,0.0003,{"v":2.96,"d":"2.9600"}]
["L5211","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","B&I","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0.04,"d":"0.0400"},null,{"v":194,"d":"194.0000"}]
["L5212","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","B&I","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0.03,"d":"0.0300"},null,{"v":143,"d":"143.0000"}]
["L5213","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","B&I","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0.024,"d":"0.0240"},null,{"v":116,"d":"116.0000"}]
["L5214","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL","B&I","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0.017,"d":"0.0170"},null,{"v":81,"d":"81.0000"}]
["L5215","Omnidirectional Interior LED with rated lumen output of 250-449 replacing incandescent or CFL","B&I","Omnidirectional Interior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0.015,"d":"0.0150"},null,{"v":73,"d":"73.0000"}]
["L5216","Decorative Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","B&I","Decorative Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0.04,"d":"0.0400"},null,{"v":194,"d":"194.0000"}]
["L5217","Decorative Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","B&I","Decorative Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0.028,"d":"0.0280"},null,{"v":134,"d":"134.0000"}]
["L5218","Decorative Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","B&I","Decorative Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0.025,"d":"0.0250"},null,{"v":120,"d":"120.0000"}]
["L5219","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL","B&I","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0.017,"d":"0.0170"},null,{"v":81,"d":"81.0000"}]
["L5220","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL","B&I","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0.015,"d":"0.0150"},null,{"v":72,"d":"72.0000"}]
["L5221","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","B&I","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":228,"d":"228.0000"}]
["L5222","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","B&I","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":168,"d":"168.0000"}]
["L5223","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","B&I","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":137,"d":"137.0000"}]
["L5224","Omnidirectional Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL","B&I","Omnidirectional Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":95,"d":"95.0000"}]
["L5226","Decorative Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","B&I","Decorative Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":228,"d":"228.0000"}]
["L5227","Decorative Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","B&I","Decorative Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":157,"d":"157.0000"}]
["L5228","Decorative Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","B&I","Decorative Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":141,"d":"141.0000"}]
["L5229","Decorative Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL","B&I","Decorative Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":95,"d":"95.0000"}]
["L5230","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL","B&I","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":84,"d":"84.0000"}]
["L5235","Refrigeration Savings for Lighting Upgrades in Freezers","B&I","Refrigeration Savings for Lighting Upgrades in Freezers",0.0005,0.0006,{"v":2.66,"d":"2.6600"}]
["L5236","Refrigeration Savings for Lighting Upgrades in Coolers","B&I","Refrigeration Savings for Lighting Upgrades in Coolers",0.0003,0.0003,{"v":1.62,"d":"1.6200"}]
["L5445","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section",0.0026,null,{"v":13,"d":"13.0000"}]
["L5446","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":15,"d":"15.0000"}]
["L5447","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7","B&I","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7",0.0034,null,{"v":30,"d":"30.0000"}]
["L5448","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section",0.0051,null,{"v":25,"d":"25.0000"}]
["L5449","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":29,"d":"29.0000"}]
["L5450","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7","B&I","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7",{"v":6.6E-3,"d":"0.0066"},null,{"v":58,"d":"58.0000"}]
["L5451","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior","B&I","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior",0.0091,0.0094,{"v":45,"d":"45.0000"}]
["L5452","4' TLED, Replacing 4' T5HO Lamp, Interior","B&I","4' TLED, Replacing 4' T5HO Lamp, Interior",0.0279,0.0286,{"v":137,"d":"137.0000"}]
["L5453","2' TLED, Replacing 2' T8 or T12 Lamp, Interior","B&I","2' TLED, Replacing 2' T8 or T12 Lamp, Interior",0.0078,{"v":0.008,"d":"0.0080"},{"v":38,"d":"38.0000"}]
["L5454","8' TLED, Replacing 8' T8 or T12 Lamp, Interior","B&I","8' TLED, Replacing 8' T8 or T12 Lamp, Interior",0.0151,0.0155,{"v":74,"d":"74.0000"}]
["L5455","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior 24/7","B&I","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior 24/7",0.0118,null,{"v":104,"d":"104.0000"}]
["L5456","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior","B&I","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior",{"v":0,"d":"0.0000"},0.0054,{"v":53,"d":"53.0000"}]
["L5457","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7","B&I","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7",0.0198,null,{"v":174,"d":"174.0000"}]
["L5458","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior","B&I","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior",{"v":0,"d":"0.0000"},null,{"v":87,"d":"87.0000"}]
["L5459","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer","B&I","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer",0.0104,0.0107,{"v":51,"d":"51.0000"}]
["L5460","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay","B&I","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay",0.0251,0.0257,{"v":123,"d":"123.0000"}]
["L5461","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay","B&I","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay",0.0783,0.0803,{"v":384,"d":"384.0000"}]
["L5559","Programming, Lighting Controls","B&I","Programming, Lighting Controls"]
["L10028","LED Fixture, Downlights, Interior","Large Industrial","LED Fixture, Downlights, Interior",0.0323,0.0323,{"v":199,"d":"199.0000"}]
["L10029","LED Fixture, Downlights, Exterior","Large Industrial","LED Fixture, Downlights, Exterior",{"v":0,"d":"0.0000"},{"v":0.036,"d":"0.0360"},{"v":350,"d":"350.0000"}]
["L10039","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior","Large Industrial","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior",0.0208,0.0208,{"v":128,"d":"128.0000"}]
["L10040","Four Pin-Base Lamp Replacing CFL, DLC Listed, Exterior","Large Industrial","Four Pin-Base Lamp Replacing CFL, DLC Listed, Exterior",{"v":0,"d":"0.0000"},0.0122,{"v":118,"d":"118.0000"}]
["L10042","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)","Large Industrial","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)",0.1984,0.1984,{"v":1222,"d":"1222.0000"}]
["L10043","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior","Large Industrial","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior",{"v":0,"d":"0.0000"},{"v":0.772,"d":"0.7720"},{"v":751,"d":"751.0000"}]
["L10211","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC","Large Industrial","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC",0.0303,0.0303,{"v":174,"d":"174.0000"}]
["L10212","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC","Large Industrial","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC",0.0973,0.0973,{"v":546,"d":"546.0000"}]
["L10213","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC","Large Industrial","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC",0.0569,0.0569,{"v":323,"d":"323.0000"}]
["L10214","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC","Large Industrial","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC",{"v":0.02,"d":"0.0200"},{"v":0.02,"d":"0.0200"},{"v":117,"d":"117.0000"}]
["L10215","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC","Large Industrial","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC",0.1789,0.1789,{"v":1012,"d":"1012.0000"}]
["L10216","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC","Large Industrial","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC",{"v":0.277,"d":"0.2770"},{"v":0.277,"d":"0.2770"},{"v":1568,"d":"1568.0000"}]
["L10217","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC","Large Industrial","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC",0.1166,0.1166,{"v":672,"d":"672.0000"}]
["L10218","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC","Large Industrial","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC",{"v":0.171,"d":"0.1710"},{"v":0.171,"d":"0.1710"},{"v":982,"d":"982.0000"}]
["L10223","Advanced Lighting Controls, Interior","Large Industrial","Advanced Lighting Controls, Interior",0.0003,0.0003,{"v":2.18,"d":"2.1800"}]
["L10224","Advanced Lighting Controls, Exterior","Large Industrial","Advanced Lighting Controls, Exterior",{"v":0,"d":"0.0000"},0.0002,{"v":1.97,"d":"1.9700"}]
["L10281","1’ to 3’ LED Linear Ambient Fixture, Interior","Large Industrial","1’ to 3’ LED Linear Ambient Fixture, Interior",{"v":0.007,"d":"0.0070"},{"v":0.007,"d":"0.0070"},{"v":43,"d":"43.0000"}]
["L10282","4' LED Linear Ambient Fixture, Interior","Large Industrial","4' LED Linear Ambient Fixture, Interior",{"v":0.014,"d":"0.0140"},{"v":0.014,"d":"0.0140"},{"v":86,"d":"86.0000"}]
["L10283","8' LED Linear Ambient Fixture, Interior","Large Industrial","8' LED Linear Ambient Fixture, Interior",{"v":0.028,"d":"0.0280"},{"v":0.028,"d":"0.0280"},{"v":173,"d":"173.0000"}]
["L10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","Large Industrial","1’ to 3’ LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},{"v":0.003,"d":"0.0030"},{"v":30,"d":"30.0000"}]
["L10285","4' LED Linear Ambient Fixture, Exterior","Large Industrial","4' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0061,{"v":59,"d":"59.0000"}]
["L10286","8' LED Linear Ambient Fixture, Exterior","Large Industrial","8' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0121,{"v":118,"d":"118.0000"}]
["L10287","General Wattage Reduction, Interior","Large Industrial","General Wattage Reduction, Interior",0.0008,0.0008,{"v":4.75,"d":"4.7500"}]
["L10288","General Wattage Reduction, Exterior","Large Industrial","General Wattage Reduction, Exterior",{"v":0,"d":"0.0000"},0.0005,{"v":4.38,"d":"4.3800"}]
["L10289","Fixture Elimination, Interior","Large Industrial","Fixture Elimination, Interior",0.0008,0.0008,{"v":4.75,"d":"4.7500"}]
["L10290","Fixture Elimination, Exterior","Large Industrial","Fixture Elimination, Exterior",{"v":0,"d":"0.0000"},0.0005,{"v":4.38,"d":"4.3800"}]
["L2482","Occupancy Sensor, LED Refrigerated Case Lights","Large Industrial","Occupancy Sensor, LED Refrigerated Case Lights",0.0075,null,{"v":65,"d":"65.0000"}]
["L2768","LED, Exit Sign, Retrofit","Large Industrial","LED, Exit Sign, Retrofit",0.0213,0.0213,{"v":187,"d":"187.0000"}]
["L3091","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay","Large Industrial","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay",0.1465,0.1465,{"v":903,"d":"903.0000"}]
["L3092","LED Fixture, <250 Watts, Replacing 320-400 Watt HID, High Bay","Large Industrial","LED Fixture, <250 Watts, Replacing 320-400 Watt HID, High Bay",0.1551,0.1551,{"v":956,"d":"956.0000"}]
["L3093","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay","Large Industrial","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay",0.2261,0.2261,{"v":1393,"d":"1393.0000"}]
["L3094","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay","Large Industrial","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay",{"v":0,"d":"0.0000"},0.0009,{"v":8.76,"d":"8.7600"}]
["L3095","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay","Large Industrial","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay",0.6297,0.6297,{"v":3881,"d":"3881.0000"}]
["L3096","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay","Large Industrial","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay",{"v":0.607,"d":"0.6070"},{"v":0.607,"d":"0.6070"},{"v":3741,"d":"3741.0000"}]
["L3097","LED Fixture, Bilevel, Stairwell and Passageway","Large Industrial","LED Fixture, Bilevel, Stairwell and Passageway",0.0262,0.0262,{"v":161,"d":"161.0000"}]
["L3111","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer","Large Industrial","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer",0.0444,0.0444,{"v":274,"d":"274.0000"}]
["L3114","LED, Horizontal Case Lighting","Large Industrial","LED, Horizontal Case Lighting",0.0174,0.0174,{"v":112,"d":"112.0000"}]
["L3393","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed","Large Industrial","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed",0.0763,null,{"v":470,"d":"470.0000"}]
["L3400","LED Fixture, 2x2, Low Output, DLC Listed","Large Industrial","LED Fixture, 2x2, Low Output, DLC Listed",0.0214,0.0214,{"v":132,"d":"132.0000"}]
["L3401","LED Fixture, 2x2, High Output, DLC Listed","Large Industrial","LED Fixture, 2x2, High Output, DLC Listed",0.0867,0.0867,{"v":534,"d":"534.0000"}]
["L3406","Daylighting Controls","Large Industrial","Daylighting Controls",0.0002,0.0002,{"v":1.33,"d":"1.3300"}]
["L3511","LED Replacement of 4’ T8 Lamps w/Integral or External Driver","Large Industrial","LED Replacement of 4’ T8 Lamps w/Integral or External Driver",0.0075,null,{"v":46,"d":"46.0000"}]
["L3512","LED Replacement of 4’ T8 Lamps utilizing existing ballast","Large Industrial","LED Replacement of 4’ T8 Lamps utilizing existing ballast",0.0083,null,{"v":51,"d":"51.0000"}]
["L3738","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section",0.0012,null,{"v":7,"d":"7.0000"}]
["L3739","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section",0.0121,null,{"v":75,"d":"75.0000"}]
["L3740","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section",{"v":0.003,"d":"0.0030"},null,{"v":19,"d":"19.0000"}]
["L3741","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section",0.0094,null,{"v":58,"d":"58.0000"}]
["L3759","LED Replacement of 4’ T8 Lamps, Direct Wire","Large Industrial","LED Replacement of 4’ T8 Lamps, Direct Wire",0.0088,null,{"v":54,"d":"54.0000"}]
["L3760","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer","Large Industrial","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0125,null,{"v":77,"d":"77.0000"}]
["L3903","LED Signage Retrofit, Interior","Large Industrial","LED Signage Retrofit, Interior",{"v":1.5E-3,"d":"0.0015"},{"v":1.5E-3,"d":"0.0015"},{"v":9.49,"d":"9.4900"}]
["L3904","LED Signage Retrofit, Exterior","Large Industrial","LED Signage Retrofit, Exterior",{"v":0,"d":"0.0000"},0.0009,{"v":8.76,"d":"8.7600"}]
["L3929","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL",{"v":0,"d":"0.0000"},null,{"v":40,"d":"40.0000"}]
["L3930","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL",{"v":0,"d":"0.0000"},null,{"v":24,"d":"24.0000"}]
["L3931","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W",{"v":0,"d":"0.0000"},null,{"v":18,"d":"18.0000"}]
["L3932","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL",0.0071,null,{"v":44,"d":"44.0000"}]
["L3933","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL",0.0042,null,{"v":26,"d":"26.0000"}]
["L3934","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W",0.0032,null,{"v":19,"d":"19.0000"}]
["L3935","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent",{"v":0,"d":"0.0000"},null,{"v":499,"d":"499.0000"}]
["L3936","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent",{"v":0,"d":"0.0000"},null,{"v":364,"d":"364.0000"}]
["L3937","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent",{"v":0,"d":"0.0000"},null,{"v":284,"d":"284.0000"}]
["L3938","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent",{"v":0,"d":"0.0000"},null,{"v":237,"d":"237.0000"}]
["L3939","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 36W – 54W Incandescent","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 36W – 54W Incandescent",{"v":0,"d":"0.0000"},null,{"v":182,"d":"182.0000"}]
["L3940","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent","Large Industrial","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent",{"v":0,"d":"0.0000"},null,{"v":114,"d":"114.0000"}]
["L3941","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W",0.0877,null,{"v":540,"d":"540.0000"}]
["L3942","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W",{"v":0.064,"d":"0.0640"},null,{"v":394,"d":"394.0000"}]
["L3943","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W",0.0499,null,{"v":308,"d":"308.0000"}]
["L3944","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W",0.0417,null,{"v":257,"d":"257.0000"}]
["L3945","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W",{"v":0.032,"d":"0.0320"},null,{"v":197,"d":"197.0000"}]
["L3946","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W","Large Industrial","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W",0.0201,null,{"v":124,"d":"124.0000"}]
["L4280","LED, Exterior Fixture, Low Output, <= 4,999 lumens","Large Industrial","LED, Exterior Fixture, Low Output, <= 4,999 lumens",{"v":0,"d":"0.0000"},0.0122,{"v":389,"d":"389.0000"}]
["L4281","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens","Large Industrial","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens",{"v":0,"d":"0.0000"},{"v":0.027,"d":"0.0270"},{"v":731,"d":"731.0000"}]
["L4282","LED, Exterior Fixture, High Output, 10,000-29,999 lumens","Large Industrial","LED, Exterior Fixture, High Output, 10,000-29,999 lumens",{"v":0,"d":"0.0000"},0.0601,{"v":1806,"d":"1806.0000"}]
["L4283","LED, Exterior Fixture, Very High Output, >= 30,000 lumens","Large Industrial","LED, Exterior Fixture, Very High Output, >= 30,000 lumens",{"v":0,"d":"0.0000"},0.1486,{"v":3279,"d":"3279.0000"}]
["L4314","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12","Large Industrial","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12",0.0242,null,{"v":149,"d":"149.0000"}]
["L4315","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, Exterior","Large Industrial","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":138,"d":"138.0000"}]
["L4316","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, 24/7","Large Industrial","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, 24/7",0.0314,null,{"v":275,"d":"275.0000"}]
["L4317","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO","Large Industrial","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO",0.0538,null,{"v":332,"d":"332.0000"}]
["L4318","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, Exterior","Large Industrial","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":306,"d":"306.0000"}]
["L4319","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, 24/7","Large Industrial","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, 24/7",0.0699,null,{"v":612,"d":"612.0000"}]
["L4320","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12","Large Industrial","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12",0.0314,null,{"v":194,"d":"194.0000"}]
["L4321","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior","Large Industrial","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":179,"d":"179.0000"}]
["L4322","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, 24/7","Large Industrial","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, 24/7",0.0408,null,{"v":358,"d":"358.0000"}]
["L4323","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO","Large Industrial","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO",{"v":0.09,"d":"0.0900"},null,{"v":554,"d":"554.0000"}]
["L4324","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior","Large Industrial","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":512,"d":"512.0000"}]
["L4325","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, 24/7","Large Industrial","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, 24/7",0.1168,null,{"v":1024,"d":"1024.0000"}]
["L4326","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12","Large Industrial","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12",0.0573,null,{"v":353,"d":"353.0000"}]
["L4327","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, Exterior","Large Industrial","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":326,"d":"326.0000"}]
["L4328","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, 24/7","Large Industrial","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, 24/7",0.0744,null,{"v":652,"d":"652.0000"}]
["L4329","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO","Large Industrial","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO",0.1158,null,{"v":714,"d":"714.0000"}]
["L4330","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, Exterior","Large Industrial","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":659,"d":"659.0000"}]
["L4331","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, 24/7","Large Industrial","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, 24/7",0.1504,null,{"v":1318,"d":"1318.0000"}]
["L4347","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay","Large Industrial","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay",0.1171,null,{"v":722,"d":"722.0000"}]
["L4348","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior","Large Industrial","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior",{"v":0,"d":"0.0000"},null,{"v":47,"d":"47.0000"}]
["L4349","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7","Large Industrial","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7",0.0107,null,{"v":94,"d":"94.0000"}]
["L4350","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior","Large Industrial","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior",{"v":0,"d":"0.0000"},null,{"v":50,"d":"50.0000"}]
["L4351","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7","Large Industrial","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7",0.0114,null,{"v":100,"d":"100.0000"}]
["L4352","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior","Large Industrial","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior",{"v":0,"d":"0.0000"},null,{"v":43,"d":"43.0000"}]
["L4353","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior, 24/7","Large Industrial","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior, 24/7",0.0098,null,{"v":86,"d":"86.0000"}]
["L4781","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour",{"v":0.004,"d":"0.0040"},null,{"v":35,"d":"35.0000"}]
["L4782","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":17,"d":"17.0000"}]
["L4783","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour",0.0122,null,{"v":107,"d":"107.0000"}]
["L4784","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":54,"d":"54.0000"}]
["L4785","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour",{"v":1.5E-3,"d":"0.0015"},null,{"v":13,"d":"13.0000"}]
["L4786","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":7,"d":"7.0000"}]
["L4787","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour",0.0158,null,{"v":138,"d":"138.0000"}]
["L4788","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":69,"d":"69.0000"}]
["L4793","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer","Large Industrial","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0093,null,{"v":57,"d":"57.0000"}]
["L4795","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay","Large Industrial","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay",0.1592,null,{"v":981,"d":"981.0000"}]
["L4796","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay","Large Industrial","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay",0.1925,null,{"v":1186,"d":"1186.0000"}]
["L4797","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) ","Large Industrial","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) ",0.0069,null,{"v":42,"d":"42.0000"}]
["L4798","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) ","Large Industrial","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) ",{"v":0.008,"d":"0.0080"},null,{"v":49,"d":"49.0000"}]
["L4799","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Large Industrial","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0079,null,{"v":49,"d":"49.0000"}]
["L4800","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) ","Large Industrial","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) ",0.0106,null,{"v":66,"d":"66.0000"}]
["L4801","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) ","Large Industrial","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) ",{"v":0.01,"d":"0.0100"},null,{"v":61,"d":"61.0000"}]
["L4802","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Large Industrial","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0097,null,{"v":60,"d":"60.0000"}]
["L4803","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) ","Large Industrial","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) ",0.0087,null,{"v":54,"d":"54.0000"}]
["L4804","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) ","Large Industrial","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) ",0.0272,null,{"v":168,"d":"168.0000"}]
["L4805","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) ","Large Industrial","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) ",0.0122,null,{"v":75,"d":"75.0000"}]
["L4806","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) ","Large Industrial","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) ",0.0286,null,{"v":176,"d":"176.0000"}]
["L4807","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) ","Large Industrial","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) ",0.0104,null,{"v":64,"d":"64.0000"}]
["L4808","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) ","Large Industrial","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) ",0.0258,null,{"v":159,"d":"159.0000"}]
["L4809","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) ","Large Industrial","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) ",0.0218,null,{"v":134,"d":"134.0000"}]
["L4810","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) ","Large Industrial","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) ",0.0169,null,{"v":104,"d":"104.0000"}]
["L4811","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Large Industrial","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0204,null,{"v":126,"d":"126.0000"}]
["L4812","Non-High Bay Occupancy/Vacancy Sensor","Large Industrial","Non-High Bay Occupancy/Vacancy Sensor",0.0002,0.0002,{"v":1.14,"d":"1.1400"}]
["L4813","LED Fixture, Track/Mono/Accent","Large Industrial","LED Fixture, Track/Mono/Accent",0.0008,0.0008,{"v":4.75,"d":"4.7500"}]
["L4830","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior","Large Industrial","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior",{"v":0,"d":"0.0000"},null,{"v":116,"d":"116.0000"}]
["L4831","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior","Large Industrial","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior",{"v":0,"d":"0.0000"},null,{"v":124,"d":"124.0000"}]
["L4832","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior","Large Industrial","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior",{"v":0,"d":"0.0000"},null,{"v":96,"d":"96.0000"}]
["L4833","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior 24/7","Large Industrial","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior 24/7",0.0265,null,{"v":232,"d":"232.0000"}]
["L4834","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior 24/7","Large Industrial","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior 24/7",0.0283,null,{"v":248,"d":"248.0000"}]
["L4835","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7","Large Industrial","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7",{"v":0.022,"d":"0.0220"},null,{"v":192,"d":"192.0000"}]
["L5061","Occupancy Sensors, On/Off, High Bay","Large Industrial","Occupancy Sensors, On/Off, High Bay",0.0003,0.0003,{"v":1.99,"d":"1.9900"}]
["L5062","Bi-Level Controls, High Bay ","Large Industrial","Bi-Level Controls, High Bay ",0.0002,0.0002,{"v":0.93,"d":"0.9300"}]
["L5063","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn","Large Industrial","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn",{"v":0,"d":"0.0000"},0.0002,{"v":1.48,"d":"1.4800"}]
["L5064","Bi-level Controls, Parking Garage Fixtures, 24 Hour","Large Industrial","Bi-level Controls, Parking Garage Fixtures, 24 Hour",0.0003,0.0003,{"v":2.96,"d":"2.9600"}]
["L5211","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Large Industrial","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0.04,"d":"0.0400"},null,{"v":247,"d":"247.0000"}]
["L5212","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Large Industrial","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0.03,"d":"0.0300"},null,{"v":182,"d":"182.0000"}]
["L5213","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Large Industrial","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0.024,"d":"0.0240"},null,{"v":148,"d":"148.0000"}]
["L5214","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL","Large Industrial","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0.017,"d":"0.0170"},null,{"v":103,"d":"103.0000"}]
["L5215","Omnidirectional Interior LED with rated lumen output of 250-449 replacing incandescent or CFL","Large Industrial","Omnidirectional Interior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0.015,"d":"0.0150"},null,{"v":93,"d":"93.0000"}]
["L5216","Decorative Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Large Industrial","Decorative Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0.04,"d":"0.0400"},null,{"v":247,"d":"247.0000"}]
["L5217","Decorative Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Large Industrial","Decorative Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0.028,"d":"0.0280"},null,{"v":170,"d":"170.0000"}]
["L5218","Decorative Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Large Industrial","Decorative Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0.025,"d":"0.0250"},null,{"v":153,"d":"153.0000"}]
["L5219","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL","Large Industrial","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0.017,"d":"0.0170"},null,{"v":103,"d":"103.0000"}]
["L5220","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL","Large Industrial","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0.015,"d":"0.0150"},null,{"v":91,"d":"91.0000"}]
["L5221","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Large Industrial","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":228,"d":"228.0000"}]
["L5222","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Large Industrial","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":168,"d":"168.0000"}]
["L5223","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Large Industrial","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":137,"d":"137.0000"}]
["L5224","Omnidirectional Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL","Large Industrial","Omnidirectional Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":95,"d":"95.0000"}]
["L5226","Decorative Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Large Industrial","Decorative Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":228,"d":"228.0000"}]
["L5227","Decorative Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Large Industrial","Decorative Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":157,"d":"157.0000"}]
["L5228","Decorative Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Large Industrial","Decorative Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":141,"d":"141.0000"}]
["L5229","Decorative Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL","Large Industrial","Decorative Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":95,"d":"95.0000"}]
["L5230","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL","Large Industrial","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":84,"d":"84.0000"}]
["L5235","Refrigeration Savings for Lighting Upgrades in Freezers","Large Industrial","Refrigeration Savings for Lighting Upgrades in Freezers",0.0006,0.0006,{"v":3.39,"d":"3.3900"}]
["L5236","Refrigeration Savings for Lighting Upgrades in Coolers","Large Industrial","Refrigeration Savings for Lighting Upgrades in Coolers",0.0003,0.0003,{"v":2.06,"d":"2.0600"}]
["L5445","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section",0.0026,null,{"v":16,"d":"16.0000"}]
["L5446","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":15,"d":"15.0000"}]
["L5447","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7","Large Industrial","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7",0.0034,null,{"v":30,"d":"30.0000"}]
["L5448","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section",0.0051,null,{"v":31,"d":"31.0000"}]
["L5449","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":29,"d":"29.0000"}]
["L5450","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7","Large Industrial","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7",{"v":6.6E-3,"d":"0.0066"},null,{"v":58,"d":"58.0000"}]
["L5451","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior","Large Industrial","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior",0.0091,0.0094,{"v":57,"d":"57.0000"}]
["L5452","4' TLED, Replacing 4' T5HO Lamp, Interior","Large Industrial","4' TLED, Replacing 4' T5HO Lamp, Interior",0.0279,0.0286,{"v":174,"d":"174.0000"}]
["L5453","2' TLED, Replacing 2' T8 or T12 Lamp, Interior","Large Industrial","2' TLED, Replacing 2' T8 or T12 Lamp, Interior",0.0078,{"v":0.008,"d":"0.0080"},{"v":49,"d":"49.0000"}]
["L5454","8' TLED, Replacing 8' T8 or T12 Lamp, Interior","Large Industrial","8' TLED, Replacing 8' T8 or T12 Lamp, Interior",0.0151,0.0155,{"v":94,"d":"94.0000"}]
["L5455","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior 24/7","Large Industrial","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior 24/7",0.0118,null,{"v":104,"d":"104.0000"}]
["L5456","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior","Large Industrial","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior",{"v":0,"d":"0.0000"},0.0054,{"v":53,"d":"53.0000"}]
["L5457","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7","Large Industrial","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7",0.0198,null,{"v":174,"d":"174.0000"}]
["L5458","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior","Large Industrial","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior",{"v":0,"d":"0.0000"},null,{"v":87,"d":"87.0000"}]
["L5459","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer","Large Industrial","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer",0.0106,0.0106,{"v":65,"d":"65.0000"}]
["L5460","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay","Large Industrial","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay",0.0254,0.0254,{"v":157,"d":"157.0000"}]
["L5461","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay","Large Industrial","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay",0.0793,0.0793,{"v":489,"d":"489.0000"}]
["L5559","Programming, Lighting Controls","Large Industrial","Programming, Lighting Controls"]
["NL10028","LED Fixture, Downlights, Interior","Agribusiness-NC","LED Fixture, Downlights, Interior",0.0171,0.0186,{"v":120,"d":"120.0000"}]
["NL10029","LED Fixture, Downlights, Exterior","Agribusiness-NC","LED Fixture, Downlights, Exterior",{"v":0,"d":"0.0000"},0.0144,{"v":140,"d":"140.0000"}]
["NL10214","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC","Agribusiness-NC","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC",0.0174,0.0189,{"v":115,"d":"115.0000"}]
["NL10281","1’ to 3’ LED Linear Ambient Fixture, Interior","Agribusiness-NC","1’ to 3’ LED Linear Ambient Fixture, Interior",0.0061,{"v":6.6E-3,"d":"0.0066"},{"v":43,"d":"43.0000"}]
["NL10282","4' LED Linear Ambient Fixture, Interior","Agribusiness-NC","4' LED Linear Ambient Fixture, Interior",0.0122,0.0133,{"v":86,"d":"86.0000"}]
["NL10283","8' LED Linear Ambient Fixture, Interior","Agribusiness-NC","8' LED Linear Ambient Fixture, Interior",0.0244,0.0266,{"v":171,"d":"171.0000"}]
["NL10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","Agribusiness-NC","1’ to 3’ LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},{"v":0.003,"d":"0.0030"},{"v":30,"d":"30.0000"}]
["NL10285","4' LED Linear Ambient Fixture, Exterior","Agribusiness-NC","4' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0061,{"v":59,"d":"59.0000"}]
["NL10286","8' LED Linear Ambient Fixture, Exterior","Agribusiness-NC","8' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0121,{"v":118,"d":"118.0000"}]
["NL2482","Occupancy Sensor, LED Refrigerated Case Lights","Agribusiness-NC","Occupancy Sensor, LED Refrigerated Case Lights",{"v":0.013,"d":"0.0130"},null,{"v":112,"d":"112.0000"}]
["NL3097","LED Fixture, Bilevel, Stairwell and Passageway","Agribusiness-NC","LED Fixture, Bilevel, Stairwell and Passageway",0.0228,0.0248,{"v":160,"d":"160.0000"}]
["NL3111","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer","Agribusiness-NC","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer",0.0386,0.0421,{"v":271,"d":"271.0000"}]
["NL3393","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed","Agribusiness-NC","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed",0.0664,null,{"v":451,"d":"451.0000"}]
["NL3400","LED Fixture, 2x2, Low Output, DLC Listed","Agribusiness-NC","LED Fixture, 2x2, Low Output, DLC Listed",0.0186,0.0203,{"v":131,"d":"131.0000"}]
["NL3401","LED Fixture, 2x2, High Output, DLC Listed","Agribusiness-NC","LED Fixture, 2x2, High Output, DLC Listed",0.0755,0.0822,{"v":529,"d":"529.0000"}]
["NL3738","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section",{"v":1E-3,"d":"0.0010"},null,{"v":7,"d":"7.0000"}]
["NL3739","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section",0.0106,null,{"v":74,"d":"74.0000"}]
["NL3740","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section",0.0026,null,{"v":19,"d":"19.0000"}]
["NL3741","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section",0.0082,null,{"v":58,"d":"58.0000"}]
["NL3760","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer","Agribusiness-NC","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0109,null,{"v":76,"d":"76.0000"}]
["NL3929","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL","Agribusiness-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL",{"v":0,"d":"0.0000"},null,{"v":40,"d":"40.0000"}]
["NL3930","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL","Agribusiness-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL",{"v":0,"d":"0.0000"},null,{"v":24,"d":"24.0000"}]
["NL3931","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W","Agribusiness-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W",{"v":0,"d":"0.0000"},null,{"v":18,"d":"18.0000"}]
["NL3932","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL","Agribusiness-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL",0.0062,null,{"v":43,"d":"43.0000"}]
["NL3933","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL","Agribusiness-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL",0.0037,null,{"v":26,"d":"26.0000"}]
["NL3934","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W","Agribusiness-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W",0.0027,null,{"v":19,"d":"19.0000"}]
["NL4280","LED, Exterior Fixture, Low Output, <= 4,999 lumens","Agribusiness-NC","LED, Exterior Fixture, Low Output, <= 4,999 lumens",{"v":0,"d":"0.0000"},0.0122,{"v":389,"d":"389.0000"}]
["NL4281","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens","Agribusiness-NC","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens",{"v":0,"d":"0.0000"},{"v":0.027,"d":"0.0270"},{"v":731,"d":"731.0000"}]
["NL4282","LED, Exterior Fixture, High Output, 10,000-29,999 lumens","Agribusiness-NC","LED, Exterior Fixture, High Output, 10,000-29,999 lumens",{"v":0,"d":"0.0000"},0.0601,{"v":1806,"d":"1806.0000"}]
["NL4283","LED, Exterior Fixture, Very High Output, >= 30,000 lumens","Agribusiness-NC","LED, Exterior Fixture, Very High Output, >= 30,000 lumens",{"v":0,"d":"0.0000"},0.1486,{"v":3279,"d":"3279.0000"}]
["NL4347","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay","Agribusiness-NC","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay",0.0804,null,{"v":564,"d":"564.0000"}]
["NL4695","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, Agriculture","Agribusiness-NC","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, Agriculture",0.1274,0.1389,{"v":1084,"d":"1084.0000"}]
["NL4696","LED Fixture, <250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture","Agribusiness-NC","LED Fixture, <250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture",{"v":0.135,"d":"0.1350"},0.1471,{"v":1227,"d":"1227.0000"}]
["NL4699","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture","Agribusiness-NC","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture",0.5479,{"v":0.597,"d":"0.5970"},{"v":3842,"d":"3842.0000"}]
["NL4701","<=180W LED, replacing or instead of 6L T8 or 4L T5HO, Agriculture","Agribusiness-NC","<=180W LED, replacing or instead of 6L T8 or 4L T5HO, Agriculture",0.0644,null,{"v":451,"d":"451.0000"}]
["NL4702","<=250W LED, replacing or instead of 8LT8 or 6LT5HO, Agriculture","Agribusiness-NC","<=250W LED, replacing or instead of 8LT8 or 6LT5HO, Agriculture",0.0804,null,{"v":564,"d":"564.0000"}]
["NL4781","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour",{"v":0.004,"d":"0.0040"},null,{"v":35,"d":"35.0000"}]
["NL4782","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":17,"d":"17.0000"}]
["NL4783","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour",0.0122,null,{"v":107,"d":"107.0000"}]
["NL4784","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":54,"d":"54.0000"}]
["NL4785","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour",{"v":1.5E-3,"d":"0.0015"},null,{"v":13,"d":"13.0000"}]
["NL4786","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":7,"d":"7.0000"}]
["NL4787","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour",0.0158,null,{"v":138,"d":"138.0000"}]
["NL4788","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":69,"d":"69.0000"}]
["NL4793","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer","Agribusiness-NC","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0081,null,{"v":57,"d":"57.0000"}]
["NL4795","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay","Agribusiness-NC","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay",{"v":0.105,"d":"0.1050"},null,{"v":737,"d":"737.0000"}]
["NL4796","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay","Agribusiness-NC","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay",0.1193,null,{"v":836,"d":"836.0000"}]
["NL4813","LED Fixture, Track/Mono/Accent","Agribusiness-NC","LED Fixture, Track/Mono/Accent",0.0007,0.0007,{"v":4.7,"d":"4.7000"}]
["NL5063","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn","Agribusiness-NC","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn",{"v":0,"d":"0.0000"},0.0002,{"v":1.48,"d":"1.4800"}]
["NL5065","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only","Agribusiness-NC","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.0461,{"v":449,"d":"449.0000"}]
["NL5066","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only","Agribusiness-NC","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.0886,{"v":863,"d":"863.0000"}]
["NL5067","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only","Agribusiness-NC","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.2156,{"v":2099,"d":"2099.0000"}]
["NL5068","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only","Agribusiness-NC","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only",{"v":0,"d":"0.0000"},0.4112,{"v":4003,"d":"4003.0000"}]
["NL5235","Refrigeration Savings for Lighting Upgrades in Freezers","Agribusiness-NC","Refrigeration Savings for Lighting Upgrades in Freezers",0.0005,0.0005,{"v":3.36,"d":"3.3600"}]
["NL5236","Refrigeration Savings for Lighting Upgrades in Coolers","Agribusiness-NC","Refrigeration Savings for Lighting Upgrades in Coolers",0.0003,0.0003,{"v":2.04,"d":"2.0400"}]
["NL5445","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section",{"v":2.3E-3,"d":"0.0023"},null,{"v":16,"d":"16.0000"}]
["NL5446","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":15,"d":"15.0000"}]
["NL5447","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7",0.0034,null,{"v":30,"d":"30.0000"}]
["NL5448","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section",0.0044,null,{"v":31,"d":"31.0000"}]
["NL5449","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":29,"d":"29.0000"}]
["NL5450","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7","Agribusiness-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7",{"v":6.6E-3,"d":"0.0066"},null,{"v":58,"d":"58.0000"}]
["NL5459","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer","Agribusiness-NC","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer",0.0092,{"v":0.01,"d":"0.0100"},{"v":64,"d":"64.0000"}]
["NL5460","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay","Agribusiness-NC","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay",0.0191,0.0208,{"v":134,"d":"134.0000"}]
["NL10028","LED Fixture, Downlights, Interior","B&I-NC","LED Fixture, Downlights, Interior",0.0194,0.0199,{"v":95,"d":"95.0000"}]
["NL10029","LED Fixture, Downlights, Exterior","B&I-NC","LED Fixture, Downlights, Exterior",{"v":0,"d":"0.0000"},0.0144,{"v":140,"d":"140.0000"}]
["NL10214","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC","B&I-NC","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC",0.0224,{"v":0.023,"d":"0.0230"},{"v":105,"d":"105.0000"}]
["NL10281","1’ to 3’ LED Linear Ambient Fixture, Interior","B&I-NC","1’ to 3’ LED Linear Ambient Fixture, Interior",0.0069,0.0071,{"v":34,"d":"34.0000"}]
["NL10282","4' LED Linear Ambient Fixture, Interior","B&I-NC","4' LED Linear Ambient Fixture, Interior",0.0138,0.0142,{"v":68,"d":"68.0000"}]
["NL10283","8' LED Linear Ambient Fixture, Interior","B&I-NC","8' LED Linear Ambient Fixture, Interior",0.0277,0.0284,{"v":136,"d":"136.0000"}]
["NL10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","B&I-NC","1’ to 3’ LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},{"v":0.003,"d":"0.0030"},{"v":30,"d":"30.0000"}]
["NL10285","4' LED Linear Ambient Fixture, Exterior","B&I-NC","4' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0061,{"v":59,"d":"59.0000"}]
["NL10286","8' LED Linear Ambient Fixture, Exterior","B&I-NC","8' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0121,{"v":118,"d":"118.0000"}]
["NL2482","Occupancy Sensor, LED Refrigerated Case Lights","B&I-NC","Occupancy Sensor, LED Refrigerated Case Lights",{"v":0.013,"d":"0.0130"},null,{"v":112,"d":"112.0000"}]
["NL3097","LED Fixture, Bilevel, Stairwell and Passageway","B&I-NC","LED Fixture, Bilevel, Stairwell and Passageway",0.0259,0.0265,{"v":127,"d":"127.0000"}]
["NL3111","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer","B&I-NC","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer",0.0438,{"v":0.045,"d":"0.0450"},{"v":215,"d":"215.0000"}]
["NL3393","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed","B&I-NC","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed",{"v":0.074,"d":"0.0740"},null,{"v":358,"d":"358.0000"}]
["NL3400","LED Fixture, 2x2, Low Output, DLC Listed","B&I-NC","LED Fixture, 2x2, Low Output, DLC Listed",0.0211,0.0217,{"v":104,"d":"104.0000"}]
["NL3401","LED Fixture, 2x2, High Output, DLC Listed","B&I-NC","LED Fixture, 2x2, High Output, DLC Listed",0.0856,0.0879,{"v":420,"d":"420.0000"}]
["NL3738","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section",0.0012,null,{"v":6,"d":"6.0000"}]
["NL3739","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section",0.0121,null,{"v":59,"d":"59.0000"}]
["NL3740","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section",{"v":0.003,"d":"0.0030"},null,{"v":15,"d":"15.0000"}]
["NL3741","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section",0.0094,null,{"v":46,"d":"46.0000"}]
["NL3929","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL","B&I-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL",{"v":0,"d":"0.0000"},null,{"v":40,"d":"40.0000"}]
["NL3930","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL","B&I-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL",{"v":0,"d":"0.0000"},null,{"v":24,"d":"24.0000"}]
["NL3931","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W","B&I-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W",{"v":0,"d":"0.0000"},null,{"v":18,"d":"18.0000"}]
["NL3932","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL","B&I-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL",0.0071,null,{"v":34,"d":"34.0000"}]
["NL3933","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL","B&I-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL",0.0042,null,{"v":21,"d":"21.0000"}]
["NL3934","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W","B&I-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W",0.0032,null,{"v":15,"d":"15.0000"}]
["NL4280","LED, Exterior Fixture, Low Output, <= 4,999 lumens","B&I-NC","LED, Exterior Fixture, Low Output, <= 4,999 lumens",{"v":0,"d":"0.0000"},0.0122,{"v":389,"d":"389.0000"}]
["NL4281","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens","B&I-NC","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens",{"v":0,"d":"0.0000"},{"v":0.027,"d":"0.0270"},{"v":731,"d":"731.0000"}]
["NL4282","LED, Exterior Fixture, High Output, 10,000-29,999 lumens","B&I-NC","LED, Exterior Fixture, High Output, 10,000-29,999 lumens",{"v":0,"d":"0.0000"},0.0601,{"v":1806,"d":"1806.0000"}]
["NL4283","LED, Exterior Fixture, Very High Output, >= 30,000 lumens","B&I-NC","LED, Exterior Fixture, Very High Output, >= 30,000 lumens",{"v":0,"d":"0.0000"},0.1486,{"v":3279,"d":"3279.0000"}]
["NL4347","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay","B&I-NC","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay",0.0924,null,{"v":448,"d":"448.0000"}]
["NL4781","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour",{"v":0.004,"d":"0.0040"},null,{"v":35,"d":"35.0000"}]
["NL4782","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":17,"d":"17.0000"}]
["NL4783","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour",0.0122,null,{"v":107,"d":"107.0000"}]
["NL4784","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":54,"d":"54.0000"}]
["NL4785","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour",{"v":1.5E-3,"d":"0.0015"},null,{"v":13,"d":"13.0000"}]
["NL4786","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":7,"d":"7.0000"}]
["NL4787","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour",0.0158,null,{"v":138,"d":"138.0000"}]
["NL4788","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":69,"d":"69.0000"}]
["NL4795","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay","B&I-NC","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay",0.1207,null,{"v":585,"d":"585.0000"}]
["NL4796","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay","B&I-NC","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay",0.1371,null,{"v":664,"d":"664.0000"}]
["NL4813","LED Fixture, Track/Mono/Accent","B&I-NC","LED Fixture, Track/Mono/Accent",0.0008,0.0008,{"v":3.73,"d":"3.7300"}]
["NL5063","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn","B&I-NC","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn",{"v":0,"d":"0.0000"},0.0002,{"v":1.48,"d":"1.4800"}]
["NL5065","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only","B&I-NC","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.0461,{"v":449,"d":"449.0000"}]
["NL5066","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only","B&I-NC","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.0886,{"v":863,"d":"863.0000"}]
["NL5067","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only","B&I-NC","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.2156,{"v":2099,"d":"2099.0000"}]
["NL5068","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only","B&I-NC","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only",{"v":0,"d":"0.0000"},0.4112,{"v":4003,"d":"4003.0000"}]
["NL5235","Refrigeration Savings for Lighting Upgrades in Freezers","B&I-NC","Refrigeration Savings for Lighting Upgrades in Freezers",0.0005,0.0006,{"v":2.66,"d":"2.6600"}]
["NL5236","Refrigeration Savings for Lighting Upgrades in Coolers","B&I-NC","Refrigeration Savings for Lighting Upgrades in Coolers",0.0003,0.0003,{"v":1.62,"d":"1.6200"}]
["NL5445","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section",0.0026,null,{"v":13,"d":"13.0000"}]
["NL5446","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":15,"d":"15.0000"}]
["NL5447","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7","B&I-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7",0.0034,null,{"v":30,"d":"30.0000"}]
["NL5448","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section",0.0051,null,{"v":25,"d":"25.0000"}]
["NL5449","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":29,"d":"29.0000"}]
["NL5450","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7","B&I-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7",{"v":6.6E-3,"d":"0.0066"},null,{"v":58,"d":"58.0000"}]
["NL5459","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer","B&I-NC","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer",0.0104,0.0107,{"v":51,"d":"51.0000"}]
["NL5460","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay","B&I-NC","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay",0.0217,0.0222,{"v":106,"d":"106.0000"}]
["NL10028","LED Fixture, Downlights, Interior","Large Industrial-NC","LED Fixture, Downlights, Interior",0.0196,0.0196,{"v":121,"d":"121.0000"}]
["NL10029","LED Fixture, Downlights, Exterior","Large Industrial-NC","LED Fixture, Downlights, Exterior",{"v":0,"d":"0.0000"},0.0144,{"v":140,"d":"140.0000"}]
["NL10214","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC","Large Industrial-NC","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC",{"v":0.02,"d":"0.0200"},{"v":0.02,"d":"0.0200"},{"v":117,"d":"117.0000"}]
["NL10281","1’ to 3’ LED Linear Ambient Fixture, Interior","Large Industrial-NC","1’ to 3’ LED Linear Ambient Fixture, Interior",{"v":0.007,"d":"0.0070"},{"v":0.007,"d":"0.0070"},{"v":43,"d":"43.0000"}]
["NL10282","4' LED Linear Ambient Fixture, Interior","Large Industrial-NC","4' LED Linear Ambient Fixture, Interior",{"v":0.014,"d":"0.0140"},{"v":0.014,"d":"0.0140"},{"v":86,"d":"86.0000"}]
["NL10283","8' LED Linear Ambient Fixture, Interior","Large Industrial-NC","8' LED Linear Ambient Fixture, Interior",{"v":0.028,"d":"0.0280"},{"v":0.028,"d":"0.0280"},{"v":173,"d":"173.0000"}]
["NL10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","Large Industrial-NC","1’ to 3’ LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},{"v":0.003,"d":"0.0030"},{"v":30,"d":"30.0000"}]
["NL10285","4' LED Linear Ambient Fixture, Exterior","Large Industrial-NC","4' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0061,{"v":59,"d":"59.0000"}]
["NL10286","8' LED Linear Ambient Fixture, Exterior","Large Industrial-NC","8' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0121,{"v":118,"d":"118.0000"}]
["NL2482","Occupancy Sensor, LED Refrigerated Case Lights","Large Industrial-NC","Occupancy Sensor, LED Refrigerated Case Lights",{"v":0.013,"d":"0.0130"},null,{"v":112,"d":"112.0000"}]
["NL3097","LED Fixture, Bilevel, Stairwell and Passageway","Large Industrial-NC","LED Fixture, Bilevel, Stairwell and Passageway",0.0262,0.0262,{"v":161,"d":"161.0000"}]
["NL3111","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer","Large Industrial-NC","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer",0.0444,0.0444,{"v":274,"d":"274.0000"}]
["NL3393","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed","Large Industrial-NC","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed",{"v":0.074,"d":"0.0740"},null,{"v":456,"d":"456.0000"}]
["NL3400","LED Fixture, 2x2, Low Output, DLC Listed","Large Industrial-NC","LED Fixture, 2x2, Low Output, DLC Listed",0.0214,0.0214,{"v":132,"d":"132.0000"}]
["NL3401","LED Fixture, 2x2, High Output, DLC Listed","Large Industrial-NC","LED Fixture, 2x2, High Output, DLC Listed",0.0867,0.0867,{"v":534,"d":"534.0000"}]
["NL3738","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section",0.0012,null,{"v":7,"d":"7.0000"}]
["NL3739","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section",0.0121,null,{"v":75,"d":"75.0000"}]
["NL3740","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section",{"v":0.003,"d":"0.0030"},null,{"v":19,"d":"19.0000"}]
["NL3741","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section",0.0094,null,{"v":58,"d":"58.0000"}]
["NL3929","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL","Large Industrial-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL",{"v":0,"d":"0.0000"},null,{"v":40,"d":"40.0000"}]
["NL3930","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL","Large Industrial-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL",{"v":0,"d":"0.0000"},null,{"v":24,"d":"24.0000"}]
["NL3931","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W","Large Industrial-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W",{"v":0,"d":"0.0000"},null,{"v":18,"d":"18.0000"}]
["NL3932","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL","Large Industrial-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL",0.0071,null,{"v":44,"d":"44.0000"}]
["NL3933","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL","Large Industrial-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL",0.0042,null,{"v":26,"d":"26.0000"}]
["NL3934","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W","Large Industrial-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W",0.0032,null,{"v":19,"d":"19.0000"}]
["NL4280","LED, Exterior Fixture, Low Output, <= 4,999 lumens","Large Industrial-NC","LED, Exterior Fixture, Low Output, <= 4,999 lumens",{"v":0,"d":"0.0000"},0.0122,{"v":389,"d":"389.0000"}]
["NL4281","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens","Large Industrial-NC","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens",{"v":0,"d":"0.0000"},{"v":0.027,"d":"0.0270"},{"v":731,"d":"731.0000"}]
["NL4282","LED, Exterior Fixture, High Output, 10,000-29,999 lumens","Large Industrial-NC","LED, Exterior Fixture, High Output, 10,000-29,999 lumens",{"v":0,"d":"0.0000"},0.0601,{"v":1806,"d":"1806.0000"}]
["NL4283","LED, Exterior Fixture, Very High Output, >= 30,000 lumens","Large Industrial-NC","LED, Exterior Fixture, Very High Output, >= 30,000 lumens",{"v":0,"d":"0.0000"},0.1486,{"v":3279,"d":"3279.0000"}]
["NL4347","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay","Large Industrial-NC","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay",0.0924,null,{"v":570,"d":"570.0000"}]
["NL4781","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour",{"v":0.004,"d":"0.0040"},null,{"v":35,"d":"35.0000"}]
["NL4782","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":17,"d":"17.0000"}]
["NL4783","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour",0.0122,null,{"v":107,"d":"107.0000"}]
["NL4784","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":54,"d":"54.0000"}]
["NL4785","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour",{"v":1.5E-3,"d":"0.0015"},null,{"v":13,"d":"13.0000"}]
["NL4786","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":7,"d":"7.0000"}]
["NL4787","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour",0.0158,null,{"v":138,"d":"138.0000"}]
["NL4788","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":69,"d":"69.0000"}]
["NL4795","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay","Large Industrial-NC","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay",0.1207,null,{"v":744,"d":"744.0000"}]
["NL4796","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay","Large Industrial-NC","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay",0.1371,null,{"v":845,"d":"845.0000"}]
["NL4813","LED Fixture, Track/Mono/Accent","Large Industrial-NC","LED Fixture, Track/Mono/Accent",0.0008,0.0008,{"v":4.75,"d":"4.7500"}]
["NL5063","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn","Large Industrial-NC","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn",{"v":0,"d":"0.0000"},0.0002,{"v":1.48,"d":"1.4800"}]
["NL5065","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only","Large Industrial-NC","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.0461,{"v":449,"d":"449.0000"}]
["NL5066","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only","Large Industrial-NC","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.0886,{"v":863,"d":"863.0000"}]
["NL5067","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only","Large Industrial-NC","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.2156,{"v":2099,"d":"2099.0000"}]
["NL5068","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only","Large Industrial-NC","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only",{"v":0,"d":"0.0000"},0.4112,{"v":4003,"d":"4003.0000"}]
["NL5235","Refrigeration Savings for Lighting Upgrades in Freezers","Large Industrial-NC","Refrigeration Savings for Lighting Upgrades in Freezers",0.0006,0.0006,{"v":3.39,"d":"3.3900"}]
["NL5236","Refrigeration Savings for Lighting Upgrades in Coolers","Large Industrial-NC","Refrigeration Savings for Lighting Upgrades in Coolers",0.0003,0.0003,{"v":2.06,"d":"2.0600"}]
["NL5445","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section",0.0026,null,{"v":16,"d":"16.0000"}]
["NL5446","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":15,"d":"15.0000"}]
["NL5447","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7",0.0034,null,{"v":30,"d":"30.0000"}]
["NL5448","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section",0.0051,null,{"v":31,"d":"31.0000"}]
["NL5449","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":29,"d":"29.0000"}]
["NL5450","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7","Large Industrial-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7",{"v":6.6E-3,"d":"0.0066"},null,{"v":58,"d":"58.0000"}]
["NL5459","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer","Large Industrial-NC","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer",0.0106,0.0106,{"v":65,"d":"65.0000"}]
["NL5460","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay","Large Industrial-NC","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay",0.0219,0.0219,{"v":135,"d":"135.0000"}]
["NL10028","LED Fixture, Downlights, Interior","Schools & Government-NC","LED Fixture, Downlights, Interior",{"v":0.015,"d":"0.0150"},0.0173,{"v":83,"d":"83.0000"}]
["NL10029","LED Fixture, Downlights, Exterior","Schools & Government-NC","LED Fixture, Downlights, Exterior",{"v":0,"d":"0.0000"},0.0144,{"v":140,"d":"140.0000"}]
["NL10214","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC","Schools & Government-NC","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC",0.0162,0.0187,{"v":84,"d":"84.0000"}]
["NL10281","1’ to 3’ LED Linear Ambient Fixture, Interior","Schools & Government-NC","1’ to 3’ LED Linear Ambient Fixture, Interior",0.0054,0.0062,{"v":29,"d":"29.0000"}]
["NL10282","4' LED Linear Ambient Fixture, Interior","Schools & Government-NC","4' LED Linear Ambient Fixture, Interior",0.0107,0.0124,{"v":59,"d":"59.0000"}]
["NL10283","8' LED Linear Ambient Fixture, Interior","Schools & Government-NC","8' LED Linear Ambient Fixture, Interior",0.0215,0.0248,{"v":118,"d":"118.0000"}]
["NL10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","Schools & Government-NC","1’ to 3’ LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},{"v":0.003,"d":"0.0030"},{"v":30,"d":"30.0000"}]
["NL10285","4' LED Linear Ambient Fixture, Exterior","Schools & Government-NC","4' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0061,{"v":59,"d":"59.0000"}]
["NL10286","8' LED Linear Ambient Fixture, Exterior","Schools & Government-NC","8' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0121,{"v":118,"d":"118.0000"}]
["NL2482","Occupancy Sensor, LED Refrigerated Case Lights","Schools & Government-NC","Occupancy Sensor, LED Refrigerated Case Lights",{"v":0.013,"d":"0.0130"},null,{"v":112,"d":"112.0000"}]
["NL3097","LED Fixture, Bilevel, Stairwell and Passageway","Schools & Government-NC","LED Fixture, Bilevel, Stairwell and Passageway",0.0201,0.0231,{"v":110,"d":"110.0000"}]
["NL3111","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer","Schools & Government-NC","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer",{"v":0.034,"d":"0.0340"},0.0392,{"v":187,"d":"187.0000"}]
["NL3393","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed","Schools & Government-NC","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed",0.0615,null,{"v":311,"d":"311.0000"}]
["NL3400","LED Fixture, 2x2, Low Output, DLC Listed","Schools & Government-NC","LED Fixture, 2x2, Low Output, DLC Listed",0.0164,0.0189,{"v":90,"d":"90.0000"}]
["NL3401","LED Fixture, 2x2, High Output, DLC Listed","Schools & Government-NC","LED Fixture, 2x2, High Output, DLC Listed",0.0665,0.0766,{"v":365,"d":"365.0000"}]
["NL3738","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section",{"v":1E-3,"d":"0.0010"},null,{"v":5,"d":"5.0000"}]
["NL3739","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section",0.0101,null,{"v":51,"d":"51.0000"}]
["NL3740","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section",0.0025,null,{"v":13,"d":"13.0000"}]
["NL3741","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section",0.0078,null,{"v":40,"d":"40.0000"}]
["NL3929","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL","Schools & Government-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL",{"v":0,"d":"0.0000"},null,{"v":40,"d":"40.0000"}]
["NL3930","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL","Schools & Government-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL",{"v":0,"d":"0.0000"},null,{"v":24,"d":"24.0000"}]
["NL3931","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W","Schools & Government-NC","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W",{"v":0,"d":"0.0000"},null,{"v":18,"d":"18.0000"}]
["NL3932","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL","Schools & Government-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL",0.0059,null,{"v":30,"d":"30.0000"}]
["NL3933","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL","Schools & Government-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL",0.0035,null,{"v":18,"d":"18.0000"}]
["NL3934","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W","Schools & Government-NC","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W",0.0026,null,{"v":13,"d":"13.0000"}]
["NL4280","LED, Exterior Fixture, Low Output, <= 4,999 lumens","Schools & Government-NC","LED, Exterior Fixture, Low Output, <= 4,999 lumens",{"v":0,"d":"0.0000"},0.0122,{"v":389,"d":"389.0000"}]
["NL4281","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens","Schools & Government-NC","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens",{"v":0,"d":"0.0000"},{"v":0.027,"d":"0.0270"},{"v":731,"d":"731.0000"}]
["NL4282","LED, Exterior Fixture, High Output, 10,000-29,999 lumens","Schools & Government-NC","LED, Exterior Fixture, High Output, 10,000-29,999 lumens",{"v":0,"d":"0.0000"},0.0601,{"v":1806,"d":"1806.0000"}]
["NL4283","LED, Exterior Fixture, Very High Output, >= 30,000 lumens","Schools & Government-NC","LED, Exterior Fixture, Very High Output, >= 30,000 lumens",{"v":0,"d":"0.0000"},0.1486,{"v":3279,"d":"3279.0000"}]
["NL4347","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay","Schools & Government-NC","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay",0.0768,null,{"v":389,"d":"389.0000"}]
["NL4781","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour",{"v":0.004,"d":"0.0040"},null,{"v":35,"d":"35.0000"}]
["NL4782","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":17,"d":"17.0000"}]
["NL4783","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour",0.0122,null,{"v":107,"d":"107.0000"}]
["NL4784","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":54,"d":"54.0000"}]
["NL4785","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour",{"v":1.5E-3,"d":"0.0015"},null,{"v":13,"d":"13.0000"}]
["NL4786","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":7,"d":"7.0000"}]
["NL4787","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour",0.0158,null,{"v":138,"d":"138.0000"}]
["NL4788","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":69,"d":"69.0000"}]
["NL4795","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay","Schools & Government-NC","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay",0.1003,null,{"v":508,"d":"508.0000"}]
["NL4796","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay","Schools & Government-NC","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay",0.1139,null,{"v":577,"d":"577.0000"}]
["NL4813","LED Fixture, Track/Mono/Accent","Schools & Government-NC","LED Fixture, Track/Mono/Accent",0.0006,0.0006,{"v":3.24,"d":"3.2400"}]
["NL5063","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn","Schools & Government-NC","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn",{"v":0,"d":"0.0000"},0.0002,{"v":1.48,"d":"1.4800"}]
["NL5065","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only","Schools & Government-NC","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.0461,{"v":449,"d":"449.0000"}]
["NL5066","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only","Schools & Government-NC","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.0886,{"v":863,"d":"863.0000"}]
["NL5067","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only","Schools & Government-NC","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only",{"v":0,"d":"0.0000"},0.2156,{"v":2099,"d":"2099.0000"}]
["NL5068","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only","Schools & Government-NC","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only",{"v":0,"d":"0.0000"},0.4112,{"v":4003,"d":"4003.0000"}]
["NL5235","Refrigeration Savings for Lighting Upgrades in Freezers","Schools & Government-NC","Refrigeration Savings for Lighting Upgrades in Freezers",0.0004,0.0005,{"v":2.31,"d":"2.3100"}]
["NL5236","Refrigeration Savings for Lighting Upgrades in Coolers","Schools & Government-NC","Refrigeration Savings for Lighting Upgrades in Coolers",0.0003,0.0003,{"v":1.41,"d":"1.4100"}]
["NL5445","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section",0.0022,null,{"v":11,"d":"11.0000"}]
["NL5446","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":15,"d":"15.0000"}]
["NL5447","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7",0.0034,null,{"v":30,"d":"30.0000"}]
["NL5448","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section",0.0042,null,{"v":21,"d":"21.0000"}]
["NL5449","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":29,"d":"29.0000"}]
["NL5450","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7","Schools & Government-NC","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7",{"v":6.6E-3,"d":"0.0066"},null,{"v":58,"d":"58.0000"}]
["NL5459","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer","Schools & Government-NC","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer",0.0081,0.0093,{"v":44,"d":"44.0000"}]
["NL5460","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay","Schools & Government-NC","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay",0.0168,0.0194,{"v":92,"d":"92.0000"}]
["L10028","LED Fixture, Downlights, Interior","Schools & Government","LED Fixture, Downlights, Interior",0.0248,0.0286,{"v":136,"d":"136.0000"}]
["L10029","LED Fixture, Downlights, Exterior","Schools & Government","LED Fixture, Downlights, Exterior",{"v":0,"d":"0.0000"},{"v":0.036,"d":"0.0360"},{"v":350,"d":"350.0000"}]
["L10039","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior","Schools & Government","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior",0.0159,0.0184,{"v":87,"d":"87.0000"}]
["L10040","Four Pin-Base Lamp Replacing CFL, DLC Listed, Exterior","Schools & Government","Four Pin-Base Lamp Replacing CFL, DLC Listed, Exterior",{"v":0,"d":"0.0000"},0.0122,{"v":118,"d":"118.0000"}]
["L10042","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)","Schools & Government","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)",{"v":0.152,"d":"0.1520"},0.1752,{"v":834,"d":"834.0000"}]
["L10043","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior","Schools & Government","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior",{"v":0,"d":"0.0000"},{"v":0.772,"d":"0.7720"},{"v":751,"d":"751.0000"}]
["L10211","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC","Schools & Government","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC",0.0241,0.0277,{"v":123,"d":"123.0000"}]
["L10212","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC","Schools & Government","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC",0.0755,{"v":0.087,"d":"0.0870"},{"v":378,"d":"378.0000"}]
["L10213","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC","Schools & Government","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC",0.0448,0.0516,{"v":227,"d":"227.0000"}]
["L10214","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC","Schools & Government","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC",0.0162,0.0187,{"v":84,"d":"84.0000"}]
["L10215","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC","Schools & Government","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC",0.1401,0.1615,{"v":708,"d":"708.0000"}]
["L10216","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC","Schools & Government","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC",{"v":0.217,"d":"0.2170"},0.2502,{"v":1096,"d":"1096.0000"}]
["L10217","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC","Schools & Government","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC",0.0931,0.1074,{"v":479,"d":"479.0000"}]
["L10218","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC","Schools & Government","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC",0.1361,0.1568,{"v":698,"d":"698.0000"}]
["L10223","Advanced Lighting Controls, Interior","Schools & Government","Advanced Lighting Controls, Interior",0.0003,0.0003,{"v":1.63,"d":"1.6300"}]
["L10224","Advanced Lighting Controls, Exterior","Schools & Government","Advanced Lighting Controls, Exterior",{"v":0,"d":"0.0000"},0.0002,{"v":1.97,"d":"1.9700"}]
["L10281","1’ to 3’ LED Linear Ambient Fixture, Interior","Schools & Government","1’ to 3’ LED Linear Ambient Fixture, Interior",0.0054,0.0062,{"v":29,"d":"29.0000"}]
["L10282","4' LED Linear Ambient Fixture, Interior","Schools & Government","4' LED Linear Ambient Fixture, Interior",0.0107,0.0124,{"v":59,"d":"59.0000"}]
["L10283","8' LED Linear Ambient Fixture, Interior","Schools & Government","8' LED Linear Ambient Fixture, Interior",0.0215,0.0248,{"v":118,"d":"118.0000"}]
["L10284","1’ to 3’ LED Linear Ambient Fixture, Exterior","Schools & Government","1’ to 3’ LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},{"v":0.003,"d":"0.0030"},{"v":30,"d":"30.0000"}]
["L10285","4' LED Linear Ambient Fixture, Exterior","Schools & Government","4' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0061,{"v":59,"d":"59.0000"}]
["L10286","8' LED Linear Ambient Fixture, Exterior","Schools & Government","8' LED Linear Ambient Fixture, Exterior",{"v":0,"d":"0.0000"},0.0121,{"v":118,"d":"118.0000"}]
["L10287","General Wattage Reduction, Interior","Schools & Government","General Wattage Reduction, Interior",0.0006,0.0007,{"v":3.24,"d":"3.2400"}]
["L10288","General Wattage Reduction, Exterior","Schools & Government","General Wattage Reduction, Exterior",{"v":0,"d":"0.0000"},0.0005,{"v":4.38,"d":"4.3800"}]
["L10289","Fixture Elimination, Interior","Schools & Government","Fixture Elimination, Interior",0.0006,0.0007,{"v":3.24,"d":"3.2400"}]
["L10290","Fixture Elimination, Exterior","Schools & Government","Fixture Elimination, Exterior",{"v":0,"d":"0.0000"},0.0005,{"v":4.38,"d":"4.3800"}]
["L2482","Occupancy Sensor, LED Refrigerated Case Lights","Schools & Government","Occupancy Sensor, LED Refrigerated Case Lights",0.0075,null,{"v":65,"d":"65.0000"}]
["L2768","LED, Exit Sign, Retrofit","Schools & Government","LED, Exit Sign, Retrofit",0.0213,0.0213,{"v":187,"d":"187.0000"}]
["L3091","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay","Schools & Government","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay",0.1122,0.1293,{"v":616,"d":"616.0000"}]
["L3092","LED Fixture, <250 Watts, Replacing 320-400 Watt HID, High Bay","Schools & Government","LED Fixture, <250 Watts, Replacing 320-400 Watt HID, High Bay",0.1188,{"v":0.137,"d":"0.1370"},{"v":652,"d":"652.0000"}]
["L3093","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay","Schools & Government","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay",0.1733,0.1997,{"v":951,"d":"951.0000"}]
["L3094","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay","Schools & Government","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay",{"v":0,"d":"0.0000"},0.0009,{"v":8.76,"d":"8.7600"}]
["L3095","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay","Schools & Government","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay",0.4825,0.5561,{"v":2649,"d":"2649.0000"}]
["L3096","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay","Schools & Government","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay",0.4651,0.5361,{"v":2553,"d":"2553.0000"}]
["L3097","LED Fixture, Bilevel, Stairwell and Passageway","Schools & Government","LED Fixture, Bilevel, Stairwell and Passageway",0.0201,0.0231,{"v":110,"d":"110.0000"}]
["L3111","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer","Schools & Government","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer",{"v":0.034,"d":"0.0340"},0.0392,{"v":187,"d":"187.0000"}]
["L3114","LED, Horizontal Case Lighting","Schools & Government","LED, Horizontal Case Lighting",0.0174,0.0174,{"v":112,"d":"112.0000"}]
["L3393","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed","Schools & Government","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed",0.0634,null,{"v":321,"d":"321.0000"}]
["L3400","LED Fixture, 2x2, Low Output, DLC Listed","Schools & Government","LED Fixture, 2x2, Low Output, DLC Listed",0.0164,0.0189,{"v":90,"d":"90.0000"}]
["L3401","LED Fixture, 2x2, High Output, DLC Listed","Schools & Government","LED Fixture, 2x2, High Output, DLC Listed",0.0665,0.0766,{"v":365,"d":"365.0000"}]
["L3406","Daylighting Controls","Schools & Government","Daylighting Controls",0.0002,0.0002,{"v":0.91,"d":"0.9100"}]
["L3511","LED Replacement of 4’ T8 Lamps w/Integral or External Driver","Schools & Government","LED Replacement of 4’ T8 Lamps w/Integral or External Driver",{"v":6.3E-3,"d":"0.0063"},null,{"v":32,"d":"32.0000"}]
["L3512","LED Replacement of 4’ T8 Lamps utilizing existing ballast","Schools & Government","LED Replacement of 4’ T8 Lamps utilizing existing ballast",0.0069,null,{"v":35,"d":"35.0000"}]
["L3738","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section",{"v":1E-3,"d":"0.0010"},null,{"v":5,"d":"5.0000"}]
["L3739","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section",0.0101,null,{"v":51,"d":"51.0000"}]
["L3740","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section",0.0025,null,{"v":13,"d":"13.0000"}]
["L3741","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section",0.0078,null,{"v":40,"d":"40.0000"}]
["L3759","LED Replacement of 4’ T8 Lamps, Direct Wire","Schools & Government","LED Replacement of 4’ T8 Lamps, Direct Wire",0.0073,null,{"v":37,"d":"37.0000"}]
["L3760","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer","Schools & Government","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0104,null,{"v":53,"d":"53.0000"}]
["L3903","LED Signage Retrofit, Interior","Schools & Government","LED Signage Retrofit, Interior",0.0012,{"v":1.4E-3,"d":"0.0014"},{"v":6.48,"d":"6.4800"}]
["L3904","LED Signage Retrofit, Exterior","Schools & Government","LED Signage Retrofit, Exterior",{"v":0,"d":"0.0000"},0.0009,{"v":8.76,"d":"8.7600"}]
["L3929","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL",{"v":0,"d":"0.0000"},null,{"v":40,"d":"40.0000"}]
["L3930","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL",{"v":0,"d":"0.0000"},null,{"v":24,"d":"24.0000"}]
["L3931","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≤ 13W",{"v":0,"d":"0.0000"},null,{"v":18,"d":"18.0000"}]
["L3932","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL",0.0059,null,{"v":30,"d":"30.0000"}]
["L3933","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL",0.0035,null,{"v":18,"d":"18.0000"}]
["L3934","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W",0.0026,null,{"v":13,"d":"13.0000"}]
["L3935","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent",{"v":0,"d":"0.0000"},null,{"v":499,"d":"499.0000"}]
["L3936","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent",{"v":0,"d":"0.0000"},null,{"v":364,"d":"364.0000"}]
["L3937","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent",{"v":0,"d":"0.0000"},null,{"v":284,"d":"284.0000"}]
["L3938","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent",{"v":0,"d":"0.0000"},null,{"v":237,"d":"237.0000"}]
["L3939","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 36W – 54W Incandescent","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 36W – 54W Incandescent",{"v":0,"d":"0.0000"},null,{"v":182,"d":"182.0000"}]
["L3940","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent","Schools & Government","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent",{"v":0,"d":"0.0000"},null,{"v":114,"d":"114.0000"}]
["L3941","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W",0.0729,null,{"v":369,"d":"369.0000"}]
["L3942","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W",0.0532,null,{"v":269,"d":"269.0000"}]
["L3943","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W",0.0415,null,{"v":210,"d":"210.0000"}]
["L3944","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W",0.0347,null,{"v":175,"d":"175.0000"}]
["L3945","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W",0.0266,null,{"v":135,"d":"135.0000"}]
["L3946","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W","Schools & Government","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W",0.0167,null,{"v":84,"d":"84.0000"}]
["L4280","LED, Exterior Fixture, Low Output, <= 4,999 lumens","Schools & Government","LED, Exterior Fixture, Low Output, <= 4,999 lumens",{"v":0,"d":"0.0000"},0.0122,{"v":389,"d":"389.0000"}]
["L4281","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens","Schools & Government","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens",{"v":0,"d":"0.0000"},null,{"v":731,"d":"731.0000"}]
["L4282","LED, Exterior Fixture, High Output, 10,000-29,999 lumens","Schools & Government","LED, Exterior Fixture, High Output, 10,000-29,999 lumens",{"v":0,"d":"0.0000"},0.0601,{"v":1806,"d":"1806.0000"}]
["L4283","LED, Exterior Fixture, Very High Output, >= 30,000 lumens","Schools & Government","LED, Exterior Fixture, Very High Output, >= 30,000 lumens",{"v":0,"d":"0.0000"},0.1486,{"v":3279,"d":"3279.0000"}]
["L4314","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12","Schools & Government","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12",0.0201,null,{"v":102,"d":"102.0000"}]
["L4315","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, Exterior","Schools & Government","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":138,"d":"138.0000"}]
["L4316","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, 24/7","Schools & Government","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12, 24/7",0.0314,null,{"v":275,"d":"275.0000"}]
["L4317","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO","Schools & Government","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO",0.0447,null,{"v":226,"d":"226.0000"}]
["L4318","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, Exterior","Schools & Government","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":306,"d":"306.0000"}]
["L4319","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, 24/7","Schools & Government","4FT Linear LED 2L, Replacing 8FT 1L T8HO or T12HO, 24/7",0.0699,null,{"v":612,"d":"612.0000"}]
["L4320","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12","Schools & Government","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12",0.0261,null,{"v":132,"d":"132.0000"}]
["L4321","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior","Schools & Government","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":179,"d":"179.0000"}]
["L4322","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, 24/7","Schools & Government","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, 24/7",0.0408,null,{"v":358,"d":"358.0000"}]
["L4323","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO","Schools & Government","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO",0.0748,null,{"v":378,"d":"378.0000"}]
["L4324","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior","Schools & Government","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":512,"d":"512.0000"}]
["L4325","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, 24/7","Schools & Government","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, 24/7",0.1168,null,{"v":1024,"d":"1024.0000"}]
["L4326","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12","Schools & Government","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12",0.0476,null,{"v":241,"d":"241.0000"}]
["L4327","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, Exterior","Schools & Government","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, Exterior",{"v":0,"d":"0.0000"},null,{"v":326,"d":"326.0000"}]
["L4328","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, 24/7","Schools & Government","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12, 24/7",0.0744,null,{"v":652,"d":"652.0000"}]
["L4329","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO","Schools & Government","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO",0.0963,null,{"v":487,"d":"487.0000"}]
["L4330","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, Exterior","Schools & Government","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, Exterior",{"v":0,"d":"0.0000"},null,{"v":659,"d":"659.0000"}]
["L4331","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, 24/7","Schools & Government","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO, 24/7",0.1504,null,{"v":1318,"d":"1318.0000"}]
["L4347","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay","Schools & Government","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay",0.0973,null,{"v":493,"d":"493.0000"}]
["L4348","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior","Schools & Government","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior",{"v":0,"d":"0.0000"},null,{"v":47,"d":"47.0000"}]
["L4349","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7","Schools & Government","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7",0.0107,null,{"v":94,"d":"94.0000"}]
["L4350","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior","Schools & Government","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior",{"v":0,"d":"0.0000"},null,{"v":50,"d":"50.0000"}]
["L4351","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7","Schools & Government","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7",0.0114,null,{"v":100,"d":"100.0000"}]
["L4352","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior","Schools & Government","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior",{"v":0,"d":"0.0000"},null,{"v":43,"d":"43.0000"}]
["L4353","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior, 24/7","Schools & Government","LED Replacement of 4-Foot T8 Lamps, w/External Driver, Exterior, 24/7",0.0098,null,{"v":86,"d":"86.0000"}]
["L4781","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour",{"v":0.004,"d":"0.0040"},null,{"v":35,"d":"35.0000"}]
["L4782","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":17,"d":"17.0000"}]
["L4783","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 24 hour",0.0122,null,{"v":107,"d":"107.0000"}]
["L4784","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":54,"d":"54.0000"}]
["L4785","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 24 hour",{"v":1.5E-3,"d":"0.0015"},null,{"v":13,"d":"13.0000"}]
["L4786","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":7,"d":"7.0000"}]
["L4787","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 24 hour",0.0158,null,{"v":138,"d":"138.0000"}]
["L4788","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section, Exterior, 12 hour",{"v":0,"d":"0.0000"},null,{"v":69,"d":"69.0000"}]
["L4793","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer","Schools & Government","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer",0.0077,null,{"v":39,"d":"39.0000"}]
["L4795","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay","Schools & Government","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay",0.1323,null,{"v":670,"d":"670.0000"}]
["L4796","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay","Schools & Government","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay",{"v":0.16,"d":"0.1600"},null,{"v":810,"d":"810.0000"}]
["L4797","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) ","Schools & Government","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) ",{"v":0.057,"d":"0.0570"},null,{"v":29,"d":"29.0000"}]
["L4798","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) ","Schools & Government","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) ",0.0067,null,{"v":34,"d":"34.0000"}]
["L4799","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Schools & Government","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",{"v":6.6E-3,"d":"0.0066"},null,{"v":33,"d":"33.0000"}]
["L4800","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) ","Schools & Government","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) ",0.0088,null,{"v":45,"d":"45.0000"}]
["L4801","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) ","Schools & Government","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) ",0.0083,null,{"v":42,"d":"42.0000"}]
["L4802","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Schools & Government","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",0.0081,null,{"v":41,"d":"41.0000"}]
["L4803","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) ","Schools & Government","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) ",0.0072,null,{"v":37,"d":"37.0000"}]
["L4804","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) ","Schools & Government","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) ",0.0226,null,{"v":114,"d":"114.0000"}]
["L4805","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) ","Schools & Government","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) ",0.0102,null,{"v":51,"d":"51.0000"}]
["L4806","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) ","Schools & Government","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) ",0.0238,null,{"v":120,"d":"120.0000"}]
["L4807","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) ","Schools & Government","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) ",0.0087,null,{"v":44,"d":"44.0000"}]
["L4808","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) ","Schools & Government","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) ",0.0214,null,{"v":108,"d":"108.0000"}]
["L4809","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) ","Schools & Government","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) ",0.0181,null,{"v":92,"d":"92.0000"}]
["L4810","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) ","Schools & Government","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) ",0.0141,null,{"v":71,"d":"71.0000"}]
["L4811","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ","Schools & Government","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) ",{"v":0.017,"d":"0.0170"},null,{"v":86,"d":"86.0000"}]
["L4812","Non-High Bay Occupancy/Vacancy Sensor","Schools & Government","Non-High Bay Occupancy/Vacancy Sensor",{"v":1E-4,"d":"0.0001"},0.0002,{"v":0.78,"d":"0.7800"}]
["L4813","LED Fixture, Track/Mono/Accent","Schools & Government","LED Fixture, Track/Mono/Accent",0.0006,0.0006,{"v":3.24,"d":"3.2400"}]
["L4830","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior","Schools & Government","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior",{"v":0,"d":"0.0000"},null,{"v":116,"d":"116.0000"}]
["L4831","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior","Schools & Government","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior",{"v":0,"d":"0.0000"},null,{"v":124,"d":"124.0000"}]
["L4832","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior","Schools & Government","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior",{"v":0,"d":"0.0000"},null,{"v":96,"d":"96.0000"}]
["L4833","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior 24/7","Schools & Government","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type A), Exterior 24/7",0.0265,null,{"v":232,"d":"232.0000"}]
["L4834","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior 24/7","Schools & Government","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C), Exterior 24/7",0.0283,null,{"v":248,"d":"248.0000"}]
["L4835","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7","Schools & Government","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7",{"v":0.022,"d":"0.0220"},null,{"v":192,"d":"192.0000"}]
["L5061","Occupancy Sensors, On/Off, High Bay","Schools & Government","Occupancy Sensors, On/Off, High Bay",0.0002,0.0003,{"v":1.23,"d":"1.2300"}]
["L5062","Bi-Level Controls, High Bay ","Schools & Government","Bi-Level Controls, High Bay ",{"v":1E-4,"d":"0.0001"},{"v":1E-4,"d":"0.0001"},{"v":0.63,"d":"0.6300"}]
["L5063","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn","Schools & Government","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn",{"v":0,"d":"0.0000"},0.0002,{"v":1.48,"d":"1.4800"}]
["L5064","Bi-level Controls, Parking Garage Fixtures, 24 Hour","Schools & Government","Bi-level Controls, Parking Garage Fixtures, 24 Hour",0.0003,0.0003,{"v":2.96,"d":"2.9600"}]
["L5211","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Schools & Government","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0.033,"d":"0.0330"},null,{"v":169,"d":"169.0000"}]
["L5212","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Schools & Government","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0.025,"d":"0.0250"},null,{"v":124,"d":"124.0000"}]
["L5213","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Schools & Government","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0.02,"d":"0.0200"},null,{"v":101,"d":"101.0000"}]
["L5214","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL","Schools & Government","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0.014,"d":"0.0140"},null,{"v":70,"d":"70.0000"}]
["L5215","Omnidirectional Interior LED with rated lumen output of 250-449 replacing incandescent or CFL","Schools & Government","Omnidirectional Interior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0.013,"d":"0.0130"},null,{"v":63,"d":"63.0000"}]
["L5216","Decorative Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Schools & Government","Decorative Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0.033,"d":"0.0330"},null,{"v":169,"d":"169.0000"}]
["L5217","Decorative Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Schools & Government","Decorative Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0.023,"d":"0.0230"},null,{"v":116,"d":"116.0000"}]
["L5218","Decorative Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Schools & Government","Decorative Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0.021,"d":"0.0210"},null,{"v":104,"d":"104.0000"}]
["L5219","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL","Schools & Government","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0.014,"d":"0.0140"},null,{"v":70,"d":"70.0000"}]
["L5220","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL","Schools & Government","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0.012,"d":"0.0120"},null,{"v":62,"d":"62.0000"}]
["L5221","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Schools & Government","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":228,"d":"228.0000"}]
["L5222","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Schools & Government","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":168,"d":"168.0000"}]
["L5223","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Schools & Government","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":137,"d":"137.0000"}]
["L5224","Omnidirectional Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL","Schools & Government","Omnidirectional Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":95,"d":"95.0000"}]
["L5226","Decorative Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL","Schools & Government","Decorative Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":228,"d":"228.0000"}]
["L5227","Decorative Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL","Schools & Government","Decorative Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":157,"d":"157.0000"}]
["L5228","Decorative Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL","Schools & Government","Decorative Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":141,"d":"141.0000"}]
["L5229","Decorative Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL","Schools & Government","Decorative Exterior LED with rated lumen output of 450-799 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":95,"d":"95.0000"}]
["L5230","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL","Schools & Government","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL",{"v":0,"d":"0.0000"},null,{"v":84,"d":"84.0000"}]
["L5235","Refrigeration Savings for Lighting Upgrades in Freezers","Schools & Government","Refrigeration Savings for Lighting Upgrades in Freezers",0.0004,0.0005,{"v":2.31,"d":"2.3100"}]
["L5236","Refrigeration Savings for Lighting Upgrades in Coolers","Schools & Government","Refrigeration Savings for Lighting Upgrades in Coolers",0.0003,0.0003,{"v":1.41,"d":"1.4100"}]
["L5445","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section",0.0022,null,{"v":11,"d":"11.0000"}]
["L5446","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":15,"d":"15.0000"}]
["L5447","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7","Schools & Government","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7",0.0034,null,{"v":30,"d":"30.0000"}]
["L5448","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section",0.0042,null,{"v":21,"d":"21.0000"}]
["L5449","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior",{"v":0,"d":"0.0000"},null,{"v":29,"d":"29.0000"}]
["L5450","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7","Schools & Government","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior 24/7",{"v":6.6E-3,"d":"0.0066"},null,{"v":58,"d":"58.0000"}]
["L5451","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior","Schools & Government","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior",0.0071,0.0082,{"v":39,"d":"39.0000"}]
["L5452","4' TLED, Replacing 4' T5HO Lamp, Interior","Schools & Government","4' TLED, Replacing 4' T5HO Lamp, Interior",0.0216,0.0249,{"v":119,"d":"119.0000"}]
["L5453","2' TLED, Replacing 2' T8 or T12 Lamp, Interior","Schools & Government","2' TLED, Replacing 2' T8 or T12 Lamp, Interior",0.0061,{"v":0.007,"d":"0.0070"},{"v":33,"d":"33.0000"}]
["L5454","8' TLED, Replacing 8' T8 or T12 Lamp, Interior","Schools & Government","8' TLED, Replacing 8' T8 or T12 Lamp, Interior",0.0117,0.0135,{"v":64,"d":"64.0000"}]
["L5455","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior 24/7","Schools & Government","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior 24/7",0.0118,null,{"v":104,"d":"104.0000"}]
["L5456","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior","Schools & Government","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior",{"v":0,"d":"0.0000"},0.0054,{"v":53,"d":"53.0000"}]
["L5457","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7","Schools & Government","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7",0.0198,null,{"v":174,"d":"174.0000"}]
["L5458","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior","Schools & Government","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior",{"v":0,"d":"0.0000"},null,{"v":87,"d":"87.0000"}]
["L5459","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer","Schools & Government","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer",0.0081,0.0093,{"v":44,"d":"44.0000"}]
["L5460","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay","Schools & Government","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay",0.0195,0.0224,{"v":107,"d":"107.0000"}]
["L5461","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay","Schools & Government","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay",0.0608,{"v":0.07,"d":"0.0700"},{"v":334,"d":"334.0000"}]
["L5559","Programming, Lighting Controls","Schools & Government","Programming, Lighting Controls"]

{"sheet":"Measure List","index":6,"n_rows":467,"n_cols":5,"rows_kept":467,"hidden":true,"merged":[[0,0,0,4]]}
["The data on this tab is used for populating the drop down boxes on the Review Sheet tab so that the \"Not Eligible\" and \"Eligible under ___\" rows don't appear.\nUpdate instructions: Update criteria list as needed on Criteria tab, then Copy/paste as values measure code & Name from column E of Criteria tab, once each for B&I/S&G/LI, Ag/Ag-Propane, and New Construction (by changing program name on Review Sheet). Delete out the \"not eligible\" and \"Eligible under ____\" prefixes from each column. Reset the named ranges below for each catalog section, and for the overall MeasuresBI, MeasuresBIR, and MeasuresBNC ranges that are the whole columns below. Named ranges include titles with ------ at beginning / end, but not bold underline column headings at top. If any new sections are needed for a program, need to define text name & named range on rows 55 to 85 of the Lookups tab. For Ag, put Ag Catalog and Ag Propane measures first. "]
["Measure Code & Name - B&I and S&G",null,"Measure Code & Name - AgV2",null,"Measure Code & Name - Business NC"]
["----------------------LIGHTING CATALOG: LED FIXTURES----------------------------",null,"----------------------AGRIBUSINESS CATALOG: MILKING EQUIPMENT -----------------------------",null,"----------------------LIGHTING CATALOG: LED FIXTURES----------------------------"]
["L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer",null,"AG3982: Well Water Plate Heat Exchanger (<135 milking cows)",null,"N-L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"]
["L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer",null,"AG3983: Well Water Plate Heat Exchanger (≥135 milking cows)",null,"N-L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer"]
["L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps",null,"N-AG3982: Well Water Plate Heat Exchanger (<135 milking cows)",null,"N-L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps",null,"N-AG3983: Well Water Plate Heat Exchanger (≥135 milking cows)",null,"N-L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["L10214: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer, w/LLLC",null,"AG5231: Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)",null,"N-L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["L10213: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer, w/LLLC",null,"AG5232: Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)",null,"N-L10282: 4' LED Linear Ambient Fixture, Interior"]
["L10211: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps, w/LLLC",null,"AG3988: Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)",null,"N-L10283: 8' LED Linear Ambient Fixture, Interior"]
["L10212: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps, w/LLLC",null,"N-AG5231: Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)",null,"N-L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior",null,"N-AG5232: Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)",null,"N-L10285: 4' LED Linear Ambient Fixture, Exterior"]
["L10282: 4' LED Linear Ambient Fixture, Interior",null,"N-AG3988: Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)",null,"N-L10286: 8' LED Linear Ambient Fixture, Exterior"]
["L10283: 8' LED Linear Ambient Fixture, Interior",null,"----------------------AGRIBUSINESS CATALOG: OTHER SPECIALTY EQUIPMENT -----------------------------",null,"N-L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"]
["L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior",null,"AG2660: Low-Energy Livestock Waterer (Heating Element Maximum of 250W)",null,"N-L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["L10285: 4' LED Linear Ambient Fixture, Exterior",null,"AG3018: Zero-Energy Livestock Waterer",null,"N-L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"]
["L10286: 8' LED Linear Ambient Fixture, Exterior",null,"N-AG3018: Zero-Energy Livestock Waterer",null,"N-L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"]
["L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture",null,"AG4939: Swine Farrowing Crate Heater, Single",null,"N-L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO"]
["L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior",null,"AG4940: Swine Farrowing Crate Heater, Double",null,"N-L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO"]
["L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture",null,"N-AG4939: Swine Farrowing Crate Heater, Single",null,"N-L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO"]
["L3903: Interior LED Signage",null,"N-AG4940: Swine Farrowing Crate Heater, Double",null,"N-L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["L3904: Exterior LED Signage",null,"AG3386: Efficient Grain Dryer (Natural Gas or Propane)",null,"N-L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID",null,"AG2434: Pump Motor Horsepower Reduction",null,"N-L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID",null,"AG4949: VFD, Irrigation Well Pump (≥500 Annual Operating Hours)",null,"N-L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID",null,"N-AG4949: VFD, Irrigation Well Pump (≥500 Annual Operating Hours)",null,"N-L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID",null,"----------------------AGRIBUSINESS CATALOG: LIGHTING --------------------------------------------",null,"N-L5065: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID",null,"L5459: 1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer",null,"N-L5066: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID",null,"L3111: 2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer",null,"N-L5067: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12",null,"L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps",null,"N-L5068: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
["L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO",null,"L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps",null,"----------------------LIGHTING CATALOG: LED LAMPS----------------------------"]
["L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO",null,"L10028: LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture",null,"----------------------LIGHTING CATALOG: CONTROLS----------------------------"]
["L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO",null,"L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior",null,"----------------------LIGHTING CATALOG: OTHER LIGHTING SOLUTIONS----------------------------"]
["L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO",null,"L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior",null,"N-L4948: Lighting Power Density (LPD) better than code requirements"]
["L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO",null,"L10282: 4' LED Linear Ambient Fixture, Interior",null,"N-L5233: Networked Lighting Controls (NLC) better than code requirements"]
["L10215: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID, w/LLLC",null,"L10283: 8' LED Linear Ambient Fixture, Interior",null,"N-R5235: Refrigeration Savings for Lighting Upgrades in Freezers"]
["L10216: ≤ 250W LED High Bay/Low Bay, replacing 400W HID, w/LLLC",null,"L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior",null,"N-R5236: Refrigeration Savings for Lighting Upgrades in Coolers"]
["L10217: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO, w/LLLC",null,"L10285: 4' LED Linear Ambient Fixture, Exterior",null,"----------------------HVAC CATALOG: HEATING SYSTEMS----------------------------"]
["L10218: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO, w/LLLC",null,"L10286: 8' LED Linear Ambient Fixture, Exterior",null,"N-H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency"]
["L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"AG4695: LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture",null,"N-H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency"]
["L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"AG4696: LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture",null,"N-H5237: High Turndown Burner, New Boiler Replacement"]
["L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"AG4697: LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture",null,"N-H2422: Infrared Heater"]
["L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"AG4698: LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture",null,"N-H5436: Unit Heater, ≥ 90% Thermal Efficiency"]
["----------------------LIGHTING CATALOG: LED LAMPS----------------------------",null,"AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture",null,"N-H2699: PTHP <8,000 BTUh, ≥10.7 EER and ≥3.1 COP   (NC =  ≥12.7 EER and ≥3.1 COP)"]
["L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID",null,"AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture",null,"N-H2702: PTHP 8,000-9,999 BTUh, ≥10.4 EER and ≥3.0 COP   (NC =  ≥12.1 EER and ≥3.0 COP)"]
["L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior",null,"L4280: Outdoor LED Fixture or Retrofit Kit – Low Output",null,"N-H2701: PTHP 10,000-12,999 BTUh, ≥9.9 EER and ≥2.9 COP   (NC =  ≥10.9 EER and ≥2.9 COP)"]
["L10039: Four-pin base LED Lamp Replacing CFL",null,"L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output",null,"N-H2700: PTHP ≥13,000 BTUh, ≥9.3 EER and ≥2.9 COP   (NC =  ≥10.3 EER and ≥2.9 COP)"]
["L10040: Four-pin base LED Lamp Replacing CFL, Exterior",null,"L4282: Outdoor LED Fixture or Retrofit Kit – High Output ",null,"N-H5081: Direct Fired Make-up Air Unit, Constant Volume"]
["L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp",null,"L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output",null,"N-H10030: Direct Fired Make-up Air Unit, Variable Air Volume"]
["L5452: 4' TLED, replacing 4' T5HO Lamp",null,"N-L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"----------------------HVAC CATALOG: COOLING SYSTEMS----------------------------"]
["L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp",null,"N-L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"N-H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["L5454: 8' TLED, replacing 8' T8 or T12 Lamp",null,"N-L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"N-H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior",null,"N-L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"N-H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior",null,"L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing existing E39 base lamp",null,"N-H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["----------------------LIGHTING CATALOG: CONTROLS----------------------------",null,"L10043: Mogul Screw-in Base (E39) replacing existing E39 base lamp, Exterior",null,"N-H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["L10223: Advanced Lighting Controls, Interior",null,"L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp",null,"N-H4368: DX Cooling ≥ 5.42 to < 11.25 tons, Min. Eff. = 16.1 IEER (additional incentive on IEER)"]
["L10224: Advanced Lighting Controls, Exterior",null,"L5452: 4' TLED, replacing 4' T5HO Lamp",null,"N-H4369: DX Cooling ≥ 11.25 to < 20.00 tons, Min. Eff. = 15.4 IEER (additional incentive on IEER)"]
["L3406: Daylighting Controls",null,"L5453: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp",null,"N-H4370: DX Cooling ≥ 20.00 to < 63.33 tons, Min. Eff. = 14.3 IEER (additional incentive on IEER)"]
["L5061: High and Low Bay On/Off Occupancy Sensor Control",null,"L5454: 8' TLED, replacing 8' T8 or T12 Lamp",null,"N-H4371: DX Cooling ≥ 63.33 tons, Min. Eff. = 9.7 EER and 11.4 IEER (additional incentive on IEER)"]
["L5062: High and Low Bay Bi-Level Occupancy Control",null,"L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior",null,"N-H10025: Air Source Heat Pump ≥ 5.42 to < 11.25 tons, Min. Eff. = 15.1 IEER (additional incentive on IEER)"]
["L4812: Non-High Bay Occupancy/Vacancy Sensor",null,"L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior",null,"N-H10026: Air Source Heat Pump ≥ 11.25 to < 20.00 tons, Min. Eff. = 14.5 IEER (additional incentive on IEER)"]
["L5063: Bi-Level Controls, Parking Garage Lighting, Dusk to Dawn",null,"AG5024: Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture",null,"N-H10027: Air Source Heat Pump ≥ 20.00 to < 63.33 tons, Min. Eff. = 13.5 IEER (additional incentive on IEER)"]
["L5064: Bi-Level Controls, Parking Garage Lighting, 24 Hour",null,"AG5025: Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture",null,"N-H4712: Air-Cooled Chiller, Path A, < 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.880 kW/ton "]
["----------------------LIGHTING CATALOG: OTHER LIGHTING SOLUTIONS----------------------------",null,"AG5026: Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture",null,"N-H4713: Air-Cooled Chiller, Path A, ≥ 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.860 kW/ton "]
["R5235: Refrigeration Savings for Lighting Upgrades in Freezers",null,"AG5027: Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture",null,"N-H4714: Air-Cooled Chiller, Path B, < 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.730 kW/ton "]
["R5236: Refrigeration Savings for Lighting Upgrades in Coolers",null,"AG5028: Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture",null,"N-H4715: Air-Cooled Chiller, Path B, ≥ 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.720 kW/ton "]
["L10289: Fixture Elimination, Interior",null,"AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture",null,"N-H4716: PD Water-Cooled, Path A, <75 tons, Full Load ≤0.720 kW/ton and IPLV ≤0.600 kW/ton"]
["L10287: General Wattage Reduction, Interior",null,"AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture",null,"N-H4717: PD Water-Cooled, Path A, ≥ 75 tons and < 150 tons, Full Load ≤0.690 kW/ton and IPLV ≤0.560 kW/ton"]
["L10290: Fixture Elimination, Exterior",null,"L10289: Fixture Elimination, Interior",null,"N-H4718: PD Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.630 kW/ton and IPLV ≤0.540 kW/ton"]
["L10288: General Wattage Reduction, Exterior",null,"L10287: General Wattage Reduction, Interior",null,"N-H4719: PD Water-Cooled, Path A, ≥ 300 tons and < 600 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.520 kW/ton"]
["----------------------HVAC CATALOG: HEATING SYSTEMS----------------------------",null,"L10290: Fixture Elimination, Exterior",null,"N-H4720: PD Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton"]
["H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency",null,"L10288: General Wattage Reduction, Exterior",null,"N-H4726: Centrifugal Water-Cooled, Path A, <150 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton"]
["H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency",null,"----------------------AGRIBUSINESS CATALOG: VENTILATION  --------------------------------------------",null,"N-H4727: Centrifugal Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton"]
["H2221: Outdoor Air Reset/Cutout Controls",null,"AG3998: Fans, High Volume Low Speed (HVLS)",null,"N-H4728: Centrifugal Water-Cooled, Path A, ≥ 300 tons and < 400 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.520 kW/ton"]
["H2205: Linkageless Controls, HVAC Boilers",null,"N-AG3998: Fans, High Volume Low Speed (HVLS)",null,"N-H4729: Centrifugal Water-Cooled, Path A, ≥ 400 tons and < 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton"]
["H2206: O₂ Trim Controls, HVAC Boilers",null,"AG5089: Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed",null,"N-H4730: Centrifugal Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton"]
["H2203: High Turndown Burner, Retrofit on Existing Boiler",null,"N-AG5089: Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed",null,"N-H4721: PD Water-Cooled, Path B, <75 tons, Full Load ≤0.780 kW/ton and IPLV ≤0.470 kW/ton"]
["H5237: High Turndown Burner, New Boiler Replacement",null,"AG5095: Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed",null,"N-H4722: PD Water-Cooled, Path B, ≥ 75 tons and < 150 tons, Full Load ≤0.750 kW/ton and IPLV ≤0.460 kW/ton"]
["H2225: Steam Trap Survey (HVAC)",null,"N-AG5095: Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed",null,"N-H4723: PD Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.680 kW/ton and IPLV ≤0.410 kW/ton"]
["H4004: Steam Trap Repair, <10 psig General Heating, 7/32\" or Smaller Trap",null,"AG5086: Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)",null,"N-H4724: PD Water-Cooled, Path B, ≥ 300 tons and < 600 tons, Full Load ≤0.6250 kW/ton and IPLV ≤0.380 kW/ton"]
["H4005: Steam Trap Repair, <10 psig General Heating, 1/4\" Trap",null,"AG5087: Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)",null,"N-H4725: PD Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton"]
["H4006: Steam Trap Repair, <10 psig General Heating, 5/16\" Trap",null,"N-AG5086: Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)",null,"N-H4731: Centrifugal Water-Cooled, Path B, <150 tons, Full Load ≤0.695 kW/ton and IPLV ≤0.410 kW/ton"]
["H4007: Steam Trap Repair, <10 psig General Heating, 3/8\" or Larger Trap",null,"N-AG5087: Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)",null,"N-H4732: Centrifugal Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.635 kW/ton and IPLV ≤0.370 kW/ton"]
["H4008: Steam Trap Repair, 10-49 psig General Heating, 7/32\" or Smaller Trap",null,"AG5090: Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)",null,"N-H4733: Centrifugal Water-Cooled, Path B, ≥ 300 tons and < 400 tons, Full Load ≤0.595 kW/ton and IPLV ≤0.360 kW/ton"]
["H4009: Steam Trap Repair, 10-49 psig General Heating, 1/4\" Trap",null,"AG5091: Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)",null,"N-H4734: Centrifugal Water-Cooled, Path B, ≥ 400 tons and < 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton"]
["H4010: Steam Trap Repair, 10-49 psig General Heating, 5/16\" Trap",null,"AG5092: Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)",null,"N-H4735: Centrifugal Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585kW/ton and IPLV ≤0.350 kW/ton"]
["H4011: Steam Trap Repair, 10-49 psig General Heating, 3/8\" or Larger Trap",null,"N-AG5090: Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)",null,"----------------------HVAC CATALOG: VENTILATION AND CONTROLS----------------------------"]
["H4012: Steam Trap Repair, 50-124 psig General Heating, 7/32\" or Smaller Trap",null,"N-AG5091: Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)",null,"N-H2314: Energy Recovery Ventilator, Sensible & Latent Heat"]
["H4013: Steam Trap Repair, 50-124 psig General Heating, 1/4\" Trap",null,"N-AG5092: Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)",null,"N-H5082: Energy Recovery Ventilator, Sensible Heat Only"]
["H4014: Steam Trap Repair, 50-124 psig General Heating, 5/16\" Trap",null,"----------------------AGRIBUSINESS CATALOG: VFD & COMPRESSED AIR  --------------------------------------------",null,"N-H2853: Demand Controlled Ventilation (DCV) for Multiple Zone RTU/AHU/Unit Ventilator"]
["H4015: Steam Trap Repair, 50-124 psig General Heating, 3/8\" or Larger Trap",null,"AG10209: VFD, Ag Water System, ≥1000 hours",null,"N-H3266: Demand Controlled Ventilation (DCV) for Single Zone RTU/AHU"]
["H4944: Steam Trap Repair, ≥125 psig General Heating, 7/32\" or Smaller Trap",null,"AG10210: VFD, Ag Water System, 500-999 hours",null,"N-H2373: Guest Room Energy Management Control (PTAC w/ elec heat)"]
["H4945: Steam Trap Repair, ≥125 psig General Heating, 1/4\" Trap",null,"AG4949: VFD, Irrigation Well Pump, ≥500 hours",null,"N-H4748: Guest Room Energy Management Control (PTHP)"]
["H4946: Steam Trap Repair, ≥125 psig General Heating, 5/16\" Trap",null,"AG3777: VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours",null,"N-H2374: Guest Room Energy Management Control (all other HVAC systems)"]
["H4947: Steam Trap Repair, ≥125 psig General Heating, 3/8\" or Larger Trap",null,"AG3835: VFD, Process Pump, Agriculture, ≥ 1000 hours",null,"N-H2640: Variable Torque VFD, Boiler Draft Fan"]
["H2429: Insulation for Steam Fittings, Natural Gas",null,"AG4414: VFD, Process Pump, Agriculture, 500-999 hours",null,"N-H2646: Variable Torque VFD, Pool Pump Motor"]
["H2430: Insulation for Steam Pipe, Natural Gas",null,"N-AG10209: VFD, Ag Water System, ≥1000 hours",null,"N-H3494: Variable Speed ECM Pump, < 100 Watts Max Input, Domestic Hot Water Recirculation"]
["H2422: Infrared Heater",null,"N-AG10210: VFD, Ag Water System, 500-999 hours",null,"N-H3495: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Domestic Hot Water Recirculation"]
["H5436: Unit Heater, ≥ 90% Thermal Efficiency",null,"N-AG4949: VFD, Irrigation Well Pump, ≥500 hours",null,"N-H3496: Variable Speed ECM Pump, > 500 Watts Max Input, Domestic Hot Water Recirculation"]
["H2699: PTHP <8,000 BTUh, ≥10.7 EER and ≥3.1 COP   (NC =  ≥12.7 EER and ≥3.1 COP)",null,"N-AG3777: VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours",null,"N-H3497: Variable Speed ECM Pump, < 100 Watts Max Input, Heating Water Circulation"]
["H2702: PTHP 8,000-9,999 BTUh, ≥10.4 EER and ≥3.0 COP   (NC =  ≥12.1 EER and ≥3.0 COP)",null,"N-AG3835: VFD, Process Pump, Agriculture, ≥ 1000 hours",null,"N-H3498: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Heating Water Circulation"]
["H2701: PTHP 10,000-12,999 BTUh, ≥9.9 EER and ≥2.9 COP   (NC =  ≥10.9 EER and ≥2.9 COP)",null,"N-AG4414: VFD, Process Pump, Agriculture, 500-999 hours",null,"N-H3499: Variable Speed ECM Pump, > 500 Watts Max Input, Heating Water Circulation"]
["H2700: PTHP ≥13,000 BTUh, ≥9.3 EER and ≥2.9 COP   (NC =  ≥10.3 EER and ≥2.9 COP)",null,"AG3836: VFD, Constant Torque, ≥1000 Annual Hours, Ag",null,"N-H3500: Variable Speed ECM Pump, < 100 Watts Max Input, Cooling Water Circulation"]
["H5081: Direct Fired Make-up Air Unit, Constant Volume",null,"AG4412: VFD, Constant Torque, 500-999 Hours, Ag",null,"N-H3501: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Cooling Water Circulation"]
["H10030: Direct Fired Make-up Air Unit, Variable Air Volume",null,"N-AG3836: VFD, Constant Torque, ≥1000 Annual Hours, Ag",null,"N-H3502: Variable Speed ECM Pump, > 500 Watts Max Input, Cooling Water Circulation"]
["----------------------HVAC CATALOG: COOLING SYSTEMS----------------------------",null,"N-AG4412: VFD, Constant Torque, 500-999 Hours, Ag",null,"N-H3503: Variable Speed ECM Pump, < 100 Watts Max Input, Water Loop Heat Pump Circulation"]
["H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"PS2196: Variable Speed Drive Air Compressor replacing Non-VSD Compressor",null,"N-H3504: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Water Loop Heat Pump Circulation"]
["H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"N-PS2196: Variable Speed Drive Air Compressor replacing Non-VSD Compressor",null,"N-H3505: Variable Speed ECM Pump, > 500 Watts Max Input, Water Loop Heat Pump Circulation"]
["H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"PS2254: No Air-Loss Condensate Drains",null,"-----------------------HVAC CATALOG: BUILDING ENVELOPE ----------------------"]
["H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"PS2257: Compressed Air Heat Recovery",null,"N-B2303: Dock Pit/Ramp External Seal, No Brush Barrier Present"]
["H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"PS3928: Vacuum Pump Heat Recovery",null,"N-B5438: Spring-loaded Overhead Door Hinge"]
["H4368: DX Cooling ≥ 5.42 to < 11.25 tons, Min. Eff. = 16.1 IEER (additional incentive on IEER)",null,"PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer",null,"-----------------------COMMERCIAL REFRIGERATION CATALOG: NON-SELF CONTAINED-----------------------"]
["H4369: DX Cooling ≥ 11.25 to < 20.00 tons, Min. Eff. = 15.4 IEER (additional incentive on IEER)",null,"----------------------AGRIBUSINESS CATALOG: COOLING & SPACE HEATING EQUIPMENT --------------------------------------------",null,"N-R2509: Reach-In Refrigerated Case with Doors replacing Open Multideck Case"]
["H4370: DX Cooling ≥ 20.00 to < 63.33 tons, Min. Eff. = 14.3 IEER (additional incentive on IEER)",null,"H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"N-R3409: Install doors on open Multideck-Style Cases"]
["H4371: DX Cooling ≥ 63.33 tons, Min. Eff. = 9.7 EER and 11.4 IEER (additional incentive on IEER)",null,"H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"N-R2271: Night Curtains for Open Multideck-Style Cases"]
["H10025: Air Source Heat Pump ≥ 5.42 to < 11.25 tons, Min. Eff. = 15.1 IEER (additional incentive on IEER)",null,"H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"-----------------------COMMERCIAL REFRIGERATION CATALOG: CONTROLS-----------------------"]
["H10026: Air Source Heat Pump ≥ 11.25 to < 20.00 tons, Min. Eff. = 14.5 IEER (additional incentive on IEER)",null,"H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"N-R2269: Evaporator Fan Control for Walk-in Cooler/Freezer"]
["H10027: Air Source Heat Pump ≥ 20.00 to < 63.33 tons, Min. Eff. = 13.5 IEER (additional incentive on IEER)",null,"H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons",null,"N-R4759: Evaporator Fan Control Reach-in Cooler/Freezer"]
["H3909: Split System A/C Condensing Unit Only, ≥11.25 tons, ≥ 11.5 EER",null,"H5428: 16 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons",null,"N-R4758: Freezer Demand Defrost"]
["H4712: Air-Cooled Chiller, Path A, < 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.880 kW/ton ",null,"H5429: 17 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons",null,"----------------------PROCESS SYSTEMS CATALOG: COMPRESSED AIR AND VACUUM-------------------------"]
["H4713: Air-Cooled Chiller, Path A, ≥ 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.860 kW/ton ",null,"H5430: 18 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons",null,"N-PS2196: Variable Speed Drive Air Compressors"]
["H4714: Air-Cooled Chiller, Path B, < 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.730 kW/ton ",null,"H5431: 19 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons",null,"N-PS4361: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Variable Torque"]
["H4715: Air-Cooled Chiller, Path B, ≥ 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.720 kW/ton ",null,"H5432: 20 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons",null,"N-PS4362: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Constant Torque"]
["H4716: PD Water-Cooled, Path A, <75 tons, Full Load ≤0.720 kW/ton and IPLV ≤0.600 kW/ton",null,"H2422: Infrared Heater (Retrofit Only)",null,"N-PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer"]
["H4717: PD Water-Cooled, Path A, ≥ 75 tons and < 150 tons, Full Load ≤0.690 kW/ton and IPLV ≤0.560 kW/ton",null,"N-H2422: Infrared Heater (NC Only)",null,"N-PS4363: Dewpoint Demand Controls for Desiccant Dryers"]
["H4718: PD Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.630 kW/ton and IPLV ≤0.540 kW/ton",null,"H2218: Hot Water Boilers, < 300 MBh input, ≥90% AFUE",null,"N-PS5441: Desiccant Compressed Air Dryer, Heated"]
["H4719: PD Water-Cooled, Path A, ≥ 300 tons and < 600 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.520 kW/ton",null,"H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency",null,"N-PS5442: Desiccant Compressed Air Dryer, Blower Purge"]
["H4720: PD Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton",null,"H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency",null,"N-PS5443: Desiccant Compressed Air Dryer, Zero Purge"]
["H4726: Centrifugal Water-Cooled, Path A, <150 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton",null,"N-H2218: Hot Water Boilers, < 300 MBh input, ≥90% AFUE",null,"N-PS2254: No Air-Loss Condensate Drains"]
["H4727: Centrifugal Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton",null,"N-H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency",null,"N-PS2255: Pressure/Flow Controllers"]
["H4728: Centrifugal Water-Cooled, Path A, ≥ 300 tons and < 400 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.520 kW/ton",null,"N-H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency",null,"N-PS2258: Compressed Air Mist Eliminators"]
["H4729: Centrifugal Water-Cooled, Path A, ≥ 400 tons and < 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton",null,"H3491: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG",null,"N-PS5444: Compressed Air Storage, Increase from ≤ 1 Gal/CFM to ≥ 3 Gal/CFM"]
["H4730: Centrifugal Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton",null,"H3492: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG",null,"N-PS2259: Air Entraining Nozzles"]
["H4721: PD Water-Cooled, Path B, <75 tons, Full Load ≤0.780 kW/ton and IPLV ≤0.470 kW/ton",null,"N-H3491: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG",null,"N-PS2257: Compressed Air Heat Recovery"]
["H4722: PD Water-Cooled, Path B, ≥ 75 tons and < 150 tons, Full Load ≤0.750 kW/ton and IPLV ≤0.460 kW/ton",null,"N-H3492: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG",null,"N-PS3928: Vacuum Pump Heat Recovery"]
["H4723: PD Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.680 kW/ton and IPLV ≤0.410 kW/ton",null,"H5436: Unit Heater, ≥90% Thermal Efficiency",null,"----------------------PROCESS SYSTEMS CATALOG: STEAM SYSTEMS-------------------------"]
["H4724: PD Water-Cooled, Path B, ≥ 300 tons and < 600 tons, Full Load ≤0.6250 kW/ton and IPLV ≤0.380 kW/ton",null,"N-H5436: Unit Heater, ≥90% Thermal Efficiency",null,"N-PS5238: High Turndown Burner, New Boiler Replacement"]
["H4725: PD Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton",null,"H5081: Direct Fired Make-up Air Unit, Constant Volume",null,"----------------------PROCESS SYSTEMS CATALOG: VFDs-------------------------"]
["H4731: Centrifugal Water-Cooled, Path B, <150 tons, Full Load ≤0.695 kW/ton and IPLV ≤0.410 kW/ton",null,"N-H5081: Direct Fired Make-up Air Unit, Constant Volume",null,"N-PS2726: Variable Frequency Drives, Variable Torque, CW Distribution Pump"]
["H4732: Centrifugal Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.635 kW/ton and IPLV ≤0.370 kW/ton",null,"H10030: Direct Fired Make-up Air Unit, Variable Air Volume",null,"N-PS2640: Variable Frequency Drives, Variable Torque, Boiler Draft Fan"]
["H4733: Centrifugal Water-Cooled, Path B, ≥ 300 tons and < 400 tons, Full Load ≤0.595 kW/ton and IPLV ≤0.360 kW/ton",null,"N-H10030: Direct Fired Make-up Air Unit, Variable Air Volume",null,"N-PS2641: Variable Frequency Drives, Variable Torque, Cooling Tower Fan"]
["H4734: Centrifugal Water-Cooled, Path B, ≥ 400 tons and < 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton",null,"----------------------AGRIBUSINESS CATALOG: WATER HEATING EQUIPMENT  --------------------------------------------",null,"N-PS2647: Variable Frequency Drives, Variable Torque, Process Fan"]
["H4735: Centrifugal Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585kW/ton and IPLV ≤0.350 kW/ton",null,"AG10032: Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)",null,"N-PS2648: Variable Frequency Drives, Variable Torque, Process Pump"]
["----------------------HVAC CATALOG: VENTILATION AND CONTROLS----------------------------",null,"AG10033: Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)",null,"N-PS3280: Variable Frequency Drives, Constant Torque, All Types"]
["H2314: Energy Recovery Ventilator, Sensible & Latent Heat",null,"N-AG10032: Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)",null,"----------------------PROCESS SYSTEMS CATALOG: DATA CENTER AND TELECOM FACILITIES-------------------------"]
["H5082: Energy Recovery Ventilator, Sensible Heat Only",null,"N-AG10033: Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)",null,"----------------------PROCESS SYSTEMS CATALOG: PROCESS SPECIALTY EQUIPMENT-------------------------"]
["H3910: HVAC Fan with ECM (≤ 1.0 hp), Heating Only",null,"AG4937: Water Heater, Ag, (Natural Gas or Propane)",null,"N-PS2490: Radiant Heater Band"]
["H3911: HVAC Fan with ECM (≤ 1.0 hp), Cooling Only",null,"N-AG4937: Water Heater, Ag, (Natural Gas or Propane)",null,"N-PS2496: Pressure Screen Rotor"]
["H3912: HVAC Fan with ECM (≤ 1.0 hp), Occupied Ventilation",null,"----------------------AG PROPANE CATALOG: SPECIALTY EQUIPMENT --------------------------------------------",null,"N-PS2538: Repulper Rotor without Extraction Plate"]
["H3913: HVAC Fan with ECM (≤ 1.0 hp), 24/7 Ventilation",null,"AG4868: Grain Dryer, Energy Efficient, Propane",null,"N-PS5210: Repulper Rotor with Extraction Plate"]
["H5435: Smart Switched Reluctance Motor, HVAC Supply Fan",null,"----------------------AG PROPANE CATALOG: VFDS AND COMPRESSED AIR --------------------------------------------",null,"N-PS4764: Spline Rotor Upgrade"]
["H3964: Advanced Rooftop Unit Controllers",null,"AG4853: Compressed Air Heat Recovery",null,"N-PS4763: HE Side Entry Agitator"]
["H2853: Demand Controlled Ventilation (DCV) for Multiple Zone RTU/AHU/Unit Ventilator",null,"N-AG4853: Compressed Air Heat Recovery",null,"N-PS4765: Industrial High Frequency Battery Charger"]
["H3266: Demand Controlled Ventilation (DCV) for Single Zone RTU/AHU",null,"PS3928: Vacuum Pump Heat Recovery",null,"N-PS3244: Process Exhaust Filtration"]
["H2373: Guest Room Energy Management Control (PTAC w/ elec heat)",null,"N-PS3928: Vacuum Pump Heat Recovery",null,"----------------------AGRIBUSINESS CATALOG: MILKING EQUIPMENT -----------------------------"]
["H4748: Guest Room Energy Management Control (PTHP)",null,"----------------------AG PROPANE CATALOG: SPACE HEATING EQUIPMENT --------------------------------------------",null,"Eligible Under AgV2: Well Water Plate Heat Exchanger (<135 milking cows)"]
["H2374: Guest Room Energy Management Control (all other HVAC systems)",null,"AG4852: Hot Water Boilers, < 300 MBh input, ≥90% AFUE",null,"Eligible Under AgV2: Well Water Plate Heat Exchanger (≥135 milking cows)"]
["H2640: Variable Torque VFD, Boiler Draft Fan",null,"AG4866: Hot Water Boilers, ≥300 MBh input, ≥90% thermal efficiency",null,"Eligible Under AgV2: Well Water Plate Heat Exchanger (<135 milking cows)"]
["H2641: Variable Torque VFD, Cooling Tower Fan",null,"N-AG4852: Hot Water Boilers, < 300 MBh input, ≥90% AFUE",null,"Eligible Under AgV2: Well Water Plate Heat Exchanger (≥135 milking cows)"]
["H2643: Variable Torque VFD, HVAC Fan",null,"N-AG4866: Hot Water Boilers, ≥300 MBh input, ≥90% thermal efficiency",null,"Eligible Under AgV2: Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)"]
["H2726: Variable Torque VFD, Chilled Water Distribution Pump",null,"AG4854: Infrared Heater (Propane Only)",null,"Eligible Under AgV2: Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)"]
["H2644: Variable Torque VFD, HVAC Heating Pump",null,"N-AG4854: Infrared Heater (Propane Only)",null,"Eligible Under AgV2: Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)"]
["H2646: Variable Torque VFD, Pool Pump Motor",null,"AG4870: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane",null,"Eligible Under AgV2: Variable Speed Control Vacuum Pump, < 500 milking cows (Dairy Farm, Parlor, Milk House)"]
["H3494: Variable Speed ECM Pump, < 100 Watts Max Input, Domestic Hot Water Recirculation",null,"AG4869: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane",null,"Eligible Under AgV2: Variable Speed Control Vacuum Pump, 500 - 2000 milking cows (Dairy Farm, Parlor, Milk House)"]
["H3495: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Domestic Hot Water Recirculation",null,"N-AG4870: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane",null,"Eligible Under AgV2: Variable Speed Control Milk Pump (Dairy Farm, Parlor, Milk House)"]
["H3496: Variable Speed ECM Pump, > 500 Watts Max Input, Domestic Hot Water Recirculation",null,"N-AG4869: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane",null,"----------------------AGRIBUSINESS CATALOG: OTHER SPECIALTY EQUIPMENT -----------------------------"]
["H3497: Variable Speed ECM Pump, < 100 Watts Max Input, Heating Water Circulation",null,"AG5437: Unit Heater, ≥ 90% Thermal Efficiency ",null,"Eligible Under AgV2: Zero-Energy Livestock Waterer"]
["H3498: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Heating Water Circulation",null,"N-AG5437: Unit Heater, ≥ 90% Thermal Efficiency ",null,"Eligible Under AgV2: Zero-Energy Livestock Waterer"]
["H3499: Variable Speed ECM Pump, > 500 Watts Max Input, Heating Water Circulation",null,"AG5407: Direct Fired Make-up Air Unit, Constant Volume",null,"Eligible Under AgV2: Swine Farrowing Crate Heater, Single"]
["H3500: Variable Speed ECM Pump, < 100 Watts Max Input, Cooling Water Circulation",null,"N-AG5407: Direct Fired Make-up Air Unit, Constant Volume",null,"Eligible Under AgV2: Swine Farrowing Crate Heater, Double"]
["H3501: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Cooling Water Circulation",null,"AG10031: Direct Fired Make-up Air Unit, Variable Air Volume",null,"Eligible Under AgV2: Swine Farrowing Crate Heater, Single"]
["H3502: Variable Speed ECM Pump, > 500 Watts Max Input, Cooling Water Circulation",null,"N-AG10031: Direct Fired Make-up Air Unit, Variable Air Volume",null,"Eligible Under AgV2: Swine Farrowing Crate Heater, Double"]
["H3503: Variable Speed ECM Pump, < 100 Watts Max Input, Water Loop Heat Pump Circulation",null,"----------------------AG PROPANE CATALOG: WATER HEATING EQUIPMENT --------------------------------------------",null,"Eligible Under AgV2: VFD, Irrigation Well Pump (≥500 Annual Operating Hours)"]
["H3504: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Water Loop Heat Pump Circulation",null,"AG10034: RHR Unit (Propane Water Heater)",null,"Eligible Under AgV2: VFD, Irrigation Well Pump (≥500 Annual Operating Hours)"]
["H3505: Variable Speed ECM Pump, > 500 Watts Max Input, Water Loop Heat Pump Circulation",null,"N-AG10034: RHR Unit (Propane Water Heater)",null,"----------------------AGRIBUSINESS CATALOG: LIGHTING --------------------------------------------"]
["-----------------------HVAC CATALOG: BUILDING ENVELOPE ----------------------",null,"AG4938: Propane Commercial Water Heater",null,"N-L5459: 1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer"]
["B2300: Dock Door Infiltration Reduction, New Install",null,"N-AG4938: Propane Commercial Water Heater",null,"N-L3111: 2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer"]
["B2301: Dock Door Infiltration Reduction, Replace Existing",null,"-------------------------------SPECIAL OFFERS AG-------------------------------",null,"N-L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["B2302: Dock Pit/Ramp External Seal, Added to Existing \"Brush\" Barrier",null,"AG4403: Refrigeration System Tune-Up, Agriculture",null,"N-L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["B2303: Dock Pit/Ramp External Seal, No Brush Barrier Present",null,"5564: Grain Dryer, Tune-up",null,"N-L10028: LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture"]
["B5438: Spring-loaded Overhead Door Hinge",null,"5565: Grain Dryer, Tune-up, Propane-Fueled",null,"N-L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["B10219: Roof Insulation, Existing Insulation <R-20",null,"5190: Pump Assessment",null,"N-L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior"]
["B10220: Roof Insulation, Existing Insulation ≥R-20",null,"5202: Bonus, VSD after Pump Assessment",null,"N-L10282: 4' LED Linear Ambient Fixture, Interior"]
["-----------------------COMMERCIAL REFRIGERATION CATALOG: NON-SELF CONTAINED-----------------------",null,"----------------------LIGHTING CATALOG: LED FIXTURES----------------------------",null,"N-L10283: 8' LED Linear Ambient Fixture, Interior"]
["R2308: ECM Evaporator Fan Motor, Walk-in Cooler, < 1/20 HP",null,"L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer",null,"N-L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior"]
["R2309: ECM Evaporator Fan Motor, Walk-in Cooler, 1/20 - 1 HP",null,"L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer",null,"N-L10285: 4' LED Linear Ambient Fixture, Exterior"]
["R2310: ECM Evaporator Fan Motor, Walk-in Freezer, < 1/20 HP",null,"L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps",null,"N-L10286: 8' LED Linear Ambient Fixture, Exterior"]
["R2311: ECM Evaporator Fan Motor, Walk-in Freezer, 1/20 - 1 HP",null,"L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps",null,"N-AG4695: LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture"]
["R2312: ECM Evaporator Fan Motor, Cooler/Freezer Case",null,"L10214: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer, w/LLLC",null,"N-AG4696: LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture"]
["R4284: PMS Evaporator Fan Motor, Cooler/Freezer Case",null,"L10213: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer, w/LLLC",null,"N-AG4701: LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture"]
["R2306: ECM Compressor Head Fan Motor",null,"L10211: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps, w/LLLC",null,"N-AG4702: LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture"]
["R2307: ECM Condenser / Condensing Unit Fan Motor",null,"L10212: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps, w/LLLC",null,"N-L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["R2509: Reach-In Refrigerated Case with Doors replacing Open Multideck Case",null,"L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior",null,"N-L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["R3409: Install doors on open Multideck-Style Cases",null,"L10282: 4' LED Linear Ambient Fixture, Interior",null,"N-L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["R2236: Case Door,Cooler,No-Heat",null,"L10283: 8' LED Linear Ambient Fixture, Interior",null,"N-L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["R2234: Case Door,Freezer,Low-Heat",null,"L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior",null,"N-AG5032: Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture"]
["R2235: Case Door,Freezer,No-Heat",null,"L10285: 4' LED Linear Ambient Fixture, Exterior",null,"N-AG5033: Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture"]
["R3114: LED, Horizontal Case Lighting, replacing Linear Fluorescent",null,"L10286: 8' LED Linear Ambient Fixture, Exterior",null,"----------------------AGRIBUSINESS CATALOG: VENTILATION  --------------------------------------------"]
["R2456: LED, Vertical Case Lighting, replacing Linear Fluorescent",null,"L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture",null,"Eligible Under AgV2: Fans, High Volume Low Speed (HVLS)"]
["R2271: Night Curtains for Open Multideck-Style Cases",null,"L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior",null,"Eligible Under AgV2: Ventilation/Exhaust Fan, Dairy, ≥ 48” with Variable Speed"]
["R3183: Strip Curtain for Walk-In Freezers and Coolers",null,"L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture",null,"Eligible Under AgV2: Ventilation/Exhaust Fan, Other (non-dairy), ≥ 48” with Variable Speed"]
["-----------------------COMMERCIAL REFRIGERATION CATALOG: CONTROLS-----------------------",null,"L3903: Interior LED Signage",null,"Eligible Under AgV2: Circulation Fan, Dairy, 36-47” (20.0 lbf/kW)"]
["R5439: Anti-Sweat Heater Controls, Freezer Case",null,"L3904: Exterior LED Signage",null,"Eligible Under AgV2: Circulation Fan, Dairy, ≥ 48” (24.5 lbf/kW)"]
["R5440: Anti-Sweat Heater Controls, Refrigerated Case",null,"L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID",null,"Eligible Under AgV2: Circulation Fan, Other (non-dairy), 24-35” (15.8 lbf/kW)"]
["R2269: Evaporator Fan Control for Walk-in Cooler/Freezer",null,"L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID",null,"Eligible Under AgV2: Circulation Fan, Other (non-dairy), 36-47” (20.0 lbf/kW)"]
["R4759: Evaporator Fan Control Reach-in Cooler/Freezer",null,"L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID",null,"Eligible Under AgV2: Circulation Fan, Other (non-dairy), ≥ 48” (24.5 lbf/kW)"]
["R4758: Freezer Demand Defrost",null,"L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID",null,"----------------------AGRIBUSINESS CATALOG: VFD & COMPRESSED AIR  --------------------------------------------"]
["R4360: Refrigeration Controls, Floating Head Pressure",null,"L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID",null,"Eligible Under AgV2: VFD, Ag Water System, ≥1000 hours"]
["----------------------PROCESS SYSTEMS CATALOG: COMPRESSED AIR AND VACUUM-------------------------",null,"L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID",null,"Eligible Under AgV2: VFD, Ag Water System, 500-999 hours"]
["PS4766: Compressed Air Leak Survey and Repair",null,"L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12",null,"Eligible Under AgV2: VFD, Ventilation/Circulation Fan, Ag, ≥1000 hours"]
["PS2196: Variable Speed Drive Air Compressors",null,"L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO",null,"Eligible Under AgV2: VFD, Process Pump, Agriculture, ≥ 1000 hours"]
["PS4361: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Variable Torque",null,"L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO",null,"Eligible Under AgV2: VFD, Process Pump, Agriculture, 500-999 hours"]
["PS4362: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Constant Torque",null,"L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO",null,"Eligible Under AgV2: VFD, Constant Torque, ≥1000 Annual Hours, Ag"]
["PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer",null,"L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO",null,"Eligible Under AgV2: VFD, Constant Torque, 500-999 Hours, Ag"]
["PS4363: Dewpoint Demand Controls for Desiccant Dryers",null,"L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO",null,"Eligible Under AgV2: Variable Speed Drive Air Compressor replacing Non-VSD Compressor"]
["PS5441: Desiccant Compressed Air Dryer, Heated",null,"L10215: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID, w/LLLC",null,"N-PS2254: No Air-Loss Condensate Drains"]
["PS5442: Desiccant Compressed Air Dryer, Blower Purge",null,"L10216: ≤ 250W LED High Bay/Low Bay, replacing 400W HID, w/LLLC",null,"N-PS2257: Compressed Air Heat Recovery"]
["PS5443: Desiccant Compressed Air Dryer, Zero Purge",null,"L10217: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO, w/LLLC",null,"N-PS3928: Vacuum Pump Heat Recovery"]
["PS2254: No Air-Loss Condensate Drains",null,"L10218: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO, w/LLLC",null,"N-PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer"]
["PS2255: Pressure/Flow Controllers",null,"L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",null,"----------------------AGRIBUSINESS CATALOG: COOLING & SPACE HEATING EQUIPMENT --------------------------------------------"]
["PS2258: Compressed Air Mist Eliminators",null,"L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",null,"N-H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["PS5444: Compressed Air Storage, Increase from ≤ 1 Gal/CFM to ≥ 3 Gal/CFM",null,"L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",null,"N-H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["PS2259: Air Entraining Nozzles",null,"L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",null,"N-H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["PS2257: Compressed Air Heat Recovery",null,"----------------------LIGHTING CATALOG: LED LAMPS----------------------------",null,"N-H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["PS3928: Vacuum Pump Heat Recovery",null,"L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID",null,"N-H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons"]
["PS2848: Compressed Air Process Load Shifting",null,"L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior",null,"N-H5428: 16 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons"]
["----------------------PROCESS SYSTEMS CATALOG: STEAM SYSTEMS-------------------------",null,"L10039: Four-pin base LED Lamp Replacing CFL",null,"N-H5429: 17 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons"]
["PS4041: Steam Trap Survey (Process)",null,"L10040: Four-pin base LED Lamp Replacing CFL, Exterior",null,"N-H5430: 18 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons"]
["PS3999: Steam Trap Repair/Replacement, Industrial, < 10 psig",null,"L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp",null,"N-H5431: 19 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons"]
["PS4000: Steam Trap Repair/Replacement, Industrial, 10-49 psig",null,"L5452: 4' TLED, replacing 4' T5HO Lamp",null,"N-H5432: 20 SEER2 and 8.5 HSPF2 A/C Split System or Single Package, < 5.42 tons"]
["PS4001: Steam Trap Repair/Replacement, Industrial, 50-124 psig",null,"L4797: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp",null,"Eligible Under AgV2: Infrared Heater (NC Only)"]
["PS4002: Steam Trap Repair/Replacement, Industrial, 125-225 psig",null,"L4809: 8' TLED, replacing 8' T8 or T12 Lamp",null,"Eligible Under AgV2: Hot Water Boilers, < 300 MBh input, ≥90% AFUE"]
["PS4003: Steam Trap Repair/Replacement, Industrial, > 225 psig",null,"L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior",null,"Eligible Under AgV3: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency"]
["PS4761: Process Boiler Combustion Upgrades, Linkageless Controls",null,"L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior",null,"Eligible Under AgV4: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency"]
["PS4762: Process Boiler Combustion Upgrades, O2 Trim Controls",null,"----------------------LIGHTING CATALOG: CONTROLS----------------------------",null,"Eligible Under AgV2: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, NG"]
["PS4760: Process Boiler Combustion Upgrades, High Turndown Burner, Retrofit on Existing Boiler",null,"L10223: Advanced Lighting Controls, Interior",null,"Eligible Under AgV2: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, NG"]
["PS5238: High Turndown Burner, New Boiler Replacement",null,"L10224: Advanced Lighting Controls, Exterior",null,"Eligible Under AgV2: Unit Heater, ≥90% Thermal Efficiency"]
["----------------------PROCESS SYSTEMS CATALOG: VFDs-------------------------",null,"L3406: Daylighting Controls",null,"Eligible Under AgV2: Direct Fired Make-up Air Unit, Constant Volume"]
["PS2726: Variable Frequency Drives, Variable Torque, CW Distribution Pump",null,"L5061: High and Low Bay On/Off Occupancy Sensor Control",null,"Eligible Under AgV2: Direct Fired Make-up Air Unit, Variable Air Volume"]
["PS2640: Variable Frequency Drives, Variable Torque, Boiler Draft Fan",null,"L5062: High and Low Bay Bi-Level Occupancy Control",null,"----------------------AGRIBUSINESS CATALOG: WATER HEATING EQUIPMENT  --------------------------------------------"]
["PS2641: Variable Frequency Drives, Variable Torque, Cooling Tower Fan",null,"L4812: Non-High Bay Occupancy/Vacancy Sensor",null,"Eligible Under AgV2: Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)"]
["PS2647: Variable Frequency Drives, Variable Torque, Process Fan",null,"L5063: Bi-Level Controls, Parking Garage Lighting, Dusk to Dawn",null,"Eligible Under AgV2: Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)"]
["PS2648: Variable Frequency Drives, Variable Torque, Process Pump",null,"L5064: Bi-Level Controls, Parking Garage Lighting, 24 Hour",null,"Eligible Under AgV2: Refrigeration Heat Recovery/RHR Unit (NG Wtr Htr)"]
["PS3280: Variable Frequency Drives, Constant Torque, All Types",null,"----------------------LIGHTING CATALOG: OTHER LIGHTING SOLUTIONS----------------------------",null,"Eligible Under AgV2: Refrigeration Heat Recovery/RHR Unit (Elec. Wtr Htr)"]
["----------------------PROCESS SYSTEMS CATALOG: DATA CENTER AND TELECOM FACILITIES-------------------------",null,"R5235: Refrigeration Savings for Lighting Upgrades in Freezers",null,"Eligible Under AgV2: Water Heater, Ag, (Natural Gas or Propane)"]
["PS4776: Air Side Economizer, Data Center/Telecom",null,"R5236: Refrigeration Savings for Lighting Upgrades in Coolers",null,"Eligible Under AgV2: Water Heater, Ag, (Natural Gas or Propane)"]
["PS2305: Energy-Efficient Drycooler, Data Center/Telecom",null,"L10289: Fixture Elimination, Interior",null,"----------------------AG PROPANE CATALOG: SPECIALTY EQUIPMENT --------------------------------------------"]
["PS4777: Efficient UPS",null,"L10287: General Wattage Reduction, Interior",null,"----------------------AG PROPANE CATALOG: VFDS AND COMPRESSED AIR --------------------------------------------"]
["PS4778: Efficient Rectifier",null,"L10290: Fixture Elimination, Exterior",null,"Eligible Under Ag Propane: Compressed Air Heat Recovery"]
["----------------------PROCESS SYSTEMS CATALOG: PROCESS SPECIALTY EQUIPMENT-------------------------",null,"L10288: General Wattage Reduction, Exterior",null,"Eligible Under Ag Propane: Vacuum Pump Heat Recovery"]
["PS2490: Radiant Heater Band",null,"----------------------HVAC CATALOG: HEATING SYSTEMS----------------------------",null,"----------------------AG PROPANE CATALOG: SPACE HEATING EQUIPMENT --------------------------------------------"]
["PS2496: Pressure Screen Rotor",null,"H10222: Hot Water Boilers, ≥300 MBh input, 90%-94% thermal efficiency",null,"Eligible Under Ag Propane: Hot Water Boilers, < 300 MBh input, ≥90% AFUE"]
["PS2538: Repulper Rotor without Extraction Plate",null,"H10207: Hot Water Boilers, ≥300 MBh input, ≥95% thermal efficiency",null,"Eligible Under Ag Propane: Hot Water Boilers, ≥300 MBh input, ≥90% thermal efficiency"]
["PS5210: Repulper Rotor with Extraction Plate",null,"H2221: Outdoor Air Reset/Cutout Controls",null,"Eligible Under Ag Propane: Infrared Heater (Propane Only)"]
["PS4764: Spline Rotor Upgrade",null,"H2205: Linkageless Controls, HVAC Boilers",null,"Eligible Under Ag Propane: Furnace with ECM, ≥90%+ AFUE, 2 stages of heat, Propane"]
["PS4763: HE Side Entry Agitator",null,"H2206: O₂ Trim Controls, HVAC Boilers",null,"Eligible Under Ag Propane: Furnace with ECM, ≥95%+ AFUE, 2 stages of heat, Propane"]
["PS4765: Industrial High Frequency Battery Charger",null,"H2203: High Turndown Burner, Retrofit on Existing Boiler",null,"Eligible Under AgV2: Direct Fired Make-up Air Unit, Constant Volume"]
["PS3244: Process Exhaust Filtration",null,"H5237: High Turndown Burner, New Boiler Replacement",null,"Eligible Under AgV2: Direct Fired Make-up Air Unit, Variable Air Volume"]
[null,null,"H2225: Steam Trap Survey (HVAC)",null,"----------------------AG PROPANE CATALOG: WATER HEATING EQUIPMENT --------------------------------------------"]
[null,null,"H4004: Steam Trap Repair, <10 psig General Heating, 7/32\" or Smaller Trap",null,"Eligible Under Ag Propane: RHR Unit (Propane Water Heater)"]
[null,null,"H4005: Steam Trap Repair, <10 psig General Heating, 1/4\" Trap",null,"Eligible Under Ag Propane: Propane Commercial Water Heater"]
[null,null,"H4006: Steam Trap Repair, <10 psig General Heating, 5/16\" Trap",null,"-------------------------------SPECIAL OFFERS AG-------------------------------"]
[null,null,"H4007: Steam Trap Repair, <10 psig General Heating, 3/8\" or Larger Trap"]
[null,null,"H4008: Steam Trap Repair, 10-49 psig General Heating, 7/32\" or Smaller Trap"]
[null,null,"H4009: Steam Trap Repair, 10-49 psig General Heating, 1/4\" Trap"]
[null,null,"H4010: Steam Trap Repair, 10-49 psig General Heating, 5/16\" Trap"]
[null,null,"H4011: Steam Trap Repair, 10-49 psig General Heating, 3/8\" or Larger Trap"]
[null,null,"H4012: Steam Trap Repair, 50-124 psig General Heating, 7/32\" or Smaller Trap"]
[null,null,"H4013: Steam Trap Repair, 50-124 psig General Heating, 1/4\" Trap"]
[null,null,"H4014: Steam Trap Repair, 50-124 psig General Heating, 5/16\" Trap"]
[null,null,"H4015: Steam Trap Repair, 50-124 psig General Heating, 3/8\" or Larger Trap"]
[null,null,"H4944: Steam Trap Repair, ≥125 psig General Heating, 7/32\" or Smaller Trap"]
[null,null,"H4945: Steam Trap Repair, ≥125 psig General Heating, 1/4\" Trap"]
[null,null,"H4946: Steam Trap Repair, ≥125 psig General Heating, 5/16\" Trap"]
[null,null,"H4947: Steam Trap Repair, ≥125 psig General Heating, 3/8\" or Larger Trap"]
[null,null,"H2429: Insulation for Steam Fittings, Natural Gas"]
[null,null,"H2430: Insulation for Steam Pipe, Natural Gas"]
[null,null,"H2422: Infrared Heater"]
[null,null,"H5436: Unit Heater, ≥ 90% Thermal Efficiency"]
[null,null,"H2699: PTHP <8,000 BTUh, ≥10.7 EER and ≥3.1 COP   (NC =  ≥12.7 EER and ≥3.1 COP)"]
[null,null,"H2702: PTHP 8,000-9,999 BTUh, ≥10.4 EER and ≥3.0 COP   (NC =  ≥12.1 EER and ≥3.0 COP)"]
[null,null,"H2701: PTHP 10,000-12,999 BTUh, ≥9.9 EER and ≥2.9 COP   (NC =  ≥10.9 EER and ≥2.9 COP)"]
[null,null,"H2700: PTHP ≥13,000 BTUh, ≥9.3 EER and ≥2.9 COP   (NC =  ≥10.3 EER and ≥2.9 COP)"]
[null,null,"H5081: Direct Fired Make-up Air Unit, Constant Volume"]
[null,null,"H10030: Direct Fired Make-up Air Unit, Variable Air Volume"]
[null,null,"----------------------HVAC CATALOG: COOLING SYSTEMS----------------------------"]
[null,null,"H5423: 16 SEER2 A/C Split System or Single Package, < 5.42 tons"]
[null,null,"H5424: 17 SEER2 A/C Split System or Single Package, < 5.42 tons"]
[null,null,"H5425: 18 SEER2 A/C Split System or Single Package, < 5.42 tons"]
[null,null,"H5426: 19 SEER2 A/C Split System or Single Package, < 5.42 tons"]
[null,null,"H5427: 20 SEER2 A/C Split System or Single Package, < 5.42 tons"]
[null,null,"H4368: DX Cooling ≥ 5.42 to < 11.25 tons, Min. Eff. = 16.1 IEER (additional incentive on IEER)"]
[null,null,"H4369: DX Cooling ≥ 11.25 to < 20.00 tons, Min. Eff. = 15.4 IEER (additional incentive on IEER)"]
[null,null,"H4370: DX Cooling ≥ 20.00 to < 63.33 tons, Min. Eff. = 14.3 IEER (additional incentive on IEER)"]
[null,null,"H4371: DX Cooling ≥ 63.33 tons, Min. Eff. = 9.7 EER and 11.4 IEER (additional incentive on IEER)"]
[null,null,"H10025: Air Source Heat Pump ≥ 5.42 to < 11.25 tons, Min. Eff. = 15.1 IEER (additional incentive on IEER)"]
[null,null,"H10026: Air Source Heat Pump ≥ 11.25 to < 20.00 tons, Min. Eff. = 14.5 IEER (additional incentive on IEER)"]
[null,null,"H10027: Air Source Heat Pump ≥ 20.00 to < 63.33 tons, Min. Eff. = 13.5 IEER (additional incentive on IEER)"]
[null,null,"H3909: Split System A/C Condensing Unit Only, ≥11.25 tons, ≥ 11.5 EER"]
[null,null,"H4712: Air-Cooled Chiller, Path A, < 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.880 kW/ton "]
[null,null,"H4713: Air-Cooled Chiller, Path A, ≥ 150 tons, Full Load ≤1.160 kW/ton, Part Load ≤0.860 kW/ton "]
[null,null,"H4714: Air-Cooled Chiller, Path B, < 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.730 kW/ton "]
[null,null,"H4715: Air-Cooled Chiller, Path B, ≥ 150 tons, Full Load ≤1.240 kW/ton, Part Load ≤0.720 kW/ton "]
[null,null,"H4716: PD Water-Cooled, Path A, <75 tons, Full Load ≤0.720 kW/ton and IPLV ≤0.600 kW/ton"]
[null,null,"H4717: PD Water-Cooled, Path A, ≥ 75 tons and < 150 tons, Full Load ≤0.690 kW/ton and IPLV ≤0.560 kW/ton"]
[null,null,"H4718: PD Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.630 kW/ton and IPLV ≤0.540 kW/ton"]
[null,null,"H4719: PD Water-Cooled, Path A, ≥ 300 tons and < 600 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.520 kW/ton"]
[null,null,"H4720: PD Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton"]
[null,null,"H4726: Centrifugal Water-Cooled, Path A, <150 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton"]
[null,null,"H4727: Centrifugal Water-Cooled, Path A, ≥ 150 tons and < 300 tons, Full Load ≤0.580 kW/ton and IPLV ≤0.550 kW/ton"]
[null,null,"H4728: Centrifugal Water-Cooled, Path A, ≥ 300 tons and < 400 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.520 kW/ton"]
[null,null,"H4729: Centrifugal Water-Cooled, Path A, ≥ 400 tons and < 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton"]
[null,null,"H4730: Centrifugal Water-Cooled, Path A, ≥ 600 tons, Full Load ≤0.530 kW/ton and IPLV ≤0.500 kW/ton"]
[null,null,"H4721: PD Water-Cooled, Path B, <75 tons, Full Load ≤0.780 kW/ton and IPLV ≤0.470 kW/ton"]
[null,null,"H4722: PD Water-Cooled, Path B, ≥ 75 tons and < 150 tons, Full Load ≤0.750 kW/ton and IPLV ≤0.460 kW/ton"]
[null,null,"H4723: PD Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.680 kW/ton and IPLV ≤0.410 kW/ton"]
[null,null,"H4724: PD Water-Cooled, Path B, ≥ 300 tons and < 600 tons, Full Load ≤0.6250 kW/ton and IPLV ≤0.380 kW/ton"]
[null,null,"H4725: PD Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton"]
[null,null,"H4731: Centrifugal Water-Cooled, Path B, <150 tons, Full Load ≤0.695 kW/ton and IPLV ≤0.410 kW/ton"]
[null,null,"H4732: Centrifugal Water-Cooled, Path B, ≥ 150 tons and < 300 tons, Full Load ≤0.635 kW/ton and IPLV ≤0.370 kW/ton"]
[null,null,"H4733: Centrifugal Water-Cooled, Path B, ≥ 300 tons and < 400 tons, Full Load ≤0.595 kW/ton and IPLV ≤0.360 kW/ton"]
[null,null,"H4734: Centrifugal Water-Cooled, Path B, ≥ 400 tons and < 600 tons, Full Load ≤0.585 kW/ton and IPLV ≤0.350 kW/ton"]
[null,null,"H4735: Centrifugal Water-Cooled, Path B, ≥ 600 tons, Full Load ≤0.585kW/ton and IPLV ≤0.350 kW/ton"]
[null,null,"----------------------HVAC CATALOG: VENTILATION AND CONTROLS----------------------------"]
[null,null,"H2314: Energy Recovery Ventilator, Sensible & Latent Heat"]
[null,null,"H5082: Energy Recovery Ventilator, Sensible Heat Only"]
[null,null,"H3910: HVAC Fan with ECM (≤ 1.0 hp), Heating Only"]
[null,null,"H3911: HVAC Fan with ECM (≤ 1.0 hp), Cooling Only"]
[null,null,"H3912: HVAC Fan with ECM (≤ 1.0 hp), Occupied Ventilation"]
[null,null,"H3913: HVAC Fan with ECM (≤ 1.0 hp), 24/7 Ventilation"]
[null,null,"H5435: Smart Switched Reluctance Motor, HVAC Supply Fan"]
[null,null,"H3964: Advanced Rooftop Unit Controllers"]
[null,null,"H2853: Demand Controlled Ventilation (DCV) for Multiple Zone RTU/AHU/Unit Ventilator"]
[null,null,"H3266: Demand Controlled Ventilation (DCV) for Single Zone RTU/AHU"]
[null,null,"H2373: Guest Room Energy Management Control (PTAC w/ elec heat)"]
[null,null,"H4748: Guest Room Energy Management Control (PTHP)"]
[null,null,"H2374: Guest Room Energy Management Control (all other HVAC systems)"]
[null,null,"H2640: Variable Torque VFD, Boiler Draft Fan"]
[null,null,"H2641: Variable Torque VFD, Cooling Tower Fan"]
[null,null,"H2643: Variable Torque VFD, HVAC Fan"]
[null,null,"H2726: Variable Torque VFD, Chilled Water Distribution Pump"]
[null,null,"H2644: Variable Torque VFD, HVAC Heating Pump"]
[null,null,"H2646: Variable Torque VFD, Pool Pump Motor"]
[null,null,"H3494: Variable Speed ECM Pump, < 100 Watts Max Input, Domestic Hot Water Recirculation"]
[null,null,"H3495: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Domestic Hot Water Recirculation"]
[null,null,"H3496: Variable Speed ECM Pump, > 500 Watts Max Input, Domestic Hot Water Recirculation"]
[null,null,"H3497: Variable Speed ECM Pump, < 100 Watts Max Input, Heating Water Circulation"]
[": ",null,"H3498: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Heating Water Circulation"]
[null,null,"H3499: Variable Speed ECM Pump, > 500 Watts Max Input, Heating Water Circulation"]
[null,null,"H3500: Variable Speed ECM Pump, < 100 Watts Max Input, Cooling Water Circulation"]
[null,null,"H3501: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Cooling Water Circulation"]
[null,null,"H3502: Variable Speed ECM Pump, > 500 Watts Max Input, Cooling Water Circulation"]
[null,null,"H3503: Variable Speed ECM Pump, < 100 Watts Max Input, Water Loop Heat Pump Circulation"]
[null,null,"H3504: Variable Speed ECM Pump, 100 - 500 Watts Max Input, Water Loop Heat Pump Circulation"]
[null,null,"H3505: Variable Speed ECM Pump, > 500 Watts Max Input, Water Loop Heat Pump Circulation"]
[null,null,"-----------------------HVAC CATALOG: BUILDING ENVELOPE ----------------------"]
[null,null,"B2300: Dock Door Infiltration Reduction, New Install"]
[null,null,"B2301: Dock Door Infiltration Reduction, Replace Existing"]
[null,null,"B2302: Dock Pit/Ramp External Seal, Added to Existing \"Brush\" Barrier"]
[null,null,"B2303: Dock Pit/Ramp External Seal, No Brush Barrier Present"]
[null,null,"B5438: Spring-loaded Overhead Door Hinge"]
[null,null,"B10219: Roof Insulation, Existing Insulation <R-20"]
[null,null,"B10220: Roof Insulation, Existing Insulation ≥R-20"]
[null,null,"-----------------------COMMERCIAL REFRIGERATION CATALOG: NON-SELF CONTAINED-----------------------"]
[null,null,"R2308: ECM Evaporator Fan Motor, Walk-in Cooler, < 1/20 HP"]
[null,null,"R2309: ECM Evaporator Fan Motor, Walk-in Cooler, 1/20 - 1 HP"]
[null,null,"R2310: ECM Evaporator Fan Motor, Walk-in Freezer, < 1/20 HP"]
[null,null,"R2311: ECM Evaporator Fan Motor, Walk-in Freezer, 1/20 - 1 HP"]
[null,null,"R2312: ECM Evaporator Fan Motor, Cooler/Freezer Case"]
[null,null,"R4284: PMS Evaporator Fan Motor, Cooler/Freezer Case"]
[null,null,"R2306: ECM Compressor Head Fan Motor"]
[null,null,"R2307: ECM Condenser / Condensing Unit Fan Motor"]
[null,null,"R2509: Reach-In Refrigerated Case with Doors replacing Open Multideck Case"]
[null,null,"R3409: Install doors on open Multideck-Style Cases"]
[null,null,"R2236: Case Door,Cooler,No-Heat"]
[null,null,"R2234: Case Door,Freezer,Low-Heat"]
[null,null,"R2235: Case Door,Freezer,No-Heat"]
[null,null,"R3114: LED, Horizontal Case Lighting, replacing Linear Fluorescent"]
[null,null,"R2456: LED, Vertical Case Lighting, replacing Linear Fluorescent"]
[null,null,"R2271: Night Curtains for Open Multideck-Style Cases"]
[null,null,"R3183: Strip Curtain for Walk-In Freezers and Coolers"]
[null,null,"-----------------------COMMERCIAL REFRIGERATION CATALOG: CONTROLS-----------------------"]
[null,null,"R5439: Anti-Sweat Heater Controls, Freezer Case"]
[null,null,"R5440: Anti-Sweat Heater Controls, Refrigerated Case"]
[null,null,"R2269: Evaporator Fan Control for Walk-in Cooler/Freezer"]
[null,null,"R4759: Evaporator Fan Control Reach-in Cooler/Freezer"]
[null,null,"R4758: Freezer Demand Defrost"]
[null,null,"R4360: Refrigeration Controls, Floating Head Pressure"]
[null,null,"----------------------PROCESS SYSTEMS CATALOG: COMPRESSED AIR AND VACUUM-------------------------"]
[null,null,"PS4766: Compressed Air Leak Survey and Repair"]
[null,null,"PS2196: Variable Speed Drive Air Compressors"]
[null,null,"PS4361: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Variable Torque"]
[null,null,"PS4362: Variable Speed Drive Vacuum Pump, ≤ 30 hp, Constant Torque"]
[null,null,"PS2264: Cycling or VFD-Controlled Refrigerated Air Dryer"]
[null,null,"PS4363: Dewpoint Demand Controls for Desiccant Dryers"]
[null,null,"PS5441: Desiccant Compressed Air Dryer, Heated"]
[null,null,"PS5442: Desiccant Compressed Air Dryer, Blower Purge"]
[null,null,"PS5443: Desiccant Compressed Air Dryer, Zero Purge"]
[null,null,"PS2254: No Air-Loss Condensate Drains"]
[null,null,"PS2255: Pressure/Flow Controllers"]
[null,null,"PS2258: Compressed Air Mist Eliminators"]
[null,null,"PS5444: Compressed Air Storage, Increase from ≤ 1 Gal/CFM to ≥ 3 Gal/CFM"]
[null,null,"PS2259: Air Entraining Nozzles"]
[null,null,"PS2257: Compressed Air Heat Recovery"]
[null,null,"PS3928: Vacuum Pump Heat Recovery"]
[null,null,"PS2848: Compressed Air Process Load Shifting"]
[null,null,"----------------------PROCESS SYSTEMS CATALOG: STEAM SYSTEMS-------------------------"]
[null,null,"PS4041: Steam Trap Survey (Process)"]
[null,null,"PS3999: Steam Trap Repair/Replacement, Industrial, < 10 psig"]
[null,null,"PS4000: Steam Trap Repair/Replacement, Industrial, 10-49 psig"]
[null,null,"PS4001: Steam Trap Repair/Replacement, Industrial, 50-124 psig"]
[null,null,"PS4002: Steam Trap Repair/Replacement, Industrial, 125-225 psig"]
[null,null,"PS4003: Steam Trap Repair/Replacement, Industrial, > 225 psig"]
[null,null,"PS4761: Process Boiler Combustion Upgrades, Linkageless Controls"]
[null,null,"PS4762: Process Boiler Combustion Upgrades, O2 Trim Controls"]
[null,null,"PS4760: Process Boiler Combustion Upgrades, High Turndown Burner, Retrofit on Existing Boiler"]
[null,null,"PS5238: High Turndown Burner, New Boiler Replacement"]
[null,null,"----------------------PROCESS SYSTEMS CATALOG: VFDs-------------------------"]
[null,null,"PS2726: Variable Frequency Drives, Variable Torque, CW Distribution Pump"]
[null,null,"PS2640: Variable Frequency Drives, Variable Torque, Boiler Draft Fan"]
[null,null,"PS2641: Variable Frequency Drives, Variable Torque, Cooling Tower Fan"]
[null,null,"PS2647: Variable Frequency Drives, Variable Torque, Process Fan"]
[null,null,"PS2648: Variable Frequency Drives, Variable Torque, Process Pump"]
[null,null,"PS3280: Variable Frequency Drives, Constant Torque, All Types"]
[null,null,"----------------------PROCESS SYSTEMS CATALOG: DATA CENTER AND TELECOM FACILITIES-------------------------"]
[null,null,"PS4776: Air Side Economizer, Data Center/Telecom"]
[null,null,"PS2305: Energy-Efficient Drycooler, Data Center/Telecom"]
[null,null,"PS4777: Efficient UPS"]
[null,null,"PS4778: Efficient Rectifier"]
[null,null,"----------------------PROCESS SYSTEMS CATALOG: PROCESS SPECIALTY EQUIPMENT-------------------------"]
[null,null,"PS2490: Radiant Heater Band"]
[null,null,"PS2496: Pressure Screen Rotor"]
[null,null,"PS2538: Repulper Rotor without Extraction Plate"]
[null,null,"PS5210: Repulper Rotor with Extraction Plate"]
[null,null,"PS4764: Spline Rotor Upgrade"]
[null,null,"PS4763: HE Side Entry Agitator"]
[null,null,"PS4765: Industrial High Frequency Battery Charger"]
[null,null,"PS3244: Process Exhaust Filtration"]
[null,null,"PS3999: Steam Trap Repair/Replacement, Industrial, < 10 psig"]
[null,null,"PS4000: Steam Trap Repair/Replacement, Industrial, 10-49 psig"]
[null,null,"PS4001: Steam Trap Repair/Replacement, Industrial, 50-124 psig"]
[null,null,"PS4002: Steam Trap Repair/Replacement, Industrial, 125-225 psig"]
[null,null,"PS4003: Steam Trap Repair/Replacement, Industrial, > 225 psig"]
[null,null,"PS4761: Process Boiler Combustion Upgrades, Linkageless Controls"]
[null,null,"PS4762: Process Boiler Combustion Upgrades, O2 Trim Controls"]
[null,null,"PS4760: Process Boiler Combustion Upgrades, High Turndown Burner, Retrofit on Existing Boiler"]
[null,null,"PS5238: High Turndown Burner, New Boiler Replacement"]
[null,null,"----------------------PROCESS SYSTEMS CATALOG: VFDs-------------------------"]
[null,null,"PS2726: Variable Frequency Drives, Variable Torque, CW Distribution Pump"]
[null,null,"PS2640: Variable Frequency Drives, Variable Torque, Boiler Draft Fan"]
[null,null,"PS2641: Variable Frequency Drives, Variable Torque, Cooling Tower Fan"]
[null,null,"PS2647: Variable Frequency Drives, Variable Torque, Process Fan"]
[null,null,"PS2648: Variable Frequency Drives, Variable Torque, Process Pump"]
[null,null,"PS3280: Variable Frequency Drives, Existing Bldg: Constant Torque, All Types"]
[null,null,"----------------------PROCESS SYSTEMS CATALOG: DATA CENTER AND TELECOM FACILITIES-------------------------"]
[null,null,"PS4776: Air Side Economizer, Data Center/Telecom"]
[null,null,"PS2305: Energy-Efficient Drycooler, Data Center/Telecom"]
[null,null,"PS4777: Efficient UPS"]
[null,null,"PS4778: Efficient Rectifier"]
[null,null,"----------------------PROCESS SYSTEMS CATALOG: PROCESS SPECIALTY EQUIPMENT-------------------------"]
[null,null,"PS2490: Radiant Heater Band"]
[null,null,"PS2496: Pressure Screen Rotor"]
[null,null,"PS2538: Repulper Rotor without Extraction Plate"]
[null,null,"PS5210: Repulper Rotor with Extraction Plate"]
[null,null,"PS4764: Spline Rotor Upgrade"]
[null,null,"PS4763: HE Side Entry Agitator"]
[null,null,"PS4765: Industrial High Frequency Battery Charger"]
[null,null,"PS3244: Process Exhaust Filtration"]

{"sheet":"Industry Std Cost","index":7,"n_rows":502,"n_cols":7,"rows_kept":502,"hidden":true}
["January 2026 Industry Standard Costs"]
[]
["Code","Measure Name","Cost per UOM","UOM","Meausre","Name"]
[598,0.5257070198862404,"Square Footage","Greenhouse Climate Controls","L5459: LED, ≤43W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer",5459,{"$f":"_xlfn.XLOOKUP(F4,$A$4:$A$502,$B$4:$B$502,\"Enter Cost\",0,1)","v":119.24241769004804}]
[1983,8980.983333333334,"Unit","Hot Water Boiler, 95%+ AFUE","L3111: LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer",3111,{"$f":"_xlfn.XLOOKUP(F5,$A$4:$A$502,$B$4:$B$502,\"Enter Cost\",0,1)","v":101.70388222432278}]
[2196,585.8025455162134,"Compressor Horsepower","Air Compressor, Variable Speed Drive, Constant Speed Replacement","L3400: 2X2 LED, ≤39W, replacing Fixture with 2 or more T8 or T12 Lamps",3400,86.67950736108713]
[2199,44.42636616215107,"Unit","Anti-sweat Heater Controls, Freezer Case, Standard Door","L3401: 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps",3401,84.21755156081447]
[2201,36.62162162162162,"Unit","Anti-sweat Heater Controls, Refrigerated Case, Standard Door","L10281: 1’ to 3’ LED Linear Ambient Fixture, Interior",10281,142.52523361522196]
[2203,121.53410491354475,"Horse Power","Boiler Burner, 10:1 High Turn Down","L10282: 4' LED Linear Ambient Fixture, Interior",10282,103.79633394099928]
[2205,683.5545283520241,"Horse Power","Boiler Control, Linkageless","L10283: 8' LED Linear Ambient Fixture, Interior",10283,162.60292104068057]
[2206,40.589819700469775,"Horse Power","Boiler Oxygen Trim Combustion Controls","L10028: LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture",10028,83.27201298058706]
[2218,51.83524424208783,"MBh Rating","Boiler, Hot Water, Modulating, >=90% AFUE, < 300 mbh","L4813: LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture",4813,4.860386712808626]
[2221,1046.05,"Control","Boiler, Outside Temperature Reset/Cutout Control","L3091: ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID",3091,203.2705701451451]
[2225,18.758544603091014,"Unit","Bonus, Steam Trap Survey","L3092: ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID",3092,207.72586149343638]
[2234,2359,"Unit","Case Door, Freezer, Low Heat","L3093: ≤ 250W LED High Bay/Low Bay, replacing 400W HID",3093,205.5338533004155]
[2235,989.64,"Unit","Case Door, Freezer, No Heat","L3094: ≤ 365W LED High Bay/Low Bay, replacing 400W HID",3094,310.59458784020774]
[2236,1030.0462464985994,"Unit","Case Door, Cooler, No Heat","L3095: ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID",3095,372.4663368436984]
[2254,475.82071428571425,"Unit","Compressed Air Condensate Drains, No Loss Drain","L3096: ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID",3096,479.70000000000005]
[2255,31.900805860805864,"Horse Power","Compressed Air Controller, Pressure/Flow Controller","L5460: ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12",5460,187.56298369703856]
[2257,188.7246915923645,"Horse Power","Compressed Air Heat Recovery, Space Heating","L5461: ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO",5461,172.6908512771471]
[2258,37.650778819203055,"Horse Power","Compressed Air Mist Eliminators","L3393: ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO",3393,200.12969403729838]
[2259,77.76,"Unit","Compressed Air Nozzles, Air Entraining","L4347: ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO",4347,237.73668173690933]
[2264,21.833376186472066,"CFM","Compressed Air, Cycling Thermal Mass Air Dryers","L4795: ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO",4795,232.89057644173758]
[2269,238.6629971590908,"Unit","Cooler Evaporator Fan Control","L4796: ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO",4796,271.58985124423964]
[2271,28.567094611528823,"Linear Feet","Cooler Night Curtains, Open Coolers","L10042: DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID",10042,135.2630035990095]
[2281,11617.977777777778,"Unit","Dishwasher, High Temp, Electric Booster, Door Type, Energy Star,  Electric","L10039: Four-pin base LED Lamp Replacing CFL",10039,18.010280623060144]
[2300,2345.875,"Unit","Dock Door Infiltration Reduction, New Install","L5451: 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp",5451,11.994201024503337]
[2301,3820.098806306307,"Unit","Dock Door Infiltration Reduction, Replace Existing","L5452: 4' TLED, replacing 4' T5HO Lamp",5452,14.170638827984217]
[2302,806.08125,"Unit","Dock Pit/Ramp External Seal, Added to Existing \"Brush\" Barrier","L4797: 2' or 3' TLED, replacing 2' or 3' T8 or T12 Lamp",4797,22.07163526228772]
[2303,2040.9132888888885,"Unit","Dock Pit/Ramp External Seal, No Brush Barrier Present","L4809: 8' TLED, replacing 8' T8 or T12 Lamp",4809,72.72500000000001]
[2306,4350.49,"Unit","ECM Compressor Fan Motor","L3903: Interior LED Signage",3903,"Enter Cost"]
[2307,5590.770434782608,"Unit","ECM Condenser/Condensing Unit Fan Motor","L10284: 1’ to 3’ LED Linear Ambient Fixture, Exterior",10284,66.38461538461539]
[2308,289.2342767295597,"Unit","ECM Evaporator Fan Motor, Walk-in Cooler, <1/20hp","L10285: 4' LED Linear Ambient Fixture, Exterior",10285,71.17940476190476]
[2309,250.47747544068136,"Unit","ECM Evaporator Fan Motor, Walk-in Cooler, 1/20hp - 1 hp","L10286: 8' LED Linear Ambient Fixture, Exterior",10286,178.7407653973933]
[2310,286.4656862745098,"Unit","ECM Evaporator Fan Motor, Walk-in Freezer, <1/20hp","L10029: LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior",10029,119.03136978471426]
[2311,304.9313893178894,"Unit","ECM Evaporator Fan Motor, Walk-in Freezer, 1/20hp - 1 hp","L3904: Exterior LED Signage",3904,2.348723063870037]
[2312,98.93333333333332,"Unit","ECM Motor, Cooler/Freezer Case","L4280: Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens",4280,167.34448455729935]
[2314,11.920249499320022,"CFM","Energy Recovery Ventilator","L4281: Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens",4281,218.02226801132377]
[2315,28.25,"Horse Power","Enter # of Hours","L4282: Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens",4282,323.89845972361394]
[2373,197.7977026855898,"Unit","Guest Room Energy Management Controls, Electric Heat PTAC Systems","L4283: Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens",4283,571.1732999351436]
[2374,347.7015972222222,"Unit","Guest Room Energy Management Controls, Not Otherwise Specified","L10043: DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior",10043,116.76904221219543]
[2422,24.05693139187575,"Capacity (Input MBh)","Infrared Heating Units, High or Low Intensity","L10040: Four-pin base LED Lamp Replacing CFL, Exterior",10040,"Enter Cost"]
[2429,27.44815340679661,"Unit","Insulation, Steam Fitting, Removable, NG","L5456: 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior",5456,10.40375]
[2430,13.40767757404665,"Unit","Insulation, Steam Piping, NG","L5458: 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior",5456,10.40375]
[2434,446.688614957265,"Horse Power","Irrigation Pressure Reduction, Nozzle Installation & Motor Downsizing"]
[2456,71.38350951974992,"Unit","LED, Reach-In Refrigerated Case, Replaces T12 or T8"]
[2490,813.793984962406,"Installed kW Of Exist. Heater Bands","Plastics Equipment, Radiant Heater Band Retrofit"]
[2496,392.2552703703704,"Horse Power","Pressure Screen Rotor"]
[2509,750.7669300015275,"Unit","Reach In Refrigerated Case w/ Doors replacing Open Multi Deck Case"]
[2538,87.664375,"Horse Power","Repulper Rotor"]
[2621,206.23583333333335,"Horse Power","Ventilation Controls, Kitchen Hood, Temp only, Adder for MUA, Retrofit"]
[2623,206.23633333333333,"Horse Power","Ventilation Controls, Kitchen Hood, Temp only, Exhaust Only, Retrofit"]
[2625,282.9896,"Horse Power","Ventilation Controls, Kitchen Hood, with Optical, Adder for MUA, Retrofit"]
[2627,4806.124100574712,"Horse Power","Ventilation Controls, Kitchen Hood, with Optical, Exhaust Only, Retrofit"]
[2639,664.4345555555554,"Horse Power","VFD, Ag Second Use Water System"]
[2640,410.52336071428584,"Horse Power","VFD, Boiler Draft Fan"]
[2641,194.25024855967072,"Horse Power","VFD, Cooling Tower Fan"]
[2643,342.13057544209715,"Horse Power","VFD, HVAC Fan"]
[2644,438.96703373015873,"Horse Power","VFD, HVAC Heating Pump"]
[2646,485.66579777777775,"Horse Power","VFD, Pool Pump Motor"]
[2647,198.5661067732634,"Horse Power","VFD, Process Fan"]
[2648,187.0840419100027,"Horse Power","VFD, Process Pump"]
[2660,727.7477659574469,"Unit","Waterer, Livestock, < 250 Watts"]
[2700,977.4127692307693,"Unit","PTHP, >=13000 Btuh"]
[2701,762.2245407066054,"Unit","PTHP, 10000-12999 Btuh"]
[2702,607.969023809524,"Unit","PTHP, 8000 - 9999 Btuh"]
[2726,340.8071167137475,"Horse Power","VFD, Chilled Water Distribution Pump"]
[2764,8527.5,"Unit","Furnace, ECM, >=95%+ AfUE, NG"]
[2768,36.83111111111111,"Unit","LED, Exit Sign, Retrofit"]
[2819,2.1475810533156516,"Unit*","Solar PV"]
[2848,769.8964164434256,"Horsepower Of Load Shifted","Compressed Air Process Load Shifting"]
[2849,0,"Unit*","Adjustment Measure"]
[2853,8.195376966537207,"CFM","Ventilation Controls, Demand Control Ventilation For Air Handling Units"]
[2927,279.0046511627907,"Unit*","Process, Not Otherwise Specified"]
[2992,7060,"Unit","Air Source Heat Pump, >= 16 SEER"]
[3018,994.0050950736717,"Unit","Waterer, Livestock, Energy Free"]
[3045,9666.007708333334,"Unit","Water Heater, High Usage, >=90% TE, NG"]
[3066,2845,"Unit","Economizer, RTU Optimization"]
[3091,203.2705701451451,"Unit","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay"]
[3092,207.72586149343638,"Unit","LED Fixture, <250 Watts, Replacing 320-400 Watt HID, High Bay"]
[3093,205.5338533004155,"Unit","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay"]
[3094,310.59458784020774,"Unit","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay"]
[3095,372.4663368436984,"Unit","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay"]
[3096,479.70000000000005,"Unit","LED Fixture, <800 Watts, Replacing 1000 Watt HID, High Bay"]
[3097,193.84462950461986,"Unit","LED Fixture, Bilevel, Stairwell and Passageway"]
[3111,101.70388222432278,"Unit","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer"]
[3114,18.79805578474514,"Linear Feet","LED, Horizontal Case Lighting"]
[3183,49.75308641975309,"Unit","Strip Curtain, Walk-In Freezers and Coolers"]
[3244,3.878821389877938,"CFM","Process Exhaust Filtration"]
[3266,3053.6472527910687,"Unit","Demand Control Ventilation, RTU Optimization"]
[3276,37.90837100574541,"MBh Rating","Boiler, Hot Water, Condensing, >=90% AFUE, >=300 mbh"]
[3277,23.990313824504927,"MBh Rating","Boiler, Hot Water, Near Condensing, >=85% AFUE, >=300 mbh"]
[3280,225.141159726907,"Horse Power","VFD, Constant Torque"]
[3281,2.5343671768113922,"Unit*","Project Assessment Incentive"]
[3383,3.7104511447760364,"Unit*","Retrocommissioning, Audit, Part 1 Incentive"]
[3384,2.4765459917941515,"Unit*","Retrocommissioning, Implementation, Part 2 Incentive"]
[3386,183.04018491052605,"Bushels Per Hour (Drying Capacity)","Grain Dryer, Energy Efficient, Hybrid"]
[3393,200.12969403729838,"Unit","LED Fixture,<=180 Watts, Replacing 4 lamp T5 or 6 lamp T8, High Bay, DLC Listed"]
[3400,86.67950736108713,"Unit","LED Fixture, 2x2, Low Output, DLC Listed"]
[3401,84.21755156081447,"Unit","LED Fixture, 2x2, High Output, DLC Listed"]
[3406,1.0766721678621178,"Unit","Daylighting Controls"]
[3409,233.64158539789793,"Unit","Retrofit Open Refrigerated Cases with Doors"]
[3412,2.0625839122553917,"Unit*","Biogas Feasibility Study Incentive"]
[3491,63.214436402666045,"MBh Rating","Furnace with ECM, ≥95%+ AFUE, NG"]
[3492,95.55681818181819,"MBh Rating","Furnace with ECM, ≥90%+ AFUE, NG"]
[3493,11924,"Unit","Parking Garage Ventilation Controls with Heating"]
[3494,369.22,"Unit","Variable Speed ECM Pump, < 100 Watts Max Input, Domestic Hot Water Recirculation"]
[3495,6485,"Unit","Variable Speed ECM Pump, 100 - 500 Watts Max Input, Domestic Hot Water Recirculation"]
[3497,1126.3725,"Unit","Variable Speed ECM Pump, < 100 Watts Max Input, Heating Water Circulation"]
[3498,1417.095,"Unit","Variable Speed ECM Pump, 100 - 500 Watts Max Input, Heating Water Circulation"]
[3499,4519.973333333333,"Unit","Variable Speed ECM Pump, > 500 Watts Max Input, Heating Water Circulation"]
[3502,2850,"Unit","Variable Speed ECM Pump, > 500 Watts Max Input, Cooling Water Circulation"]
[3511,26.76245816118047,"Unit","LED Replacement of 4’ T8 Lamps w/Integral or External Driver"]
[3512,12.283588396933938,"Unit","LED Replacement of 4’ T8 Lamps utilizing existing ballast"]
[3681,288,"Unit","Spring-loaded Garage Door Hinge, 60 Degree Indoor Temperature Setpoint"]
[3682,115.27,"Unit","Spring-loaded Garage Door Hinge, 65 Degree Indoor Temperature Setpoint"]
[3684,11933.333333333334,"Unit","3684"]
[3703,7.066405177597333,"Square Feet Of Insulation","Insulation, Wall, NG heat with Cooling"]
[3704,1.9791666666666667,"Square Feet Of Insulation","Insulation, Wall, NG heat without Cooling"]
[3705,6.428571428571429,"Square Feet Of Insulation","Insulation, Wall, Electric heat with Cooling"]
[3707,1.9212161324045154,"Square Feet Of Insulation","Insulation, Attic, NG heat with Cooling, Existing Insulation ≤R-11"]
[3708,1.815925925925926,"Square Feet Of Insulation","Insulation, Attic, NG heat without Cooling, Existing Insulation ≤R-11"]
[3709,1.6054950123263014,"Square Feet Of Insulation","Insulation, Attic, NG heat with Cooling, Existing Insulation R-12 to R-19"]
[3710,4.762794860368389,"Square Feet Of Insulation","Insulation, Attic, NG heat without Cooling, Existing Insulation R-12 to R-19"]
[3711,1.254692437511403,"Square Feet Of Insulation","Insulation, Attic, Electric heat with Cooling, Existing Insulation ≤R-11"]
[3713,1.4998084254267536,"Square Feet Of Insulation","Insulation, Attic, Electric heat with Cooling, Existing Insulation R-12 to R-19"]
[3738,34.65429487179487,"Linear Feet","LED Fixture, Linear Ambient, Replacing 1 or 2 T5 lamp(s) in Cross Section"]
[3739,29.462188055000556,"Linear Feet","LED Fixture, Linear Ambient, Replacing 3 or 4 T5 lamps in Cross Section"]
[3740,22.88202277336959,"Linear Feet","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section"]
[3741,24.783734632415168,"Linear Feet","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/12 lamps in Cross Section"]
[3759,11.106545541933762,"Unit","LED Replacement of 4’ T8 Lamps, Direct Wire"]
[3760,102.89794985911631,"Unit","LED Troffer, 1x4, Replacing 4' 1-2 Lamp T8 Troffer"]
[3777,508.7360765016746,"Horse Power","VFD, High Speed Ventilation/Circulation Fan, Ag"]
[3780,6252.5,"Unit","Hot Water Boiler, Tier 2, 95%+ AFUE"]
[3835,172.03141383219958,"Horse Power","VFD, Process Pump, Agriculture"]
[3836,425.95971895711494,"Horse Power","VFD, Constant Torque, Agriculture"]
[3874,4683.423,"Unit","Ductless Minisplit Heat Pump, replacing Electric Resistance and CAC"]
[3875,6376.55,"Unit","Ductless Minisplit Heat Pump, replacing Electric Resistance and Room AC"]
[3877,9471.344,"Unit","Ductless Minisplit Heat Pump, replacing Electric Resistance and no AC"]
[3904,2.348723063870037,"Unit","LED Signage Retrofit, Exterior"]
[3909,1382.0457402168447,"Tons","A/C Split System, Condensing Unit Only, High Efficiency"]
[3910,2144.799155844156,"Horse Power","ECM HVAC Fan Motors, Heating"]
[3912,9052.371085742405,"Horse Power","ECM HVAC Fan Motors, Occupied Ventilation"]
[3913,6202.037878787878,"Horse Power","ECM HVAC Fan Motors, 24/7 Ventilation"]
[3928,134.51388888888889,"Horse Power","Vacuum Pump Heat Recovery, Space Heating"]
[3929,17.349999999999998,"Unit","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, ≥ 23W CFL"]
[3930,34.5,"Unit","LED Lamp, ENERGY STAR, Replacing Exterior Directional CFL, 14W-22W CFL"]
[3932,20.861793619791666,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≥ 23W CFL"]
[3933,12.665716783216784,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, 14W-22W CFL"]
[3934,8.38,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional CFL, ≤ 13W"]
[3935,58.5175,"Unit","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 120W – 250W Incandescent"]
[3936,61.599782608695655,"Unit","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 100W – 119W Incandescent"]
[3937,28.618303571428573,"Unit","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 75W – 99W Incandescent"]
[3938,10,"Unit","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, 55W – 74W Incandescent"]
[3940,13.417692307692308,"Unit","LED Lamp, ENERGY STAR, Replacing Exterior Directional Incandescent, ≤ 35W Incandescent"]
[3941,27.232538527836024,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 120W – 250W"]
[3942,16.750483333333335,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 100W – 119W"]
[3943,14.024304433197258,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 75W – 99W"]
[3944,9.936264095375952,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 55W – 74W"]
[3945,13.448981481481484,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, 36W – 54W"]
[3946,12,"Unit","LED Lamp, ENERGY STAR, Replacing Interior Directional Incandescent, ≤ 35W"]
[3947,51.21010714285713,"Unit","LED Lamp, ENERGY STAR, 1,600 – 1,999 Lumens, Exterior"]
[3948,33.14666666666667,"Unit","LED Lamp, ENERGY STAR, 1,100 – 1,599 Lumens, Exterior"]
[3949,25.21428571428572,"Unit","LED Lamp, ENERGY STAR, 800 – 1,099 Lumens, Exterior"]
[3952,11.423430438168536,"Unit","LED Lamp, ENERGY STAR, Replacing Omnidirectional and Decorative Incand. or CFL, 1,600 – 1,999 Lumens"]
[3953,12.325127053265097,"Unit","LED Lamp, ENERGY STAR, Replacing Omnidirectional and Decorative Incand. or CFL, 1,100 – 1,599 Lumens"]
[3954,8.080806817007808,"Unit","LED Lamp, ENERGY STAR, Replacing Omnidirectional and Decorative Incand. or CFL, 800 – 1,099 Lumens"]
[3955,8.279809701492537,"Unit","LED Lamp, ENERGY STAR, Replacing Omnidirectional and Decorative Incand. or CFL, 450 – 799 Lumens"]
[3956,5.661496598639455,"Unit","LED Lamp, ENERGY STAR, Replacing Omnidirectional and Decorative Incand. or CFL, 250 – 449 Lumens"]
[3962,0.4782666058794911,"Watts Reduced Per Lamp","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)"]
[3963,0.6661833469590055,"Watts Reduced Per Lamp","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior"]
[3964,661.5689485907359,"Tons","Advanced Rooftop Unit Controller"]
[3978,45.95372411315671,"Unit","Occupancy Sensors, On/Off, High Bay, General"]
[3979,48.13270393192489,"Unit","Bi-Level Controls, High Bay, General"]
[3982,55.2451313417942,"Milking Cows","Plate Heat Exchanger and Well Water Pre-Cooler (<135 milking cows)"]
[3983,19.49242894568133,"Milking Cows","Plate Heat Exchanger and Well Water Pre-Cooler (≥135 milking cows)"]
[3987,15.77587137732872,"Milking Cows","3987"]
[3988,9.059661185828539,"Milking Cows","VFD, Dairy Milk Pump, Agriculture"]
[3989,9.304510015466004,"Milking Cows","Refrigeration Heat Recovery, NG WH, w/ a pre-cooler and VFD on milk pump, Ag"]
[3990,19.08213549465241,"Milking Cows","Refrigeration Heat Recovery, NG WH, w/ a pre-cooler, Ag"]
[3991,14.778416349206351,"Milking Cows","Refrigeration Heat Recovery, NG WH, w/ no pre-cooler, Ag"]
[3992,21.355216478696743,"Milking Cows","Refrigeration Heat Recovery, Elec WH, w/ a pre-cooler and VFD on milk pump, Ag"]
[3993,46.42266483516483,"Milking Cows","Refrigeration Heat Recovery, Elec WH, w/ a pre-cooler, Ag"]
[3994,40.120043677144515,"Milking Cows","Refrigeration Heat Recovery, Elec WH, w/ no pre-cooler, Ag"]
[3998,261.30129193740527,"Fan Diameter In Feet","Fans, High Volume Low Speed (HVLS), General"]
[3999,181.97520833333334,"Unit","Steam Trap Repair, < 10 psig, Industrial"]
[4000,209.58563148445307,"Unit","Steam Trap Repair, 10-49 psig, Industrial"]
[4001,253.48137361453936,"Unit","Steam Trap Repair, 50-124 psig, Industrial"]
[4002,323.0588736263736,"Unit","Steam Trap Repair, 125-225 psig, Industrial"]
[4003,3237.5,"Unit","Steam Trap Repair, > 225 psig, Industrial"]
[4004,178.33815726881937,"Unit","Steam Trap Repair, < 10 psig, General Heating, 7/32\" or Smaller"]
[4005,88.70744946823041,"Unit","Steam Trap Repair, < 10 psig, General Heating, 1/4\""]
[4006,185.62747435897438,"Unit","Steam Trap Repair, < 10 psig, General Heating, 5/16\""]
[4007,236.60667384012345,"Unit","Steam Trap Repair, < 10 psig, General Heating, 3/8\" or Larger"]
[4008,157.51398559123447,"Unit","Steam Trap Repair, 10-49 psig, General Heating, 7/32\" or Smaller"]
[4009,75.11051127381938,"Unit","Steam Trap Repair, 10-49 psig, General Heating, 1/4\""]
[4010,17.082180288044487,"Unit","Steam Trap Repair, 10-49 psig, General Heating, 5/16\""]
[4011,160.74534409557526,"Unit","Steam Trap Repair, 10-49 psig, General Heating, 3/8\" or Larger"]
[4012,381.98,"Unit","Steam Trap Repair, 50-124 psig, General Heating, 7/32\" or Smaller"]
[4013,128.505,"Unit","Steam Trap Repair, 50-124 psig, General Heating, 1/4\""]
[4014,547.35,"Unit","Steam Trap Repair, 50-124 psig, General Heating, 5/16\""]
[4015,465,"Unit","Steam Trap Repair, 50-124 psig, General Heating, 3/8\" or Larger"]
[4040,1,"Unit*","Emerging Technology Demonstration"]
[4041,16.975468584795976,"Unit","Bonus, Steam Trap Survey, Industrial"]
[4043,562.327417929293,"Horse Power","VFD, Ag Primary Use Water System"]
[4280,167.34448455729935,"Unit","LED, Exterior Fixture, Low Output, <= 4,999 lumens"]
[4281,218.02226801132377,"Unit","LED, Exterior Fixture, Mid Output, 5,000-9,999 lumens"]
[4282,323.89845972361394,"Unit","LED, Exterior Fixture, High Output, 10,000-29,999 lumens"]
[4283,571.1732999351436,"Unit","LED, Exterior Fixture, Very High Output, >= 30,000 lumens"]
[4314,56.75963333333334,"Unit","4FT Linear LED 2L, Replacing 8FT 1L T8 or T12"]
[4320,83.59539145914455,"Unit","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12"]
[4321,62.550000000000004,"Unit","4FT Linear LED 4L, Replacing 8FT 2L T8 or T12, Exterior"]
[4323,102.99759243482579,"Unit","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO"]
[4324,79.8348717948718,"Unit","4FT Linear LED 4L, Replacing 8FT 2L T8HO or T12HO, Exterior"]
[4326,52.98428571428571,"Unit","4FT Linear LED 2L, Replacing 8FT 2L T8 or T12"]
[4329,91.44446280991735,"Unit","4FT Linear LED 2L, Replacing 8FT 2L T8HO or T12HO"]
[4347,237.73668173690933,"Unit","LED Fixture, ≤250 Watts, Replacing 8-lamp T8 or 6-lamp T5HO, High Bay"]
[4348,8.88,"Unit","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior"]
[4349,5.5,"Unit","LED Replacement of 4-Foot T8 Lamps Utilizing Existing Ballast, Exterior, 24/7"]
[4350,11.916666666666666,"Unit","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior"]
[4351,9.401463675213675,"Unit","LED Replacement of 4-Foot T8 Lamps, Direct Wire, Exterior, 24/7"]
[4354,2.0589405984103006,"Watts Reduced Per Fixture","LED Fixture, Downlights, Interior"]
[4356,1.3720890356682836,"Watts Reduced Per Fixture","LED Fixture, Downlights, Exterior"]
[4360,608.5933852386476,"Horse Power","Refrigeration Controls, Floating Head Pressure"]
[4361,315.88632252992494,"Horse Power","VSD Vacuum Pump, ≤ 30 hp, Variable Torque"]
[4362,1049.2179838709676,"Horse Power","VSD Vacuum Pump, ≤ 30 hp, Constant Torque"]
[4363,33.40350069147958,"CFM","Dew Point Controls for Desiccant Dryers"]
[4368,1488.1792858694464,"Tons","A/C Split or Packaged System, High Efficiency, ≥ 5.42 to < 11.25 tons "]
[4369,1421.4360494462283,"Tons","A/C Split or Packaged System, High Efficiency, ≥ 11.25 to < 20.00 tons"]
[4370,2384.825126258291,"Tons","A/C Split or Packaged System, High Efficiency, ≥ 20.00 to < 63.33 tons"]
[4371,2238.6386573542577,"Tons","A/C Split or Packaged System, High Efficiency, ≥ 63.33 tons"]
[4375,170.9975,"Tstat","Smart Thermostat, Natural Gas Boiler"]
[4376,201.24678571428572,"Unit","Smart Thermostat, Natural Gas Furnace w/ AC"]
[4377,156.04797872340433,"Unit","Smart Thermostat, Natural Gas Rooftop Unit w/ AC"]
[4403,2.16777863734993,"# of Milking Cows per Compressor","Refrigeration System Tune-Up, Agriculture"]
[4412,172.101590909091,"Horse Power","VFD, Constant Torque, Agriculture, Low HOU"]
[4413,109.23005555555552,"Horse Power","VFD, High Speed Ventilation/Circulation Fan, Ag, Low HOU"]
[4414,305.4572583333333,"Horse Power","VFD, Process Pump, Agriculture, Low HOU"]
[4419,0.4298993260796239,"Boiler Capacity (MBh)","Boiler Tune Up, Non-EBTU"]
[4669,2.425230158730159,"Unit*","Wastewater Plant Energy Assessment"]
[4695,196.0026459245353,"Unit","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, Agriculture"]
[4696,226.82872242843274,"Unit","LED Fixture, <250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture"]
[4697,207.59700971598764,"Unit","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
[4698,251.49491358024693,"Unit","LED Fixture, <365 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
[4699,274.72175,"Unit","LED Fixture, <500 Watts, Replacing 1000 Watt HID, High Bay, Agriculture"]
[4701,223.95352482862,"Unit","<=180W LED, replacing or instead of 6L T8 or 4L T5HO, Agriculture"]
[4702,216.29219651553308,"Unit","<=250W LED, replacing or instead of 8LT8 or 6LT5HO, Agriculture"]
[4703,0.5068270496108749,"Watts Reduced Per Lamp","DLC Listed, Mogul Screw-Base (E39) lamp replacing HID (various), Agriculture"]
[4707,29.782989689715265,"Unit*","Bonus, Early Completion, 25%"]
[4708,84.40008252208874,"Unit*","Bonus, Early Completion, 10%"]
[4712,1114.627247798755,"Tons","Chiller, Air-Cooled <150 tons, Path A"]
[4713,813.0261113713343,"Tons","Chiller, Air-Cooled ≥150 tons, Path A"]
[4714,929.0189310595935,"Tons","Chiller, Air-Cooled <150 tons, Path B"]
[4715,626.6123742098528,"Tons","Chiller, Air-Cooled ≥150 tons, Path B"]
[4716,3791.015625,"Tons","Chiller, Positive Displacement, Water-Cooled <75 tons, Path A"]
[4717,1471.1245421245421,"Tons","Chiller, Positive Displacement, Water-Cooled ≥75 and <150 tons, Path A"]
[4718,1385.9554311926606,"Tons","Chiller, Positive Displacement, Water-Cooled ≥150 and <300 tons, Path A"]
[4719,358.99,"Tons","Chiller, Positive Displacement, Water-Cooled ≥300 and <600 tons, Path A"]
[4723,524.6277777777777,"Tons","Chiller, Positive Displacement, Water-Cooled ≥150 and <300 tons, Path B"]
[4727,1144.2110204081632,"Tons","Chiller, Centrifugal, Water-Cooled ≥150 and <300 tons, Path A"]
[4730,500.5590083333334,"Tons","Chiller, Centrifugal, Water-Cooled ≥600, Path A"]
[4733,677.8348593097794,"Tons","Chiller, Centrifugal, Water-Cooled ≥300 and <400 tons, Path B"]
[4734,387.3211111111111,"Tons","Chiller, Centrifugal, Water-Cooled ≥400 and <600 tons, Path B"]
[4735,1153,"Tons","Chiller, Centrifugal, Water-Cooled ≥600, Path B"]
[4737,1544.1362143327776,"Tons","A/C Split System, ≤ 65 MBh, SEER 16"]
[4738,2277.9508994708995,"Tons","A/C Split System, ≤ 65 MBh, SEER 17"]
[4739,1436.7866666666669,"Tons","A/C Split System, ≤ 65 MBh, SEER 18"]
[4741,959.2741379310345,"Tons","A/C Single Package, ≤ 65 MBh, SEER 16"]
[4742,1310.6540487162606,"Tons","A/C Single Package, ≤ 65 MBh, SEER 17"]
[4743,1741,"Tons","A/C Single Package, ≤ 65 MBh, SEER 18"]
[4745,1273.7089147286822,"Tons","Air-Source Heat Pump, ≤ 65 MBh, SEER 16 and 9.0 HSPF"]
[4746,2152.962962962963,"Tons","Air-Source Heat Pump, ≤ 65 MBh, SEER 17 and 9.0 HSPF"]
[4747,2470.3059110449735,"Tons","Air-Source Heat Pump, ≤ 65 MBh, SEER 18 and 9.0 HSPF"]
[4748,245.9975,"Unit","Guest Room Energy Management Controls, PTHP Systems"]
[4749,1.0907053652101986,"Conditioned Sq Ft","Air Sealing, Natural Gas Heat with Cooling"]
[4750,2.3054786945081065,"Conditioned Sq Ft","Air Sealing, Natural Gas Heat without Cooling"]
[4751,1.3536533831435105,"Conditioned Sq Ft","Air Sealing, Electric Heat with Cooling"]
[4753,17.08893361865136,"Capacity (Input MBh)","Unit Heater, ≥90% Thermal Efficiency, Heating Setpoint = 70°F   "]
[4754,28.1211727931983,"Capacity (Input MBh)","Unit Heater, ≥90% Thermal Efficiency, Heating Setpoint = 65°F   "]
[4758,701.5989860198811,"kW Controlled","Demand Defrost Controls, Freezer"]
[4759,15,"Unit","Evaporator Fan Control, Reach-in Cooler or Freezer"]
[4760,93.24801552784838,"Horse Power","Process Boiler Burner, 10:1 High Turn Down"]
[4761,65.72201685571756,"Horse Power","Process Boiler Control, Linkageless"]
[4762,38.364593265601066,"Horse Power","Process Boiler, Oxygen Trim Combustion Controls"]
[4763,916.4146550877192,"Horse Power","High Efficiency Side Entry Agitator"]
[4764,64.93561875,"Horse Power","Spline Rotor Upgrade for Refiners"]
[4765,134.69906577408923,"kW-hour of battery charger capacity","Battery Charger, Industrial, High Frequency"]
[4766,14.130187503596064,"Horse Power","Compressed Air System Leak Survey and Repair"]
[4770,5153.846153846153,"Tons","A/C Split System, ≤ 65 MBh, SEER 17, Data Center/Telecom"]
[4776,1061.204375,"Tons","Air Side Economizer, Data Center/Telecom"]
[4777,549.9999999999999,"kW Capacity","Efficient UPS"]
[4779,0.7567118715702211,"Watts Reduced Per Fixture","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior"]
[4781,38.699999999999996,"Linear Feet","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 24 hour"]
[4782,19.96406746031746,"Linear Feet","LED Fixture, Linear Ambient, Replacing 1 or 2 T8/T12 lamp(s) in Cross Section, Exterior, 12 hour"]
[4784,26.715,"Linear Feet","LED Fixture, Linear Ambient, Replacing 3 or 4 T8/T12 lamps in Cross Section, Exterior, 12 hour"]
[4793,108.90926919079769,"Unit","LED Troffer, 2x4, Replacing 4' 1-2 Lamp T8 Troffer"]
[4795,232.89057644173758,"Unit","LED Fixture, ≤ 300 Watts, Replacing 10-Lamp T8 or 8-Lamp T5HO, High Bay"]
[4796,271.58985124423964,"Unit","LED Fixture, ≤ 350 Watts, Replacing 12-Lamp T8 or 10-Lamp T5HO, High Bay"]
[4797,22.07163526228772,"Unit","LED Replacement of 2' T8 or T12 Lamp w/External Driver (UL Type C) "]
[4798,11.396031329330576,"Unit","LED Replacement of 2' T8 or T12 Lamp, Direct Wire (UL Type B) "]
[4799,24.404180730159766,"Unit","LED Replacement of 2' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) "]
[4800,41.99,"Unit","LED Replacement of U-Bend T8 or T12 Lamp w/External Driver (UL Type C) "]
[4801,19.860746927236978,"Unit","LED Replacement of U-Bend T8 or T12 Lamp, Direct Wire (UL Type B) "]
[4802,29.99046466725067,"Unit","LED Replacement of U-Bend T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) "]
[4803,43.7,"Unit","LED Replacement of 4' T5 Lamp w/External Driver (UL Type C) "]
[4804,14.027333333333335,"Unit","LED Replacement of 4' T5HO Lamp w/External Driver (UL Type C) "]
[4805,13.626716826237402,"Unit","LED Replacement of 4' T5 Lamp, Direct Wire (UL Type B) "]
[4806,16.163000326658576,"Unit","LED Replacement of 4' T5HO Lamp, Direct Wire (UL Type B) "]
[4807,24.030136054421767,"Unit","LED Replacement of 4' T5 Lamp Utilizing Existing Ballast (UL Type A) "]
[4808,14.618427195768291,"Unit","LED Replacement of 4' T5HO Lamp Utilizing Existing Ballast (UL Type A) "]
[4809,72.72500000000001,"Unit","LED Replacement of 8' T8 or T12 Lamp w/External Driver (UL Type C) "]
[4810,32.69574108103688,"Unit","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B) "]
[4811,65.1475,"Unit","LED Replacement of 8' T8 or T12 Lamp Utilizing Existing Ballast (UL Type A) "]
[4812,0.9827026373077955,"Watts Controlled","Non-High Bay Occupancy/Vacancy Sensor"]
[4813,4.860386712808626,"Watts Reduced Per Fixture","LED Fixture, Track/Mono/Accent"]
[4829,0,"Unit*","Bonus, Agribusiness Trade Ally"]
[4832,18.333333333333332,"Unit","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior"]
[4835,24.925,"Unit","LED Replacement of 8' T8 or T12 Lamp, Direct Wire (UL Type B), Exterior 24/7"]
[4844,0,"Unit*","Farm Disaster Bonus"]
[4901,234.20199999999997,"Unit","Grain Dryer Tune-Up"]
[4925,934,"Unit","Circulation Fan, High-Speed High-Efficiency, >=53 inches, Ag, Efficiency Level 1"]
[4937,8048.54623809524,"Unit","Water Heater, Dual Thermostat, Ag, NG"]
[4939,174.10000000000002,"Unit","Swine Farrowing Crate Heaters w/Controls, Single"]
[4940,220.08,"Unit","Swine Farrowing Crate Heaters w/Controls, Double"]
[4942,14382.574074074075,"Unit","Water Heater, High Usage >= 90% Thermal Efficiency, Tankless, NG"]
[4943,860,"Unit","4943"]
[4944,2.454363119468744,"Unit","≥125 psig General Heating Steam Trap, ≤ 7/32” Orifice"]
[4945,1.299728431167746,"Unit","≥125 psig General Heating Steam Trap, 1/4” Orifice"]
[4946,8.906905640484977,"Unit","≥125 psig General Heating Steam Trap, 5/16” Orifice"]
[4947,359.890625,"Unit","≥125 psig General Heating Steam Trap, ≥ 3/8” Orifice"]
[4948,0.5125385320255726,"kWh Below Code","Interior New Construction Lighting LPD Below Code"]
[4949,188.28732454106276,"HP","VFD, Variable Torque, Irrigation Well Pump, >500 HOU"]
[4950,4602.875,"Unit","MF NG Furnace, Multi-stage+, 95% AFUE"]
[4951,5500.6943575419,"Unit","MF NG Furnace, Multi-stage+, 96% AFUE"]
[4952,6884.628958333334,"Unit","MF NG Furnace, Multi-stage+, 97% AFUE"]
[4953,8222.742222222221,"Unit","MF NG Furnace, Multi-stage+, 98%+ AFUE"]
[4955,5326.111111111111,"Unit","MF NG Furnace, Multi-stage+, Tier 2, 96% AFUE"]
[4956,5058,"Unit","MF NG Furnace, Multi-stage+, Tier 2, 97% AFUE"]
[4957,6046.5,"Unit","MF NG Furnace, Multi-stage+, Tier 2, 98%+ AFUE"]
[4958,4475.207692307692,"Unit","MF NG Furnace, Single-stage, 95% AFUE"]
[4959,3612.628571428568,"Unit","MF NG Furnace, Single-stage, 96% AFUE"]
[4960,2971.4285714285716,"Unit","MF NG Furnace, Single-stage, Tier 2, 95% AFUE"]
[4961,4375.9,"Unit","MF NG Furnace, Single-stage, Tier 2, 96% AFUE"]
[5008,3793.935,"Unit","Heat Pump Water Heater: 3.3 UEF"]
[5022,11405.070000000002,"Unit","Ductless Minisplit Heat Pump, Replacing Gas Furnace and CAC"]
[5023,4382.978,"Unit","Ductless Minisplit Heat Pump, Replacing Gas Boiler and CAC"]
[5024,670.715,"Unit","Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1,000W HID, Agriculture"]
[5026,841.5,"Unit","Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1,000W HID, Agriculture"]
[5027,241.875,"Unit","Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture"]
[5028,256.28625,"Unit","Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture"]
[5029,1.6283695438330061,"Total Watts Reduced","CLS, Fixture or Retrofit Kit Only"]
[5030,3.518534203559263,"Total Watts Reduced","CLS, Fixture or Retrofit Kit/Lamp with Connected Controls, Exterior"]
[5031,3.5508572914189376,"Total Watts Reduced","CLS, Fixture or Retrofit Kit/Lamp with Connected Controls, Interior"]
[5032,0.14400694104840078,"kWh Savings","Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture"]
[5033,0.43913694880415804,"kWh Savings","Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture"]
[5061,0.38932693952685965,"Watts Controlled","Occupancy Sensors, On/Off, High Bay"]
[5062,0.34785930568769446,"Watts Controlled","Bi-Level Controls, High Bay "]
[5063,0.6374372541039207,"Watts Controlled","Bi-level Controls, Parking Garage Fixtures, Dusk to Dawn"]
[5064,0.4928217948717949,"Watts Controlled","Bi-level Controls, Parking Garage Fixtures, 24 Hour"]
[5065,544.3,"Unit","LED, Exterior Fixture w/ NLC, Low Output, <= 4,999 lumens, NC Only"]
[5066,314.94248733535966,"Unit","LED, Exterior Fixture w/ NLC, Mid Output, 5,000-9,999 lumens, NC Only"]
[5067,514.1962500000001,"Unit","LED, Exterior Fixture w/ NLC, High Output, 10,000-29,999 lumens, NC Only"]
[5068,600.5633333333334,"Unit","LED, Exterior Fixture w/ NLC, Very High Output, >= 30,000 lumens, NC Only"]
[5069,3200,"Tons","A/C Split System, ≤ 65 MBh, SEER 19"]
[5070,1668.060238095238,"Tons","A/C Split System, ≤ 65 MBh, SEER 20"]
[5072,1825.6410256410256,"Tons","A/C Single Package, ≤ 65 MBh, SEER 20"]
[5073,1867.8854444444441,"Tons","Air-Source Heat Pump, ≤ 65 MBh, SEER 19 and 9.0 HSPF"]
[5074,3738.343344444444,"Tons","Air-Source Heat Pump, ≤ 65 MBh, SEER 20 and 9.0 HSPF"]
[5076,3925,"Tons","A/C Split System, ≤ 65 MBh, SEER 20, Data Center/Telecom"]
[5079,77.68697478991596,"Tstat","Smart Thermostat, Natural Gas Unit Heater, Standard Efficiency"]
[5081,4.270319613150269,"CFM","Direct Fired Make-up Air Unit, Constant Volume, Natural Gas"]
[5082,18.211477465110956,"CFM","Energy Recovery Ventilator, Sensible Heat Only"]
[5083,13691.599999999999,"Unit","Water Heater, High Usage, ≥ 95% TE, K-12 School, NG"]
[5084,8424.377142857144,"Unit","Water Heater, High Usage ≥ 90% Thermal Efficiency, Indirect, NG"]
[5086,725.3861111111112,"Unit","Circulation Fan, High-Speed High-Efficiency, Fixed Speed, 36-47 inches, Dairy"]
[5087,1171.7929515134254,"Unit","Circulation Fan, High-Speed High-Efficiency, Fixed Speed, ≥ 48 inches, Dairy"]
[5088,1293.9055555555558,"Unit","Ventilation Fan, High-Speed High-Efficiency, Fixed Speed, ≥ 48 inches, Dairy"]
[5089,3037.513947944669,"Unit","Ventilation Fan, High-Speed High-Efficiency, Variable Speed, ≥ 48 inches, Dairy"]
[5092,945.7,"Unit","Circulation Fan, High-Speed High-Efficiency, Fixed Speed, ≥ 48 inches, Non-Dairy"]
[5094,2137.9045454545453,"Unit","Ventilation Fan, High-Speed High-Efficiency, Fixed Speed, ≥ 48 inches, Non-Dairy"]
[5095,3032.202348039216,"Unit","Ventilation Fan, High-Speed High-Efficiency, Variable Speed, ≥ 48 inches, Non-Dairy"]
[5159,0,"Total Incentive","Bonus, Natural Gas, Agriculture"]
[5162,0,"Unit","SEM Staffing"]
[5163,9918.333333333334,"Unit","Air-Source Heat Pump Replacing Gas Furnace and CAC"]
[5167,3.125,"Unit","Insulation, Attic, NG heat with Cooling, Existing Insulation R-20 to R-38"]
[5188,50.58399226818334,"Unit*","PEP, Multifamily, New Construction"]
[5190,558.9452380952381,"Unit","Pump Assessment"]
[5191,10952.800000000001,"Unit","MF, Air Source Heat Pump, >= 16 SEER"]
[5192,12061.574108843537,"Unit","MF, Air Source Heat Pump replacing gas furnace and CAC"]
[5193,14651.666666666666,"Unit","MF, Air Source Heat Pump replacing gas furnace no CAC"]
[5195,0,"Unit*","Bonus, Custom Incentive"]
[5205,1.4174225490196077,"Unit*","School Energy Challenge, Installation Reimbursement"]
[5211,13.016407407407407,"Unit","Omnidirectional Interior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL"]
[5212,13.833491001751868,"Unit","Omnidirectional Interior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL"]
[5213,7.041111883684807,"Unit","Omnidirectional Interior LED with rated lumen output of 800-1,099 replacing incandescent or CFL"]
[5214,3.6527083333333334,"Unit","Omnidirectional Interior LED with rated lumen output of 450-799 replacing incandescent or CFL"]
[5219,4.550833333333333,"Unit","Decorative Interior LED with rated lumen output of 450-799 replacing incandescent or CFL"]
[5220,6.1899999999999995,"Unit","Decorative Interior LED with rated lumen output of 250-449 replacing incandescent or CFL"]
[5221,30.168888888888887,"Unit","Omnidirectional Exterior LED with rated lumen output of 1,600-1,999 replacing incandescent or CFL"]
[5222,8.1,"Unit","Omnidirectional Exterior LED with rated lumen output of 1,100-1,599 replacing incandescent or CFL"]
[5223,6.593333333333334,"Unit","Omnidirectional Exterior LED with rated lumen output of 800-1,099 replacing incandescent or CFL"]
[5230,5,"Unit","Decorative Exterior LED with rated lumen output of 250-449 replacing incandescent or CFL"]
[5231,25.6287776118,"Milking Cows","Variable Speed Control Vacuum Pump, < 500 cows"]
[5232,9.30835552588361,"Milking Cows","Variable Speed Control Vacuum Pump, 500 - 2000 cows"]
[5233,2.69518119787718,"kWh Below Code","Networked Lighting Controls, better than code, new construction"]
[5234,84.63764222861509,"MBh Rating","Boiler, 95%+ Efficient, With DHW, Multifamily, NG"]
[5235,1.6273806284323002,"Lighting Watts Reduced","Refrigeration Savings for Lighting Upgrades in Freezers"]
[5236,1.361536719288421,"Lighting Watts Reduced","Refrigeration Savings for Lighting Upgrades in Coolers"]
[5237,173.11715577599267,"Horse Power","Boiler Burner, 10:1 High Turn Down, New Boiler"]
[5238,1026.8922643714802,"Horse Power","Process Boiler Burner, 10:1 High Turn Down, New Boiler"]
[5254,443.2307692307692,"Unit","Smart Thermostat, Existing Air-Source Heat Pump, Contractor Install"]
[5255,89.99,"Unit","Smart Thermostat, Existing Air-Source Heat Pump, Retail Purchase"]
[5257,99,"Unit","Smart Thermostat, Existing Natural Gas Boiler, Retail Purchase"]
[5258,393.74145454545453,"Unit","Smart Thermostat, Existing Natural Gas Furnace, Contractor Install"]
[5259,133.15823529411753,"Unit","Smart Thermostat, Existing Natural Gas Furnace, Retail Purchase"]
[5321,10456,"Unit","Ground Source Heat Pump, With Gas Service"]
[5357,3199.6800000000003,"Unit","Automatic Sash Closer, Lab Energy Efficiency"]
[5358,550.5555555555555,"Unit","Automatic Flow Reducer, Lab Energy Efficiency"]
[5370,61.05999999999996,"Unit","Farmhouse Pack, Electric Only"]
[5374,2500,"Unit*","Solar Ready"]
[5388,1.428811,"Unit*","Tribal Nation Energy Plan Incentive"]
[5396,2.8136833746327974,"Unit*","Tribal Nation Project Development Incentive"]
[5400,1.0833541852844801,"Unit*","Project Assessment Incentive, SEM Bonus"]
[5423,1645.3738322536365,"Tons","A/C Split System or Single Package, ≤ 65 MBh, SEER2 16"]
[5424,1773.1199599800048,"Tons","A/C Split System or Single Package, ≤ 65 MBh, SEER2 17"]
[5425,2792.2680793934965,"Tons","A/C Split System or Single Package, ≤ 65 MBh, SEER2 18"]
[5426,2173.085114197531,"Tons","A/C Split System or Single Package, ≤ 65 MBh, SEER2 19"]
[5427,2472.042790627362,"Tons","A/C Split System or Single Package, ≤ 65 MBh, SEER2 20"]
[5428,307.6923076923077,"Tons","Air-Source Heat Pump, Split System, ≤ 65 MBh, SEER2 16 and 8.5 HSPF2"]
[5429,1984.4897368421052,"Tons","Air-Source Heat Pump, Split System, ≤ 65 MBh, SEER2 17 and 8.5 HSPF2"]
[5430,6119.307464726631,"Tons","Air-Source Heat Pump, Split System, ≤ 65 MBh, SEER2 18 and 8.5 HSPF2"]
[5431,3936.553978379857,"Tons","Air-Source Heat Pump, Split System, ≤ 65 MBh, SEER2 19 and 8.5 HSPF2"]
[5432,3756.2733554191577,"Tons","Air-Source Heat Pump, Split System, ≤ 65 MBh, SEER2 20 and 8.5 HSPF2"]
[5436,19.814348781697433,"Capacity (Input MBh)","Unit Heater, ≥90% Thermal Efficiency"]
[5438,177.8,"Unit","Spring-loaded Garage Door Hinge"]
[5440,35,"Unit","Anti-sweat Heater Controls, Refrigerated Case"]
[5441,53.31466666666666,"CFM","Desiccant Compressed Air Dryer, Heated"]
[5444,95.08,"Horse Power","Compressed Air Storage, Increase from ≤ 1 Gal/CFM to ≥ 3 Gal/CFM"]
[5445,26.602687811267664,"Linear Feet","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section"]
[5446,18.797980667701857,"Linear Feet","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior"]
[5447,162.893125,"Linear Feet","LED Fixture, Linear Ambient, Replacing 1 or 2 Lamp(s) in Cross Section, Exterior 24/7"]
[5448,25.00478138961013,"Linear Feet","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section"]
[5449,41.573750000000004,"Linear Feet","LED Fixture, Linear Ambient, Replacing 3 or 4 Lamps in Cross Section, Exterior"]
[5451,11.994201024503337,"Unit","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Interior"]
[5452,14.170638827984217,"Unit","4' TLED, Replacing 4' T5HO Lamp, Interior"]
[5453,10.454737406895603,"Unit","2' TLED, Replacing 2' T8 or T12 Lamp, Interior"]
[5454,28.26372557961915,"Unit","8' TLED, Replacing 8' T8 or T12 Lamp, Interior"]
[5456,10.40375,"Unit","4' or U-Bend TLED, ≤24W, Replacing 4' or U-Bend T5, T8 or T12 Lamp, Exterior"]
[5457,35,"Unit","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior 24/7"]
[5458,30,"Unit","8' TLED, Replacing 8' T8 or T12 Lamp, Exterior"]
[5459,119.24241769004804,"Unit","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer"]
[5460,187.56298369703856,"Unit","LED Fixture, ≤ 85 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12, High Bay"]
[5461,172.6908512771471,"Unit","LED Fixture, ≤ 125 Watts, Replacing 4 Lamp 4' or 2 Lamp 8' T12HO, High Bay"]
[5532,474.91499999999996,"Unit","PEM Recognition Incentive"]
[5533,1150,"Unit","PEM Training Incentive"]
[5550,7983.8775000000005,"Unit","Ductless Minisplit Heat Pump, >= 16 SEER2"]
[5564,0.8969408916761403,"# of corn acres planted","Grain Dryer Tune-Up"]
[5575,442.22909090909087,"Unit","Compressed Air System Leak Survey and Repair, Dairy Operations"]
[10005,14771.435,"Per water heater","Water Heater, ≥90% TE, NG Indirect, ≥80 gal capacity"]
[10006,7986,"Per water heater","Water Heater, ≥90% TE, NG Indirect, <80 gal capacity"]
[10025,1794.75,"Tons","Commercial Air Source Heat Pumps, ≥ 5.42 to < 11.25 tons"]
[10026,1318.4627354235972,"Tons","Commercial Air Source Heat Pumps, ≥ 11.25 to < 20.00 tons"]
[10028,83.27201298058706,"Unit","LED Fixture, Downlights, Interior"]
[10029,119.03136978471426,"Unit","LED Fixture, Downlights, Exterior"]
[10030,5.172468795879927,"CFM","Direct Fired Make-up Air Unit, Variable Air Volume"]
[10032,5470.228571428571,"Milking Cows","Refrigeration Heat Recovery, NG WH, Ag"]
[10033,4897.429,"Milking Cows","Refrigeration Heat Recovery, Electric WH, Ag"]
[10035,1,"Unit*","Bonus, 123 Energy Audit, 10%"]
[10039,18.010280623060144,"Unit","Four Pin-Base Lamp Replacing CFL, DLC Listed, Interior"]
[10041,227.84330188679232,"Unit","Smart Thermostat, Natural Gas Heat Source"]
[10042,135.2630035990095,"Unit","LED Lamp, DLC, High/Low-Bay Mogul Screw-Base (E39)"]
[10043,116.76904221219543,"Unit","LED Lamp, DLC, Mogul Screw-Base (E39), Exterior"]
[10045,49.575,"Unit","Thermostatic Radiator Valve"]
[10048,3725,"Unit","MF NG Furnace, Single-Stage, 97% AFUE"]
[10051,9683.184285714286,"Unit","MF, Air-Source Heat Pump replacing Electric Resistance"]
[10052,238.77391044776095,"Unit","Smart Thermostat, Gas and Electric"]
[10053,244.37555555555556,"Unit","Smart Thermostat, Electric only"]
[10207,47.57382266271005,"MBh Rating","Boiler, Hot Water, Condensing, >=95% TE, >=300 MBh"]
[10209,613.7014888888888,"Horse Power","VFD, Agriculture Water System"]
[10211,120.56494545990567,"Unit","LED Fixture, 2x2, Low Output, DLC Listed, w/LLLC"]
[10212,113.93606060606061,"Unit","LED Fixture, 2x2 High Output, DLC Listed, w/LLLC"]
[10213,125.52980882623801,"Unit","LED Troffer, 2x4, Replacing 4' 3-4 Lamp T8 Troffer, w/LLLC"]
[10214,118.47500000000001,"Unit","LED Troffer, 1x4 or 2x4, Replacing 4' 1 or 2 Lamp T8 Troffer, w/LLLC"]
[10215,227.33,"Unit","LED Fixture, <155 Watts, Replacing 250 Watt HID, High Bay, w/LLLC"]
[10216,196.81133333333335,"Unit","LED Fixture, <250 Watts, Replacing 400 Watt HID, High Bay, w/LLLC"]
[10217,274.12586351430105,"Unit","LED Fixture, <=180 Watts, Replacing 4 lamp T5HO or 6 lamp T8, High Bay, DLC Listed, w/LLLC"]
[10218,328.42801282051283,"Unit","LED Fixture, <=250 Watts, Replacing 6-lamp T5HO or 8-lamp T8, High Bay, DLC Listed, w/LLLC"]
[10219,9.17018611370663,"Square Footage","Roof Insulation, Existing Insulation <R-20"]
[10220,3.3886293187303616,"Square Footage","Roof Insulation, Existing Insulation >=R-20"]
[10222,41.84047295238095,"MBh Rating","Boiler, Hot Water, Condensing, 90% - 94% TE, >=300 MBh"]
[10223,2.632504201403938,"Watts Controlled","Advanced Lighting Controls, Interior"]
[10224,0.3221307156780841,"Watts Controlled","Advanced Lighting Controls, Exterior"]
[10281,142.52523361522196,"Unit","1’ to 3’ LED Linear Ambient Fixture, Interior"]
[10282,103.79633394099928,"Unit","4' LED Linear Ambient Fixture, Interior"]
[10283,162.60292104068057,"Unit","8' LED Linear Ambient Fixture, Interior"]
[10284,66.38461538461539,"Unit","1’ to 3’ LED Linear Ambient Fixture, Exterior"]
[10285,71.17940476190476,"Unit","4' LED Linear Ambient Fixture, Exterior"]
[10286,178.7407653973933,"Unit","8' LED Linear Ambient Fixture, Exterior"]
[10287,1.4394975369750822,"Total Watts Reduced","General Wattage Reduction, Interior"]
[10288,3.0823635121214847,"Total Watts Reduced","General Wattage Reduction, Exterior"]
[10289,0.6455166542897102,"Unit","Fixture Elimination, Interior"]
[10290,3.5836177474402731E-4,"Unit","Fixture Elimination, Exterior"]

{"sheet":"2025 Default Wattage Guide","index":8,"n_rows":131,"n_cols":6,"rows_kept":131,"hidden":true,"merged":[[0,0,0,5],[1,0,1,2],[1,4,1,5],[3,1,4,1],[3,2,4,2],[5,1,6,1],[5,2,6,2],[6,4,7,4],[6,5,7,5],[7,1,8,1],[7,2,8,2],[8,4,9,4],[8,5,9,5],[9,1,10,1],[9,2,10,2],[10,4,11,4],[10,5,11,5],[11,1,12,1],[11,2,12,2],[12,4,13,4],[12,5,13,5],[13,1,14,1],[13,2,14,2],[14,4,15,4],[14,5,15,5],[15,1,16,1],[15,2,16,2],[16,4,17,4],[16,5,17,5],[17,1,18,1],[17,2,18,2],[18,4,19,4],[18,5,19,5],[19,1,20,1],[19,2,20,2],[20,4,21,4],[20,5,21,5],[21,1,22,1],[21,2,22,2],[22,4,23,4],[22,5,23,5],[23,1,24,1],[23,2,24,2],[24,4,25,4],[24,5,25,5],[25,1,26,1],[25,2,26,2],[26,4,27,4],[26,5,27,5],[28,0,28,1],[29,1,31,1],[29,2,31,2],[31,4,32,4],[31,5,32,5],[32,1,33,1],[32,2,33,2],[33,4,34,4],[33,5,34,5],[34,1,35,1],[34,2,35,2],[35,4,36,4],[35,5,36,5],[36,1,37,1],[36,2,37,2],[37,4,38,4],[37,5,38,5],[38,1,39,1],[38,2,39,2],[39,4,40,4],[39,5,40,5],[40,1,41,1],[40,2,41,2],[41,4,42,4],[41,5,42,5],[42,1,43,1],[42,2,43,2],[43,4,44,4],[43,5,44,5],[44,1,45,1],[44,2,45,2],[45,4,46,4],[45,5,46,5],[46,1,47,1],[46,2,47,2],[47,4,48,4],[47,5,48,5],[51,1,52,1],[51,2,52,2],[52,4,53,4],[52,5,53,5]]}
[]
["*******FOR COMMON CFL DOWNLIGHTS*******",{"$nulls":3},"*******FOR COMMON LINEAR FLUORESCENT SYSTEMS*******"]
[null,"Existing Lamp Conﬁguration","Total System Wattage",null,"Existing Lamp Conﬁguration","Total System Wattage"]
[null,"(1) 13W CFL",16]
[{"$nulls":4},"*******4-Foot Fixtures*******"]
[null,"(1) 18W CFL",23]
[{"$nulls":4},"1L F32 T8 Normal BF",33]
[null,"(1) 26W CFL",31]
[{"$nulls":4},"1L F34 T12",39]
[null,"(1) 32W CFL",35]
[{"$nulls":4},"1L F40 T12",39]
[null,"(1) 42W CFL",46]
[{"$nulls":4},"1L F54 T5HO",62]
[null,"(1) 36/39W 2G11 CFL",51]
[{"$nulls":4},"2L F32 T8 Normal BF",61]
[null,"(1) 40W 2G11 CFL",48]
[{"$nulls":4},"2L FU32T8/6",55]
[null,"(1) 55W 2G11 CFL",58]
[{"$nulls":4},"2L F34 T12",66]
[null,"(2) 13W CFL",32]
[{"$nulls":4},"2L F40 T12",79]
[null,"(2) 18 W CFL",46]
[{"$nulls":4},"2L FU40T12",72]
[null,"(2) 26W CFL",62]
[{"$nulls":4},"2L F54 T5HO",117]
[null,"(2) 32W CFL",70]
[{"$nulls":4},"3L F32 T8 Normal BF",91]
[]
["*******FOR COMMON HID SYSTEMS*******",{"$nulls":3},"3L F34 T12",103]
[null,"Existing Lamp Conﬁguration","Total System Wattage"]
[{"$nulls":4},"3L F40 T12",124]
[{"$nulls":4},"4L F54 T5HO",234]
[null,"50W HID",65]
[{"$nulls":4},"4L F32 T8 Normal BF",120]
[null,"70W HID",94]
[{"$nulls":4},"4L F32 T8 High BF",151]
[null,"100W HID",126]
[{"$nulls":4},"4L F34 T12",136]
[null,"125W HID",146]
[{"$nulls":4},"4L F40 T12",153]
[null,"150W HID",179]
[{"$nulls":4},"6L F54 T5HO",355]
[null,"175W HID",210]
[{"$nulls":4},"6L F32 T8 High BF",224]
[null,"200W HID",232]
[{"$nulls":4},"8L F54 T5HO",468]
[null,"250W HID",293]
[{"$nulls":4},"8L F32 T8 High BF",291]
[null,"320W HID",356]
[null,"400W HID",455,null,"10L F54 T5HO",585]
[null,"750W HID",812,null,"10L F32 T8 High BF",368]
[null,"1,000W HID",{"v":1079,"d":"1,079"}]
[{"$nulls":4},"12L F32 T8 High BF",442]
[]
[{"$nulls":4},"*******8-Foot Fixtures*******"]
[{"$nulls":4},"1L F96T8",61]
[{"$nulls":4},"2L F96T8",107]
[{"$nulls":4},"1L F96T12",69]
[{"$nulls":4},"1L F96T12/HO",115]
[{"$nulls":4},"2L F96T12",109]
[{"$nulls":4},"2L F96T12/HO",190]
[]
[]
[]
[]
[null,"*******FOR CFL DOWNLIGHTS*******","Wattage"]
[null,"(1) 13W CFL",16]
[null,"(1) 18W CFL",23]
[null,"(1) 26W CFL",31]
[null,"(1) 32W CFL",35]
[null,"(1) 42W CFL",46]
[null,"(1) 36/39W 2G11 CFL",51]
[null,"(1) 40W 2G11 CFL",48]
[null,"(1) 55W 2G11 CFL",58]
[null,"(2) 13W CFL",32]
[null,"(2) 18 W CFL",46]
[null,"(2) 26W CFL",62]
[null,"(2) 32W CFL",70]
[null,"*******FOR HID SYSTEMS*******"]
[null,"50W HID",65]
[null,"70W HID",94]
[null,"100W HID",126]
[null,"125W HID",146]
[null,"150W HID",179]
[null,"175W HID",210]
[null,"200W HID",232]
[null,"250W HID",293]
[null,"320W HID",356]
[null,"400W HID",455]
[null,"750W HID",812]
[null,"1,000W HID",{"v":1079,"d":"1,079"}]
[null,"*******FOR LINEAR FLUORESCENT SYSTEMS*******"]
[null,"*******Linear Replacement Lamps********"]
[null,"4' or U-Bend T5, T8, or T12 Lamp","Enter Wattage"]
[null,"4' T5HO Lamp","Enter Wattage"]
[null,"2' or 3' T8 or T12 Lamp","Enter Wattage"]
[null,"8' T8 or T12 Lamp","Enter Wattage"]
[null,"*******4-Foot Fixtures*******"]
[null,"1L F32 T8 Normal BF Fixture",33]
[null,"1L F34 T12 Fixture",39]
[null,"1L F40 T12 Fixture",39]
[null,"1L F54 T5HO Fixture",62]
[null,"2L F32 T8 Normal BF Fixture",61]
[null,"2L FU32T8/6 Fixture",55]
[null,"2L F34 T12 Fixture",66]
[null,"2L F40 T12 Fixture",79]
[null,"2L FU40T12 Fixture",72]
[null,"2L F54 T5HO Fixture",117]
[null,"3L F32 T8 Normal BF Fixture",91]
[null,"3L F34 T12 Fixture",103]
[null,"3L F40 T12 Fixture",124]
[null,"4L F54 T5HO Fixture",234]
[null,"4L F32 T8 Normal BF Fixture",120]
[null,"4L F32 T8 High BF Fixture",151]
[null,"4L F34 T12 Fixture",136]
[null,"4L F40 T12 Fixture",153]
[null,"6L F54 T5HO Fixture",355]
[null,"6L F32 T8 High BF Fixture",224]
[null,"8L F54 T5HO Fixture",468]
[null,"8L F32 T8 High BF Fixture",291]
[null,"10L F54 T5HO Fixture",585]
[null,"10L F32 T8 High BF Fixture",368]
[null,"12L F32 T8 High BF Fixture",442]
[null,"*******8-Foot Fixtures*******"]
[null,"1L F96T8 Fixture",61]
[null,"2L F96T8 Fixture",107]
[null,"1L F96T12 Fixture",69]
[null,"1L F96T12/HO Fixture",115]
[null,"2L F96T12 Fixture",109]
[null,"2L F96T12/HO Fixture",190]
[null,"Other Fixture","Manual Input"]

{"sheet":"S&G Interior Measures","index":9,"n_rows":38,"n_cols":2,"rows_kept":38,"hidden":true}
["Column1.1","Column1.2"]
["L5459"," LED, <44W, 1x4 or 2X4 product replacing 1- or 2-lamp T8 or T12 troffer"]
["L3111"," LED, ≤55W, 2X4 product replacing 3- or 4-lamp T8 or T12 troffer"]
["L3400"," 2X2 LED, ≤36W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["L3401"," 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["L5445"," LED Fixture ≤10W/FT Replacing 1- or 2-lamp T5, T8 or T12 Lamp(s) in Cross Section"]
["L5448"," LED Fixture ≤24W/FT Replacing 3- or 4-lamp T5, T8 or T12 Lamps in Cross Section"]
["L4314"," 4’ 2 Lamp TLED ≤24W replacing 8’ 1 Lamp T8 or T12"]
["L4317"," 4’ 2 Lamp TLED ≤24W replacing 8’ 1 Lamp T8HO or T12HO"]
["L4320"," 4’ 4 Lamp TLED ≤24W replacing 8’ 2 Lamp T8 or T12"]
["L4323"," 4’ 4 Lamp TLED ≤24W replacing 8’ 2 Lamp T8HO or T12HO"]
["L4326"," 4’ 2 Lamp TLED ≤24W replacing 8’ 2 Lamp T8 or T12"]
["L4329"," 4’ 2 Lamp TLED ≤24W replacing 8’ 2 Lamp T8HO or T12HO"]
["L3091"," ≤ 155W LED High Bay/Low Bay, replacing or instead of 250W HID"]
["L3092"," ≤ 250W LED High Bay/Low Bay, instead of 320-399W HID"]
["L3093"," ≤ 250W LED High Bay/Low Bay, replacing 400W HID"]
["L3094"," ≤ 365W LED High Bay/Low Bay, replacing 400W HID"]
["L3095"," ≤ 500W LED High Bay/Low Bay, replacing or instead of 1000W HID"]
["L3096"," ≤ 800W LED High Bay/Low Bay, replacing or instead of 1000W HID"]
["L3393"," ≤ 180W LED High Bay/Low Bay, replacing or instead of 6L T8 or 4L T5HO"]
["L4347"," ≤ 250W LED High Bay/Low Bay, replacing or instead of 8L T8 or 6L T5HO"]
["L4795"," ≤ 300W LED High Bay/Low Bay, replacing or instead of 10L T8 or 8L T5HO"]
["L4796"," ≤ 350W LED High Bay/Low Bay, replacing or instead of 12L T8 or 10L T5HO"]
["L5460"," ≤ 85W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T8 or T12"]
["L5461"," ≤ 125W LED High Bay/Low Bay, replacing 4 Lamp 4' or 2 Lamp 8' T12HO"]
["R5235"," Refrigeration Savings for Lighting Upgrades in Freezers"]
["R5236"," Refrigeration Savings for Lighting Upgrades in Coolers"]
["L4354"," LED Downlight Fixtures replacing or instead of Incandescent, CFL, or HID fixture"]
["L4813"," LED Track/Mono/Accent fixtures replacing incandescent, CFL, or HID fixture"]
["L3097"," LED Stairwell or Passageway Fixture"]
["L3903"," Interior LED Signage"]
["L3962"," DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID"]
["L4779"," Four-pin base LED Lamp Replacing CFL"]
["L5451"," 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp"]
["L5452"," 4' TLED, replacing 4' T5HO Lamp"]
["L5453"," 2' TLED, replacing 2' T8 or T12 Lamp"]
["L5454"," 8' TLED, replacing 8' T8 or T12 Lamp"]
["L5029"," CLS Fixture or Retrofit Kit Upgrade"]

{"sheet":"S&G Exterior Measures","index":10,"n_rows":28,"n_cols":2,"rows_kept":28,"hidden":true}
["Column1.1","Column1.2"]
["L4280"," Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["L4281"," Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["L4282"," Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["L4283"," Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["L4356"," LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["L5446"," LED Fixture ≤ 10 W/ft Replacing or Instead of 1L or 2L T5, T8, or T12 in Cross Section - 12 Hours/Day"]
["L5447"," LED Fixture ≤ 10 W/ft Replacing or Instead of 1L or 2L T5, T8, or T12 in Cross Section - 24 Hours/Day"]
["L5449"," LED Fixture ≤ 24 W/ft Replacing or Instead of 3L or 4L T5, T8, or T12 in Cross Section - 12 Hours/Day"]
["L5450"," LED Fixture ≤ 24 W/ft Replacing or Instead of 3L or 4L T5, T8, or T12 in Cross Section - 24 Hours/Day"]
["L4316"," 4' 2-lamp TLED <24W replacing 8' 1-lamp T8 or T12, 24 Hour, Exterior"]
["L4315"," 4' 2-lamp TLED <24W replacing 8' 1-lamp T8 or T12, Dusk to Dawn, Exterior"]
["L4319"," 4' 2-lamp TLED <24W replacing 8' 1-lamp T8HO or T12HO, 24 Hour, Exterior"]
["L4318"," 4' 2-lamp TLED <24W replacing 8' 1-lamp T8HO or T12HO, Dusk to Dawn, Exterior"]
["L4322"," 4’ 4-lamp TLED <24W replacing 8' 2-lamp T8 or T12, 24 Hour, Exterior"]
["L4321"," 4’ 4-lamp TLED <24W replacing 8' 2-lamp T8 or T12, Dusk to Dawn, Exterior"]
["L4325"," 4' 4-lamp TLED <24W replacing 8' 2-lamp T8HO or T12HO, 24 Hour, Exterior"]
["L4324"," 4' 4-lamp TLED <24W replacing 8' 2-lamp T8HO or T12HO, Dusk to Dawn, Exterior"]
["L4328"," 4' 2-lamp TLED <24W replacing 8' 2-lamp T8 or T12, 24 Hour, Exterior"]
["L4327"," 4' 2-lamp TLED <24W replacing 8' 2-lamp T8 or T12, Dusk to Dawn, Exterior"]
["L4331"," 4' 2-lamp TLED <24W replacing 8' 2-lamp T8HO or T12HO, 24 Hour, Exterior"]
["L4330"," 4' 2-lamp TLED <24W replacing 8' 2-lamp T8HO or T12HO, Dusk to Dawn, Exterior"]
["L3904"," Exterior LED Signage"]
["L3963"," DLC listed, Mogul Screw-Base (E39) lamp replacing HID, Exterior"]
["L5455"," 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, 24 hour, Exterior"]
["L5456"," 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["L5457"," 8' TLED, replacing 8' T8 or T12 Lamp, 24 Hour, Exterior"]
["L5458"," 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]

{"sheet":"Ag Measures","index":11,"n_rows":73,"n_cols":2,"rows_kept":73,"hidden":true}
["Column1.1","Column1.2"]
["L5459"," 1X4 or 2X4 LED, ≤43W, replacing 1- or 2-lamp T8 or T12 troffer"]
["L3111"," 2X4 LED, ≤55W, replacing 3- or 4-lamp T8 or T12 troffer"]
["L3400"," 2X2 LED, ≤36W, replacing Fixture with 2 or more T8 or T12 Lamps"]
["L3401"," 2X2 LED, ≤85W, replacing Fixture with 2 or more 2G11 base Lamps"]
["L5445"," LED Fixture ≤10W/FT Replacing 1- or 2-lamp T5, T8 or T12 Lamp(s) in Cross Section"]
["L5448"," LED Fixture ≤24W/FT replacing 3- or 4-lamp T8 or T12 Lamps in Cross Section"]
["L4314"," 4’ 2 Lamp TLED <24W replacing 8’ 1 Lamp T8 or T12"]
["L4317"," 4’ 2 Lamp TLED <24W replacing 8’ 1 Lamp T8HO or T12HO"]
["L4320"," 4’ 4 Lamp TLED <24W replacing 8’ 2 Lamp T8 or T12"]
["L4323"," 4’ 4 Lamp TLED <24W replacing 8’ 2 Lamp T8HO or T12HO"]
["L4326"," 4’ 2 Lamp TLED <24W replacing 8’ 2 Lamp T8 or T12"]
["L4329"," 4’ 2 Lamp TLED <24W replacing 8’ 2 Lamp T8HO or T12HO"]
["AG4695"," LED Fixture, ≤155 Watts, Replacing 250 Watt HID, High Bay, Agriculture"]
["AG4696"," LED Fixture, ≤250 Watts, Replacing 320-399 Watt HID, High Bay, Agriculture"]
["AG4697"," LED Fixture, ≤250 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
["AG4698"," LED Fixture, ≤365 Watts, Replacing 400 Watt HID, High Bay, Agriculture"]
["AG4701"," LED Fixture, ≤180W LED, replacing 6L T8 or 4L T5HO, High Bay, Agriculture"]
["AG4702"," LED Fixture, ≤250W LED, replacing 8LT8 or 6LT5HO, High Bay, Agriculture"]
["L4354"," LED Downlight Fixtures replacing Incandescent, CFL, or HID fixture"]
["L3962"," DLC listed, Mogul Screw-Base (E39) LED lamp replacing HID"]
["L5451"," 4' or U-Bend TLED, ≤24W, replacing 4' or U-Bend T5, T8, or T12 Lamp"]
["L5452"," 4' TLED, replacing 4' T5HO Lamp"]
["L5453"," 2' TLED, replacing 2' T8 or T12 Lamp"]
["L5454"," 8' TLED, replacing 8' T8 or T12 Lamp"]
["N-L4948"," Lighting Power Density (LPD) better than code requirements"]
["AG4703"," DLC Listed, Mogul Screw-Base (E39) replacing existing E39 base lamp, Agriculture"]
["L4280"," Outdoor LED Fixture or Retrofit Kit – Low Output"]
["L4281"," Outdoor LED Fixture or Retrofit Kit – Mid Output"]
["L4282"," Outdoor LED Fixture or Retrofit Kit – High Output "]
["L4283"," Outdoor LED Fixture or Retrofit Kit – Very High Output"]
["N-L4280"," Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens"]
["N-L4281"," Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens"]
["N-L4282"," Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens"]
["N-L4283"," Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens"]
["N-L5065"," Outdoor LED Fixture or Retrofit Kit – Low Output ≤4,999 lumens, with NLC"]
["N-L5066"," Outdoor LED Fixture or Retrofit Kit – Mid Output 5,000 – 9,999 lumens, with NLC"]
["N-L5067"," Outdoor LED Fixture or Retrofit Kit – High Output 10,000 – 29,999 lumens, with NLC"]
["N-L5068"," Outdoor LED Fixture or Retrofit Kit – Very High Output ≥30,000 lumens, with NLC"]
["L4356"," LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["N-L4356"," LED Downlight Fixtures replacing or instead of Incandescent, CFL or HID fixture, Exterior"]
["L5446"," LED Fixture ≤ 10 W/ft Replacing or Instead of 1L or 2L T5, T8, or T12 in Cross Section - 12 Hours/Day"]
["L5447"," LED Fixture ≤ 10 W/ft Replacing or Instead of 1L or 2L T5, T8, or T12 in Cross Section - 24 Hours/Day"]
["L5449"," LED Fixture ≤ 24 W/ft Replacing or Instead of 3L or 4L T5, T8, or T12 in Cross Section - 12 Hours/Day"]
["L5450"," LED Fixture ≤ 24 W/ft Replacing or Instead of 3L or 4L T5, T8, or T12 in Cross Section - 24 Hours/Day"]
["N-L5446"," LED Fixture ≤ 10 W/ft Replacing or Instead of 1L or 2L T5, T8, or T12 in Cross Section - 12 Hours/Day"]
["N-L5447"," LED Fixture ≤ 10 W/ft Replacing or Instead of 1L or 2L T5, T8, or T12 in Cross Section - 24 Hours/Day"]
["N-L5449"," LED Fixture ≤ 24 W/ft Replacing or Instead of 3L or 4L T5, T8, or T12 in Cross Section - 12 Hours/Day"]
["N-L5450"," LED Fixture ≤ 24 W/ft Replacing or Instead of 3L or 4L T5, T8, or T12 in Cross Section - 24 Hours/Day"]
["L4316"," 4' 2-lamp TLED <24W replacing 8' 1-lamp T8 or T12, 24 Hour, Exterior"]
["L4315"," 4' 2-lamp TLED <24W replacing 8' 1-lamp T8 or T12, Dusk to Dawn, Exterior"]
["L4319"," 4' 2-lamp TLED <24W replacing 8' 1-lamp T8HO or T12HO, 24 Hour, Exterior"]
["L4318"," 4' 2-lamp TLED <24W replacing 8' 1-lamp T8HO or T12HO, Dusk to Dawn, Exterior"]
["L4322"," 4’ 4-lamp TLED <24W replacing 8' 2-lamp T8 or T12, 24 Hour, Exterior"]
["L4321"," 4’ 4-lamp TLED <24W replacing 8' 2-lamp T8 or T12, Dusk to Dawn, Exterior"]
["L4325"," 4' 4-lamp TLED <24W replacing 8' 2-lamp T8HO or T12HO, 24 Hour, Exterior"]
["L4324"," 4' 4-lamp TLED <24W replacing 8' 2-lamp T8HO or T12HO, Dusk to Dawn, Exterior"]
["L4328"," 4' 2-lamp TLED <24W replacing 8' 2-lamp T8 or T12, 24 Hour, Exterior"]
["L4327"," 4' 2-lamp TLED <24W replacing 8' 2-lamp T8 or T12, Dusk to Dawn, Exterior"]
["L4331"," 4' 2-lamp TLED <24W replacing 8' 2-lamp T8HO or T12HO, 24 Hour, Exterior"]
["L4330"," 4' 2-lamp TLED <24W replacing 8' 2-lamp T8HO or T12HO, Dusk to Dawn, Exterior"]
["L3963"," Mogul Screw-in Base (E39) replacing existing E39 base lamp, Exterior"]
["L5455"," 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, 24 hour, Exterior"]
["L5456"," 4' or U-Bend TLED ≤24W, replacing 4' or U-Bend T5, T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["L5457"," 8' TLED, replacing 8' T8 or T12 Lamp, 24 Hour, Exterior"]
["L5458"," 8' TLED, replacing 8' T8 or T12 Lamp, Dusk to Dawn, Exterior"]
["AG5024"," Horticultural Lighting, Non-stacked Indoor, <700W LED, replacing 1000W HID, Agriculture"]
["AG5025"," Horticultural Lighting, Non-stacked Indoor, <400W LED, replacing 600W HID, Agriculture"]
["AG5026"," Horticultural Lighting, Supplemented Greenhouse, <700W LED, replacing 1000W HID, Agriculture"]
["AG5027"," Horticultural Lighting, Supplemented Greenhouse, <400W LED, replacing 600W HID, Agriculture"]
["AG5028"," Horticultural Lighting, Supplemented Greenhouse, <250W LED, replacing 400W HID, Agriculture"]
["AG5032"," Horticultural Lighting, Non-stacked Indoor, Grow Light System, Agriculture"]
["AG5033"," Horticultural Lighting, Supplemented Greenhouse, Grow Light System, Agriculture"]

{"sheet":"Wattage Guide","index":12,"n_rows":304,"n_cols":9,"rows_kept":304,"hidden":true,"merged":[[3,1,3,3],[3,6,3,8]]}
["Focus on Energy AgSG Lighting Tool"]
["Directions: Use the filters to narrow your search for default lighting input wattage consumptions."]
[]
[null,"Existing Lighting",{"$nulls":4},"Proposed Lighting"]
[null,"Type","Lighting Detail","Existing Wattage",null,null,"Type","Lighting Detail","Proposed Wattage"]
[null,null,"CFL Lamps (Screw in and Pin base)",{"$nulls":4},"CFL Lamps (screw and pin based)"]
[null,"CFL","CFL, screw in ≤ 32 watts","Manual Entry",null,null,"CFL","CFL, screw in ≤ 32 watts","Manual Entry"]
[null,"CFL","Cold Cathode CFL, screw in ≤ 32 watts","Manual Entry",null,null,"CFL","CFL Reflector Flood, screw in ≤ 32 watts","Manual Entry"]
[null,"CFL","CFL Reflector Flood, screw in ≤ 32 watts","Manual Entry",null,null,"CFL","CFL, screw in, 33 to 115 watts","Manual Entry"]
[null,"CFL","CFL, screw in, 33 to 115 watts","Manual Entry",null,null,"CFL","Hard-wired CFL, pin-based CFL Lamps","Manual Entry"]
[null,"CFL","Hard-wired CFL, pin-based CFL Lamps","Manual Entry",null,null,"CFL","14 watt Pin Based CFL",{"v":18,"d":"18.0"}]
[null,"CFL","14 watt Pin Based CFL",18,null,null,"CFL","15 watt Pin Based CFL",{"v":20,"d":"20.0"}]
[null,"CFL","15 watt Pin Based CFL",20,null,null,"CFL","16 watt Pin Based CFL",{"v":22,"d":"22.0"}]
[null,"CFL","16 watt Pin Based CFL",22,null,null,"CFL","21 watt Pin Based CFL",{"v":24,"d":"24.0"}]
[null,"CFL","18 watt Pin Based CFL",23,null,null,"CFL","23 watt Pin Based CFL",{"v":27,"d":"27.0"}]
[null,"CFL","21 watt Pin Based CFL",24,null,null,"CFL","27 watt Pin Based CFL",{"v":29,"d":"29.0"}]
[null,"CFL","23 watt Pin Based CFL",27,null,null,"CFL","28 watt Pin Based CFL",{"v":33,"d":"33.0"}]
[null,"CFL","26 watt Pin Based CFL",31,null,null,"CFL","33 watt Pin Based CFL",{"v":35,"d":"35.0"}]
[null,"CFL","27 watt Pin Based CFL",29,null,null,"CFL","38 watt Pin Based CFL",{"v":40,"d":"40.0"}]
[null,"CFL","28 watt Pin Based CFL",33,{"$nulls":3},"Fluorescent 2x4 Troffer Fixtures"]
[null,"CFL","32 watt Pin Based CFL",35,null,null,"Fluorescent 2x4","High Performance Troffer, 2 Lamp F28T5 2x4",{"v":63,"d":"63.0"}]
[null,"CFL","33 watt Pin Based CFL",35,null,null,"Fluorescent 2x4","High Performance Troffer, 2 Lamp HPT8 2x4",54.5]
[null,"CFL","38 watt Pin Based CFL",40,null,null,"Fluorescent 2x4","High Performance Troffer, 2 Lamp HPT8 2x4 (Low BF)",{"v":48,"d":"48.0"}]
[null,"CFL","42 watt Pin Based CFL",46,null,null,"Fluorescent 2x4","High Performance Troffer, 2 Lamp T8 25 watt 2x4",{"v":43,"d":"43.0"}]
[null,null,"Fluorescent Fixtures",{"$nulls":3},"Fluorescent 2x4","High Performance Troffer, 2 Lamp T8 25 watt 2x4 (Low BF)",{"v":38,"d":"38.0"}]
[null,"T12 2ft","2' 1 Lamp T12",22.8,null,null,"Fluorescent 2x4","High Performance Troffer, 2 Lamp T8 28 watt 2x4",{"v":48,"d":"48.0"}]
[null,"T12 2ft","2' 2 Lamp T12",51.7,null,null,"Fluorescent 2x4","High Performance Troffer, 2 Lamp T8 28 watt 2x4 (Low BF)",{"v":43,"d":"43.0"}]
[null,"T12 2ft","2' 3 Lamp T12",67.5,{"$nulls":3},"Fluorescent Fixtures"]
[null,"T12 2ft","2' 4 Lamp T12",95.5,null,null,"T5 2ft","2', 6 Lamp T5 HO ",{"v":160,"d":"160.0"}]
[null,"T12 2ft","2' 6 Lamp T12",{"v":146,"d":"146.0"},null,null,"T5 2ft","2', 4 Lamp T5 HO ",104.5]
[null,"T12 2ft","2' 1 Lamp T12 HO (35w)",{"v":63,"d":"63.0"},null,null,"T5 2ft","2', 3 Lamp T5 HO ",79.5]
[null,"T12 2ft","2' 2 Lamp T12 HO (35w)",92.4,null,null,"T5 2ft","2', 2 Lamp T5 HO ",53.2]
[null,"T12 2ft","2' 1 Lamp T12 HO (50w)",{"v":71,"d":"71.0"},null,null,"T5 2ft","2', 1 Lamp T5 HO",{"v":27,"d":"27.0"}]
[null,"T12 2ft","2' 2 Lamp T12 HO (50w)",{"v":112,"d":"112.0"},null,null,"T5 4ft","(two fixtures) 4', 6 Lamp T5 HO High Bay",{"v":710,"d":"710.0"}]
[null,"T12 3ft","3' 1 Lamp T12",{"v":38.56666666666667,"d":"38.6"},null,null,"T5 4ft","4', 10 Lamp F54 T5HO High Bay",{"v":585,"d":"585.0"}]
[null,"T12 3ft","3' 2 Lamp T12",{"v":70,"d":"70.0"},null,null,"T5 4ft","4', 8 Lamp T5HO High Bay",{"v":585,"d":"585.0"}]
[null,"T12 3ft","3' 3 Lamp T12",{"v":110,"d":"110.0"},null,null,"T5 4ft","(two fixtures) 4', 4 Lamp T5 HO High Bay",{"v":468,"d":"468.0"}]
[null,"T12 3ft","3' 4 Lamp T12",{"v":144,"d":"144.0"},null,null,"T5 4ft","(two fixtures) 4' 6 Lamp T8 High Bay",{"v":448,"d":"448.0"}]
[null,"T12 3ft","3' 6 Lamp T12",{"v":225,"d":"225.0"},null,null,"T5 4ft","4', 10 Lamp T8, High Bay",{"v":370,"d":"370.0"}]
[null,"T12 4ft","4' 1 Lamp T12 (34w)",{"v":38.666666666666664,"d":"38.7"},null,null,"T5 4ft","4', 6 Lamp T5 HO High Bay",354.5]
[null,"T12 4ft","4' 2 Lamp T12 (34w)",{"v":66.33333333333333,"d":"66.3"},null,null,"T5 4ft","4', 4 Lamp T5 HO High Bay",{"v":234,"d":"234.0"}]
[null,"T12 4ft","4' 3 Lamp T12 (34w)",{"v":103.33333333333333,"d":"103.3"},null,null,"T5 4ft","4' 4 Lamp T5 HO",{"v":234,"d":"234.0"}]
[null,"T12 4ft","4' 4 Lamp T12 (34w)",{"v":135.66666666666666,"d":"135.7"},null,null,"T5 4ft","4', 3 Lamp T5 HO High Bay",{"v":179,"d":"179.0"}]
[null,"T12 4ft","4' 1 Lamp T12 (40w)",39.3,null,null,"T5 4ft","4' 3 Lamp T5 HO",{"v":179,"d":"179.0"}]
[null,"T12 4ft","4' 2 Lamp T12 (40w)",{"v":78.75,"d":"78.8"},null,null,"T5 4ft","4', 4 Lamp F28 T5",{"v":126,"d":"126.0"}]
[null,"T12 4ft","4' 3 Lamp T12 (40w)",{"v":124,"d":"124.0"},null,null,"T5 4ft","4', 4 Lamp F28 T5 ",{"v":126,"d":"126.0"}]
[null,"T12 4ft","4' 4 Lamp T12 (40w)",{"v":153,"d":"153.0"},null,null,"T5 4ft","4', 2 Lamp T5 HO High Bay",{"v":117,"d":"117.0"}]
[null,"T12 4ft","4' 1 Lamp T12 HO",76.3,null,null,"T5 4ft","4' 2 Lamp T5 HO",{"v":117,"d":"117.0"}]
[null,"T12 4ft","4' 2 Lamp T12 HO",{"v":134.26666666666668,"d":"134.3"},null,null,"T5 4ft","4', 3 Lamp F28 T5",95.5]
[null,"T12 4ft","4' 3 Lamp T12 HO",216.8,null,null,"T5 4ft","4', 3 Lamp F28 T5 ",95.5]
[null,"T12 4ft","4' 4 Lamp T12 HO",276.3,null,null,"T5 4ft","4', 2 Lamp F28 T5",{"v":63,"d":"63.0"}]
[null,"T12 4ft","4' 1 Lamp T12 VHO",{"v":140,"d":"140.0"},null,null,"T5 4ft","4', 2 Lamp F28 T5 ",{"v":63,"d":"63.0"}]
[null,"T12 4ft","4' 2 Lamp T12 VHO",{"v":252,"d":"252.0"},null,null,"T5 4ft","4', 1 Lamp F54 T5HO",{"v":62,"d":"62.0"}]
[null,"T12 4ft","4' 3 Lamp T12 VHO",{"v":377,"d":"377.0"},null,null,"T5 4ft","4' 1 Lamp T5 HO",{"v":62,"d":"62.0"}]
[null,"T12 4ft","4' 4 Lamp T12 VHO",{"v":484,"d":"484.0"},null,null,"T5 4ft","4', 1 Lamp F28 T5",32.5]
[null,"T12 5ft","5' 1 Lamp T12",53.5,null,null,"T5 4ft","4', 1 Lamp F28 T5 ",32.5]
[null,"T12 5ft","5' 2 Lamp T12",{"v":108,"d":"108.0"},null,null,"T8 4ft","4', 8 Lamp T8, High Bay",{"v":291,"d":"291.0"}]
[null,"T12 6ft","6' 1 Lamp T12",{"v":73.03333333333333,"d":"73.0"},null,null,"T8 4ft","4' 6 Lamp T8 ",{"v":224,"d":"224.0"}]
[null,"T12 6ft","6' 2 Lamp T12",{"v":114.33333333333333,"d":"114.3"},null,null,"T8 4ft","4', 6 Lamp T8, High Bay",223.5]
[null,"T12 6ft","6' 3 Lamp T12",{"v":189,"d":"189.0"},null,null,"T8 4ft","4', 6 Lamp T8 (HP), High BF (Non-High Bay)",{"v":218,"d":"218.0"}]
[null,"T12 6ft","6' 4 Lamp T12",{"v":230,"d":"230.0"},null,null,"T8 4ft","4', 6 Lamp T8 (HP) Normal BF (Non-High Bay)",{"v":164,"d":"164.0"}]
[null,"T12 8ft","8' 1 Lamp T12",{"v":68.83333333333333,"d":"68.8"},null,null,"T8 4ft","4', 4 Lamp T8, High Bay",150.5]
[null,"T12 8ft","8' 2 Lamp T12",{"v":109.33333333333333,"d":"109.3"},null,null,"T8 4ft","4', 4 Lamp T8 (HP), High BF",{"v":145,"d":"145.0"}]
[null,"T12 8ft","8' 3 Lamp T12",{"v":179,"d":"179.0"},null,null,"T8 4ft","4', 4 Lamp T8 28 watt, (HP) High BF",{"v":131,"d":"131.0"}]
[null,"T12 8ft","8' 4 Lamp T12",{"v":233,"d":"233.0"},null,null,"T8 4ft","4', 4 Lamp T8 25 watt, (HP) High BF",{"v":122,"d":"122.0"}]
[null,"T12 8ft","8' 1 Lamp T12 HO",114.5,null,null,"T8 4ft","4' 4 Lamp T8",{"v":120.03333333333335,"d":"120.0"}]
[null,"T12 8ft","8' 2 Lamp T12 HO",189.6,null,null,"T8 4ft","4', 3 Lamp T8 (HP), High BF",{"v":109,"d":"109.0"}]
[null,"T12 8ft","8' 3 Lamp T12 HO",{"v":319,"d":"319.0"},null,null,"T8 4ft","4', 4 Lamp T8 (HP) Normal BF",107.5]
[null,"T12 8ft","8' 4 Lamp T12 HO",{"v":414,"d":"414.0"},null,null,"T8 4ft","4', 3 Lamp T8 28 watt, (HP) High BF",{"v":96,"d":"96.0"}]
[null,"T12 8ft","8' 1 Lamp T12 VHO",201.5,null,null,"T8 4ft","4', 4 Lamp T8 (HP) Low BF",{"v":95,"d":"95.0"}]
[null,"T12 8ft","8' 2 Lamp T12 VHO",{"v":389.15,"d":"389.2"},null,null,"T8 4ft","4', 4 Lamp T8 28 watt, (HP) Normal BF",{"v":94,"d":"94.0"}]
[null,"T12 8ft","8' 3 Lamp T12 VHO",567.5,null,null,"T8 4ft","4', 3 Lamp T8 25 watt, (HP) High BF",{"v":93,"d":"93.0"}]
[null,"T12 8ft","8' 4 Lamp T12 VHO",{"v":760,"d":"760.0"},null,null,"T8 4ft","4' 3 Lamp T8 ",{"v":90.96666666666665,"d":"91.0"}]
[null,"T12 U Bent","U Bent T12 1 Lamp",{"v":43,"d":"43.0"},null,null,"T8 4ft","4', 4 Lamp T8 25 watt, (HP) Normal BF",{"v":85,"d":"85.0"}]
[null,"T12 U Bent","U Bent T12 2 Lamp",{"v":72,"d":"72.0"},null,null,"T8 4ft","4', 4 Lamp T8 28 watt, (HP) Low BF",{"v":83,"d":"83.0"}]
[null,"T12 U Bent","U Bent T12 3 Lamp",{"v":115,"d":"115.0"},null,null,"T8 4ft","4', 3 Lamp T8 (HP) Normal BF",{"v":81.55,"d":"81.6"}]
[null,"T5 2ft","2' 1 Lamp T5",{"v":16,"d":"16.0"},null,null,"T8 4ft","4', 4 Lamp T8 25 watt, (HP) Low BF",{"v":75,"d":"75.0"}]
[null,"T5 2ft","2' 2 Lamp T5",30.5,null,null,"T8 4ft","4', 2 Lamp T8 (HP), High BF",73.5]
[null,"T5 2ft","2' 3 Lamp T5",{"v":51,"d":"51.0"},null,null,"T8 4ft","4', 3 Lamp T8 28 watt, (HP) Normal BF",{"v":72,"d":"72.0"}]
[null,"T5 2ft","2' 4 Lamp T5",{"v":66,"d":"66.0"},null,null,"T8 4ft","4', 3 Lamp T8 (HP) Low BF",71.5]
[null,"T5 2ft","2', 1 Lamp T5 HO",{"v":27,"d":"27.0"},null,null,"T8 4ft","4', 2 Lamp T8 28 watt, (HP) High BF",{"v":65,"d":"65.0"}]
[null,"T5 2ft","2', 2 Lamp T5 HO",53.2,null,null,"T8 4ft","4', 3 Lamp T8 25 watt, (HP) Normal BF",{"v":64,"d":"64.0"}]
[null,"T5 2ft","2', 3 Lamp T5 HO",79.5,null,null,"T8 4ft","4', 3 Lamp T8 28 watt, (HP) Low BF",{"v":63,"d":"63.0"}]
[null,"T5 2ft","2', 4 Lamp T5 HO",104.5,null,null,"T8 4ft","4' 2 Lamp T8 ",61.4]
[null,"T5 2ft","2', 6 Lamp T5 HO",{"v":160,"d":"160.0"},null,null,"T8 4ft","4', 2 Lamp T8 25 watt, (HP) High BF",{"v":60,"d":"60.0"}]
[null,"T5 3ft","3' 1 Lamp T5",25.1,null,null,"T8 4ft","4', 3 Lamp T8 25 watt, (HP) Low BF",{"v":57,"d":"57.0"}]
[null,"T5 3ft","3' 2 Lamp T5",{"v":48.45,"d":"48.5"},null,null,"T8 4ft","4', 2 Lamp T8 (HP) Normal BF",54.5]
[null,"T5 3ft","3' 3 Lamp T5",{"v":73,"d":"73.0"},null,null,"T8 4ft","4', 2 Lamp T8 (HP) Low BF",{"v":48,"d":"48.0"}]
[null,"T5 3ft","3' 4 Lamp T5",{"v":96,"d":"96.0"},null,null,"T8 4ft","4', 2 Lamp T8 28 watt, (HP) Normal BF",{"v":48,"d":"48.0"}]
[null,"T5 3ft","3' 1 Lamp T5 HO",43.2,null,null,"T8 4ft","4', 2 Lamp T8 25 watt, (HP) Normal BF",{"v":43,"d":"43.0"}]
[null,"T5 3ft","3' 2 Lamp T5 HO",85.5,null,null,"T8 4ft","4', 2 Lamp T8 28 watt, (HP) Low BF",{"v":43,"d":"43.0"}]
[null,"T5 3ft","3' 3 Lamp T5 HO",{"v":130,"d":"130.0"},null,null,"T8 4ft","4', 2 Lamp T8 25 watt, (HP) Low BF",{"v":38,"d":"38.0"}]
[null,"T5 3ft","3' 4 Lamp T5 HO",{"v":172,"d":"172.0"},null,null,"T8 4ft","4', 1 Lamp T8 (HP) High BF",{"v":37,"d":"37.0"}]
[null,"T5 4ft","4' 1 Lamp T5 (28w)",32.5,null,null,"T8 4ft","4', 1 Lamp T8 28 watt, (HP) High BF",{"v":33,"d":"33.0"}]
[null,"T5 4ft","4' 2 Lamp T5 (28w)",{"v":63,"d":"63.0"},null,null,"T8 4ft","4' 1 Lamp T8 ",{"v":32.699999999999996,"d":"32.7"}]
[null,"T5 4ft","4' 3 Lamp T5 (28w)",95.5,null,null,"T8 4ft","4', 1 Lamp T8 25 watt, (HP) High BF",{"v":31,"d":"31.0"}]
[null,"T5 4ft","4' 4 Lamp T5 (28w)",{"v":126,"d":"126.0"},null,null,"T8 4ft","4', 1 Lamp T8 (HP) Normal BF",{"v":28,"d":"28.0"}]
[null,"T5 4ft","4' 1 Lamp T5 HO",{"v":62,"d":"62.0"},null,null,"T8 4ft","4', 1 Lamp T8 (HP) Low BF",26.5]
[null,"T5 4ft","4' 2 Lamp T5 HO",{"v":117,"d":"117.0"},null,null,"T8 4ft","4', 1 Lamp T8 28 watt, (HP) Normal BF",{"v":25,"d":"25.0"}]
[null,"T5 4ft","4' 3 Lamp T5 HO",{"v":179,"d":"179.0"},null,null,"T8 4ft","4', 1 Lamp T8 25 watt, (HP) Normal BF",22.5]
[null,"T5 4ft","4', 4 Lamp T5 HO High Bay",{"v":234,"d":"234.0"},null,null,"T8 4ft","4', 1 Lamp T8 28 watt, (HP) Low BF",{"v":22,"d":"22.0"}]
[null,"T5 4ft","4' 6 Lamp T5 HO (54w) High Bay",354.5,null,null,"T8 4ft","4', 1 Lamp T8 25 watt, (HP) Low BF",20.5]
[null,"T5 4ft","4' 8 Lamp T5 HO (54w) High Bay",{"v":585,"d":"585.0"},null,null,"T8 8ft","8', 4 Lamp T8 (54W)",{"v":201,"d":"201.0"}]
[null,"T8 2ft","2' 1 Lamp T8",20.2,null,null,"T8 8ft","8', 3 Lamp T8 (54W)",{"v":160,"d":"160.0"}]
[null,"T8 2ft","2' 2 Lamp T8",{"v":36.333333333333336,"d":"36.3"},null,null,"T8 8ft","8', 2 Lamp T8 (54W)",{"v":100,"d":"100.0"}]
[null,"T8 2ft","2' 3 Lamp T8",{"v":52,"d":"52.0"},null,null,"T8 8ft","8', 1 Lamp T8 (54W)",{"v":60,"d":"60.0"}]
[null,"T8 2ft","2' 4 Lamp T8",{"v":66.33333333333333,"d":"66.3"},{"$nulls":3},"Fluorescent Replacement Lamps"]
[null,"T8 3ft","3' 1 Lamp T8",{"v":26.733333333333334,"d":"26.7"},null,null,"T5 4ft Lamp Only","4' T5, 26 watt Lamp Only",{"v":26,"d":"26.0"}]
[null,"T8 3ft","3' 2 Lamp T8",{"v":50.166666666666664,"d":"50.2"},null,null,"T5 4ft Lamp Only","4' T5HO, 51 watt Lamp Only",{"v":51,"d":"51.0"}]
[null,"T8 3ft","3' 3 Lamp T8",{"v":72.66666666666667,"d":"72.7"},null,null,"T5 4ft Lamp Only","4' T5HO, 49 watt Lamp Only",{"v":49,"d":"49.0"}]
[null,"T8 3ft","3' 4 Lamp T8",{"v":96.33333333333333,"d":"96.3"},null,null,"T5 4ft Lamp Only","4' T5HO, 47 watt Lamp Only",{"v":47,"d":"47.0"}]
[null,"T8 3ft","3' 6 Lamp T8",{"v":135,"d":"135.0"},null,null,"T5 4ft Lamp Only","4' T5HO, 44 watt Lamp Only",{"v":44,"d":"44.0"}]
[null,"T8 4ft","4' 1 Lamp T8 (25w)",{"v":25,"d":"25.0"},null,null,"T8 4ft Lamp Only","4' T8, 28 watt Lamp Only",{"v":25,"d":"25.0"}]
[null,"T8 4ft","4' 2 Lamp T8 (25w)",44.5,null,null,"T8 4ft Lamp Only","4' T8, 25 watt Lamp Only",{"v":22,"d":"22.0"}]
[null,"T8 4ft","4' 3 Lamp T8 (25w)",64.5,null,null,"T8 8ft Lamp Only","8' T8, 54 watt Lamp Only",{"v":48,"d":"48.0"}]
[null,"T8 4ft","4' 4 Lamp T8 (25w)",85.5,null,null,"T8 8ft Lamp Only","8' T8, 51 watt Lamp Only",{"v":45,"d":"45.0"}]
[null,"T8 4ft","4' 4 Lamp T8 (25w) High Bay",122.5,null,null,"T8 8ft Lamp Only","8' T8, 50 watt Lamp Only",{"v":44,"d":"44.0"}]
[null,"T8 4ft","4' 1 Lamp T8 (28w)",25.5,null,null,"T8 8ft Lamp Only","8' T8, 49 watt Lamp Only",{"v":43,"d":"43.0"}]
[null,"T8 4ft","4' 2 Lamp T8 (28w)",{"v":50,"d":"50.0"},{"$nulls":3},"HID (Metal Halide) Fixtures"]
[null,"T8 4ft","4' 3 Lamp T8 (28w)",{"v":74,"d":"74.0"},null,null,"PSMH","Pulse Start Metal Halide, 50 watts",{"v":67,"d":"67.0"}]
[null,"T8 4ft","4' 4 Lamp T8 (28w)",{"v":98,"d":"98.0"},null,null,"PSMH","Pulse Start Metal Halide, 70 watts",87.5]
[null,"T8 4ft","4' 4 Lamp T8 (28w) High Bay",129.5,null,null,"PSMH","Pulse Start Metal Halide, 100 watts",{"v":123,"d":"123.0"}]
[null,"T8 4ft","4' 6 Lamp T8 (28w) High Bay",{"v":194,"d":"194.0"},null,null,"PSMH","Pulse Start Metal Halide, 125 watts",145.5]
[null,"T8 4ft","4' 1 Lamp T8 (30w)",29.5,null,null,"PSMH","Pulse Start Metal Halide, 150 watts",{"v":181,"d":"181.0"}]
[null,"T8 4ft","4' 2 Lamp T8 (30w)",{"v":63.699999999999996,"d":"63.7"},null,null,"PSMH","Pulse Start Metal Halide, 175 watts",198.5]
[null,"T8 4ft","4' 3 Lamp T8 (30w)",{"v":79,"d":"79.0"},null,null,"PSMH","Pulse Start Metal Halide, 200 watts",{"v":225,"d":"225.0"}]
[null,"T8 4ft","4' 4 Lamp T8 (30w)",{"v":105,"d":"105.0"},null,null,"PSMH","Pulse Start Metal Halide, 250 watts",{"v":281,"d":"281.0"}]
[null,"T8 4ft","4' 1 Lamp T8",{"v":32.699999999999996,"d":"32.7"},null,null,"PSMH","Pulse Start Metal Halide, 320 watts",{"v":356,"d":"356.0"}]
[null,"T8 4ft","4' 2 Lamp T8",61.4,null,null,"PSMH","Pulse Start Metal Halide, 350 watts",392.5]
[null,"T8 4ft","4' 3 Lamp T8",{"v":90.96666666666665,"d":"91.0"},null,null,"PSMH","Pulse Start Metal Halide, 400 watts",{"v":445,"d":"445.0"}]
[null,"T8 4ft","4' 4 Lamp T8",{"v":120.03333333333335,"d":"120.0"},null,null,"PSMH","Pulse Start Metal Halide, 450 watts",{"v":493,"d":"493.0"}]
[null,"T8 4ft","4' 4 Lamp T8 High Bay",150.5,null,null,"PSMH","Pulse Start Metal Halide, 575 watts",{"v":640,"d":"640.0"}]
[null,"T8 4ft","4' 6 Lamp T8 High Bay",223.5,null,null,"PSMH","Pulse Start Metal Halide, 750 watts",{"v":812,"d":"812.0"}]
[null,"T8 4ft","4' 8 Lamp T8 High Bay",{"v":291,"d":"291.0"},null,null,"PSMH","Pulse Start Metal Halide, 775 watts",{"v":855,"d":"855.0"}]
[null,"T8 5ft","5' 1 Lamp T8",{"v":36,"d":"36.0"},null,null,"PSMH","Pulse Start Metal Halide, 875 watts",{"v":950,"d":"950.0"}]
[null,"T8 5ft","5' 2 Lamp T8",{"v":72,"d":"72.0"},null,null,"PSMH","Pulse Start Metal Halide, 1000 watts",{"v":1080,"d":"1080.0"}]
[null,"T8 5ft","5' 3 Lamp T8",{"v":106,"d":"106.0"},null,null,"PSMH","Electronic Pulse Start Metal Halide, 320 watts",{"v":344,"d":"344.0"}]
[null,"T8 5ft","5' 4 Lamp T8",{"v":134,"d":"134.0"},null,null,"PSMH","Electronic Pulse Start Metal Halide, 320 watts (Exterior)",{"v":344,"d":"344.0"}]
[null,"T8 8ft","8' 1 Lamp T8 (57W)",{"v":51,"d":"51.0"},null,null,"CMH","Ceramic Metal Halide, ≤ 25 watts","Manual Entry"]
[null,"T8 8ft","8' 1 Lamp T8 (57W)",{"v":100,"d":"100.0"},null,null,"CMH","Ceramic Metal Halide, 39 watts",{"v":46,"d":"46.0"}]
[null,"T8 8ft","8' 1 Lamp T8 (59W)",{"v":61,"d":"61.0"},null,null,"CMH","Ceramic Metal Halide, 50 watts",{"v":55,"d":"55.0"}]
[null,"T8 8ft","8' 2 Lamp T8 (59W)",106.5,null,null,"CMH","Ceramic Metal Halide, 60 watts",{"v":67,"d":"67.0"}]
[null,"T8 8ft","8' 3 Lamp T8 (59W)",{"v":167,"d":"167.0"},null,null,"CMH","Ceramic Metal Halide, 90 watts",{"v":99,"d":"99.0"}]
[null,"T8 8ft","8' 4 Lamp T8 (59W)",{"v":219,"d":"219.0"},null,null,"CMH","Ceramic Metal Halide, 100 watts",{"$f":"1.1*100","v":{"v":110.00000000000001,"d":"110.0"}}]
[null,"T8 U Bent","U Bent T8 1 Lamp",{"v":29,"d":"29.0"},null,null,"CMH","Ceramic Metal Halide, 140 watts",{"v":154,"d":"154.0"}]
[null,"T8 U Bent","U Bent T8 2 Lamp",{"v":55,"d":"55.0"},null,null,"CMH","Ceramic Metal Halide, 150 watts",{"v":185,"d":"185.0"}]
[null,"T8 U Bent","U Bent T8 3 Lamp",{"v":81,"d":"81.0"},null,null,"CMH","Ceramic Metal Halide, 210 watts",{"v":229,"d":"229.0"}]
[null,null,"Fluorescent Lamps",{"$nulls":3},"CMH","Ceramic Metal Halide, 220 watts",{"v":242,"d":"242.0"}]
[null,"Fluorescent Lamps","4' T5, 28 watt Lamp Only",{"v":28,"d":"28.0"},null,null,"CMH","Ceramic Metal Halide, 270 watts",{"v":290,"d":"290.0"}]
[null,"Fluorescent Lamps","4' T5HO, 54 watt Lamp Only",{"v":54,"d":"54.0"},null,null,"CMH","Ceramic Metal Halide, 315 watts",{"v":343,"d":"343.0"}]
[null,"Fluorescent Lamps","4' T8, 32 watt Lamp Only",{"v":28,"d":"28.0"},null,null,"CMH","Ceramic Metal Halide, 575 watts",{"v":640,"d":"640.0"}]
[null,"Fluorescent Lamps","8' T8, 59 watt Lamp Only",{"v":52,"d":"52.0"},{"$nulls":3},"HID Replacement Lamps"]
[null,"Fluorescent Lamps","4' T12, Lamp Only",{"v":34,"d":"34.0"},null,null,"HID Lamps","145W HID RW Direct Replacement Lamp",{"v":174,"d":"174.0"}]
[null,null,"Fluorescent Linear Ambient Fixtures",{"$nulls":3},"HID Lamps","150W HID RW Direct Replacement Lamp",{"v":180,"d":"180.0"}]
[null,"Linear Ambient Fluorescent","T5 Linear Ambient Fixt, per ft, 1 Lamp Cross Section",{"$f":"32.5/4","v":{"v":8.125,"d":"8.1"}},null,null,"HID Lamps","205W HID RW Direct Replacement Lamp",{"v":235,"d":"235.0"}]
[null,"Linear Ambient Fluorescent","T5 Linear Ambient Fixt, per ft, 2 Lamp Cross Section",{"$f":"63/4","v":{"v":15.75,"d":"15.8"}},null,null,"HID Lamps","220W HID RW Direct Replacement Lamp ",{"v":242,"d":"242.0"}]
[null,"Linear Ambient Fluorescent","T5 Linear Ambient Fixt, per ft, 3 Lamp Cross Section",{"$f":"95.5/4","v":{"v":23.875,"d":"23.9"}},null,null,"HID Lamps","260W HID RW Direct Replacement Lamp ",{"v":299,"d":"299.0"}]
[null,"Linear Ambient Fluorescent","T5 Linear Ambient Fixt, per ft, 4 Lamp Cross Section",{"$f":"126/4","v":31.5},null,null,"HID Lamps","330W HID RW Direct Replacement Lamp",{"v":380,"d":"380.0"}]
[null,"Linear Ambient Fluorescent","T8 Linear Ambient Fixt, per ft, 1 Lamp Cross Section",{"$f":"32.7/4","v":{"v":8.175,"d":"8.2"}},null,null,"HID Lamps","360W HID RW Direct Replacement Lamp ",{"v":414,"d":"414.0"}]
[null,"Linear Ambient Fluorescent","T8 Linear Ambient Fixt, per ft, 2 Lamp Cross Section",{"$f":"61.4/4","v":{"v":15.35,"d":"15.4"}},null,null,"HID Lamps","830W HID RW Direct Replacement Lamp",{"v":896,"d":"896.0"}]
[null,"Linear Ambient Fluorescent","T8 Linear Ambient Fixt, per ft, 3 Lamp Cross Section",{"$f":"90.9666666666667/4","v":{"v":22.741666666666674,"d":"22.7"}},null,null,"HID Lamps","860W HID RW Direct Replacement Lamp",{"v":928,"d":"928.0"}]
[null,"Linear Ambient Fluorescent","T8 Linear Ambient Fixt, per ft, 4 Lamp Cross Section",{"$f":"120.033333333333/4","v":{"v":30.00833333333325,"d":"30.0"}},{"$nulls":3},"Induction Fixtures"]
[null,"Linear Ambient Fluorescent","HPT8 Linear Ambient Fixt, per ft, 1 Lamp Cross Section",{"$f":"28/4","v":{"v":7,"d":"7.0"}},null,null,"Induction","Induction, 35 watts",{"v":39,"d":"39.0"}]
[null,"Linear Ambient Fluorescent","HPT8 Linear Ambient Fixt, per ft, 2 Lamp Cross Section",{"$f":"54.5/4","v":{"v":13.625,"d":"13.6"}},null,null,"Induction","Induction, 55 watts",{"v":58,"d":"58.0"}]
[null,"Linear Ambient Fluorescent","HPT8 Linear Ambient Fixt, per ft, 3 Lamp Cross Section",{"$f":"81.55/4","v":{"v":20.3875,"d":"20.4"}},null,null,"Induction","Induction, 70 watts",{"v":77,"d":"77.0"}]
[null,"Linear Ambient Fluorescent","HPT8 Linear Ambient Fixt, per ft, 4 Lamp Cross Section",{"$f":"107.5/4","v":{"v":26.875,"d":"26.9"}},null,null,"Induction","Induction, 85 watts",89.5]
[null,"Linear Ambient Fluorescent","RWT8 (28W) Linear Ambient Fixt, per ft, 1 Lamp Cross Section",{"$f":"25.5/4","v":{"v":6.375,"d":"6.4"}},null,null,"Induction","Induction, 100 watts",106.5]
[null,"Linear Ambient Fluorescent","RWT8 (28W) Linear Ambient Fixt, per ft, 2 Lamp Cross Section",{"$f":"50/4","v":12.5},null,null,"Induction","Induction, 120 watts",{"v":132,"d":"132.0"}]
[null,"Linear Ambient Fluorescent","RWT8 (28W) Linear Ambient Fixt, per ft, 3 Lamp Cross Section",{"$f":"74/4","v":18.5},null,null,"Induction","Induction, 125 watts",137.5]
[null,"Linear Ambient Fluorescent","RWT8 (28W) Linear Ambient Fixt, per ft, 4 Lamp Cross Section",{"$f":"98/4","v":24.5},null,null,"Induction","Induction, 150 watts",160.5]
[null,"Linear Ambient Fluorescent","RWT8 (25W) Linear Ambient Fixt, per ft, 1 Lamp Cross Section",{"$f":"25/4","v":{"v":6.25,"d":"6.3"}},null,null,"Induction","Induction, 165 watts",173.5]
[null,"Linear Ambient Fluorescent","RWT8 (25W) Linear Ambient Fixt, per ft, 2 Lamp Cross Section",{"$f":"44.5/4","v":{"v":11.125,"d":"11.1"}},null,null,"Induction","Induction, 200 watts",{"v":220,"d":"220.0"}]
[null,"Linear Ambient Fluorescent","RWT8 (25W) Linear Ambient Fixt, per ft, 3 Lamp Cross Section",{"$f":"64.5/4","v":{"v":16.125,"d":"16.1"}},null,null,"Induction","Induction, 225 watts",{"v":248,"d":"248.0"}]
[null,"Linear Ambient Fluorescent","RWT8 (25W) Linear Ambient Fixt, per ft, 4 Lamp Cross Section",{"$f":"85.5/4","v":{"v":21.375,"d":"21.4"}},null,null,"Induction","Induction, 250 watts",{"v":275,"d":"275.0"}]
[null,"Linear Ambient Fluorescent","T12 Linear Ambient Fixt, per ft, 1 Lamp Cross Section",{"$f":"38.6666666666667/4","v":{"v":9.666666666666675,"d":"9.7"}},null,null,"Induction","Induction, 300 watts",{"v":330,"d":"330.0"}]
[null,"Linear Ambient Fluorescent","T12 Linear Ambient Fixt, per ft, 2 Lamp Cross Section",{"$f":"66.3333333333333/4","v":{"v":16.583333333333325,"d":"16.6"}},null,null,"Induction","Induction, 750 watts",{"v":825,"d":"825.0"}]
[null,"Linear Ambient Fluorescent","T12 Linear Ambient Fixt, per ft, 3 Lamp Cross Section",{"$f":"103.333333333333/4","v":{"v":25.83333333333325,"d":"25.8"}},{"$nulls":3},"LED Fixtures"]
[null,"Linear Ambient Fluorescent","T12 Linear Ambient Fixt, per ft, 4 Lamp Cross Section",{"$f":"135.666666666667/4","v":{"v":33.91666666666675,"d":"33.9"}},null,null,"LED","LED Stairwell & Passageway Fixture w/occ sensor (DLC listed)","Manual Entry"]
[null,null,"HID Fixtures",{"$nulls":3},"LED","Linear Fluorescent Stairwell & Passageway Fixture w/occ sensor","Manual Entry"]
[null,"Mercury Vapor","Mercury Vapor, 40 watts",{"v":50,"d":"50.0"},null,null,"LED","Interior LED Lamp, Replacing Incand. ≤40W (ENERGY STAR)","Manual Entry"]
[null,"Mercury Vapor","Mercury Vapor, 50 watts",74.5,null,null,"LED","Interior LED Lamp, Replacing Incand. >40W (ENERGY STAR)","Manual Entry"]
[null,"Mercury Vapor","Mercury Vapor, 75 watts",{"v":94,"d":"94.0"},null,null,"LED","Interior LED Lamp, Replacing CFL <23W (ENERGY STAR)","Manual Entry"]
[null,"Mercury Vapor","Mercury Vapor, 100 watts",123.5,null,null,"LED","Interior LED Lamp, Replacing CFL ≥23W (ENERGY STAR)","Manual Entry"]
[null,"Mercury Vapor","Mercury Vapor, 175 watts",{"v":205,"d":"205.0"},null,null,"LED","LED Downlight, ≤ 18W, replacing incandescent (ENERGY STAR Listed)","Manual Entry"]
[null,"Mercury Vapor","Mercury Vapor, 250 watts",287.5,null,null,"LED","LED Accent Light, ≤ 18W, replacing incand. (DLC or Estar Listed)","Manual Entry"]
[null,"Mercury Vapor","Mercury Vapor, 400 watts",454.5,null,null,"LED","LED Track/Monopoint, ≤ 18W, replacing incand. (DLC or Estar Listed)","Manual Entry"]
[null,"Mercury Vapor","Mercury Vapor, 1000 watts",1077.5,null,null,"LED","LED Pole Mounted Fixture (DLC listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 35 watts",44.5,null,null,"LED","LED Wall-pack Fixture (DLC listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 50 watts",{"v":65,"d":"65.0"},null,null,"LED","LED Parking Garage Fixture, 24 Hour (DLC listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 70 watts",90.5,null,null,"LED","LED Parking Garage Fixture, Dusk to Dawn (DLC listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 100 watts",{"v":133,"d":"133.0"},null,null,"LED","LED Flood Light (DLC listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 150 watts",{"v":188,"d":"188.0"},null,null,"LED","LED Canopy Fixture (DLC listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 200 watts",{"v":245,"d":"245.0"},null,null,"LED","LED Downlight, > 18W, replacing incandescent or HID (ENERGY STAR Listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 250 watts",{"v":295,"d":"295.0"},null,null,"LED","LED Accent Light, > 18W, replacing incand. or HID (DLC or Estar Listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 310 watts",{"v":365,"d":"365.0"},null,null,"LED","LED Track/Monopoint Fixture, > 18W, replacing incand. or HID (DLC or Estar Listed)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 360 watts",{"v":414,"d":"414.0"},null,null,"LED","LED High Performance 2x4 Troffer (DLC listed, ≤55W)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 400 watts",{"v":461,"d":"461.0"},null,null,"LED","LED High Performance 1x4 Troffer (DLC listed, ≤25W)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 600 watts",{"v":665,"d":"665.0"},null,null,"LED","LED High Performance 2x2 Troffer (DLC listed, ≤36W)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 750 watts",{"v":840,"d":"840.0"},null,null,"LED","LED High Performance 2x2 Troffer (DLC listed, ≤85W)","Manual Entry"]
[null,"High Pressure Sodium","High Pressure Sodium, 1000 watts",{"v":1100,"d":"1100.0"},null,null,"LED","LED High Bay Fixture, ≤ 155 watts (DLC listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 20/22 watts",{"v":25,"d":"25.0"},null,null,"LED","LED High Bay Fixture, ≤ 250 watts (DLC listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 32 watts",{"v":40,"d":"40.0"},null,null,"LED","LED High Bay Fixture, ≤ 365 watts (DLC listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 35/39 watts",{"v":52,"d":"52.0"},null,null,"LED","LED High Bay Fixture, ≤ 500 watts (DLC listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 50 watts",64.5,null,null,"LED","LED High Bay Fixture, ≤ 800 watts (DLC listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 70 watts",93.5,null,null,"LED","LED Exit Fixture or Retrofit Kit","Manual Entry"]
[null,"Metal Halide","Metal Halide, 100 watts",{"v":126,"d":"126.0"},null,null,"LED","LED Lamp (Energy Star)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 150 watts",178.5,null,null,"LED","LED High Bay ≤ 180 watts, replacing Linear Fluorescent High Bay","Manual Entry"]
[null,"Metal Halide","Metal Halide, 175 watts",209.5,null,null,"LED","Exterior LED Downlight  ≤ 18 watts (Estar Listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 200 watts",{"v":232,"d":"232.0"},null,null,"LED","Exterior LED Downlight  > 18 watts (Estar Listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 250 watts",{"v":293,"d":"293.0"},null,null,"LED","Exterior LED Downlight ≥ 4000 Lumens ≤ 100 watts (Estar Listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 400 watts",{"v":455,"d":"455.0"},null,null,"LED","Exterior LED Downlight ≥ 6000 Lumens (Estar Listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 1000 watts",1078.5,null,null,"LED","LED Downlight, Interior, ≤ 18W, replacing CFL (ENERGY STAR Listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 1500 watts",{"v":1609,"d":"1609.0"},null,null,"LED","LED Downlight, Interior, > 18W, replacing CFL (ENERGY STAR Listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 1650 watts",{"v":1765,"d":"1765.0"},null,null,"LED","LED Downlight, Interior, ≥ 4000 Lumens ≤ 100W, replacing HID (Estar Listed)","Manual Entry"]
[null,"Metal Halide","Metal Halide, 2000 watts",{"v":2140,"d":"2140.0"},null,null,"LED","LED Downlight, Interior, ≥ 6000 Lumens, replacing HID (Estar Listed)","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 50 watts",{"v":67,"d":"67.0"},null,null,"LED","Interior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp ","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 70 watts",87.5,null,null,"LED","Interior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp, Enter # of 1 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 100 watts",{"v":123,"d":"123.0"},null,null,"LED","Interior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp, Enter # of 2 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 125 watts",145.5,null,null,"LED","Interior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp, Enter # of 3 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 150 watts",{"v":181,"d":"181.0"},null,null,"LED","Interior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp, Enter # of 4 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 175 watts",198.5,null,null,"LED","Interior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp, Enter # of 6 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 200 watts",{"v":225,"d":"225.0"},null,null,"LED","Interior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp, Enter # of 8 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 250 watts",{"v":281,"d":"281.0"},null,null,"LED","Interior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp, Enter # of 10 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 320 watts",{"v":356,"d":"356.0"},null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T8 or T12 Lamp","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 350 watts",392.5,null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T8 or T12 Lamp ","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 400 watts",{"v":445,"d":"445.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T12 Lamp, Enter # of 1 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 450 watts",{"v":493,"d":"493.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T12 Lamp, Enter # of 2 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 750 watts",{"v":812,"d":"812.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T12 Lamp, Enter # of 3 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 775 watts",{"v":855,"d":"855.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T12 Lamp, Enter # of 4 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 875 watts",{"v":950,"d":"950.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T8 Lamp, Enter # of 1 Lamp Fixtures","Manual Entry"]
[null,"PSMH","Pulse Start Metal Halide, 1000 watts",{"v":1080,"d":"1080.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T8 Lamp, Enter # of 2 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  39 watts",{"v":46,"d":"46.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T8 Lamp, Enter # of 3 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  50 watts",{"v":55,"d":"55.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T8 Lamp, Enter # of 4 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  60 watts",{"v":67,"d":"67.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T8 Lamp, Enter # of 6 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  90 watts",{"v":99,"d":"99.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T8 Lamp, Enter # of 8 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  140 watts",{"v":154,"d":"154.0"},null,null,"LED","Interior 4' T8 LED Direct Wire, Replacing 4’ T8 Lamp, Enter # of 10 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  150 watts",{"v":185,"d":"185.0"},null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T12 Lamp, Enter # of 1 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  210 watts",{"v":229,"d":"229.0"},null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T12 Lamp, Enter # of 2 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  220 watts",{"v":242,"d":"242.0"},null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T12 Lamp, Enter # of 3 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  270 watts",{"v":290,"d":"290.0"},null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T12 Lamp, Enter # of 4 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  315 watts",{"v":343,"d":"343.0"},null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T8 Lamp, Enter # of 1 Lamp Fixtures","Manual Entry"]
[null,"CMH","Ceramic Metal Halide,  575 watts",{"v":640,"d":"640.0"},null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T8 Lamp, Enter # of 2 Lamp Fixtures","Manual Entry"]
[null,"Neon","Neon, 9mm (watts per linear foot)",14.7,null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T8 Lamp, Enter # of 3 Lamp Fixtures","Manual Entry"]
[null,"Neon","Neon, 10mm (watts per linear foot)",12.5,null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T8 Lamp, Enter # of 4 Lamp Fixtures","Manual Entry"]
[null,"Neon","Neon, 11mm (watts per linear foot)",10.1,null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T8 Lamp, Enter # of 6 Lamp Fixtures","Manual Entry"]
[null,"Neon","Neon, 12mm (watts per linear foot)",8.1,null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T8 Lamp, Enter # of 8 Lamp Fixtures","Manual Entry"]
[null,"Neon","Neon, 13mm (watts per linear foot)",7.4,null,null,"LED","Interior 4' T8 LED w/External Driver, Replacing 4’ T8 Lamp, Enter # of 10 Lamp Fixtures","Manual Entry"]
[null,"Neon","Neon, 14mm (watts per linear foot)",{"v":7,"d":"7.0"},null,null,"LED","Exterior 4' T8 LED w/External Driver, Replacing 4’ T8 or T12 Lamp","Manual Entry"]
[null,"Neon","Neon, 15mm (watts per linear foot)",6.8,null,null,"LED","Exterior 4' T8 LED Using Existing Ballast, Replacing 4’ T8 Lamp ","Manual Entry"]
[null,"Neon","Neon, 18mm (watts per linear foot)",5.8,null,null,"LED","Exterior 4' T8 LED Direct Wire, Replacing 4’ T8 or T12 Lamp","Manual Entry"]
[null,"Neon","Neon, 20mm (watts per linear foot)",4.8,null,null,"LED","LED Linear Ambient Fixt, per ft, Replace 1 or 2-lamp T8/T12 Lamp(s) in Cross Section","Manual Entry"]
[null,"Neon","Neon, 22mm (watts per linear foot)",{"v":4,"d":"4.0"},null,null,"LED","LED Linear Ambient Fixt, per ft, Replace 3 or 4-lamp T8/T12 Lamps in Cross Section","Manual Entry"]
[null,"Neon","Neon, 25mm (watts per linear foot)",3.2,null,null,"LED","LED Linear Ambient Fixt, per ft, Replace 1 or 2-lamp T5 Lamp(s) in Cross Section","Manual Entry"]
[null,null,"HID Lamps",{"$nulls":3},"LED","LED Linear Ambient Fixt, per ft, Replace 3 or 4-lamp T5 Lamp(s) in Cross Section","Manual Entry"]
[null,"HID Lamps Only","175W HID Lamp Only",210,null,null,"LED","Exterior LED Lamp, Replacing Incand. ≤40W (ENERGY STAR)","Manual Entry"]
[null,"HID Lamps Only","250W HID Lamp Only",293,null,null,"LED","Exterior LED Lamp, Replacing Incand. >40W (ENERGY STAR)","Manual Entry"]
[null,"HID Lamps Only","320W HID Lamp Only",356]
[null,"HID Lamps Only","400W HID Lamp Only",455]
[null,"HID Lamps Only","1000W HID Lamp Only",1079]
[null,null,"Incandescent Lamps"]
[null,"Incandescent","Incandescent, 25W",25]
[null,"Incandescent","Incandescent, 29W",29]
[null,"Incandescent","Incandescent, 35W",35]
[null,"Incandescent","Incandescent, 40W",40]
[null,"Incandescent","Incandescent, 43W",43]
[null,"Incandescent","Incandescent, 50W",50]
[null,"Incandescent","Incandescent, 53W",53]
[null,"Incandescent","Incandescent, 60W",60]
[null,"Incandescent","Incandescent, 65W",65]
[null,"Incandescent","Incandescent, 73W",73]
[null,"Incandescent","Incandescent, 75W",75]
[null,"Incandescent","Incandescent, 85W",85]
[null,"Incandescent","Incandescent, 90W",90]
[null,"Incandescent","Incandescent, 100W",100]
[null,null,"Induction Fixtures"]
[null,"Induction","Induction, 35 watts",{"v":39,"d":"39.0"}]
[null,"Induction","Induction, 55 watts",{"v":58,"d":"58.0"}]
[null,"Induction","Induction, 70 watts",{"v":77,"d":"77.0"}]
[null,"Induction","Induction, 85 watts",89.5]
[null,"Induction","Induction, 100 watts",106.5]
[null,"Induction","Induction, 120 watts",{"v":132,"d":"132.0"}]
[null,"Induction","Induction, 125 watts",137.5]
[null,"Induction","Induction, 150 watts",160.5]
[null,"Induction","Induction, 165 watts",173.5]
[null,"Induction","Induction, 200 watts",{"v":220,"d":"220.0"}]
[null,"Induction","Induction, 225 watts",{"v":248,"d":"248.0"}]
[null,"Induction","Induction, 250 watts",{"v":275,"d":"275.0"}]
[null,"Induction","Induction, 300 watts",{"v":330,"d":"330.0"}]
[null,"Induction","Induction, 750 watts",{"v":825,"d":"825.0"}]
[null,null,"Miscellaneous"]
[null,"Miscellaneous","1x FT/BX/PL-L 40 watt Lamps",36]
[null,"Miscellaneous","2x FT/BX/PL-L 40 watt Lamps",72]
[null,"Miscellaneous","3x FT/BX/PL-L 40 watt Lamps",102]
[null,"Miscellaneous","4x FT/BX/PL-L 40 watt Lamps",144]
[null,"Miscellaneous","1x FT/BX/PL-L 50 watt Lamps",54]
[null,"Miscellaneous","2x FT/BX/PL-L 50 watt Lamps",108]
[null,"Miscellaneous","3x FT/BX/PL-L 50 watt Lamps",162]
[null,"Miscellaneous","4x FT/BX/PL-L 50 watt Lamps",216]
[null,"Miscellaneous","1x FT/BX/PL-L 55 watt Lamps",62]
[null,"Miscellaneous","2x FT/BX/PL-L 55 watt Lamps",112]
[null,"Miscellaneous","3x FT/BX/PL-L 55 watt Lamps",168]
[null,"Miscellaneous","4x FT/BX/PL-L 55 watt Lamps",224]
[null,"Miscellaneous","Exit Sign - Incandescent or CFL","Manual Entry"]
[null,"Miscellaneous","Other","Manual Entry"]